# Static Call Graph for image .\Objects\Fls_Demo.axf

#<CALLGRAPH># ARM Linker, 6180002: Last Updated: Mon Jan 15 10:57:23 2024

### Maximum Stack Usage = 264 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ Fls_MainFunction ⇒ Fls_ProcessRequestedJobs ⇒ Fls_DoJobDataTransfer ⇒ Fls_ProcessJobDataTransfer ⇒ Fls_ExecuteJobRdBlankCheckComp ⇒ Fls_Lld_ReadFlash ⇒ Fls_Lld_ReadUserPartition ⇒ Fls_Lld_ValidFlash ⇒ Fls_Lld_ValidDFlash

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ACMP0_IRQHandler ⇒ ACMP0_IRQHandler
- DefaultISR ⇒ DefaultISR

  ### Function Pointers

  - ACMP0_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - ADC0_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - BusFault_Handler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - CAN0_Error_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - CAN0_ORed_0_15_MB_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - CAN0_ORed_16_31_MB_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - CAN0_ORed_32_47_MB_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - CAN0_ORed_48_63_MB_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - CAN0_ORed_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - CAN0_Wake_Up_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - CAN1_Error_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - CAN1_ORed_0_15_MB_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - CAN1_ORed_16_31_MB_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - CAN1_ORed_32_47_MB_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - CAN1_ORed_48_63_MB_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - CAN1_ORed_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - CAN1_Wake_Up_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - DMA0_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - DMA1_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - DMA2_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - DMA3_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - DMA_Error_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - EFM_Ecc_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - EFM_Error_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - EFM_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - EMU_DB_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - EMU_SB_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - GPIOA_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - GPIOB_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - GPIOC_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - GPIOD_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - GPIOE_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - HCU_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - HardFault_Handler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - I2C0_Master_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - I2C0_Slave_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - I2C1_Master_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - MPWM0_Ch0_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - MPWM0_Ch0_Ovf_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - MPWM0_Ch1_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - MPWM0_Ch1_Ovf_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - MPWM0_Ch2_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - MPWM0_Ch2_Ovf_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - MPWM0_Ch3_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - MPWM0_Ch3_Ovf_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - MPWM0_Ch4_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - MPWM0_Ch4_Ovf_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - MPWM0_Ch5_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - MPWM0_Ch5_Ovf_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - MPWM0_Ch6_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - MPWM0_Ch6_Ovf_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - MPWM0_Ch7_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - MPWM0_Ch7_Ovf_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - MemManage_Handler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - NMI_Handler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - PCU_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - PendSV_Handler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved10_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved11_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved12_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved13_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved14_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved15_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved16_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved17_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved18_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved19_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved20_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved21_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved22_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved23_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved24_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved25_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved26_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved27_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved28_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved29_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved30_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved31_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved32_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved33_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved34_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved35_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved36_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved37_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved38_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved39_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved40_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved41_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved42_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved43_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved44_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved45_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved46_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved47_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved48_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved49_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved50_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved51_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved52_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved53_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved54_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved55_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved56_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved57_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved58_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved59_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved5_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved60_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved61_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved62_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved63_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved64_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved65_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved66_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved67_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved68_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved69_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved6_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved70_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved71_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved72_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved73_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved74_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved75_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved76_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved77_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved78_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved79_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved7_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved80_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved81_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved82_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved83_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved84_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved8_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reserved9_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Reset_Handler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - SCU_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - SPI0_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - SPI1_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - SPI2_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - SVC_Handler from exceptions.o(.text.SVC_Handler) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - SysTick_Handler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - SystemInit from system_ytm32b1mc0.o(.mcal_text) referenced from ytm32b1mc0_startup_armc.o(.text)
  - TRNG_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - UART0_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - UART1_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - UART2_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - UsageFault_Handler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - Wdg_Mld_Isr from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from ytm32b1mc0_startup_armc.o(.text)
  - eTMR0_Ch0_Ch1_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - eTMR0_Ch2_Ch3_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - eTMR0_Ch4_Ch5_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - eTMR0_Ch6_Ch7_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - eTMR0_Fault_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - eTMR0_Ovf_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - eTMR1_Ch0_Ch1_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - eTMR1_Ch2_Ch3_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - eTMR1_Ch4_Ch5_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - eTMR1_Ch6_Ch7_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - eTMR1_Fault_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - eTMR1_Ovf_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - init_data_bss from startup.o(.mcal_text) referenced from ytm32b1mc0_startup_armc.o(.text)
  - lpTMR0_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - main from main.o(.text.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)
  - pTMR_Ch0_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - pTMR_Ch1_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - pTMR_Ch2_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)
  - pTMR_Ch3_IRQHandler from ytm32b1mc0_startup_armc.o(.text) referenced from ytm32b1mc0_startup_armc.o(RESET)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry4.o(.ARM.Collect$$$$00000003))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Fls_Init (Thumb, 180 bytes, Stack size 16 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Fls_Init ⇒ Fls_Lld_Init ⇒ Fls_Lld_SetProtectReg
  [Calls]
  - >> Fls_Lld_Init
  [Called By]
  - >> Board_Init

  Fls_Erase (Thumb, 172 bytes, Stack size 24 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 48
  - Call Chain = Fls_Erase ⇒ Fls_IsSectorEndAddrAligned ⇒ Fls_GetSectorIndexByAddr
  [Calls]
  - >> SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_02
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_02
  - >> Fls_GetSectorIndexByAddr
  - >> Fls_IsSectorEndAddrAligned
  - >> Fls_IsSectorStartAddrAligned
  [Called By]
  - >> main

  Fls_Write (Thumb, 198 bytes, Stack size 32 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 56
  - Call Chain = Fls_Write ⇒ Fls_IsSectorAddrPageAligned ⇒ Fls_GetSectorIndexByAddr
  [Calls]
  - >> SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_03
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_03
  - >> Fls_IsSectorAddrPageAligned
  - >> Fls_GetSectorIndexByAddr
  [Called By]
  - >> main

  Fls_Cancel (Thumb, 178 bytes, Stack size 8 bytes, fls.o(.mcal_text), UNUSED)
  [Calls]

  - >> Fls_Lld_Cancel
  - >> Fls_GetLldJobResult

  Fls_GetStatus (Thumb, 72 bytes, Stack size 4 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 4
  - Call Chain = Fls_GetStatus
  [Called By]
  - >> main

  Fls_GetJobResult (Thumb, 48 bytes, Stack size 4 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 4
  - Call Chain = Fls_GetJobResult
  [Called By]
  - >> main

  Fls_Read (Thumb, 192 bytes, Stack size 32 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 56
  - Call Chain = Fls_Read ⇒ Fls_IsAddrInRange ⇒ Fls_GetSectorIndexByAddr
  [Calls]
  - >> SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_06
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_06
  - >> Fls_IsAddrInRange
  - >> Fls_GetSectorIndexByAddr
  [Called By]
  - >> main

  Fls_MainFunction (Thumb, 136 bytes, Stack size 16 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 240
  - Call Chain = Fls_MainFunction ⇒ Fls_ProcessRequestedJobs ⇒ Fls_DoJobDataTransfer ⇒ Fls_ProcessJobDataTransfer ⇒ Fls_ExecuteJobRdBlankCheckComp ⇒ Fls_Lld_ReadFlash ⇒ Fls_Lld_ReadUserPartition ⇒ Fls_Lld_ValidFlash ⇒ Fls_Lld_ValidDFlash
  [Calls]
  - >> Fls_Lld_MainFunction
  - >> Fls_MainFunctionCheckJobResult
  - >> Fls_ProcessRequestedJobs
  - >> Fls_ClrLldJobResult
  - >> Fls_GetLldJobResult
  [Called By]
  - >> main

  Fls_Compare (Thumb, 190 bytes, Stack size 32 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 56
  - Call Chain = Fls_Compare ⇒ Fls_IsAddrInRange ⇒ Fls_GetSectorIndexByAddr
  [Calls]
  - >> SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_04
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_04
  - >> Fls_IsAddrInRange
  - >> Fls_GetSectorIndexByAddr
  [Called By]
  - >> main

  Fls_BlankCheck (Thumb, 174 bytes, Stack size 24 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 48
  - Call Chain = Fls_BlankCheck ⇒ Fls_IsAddrInRange ⇒ Fls_GetSectorIndexByAddr
  [Calls]
  - >> SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_05
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_05
  - >> Fls_IsAddrInRange
  - >> Fls_GetSectorIndexByAddr
  [Called By]
  - >> main

  Fls_Lld_GetOneBitEccErrFlag (Thumb, 8 bytes, Stack size 8 bytes, fls_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Fls_Lld_GetRecoverr

  Fls_Lld_GetTwoBitEccErrFlag (Thumb, 8 bytes, Stack size 8 bytes, fls_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Fls_Lld_GetUnrecoverr

  Fls_Lld_ClearOneBitEccErrFlag (Thumb, 8 bytes, Stack size 8 bytes, fls_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Fls_Lld_ClearRecoverr

  Fls_Lld_ClearTwoBitEccErrFlag (Thumb, 8 bytes, Stack size 8 bytes, fls_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Fls_Lld_ClearUnrecoverr

  Fls_Lld_GetEccErrAddr (Thumb, 8 bytes, Stack size 8 bytes, fls_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Fls_Lld_GetEccErrorAddrReg

  Fls_Lld_Init (Thumb, 142 bytes, Stack size 16 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Fls_Lld_Init ⇒ Fls_Lld_SetProtectReg
  [Calls]
  - >> Fls_Lld_SetProtectReg
  - >> Fls_Lld_ClearRegSTS
  - >> Fls_Lld_CheckIdle
  [Called By]
  - >> Fls_Init

  Fls_Lld_SectorErase (Thumb, 342 bytes, Stack size 16 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 44
  - Call Chain = Fls_Lld_SectorErase ⇒ Fls_Lld_LoadCommandSync ⇒ Fls_Lld_CheckErrorFlag
  [Calls]
  - >> SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_00
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_00
  - >> Fls_Lld_LoadCommandSync (via Veneer)
  - >> Fls_Lld_LoadCommand
  - >> Fls_Lld_UnLockCMD
  - >> ARM_MPU_Enable
  - >> Fls_Lld_JudgeSetAddr
  - >> Fls_Lld_ClearWE
  - >> Fls_Lld_SetWE
  - >> ARM_MPU_Disable
  - >> Fls_Lld_EFMNopCommand
  - >> Fls_Lld_ValidFlash
  - >> Fls_Lld_ClearRegSTS
  - >> Fls_Lld_CheckIdle
  [Called By]
  - >> Fls_ExecuteJobErase

  Fls_Lld_ReadFlash (Thumb, 86 bytes, Stack size 24 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 104
  - Call Chain = Fls_Lld_ReadFlash ⇒ Fls_Lld_ReadUserPartition ⇒ Fls_Lld_ValidFlash ⇒ Fls_Lld_ValidDFlash
  [Calls]
  - >> Fls_Lld_LoadAESKey
  - >> Fls_Lld_ValidNVRFlash
  - >> Fls_Lld_ReadUserPartition
  - >> Fls_Lld_ValidFlash
  [Called By]
  - >> Fls_ExecuteJobRdBlankCheckComp

  Fls_Lld_CompareFlash (Thumb, 156 bytes, Stack size 24 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 92
  - Call Chain = Fls_Lld_CompareFlash ⇒ Fls_Lld_CompareCheck ⇒ Fls_Lld_ComputeReadSize
  [Calls]
  - >> Fls_Lld_BlankCheck
  - >> Fls_Lld_CompareCheck
  - >> Fls_Lld_ValidFlash
  [Called By]
  - >> Fls_ExecuteJobRdBlankCheckComp

  Fls_Lld_BlankCheck (Thumb, 232 bytes, Stack size 40 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 60
  - Call Chain = Fls_Lld_BlankCheck ⇒ Fls_Lld_ComputeReadSize
  [Calls]
  - >> Fls_Lld_ComputeReadSize
  [Called By]
  - >> Fls_Lld_CompareFlash

  Fls_Lld_MainFunction (Thumb, 560 bytes, Stack size 16 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 52
  - Call Chain = Fls_Lld_MainFunction ⇒ Fls_Lld_SectorWriteStatus ⇒ Fls_Lld_GetCtrlStatus ⇒ Fls_Lld_CheckErrorFlag
  [Calls]
  - >> Fls_Lld_SectorWriteStatus
  - >> Fls_Lld_SectorEraseStatus
  - >> Det_ReportTransientFault
  - >> Det_ReportRuntimeError
  [Called By]
  - >> Fls_MainFunction

  Fls_Lld_SectorWrite (Thumb, 384 bytes, Stack size 32 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 64
  - Call Chain = Fls_Lld_SectorWrite ⇒ Fls_Lld_WriteDataPage ⇒ Fls_Lld_JudgeSetAddr
  [Calls]
  - >> SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_01
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_01
  - >> Fls_Lld_WriteRstCheck
  - >> Fls_Lld_WriteDataPage
  - >> Fls_Lld_AddrCheckPreWrite
  - >> Fls_Lld_LoadCommandSync (via Veneer)
  - >> Fls_Lld_LoadCommand
  - >> Fls_Lld_UnLockCMD
  - >> Fls_Lld_EFMNopCommand
  - >> Fls_Lld_ValidFlash
  - >> Fls_Lld_CheckIdle
  [Called By]
  - >> Fls_ExecuteJobWrite

  Fls_Lld_Cancel (Thumb, 108 bytes, Stack size 24 bytes, fls_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Fls_Lld_CheckIdle
  [Called By]
  - >> Fls_Cancel

  Fls_Lld_GetPhycSectorSize (Thumb, 46 bytes, Stack size 16 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Fls_Lld_GetPhycSectorSize ⇒ Fls_Lld_ValidPFlash
  [Calls]
  - >> Fls_Lld_ValidPFlash
  [Called By]
  - >> Fls_ExecuteJobErase

  Fls_schm_read_msr (Thumb, 14 bytes, Stack size 4 bytes, schm_fls.o(.mcal_text))
  [Stack]

  - Max Depth = 4
  - Call Chain = Fls_schm_read_msr
  [Called By]
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_01
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_07
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_00
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_05
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_04
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_06
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_03
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_02

  SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_00 (Thumb, 64 bytes, Stack size 8 bytes, schm_fls.o(.mcal_text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_00 ⇒ Fls_schm_read_msr
  [Calls]
  - >> Fls_schm_read_msr
  [Called By]
  - >> Fls_Lld_SectorErase

  SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_00 (Thumb, 52 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_Lld_SectorErase

  SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_01 (Thumb, 64 bytes, Stack size 8 bytes, schm_fls.o(.mcal_text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_01 ⇒ Fls_schm_read_msr
  [Calls]
  - >> Fls_schm_read_msr
  [Called By]
  - >> Fls_Lld_SectorWrite

  SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_01 (Thumb, 52 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_Lld_SectorWrite

  SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_02 (Thumb, 64 bytes, Stack size 8 bytes, schm_fls.o(.mcal_text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_02 ⇒ Fls_schm_read_msr
  [Calls]
  - >> Fls_schm_read_msr
  [Called By]
  - >> Fls_Erase

  SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_02 (Thumb, 52 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_Erase

  SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_03 (Thumb, 64 bytes, Stack size 8 bytes, schm_fls.o(.mcal_text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_03 ⇒ Fls_schm_read_msr
  [Calls]
  - >> Fls_schm_read_msr
  [Called By]
  - >> Fls_Write

  SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_03 (Thumb, 52 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_Write

  SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_04 (Thumb, 64 bytes, Stack size 8 bytes, schm_fls.o(.mcal_text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_04 ⇒ Fls_schm_read_msr
  [Calls]
  - >> Fls_schm_read_msr
  [Called By]
  - >> Fls_Compare

  SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_04 (Thumb, 52 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_Compare

  SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_05 (Thumb, 64 bytes, Stack size 8 bytes, schm_fls.o(.mcal_text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_05 ⇒ Fls_schm_read_msr
  [Calls]
  - >> Fls_schm_read_msr
  [Called By]
  - >> Fls_BlankCheck

  SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_05 (Thumb, 52 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_BlankCheck

  SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_06 (Thumb, 64 bytes, Stack size 8 bytes, schm_fls.o(.mcal_text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_06 ⇒ Fls_schm_read_msr
  [Calls]
  - >> Fls_schm_read_msr
  [Called By]
  - >> Fls_Read

  SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_06 (Thumb, 52 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_Read

  SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_07 (Thumb, 64 bytes, Stack size 8 bytes, schm_fls.o(.mcal_text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_07 ⇒ Fls_schm_read_msr
  [Calls]
  - >> Fls_schm_read_msr
  [Called By]
  - >> Fls_Lld_LoadAESKey

  SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_07 (Thumb, 52 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_Lld_LoadAESKey

  init_data_bss (Thumb, 440 bytes, Stack size 52 bytes, startup.o(.mcal_text))
  [Stack]

  - Max Depth = 52
  - Call Chain = init_data_bss
  [Address Reference Count : 1]
  - ytm32b1mc0_startup_armc.o(.text)

  SystemInit (Thumb, 52 bytes, Stack size 0 bytes, system_ytm32b1mc0.o(.mcal_text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(.text)

  SystemCoreClockUpdate (Thumb, 20 bytes, Stack size 0 bytes, system_ytm32b1mc0.o(.mcal_text), UNUSED)

  Mcu_GetPllStatus (Thumb, 16 bytes, Stack size 4 bytes, mcu.o(.mcal_text), UNUSED)

  Mcu_GetResetReason (Thumb, 42 bytes, Stack size 16 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_GetResetValue

  Mcu_Init (Thumb, 86 bytes, Stack size 16 bytes, mcu.o(.mcal_text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Mcu_Init ⇒ Mcu_Lld_SetRcu
  [Calls]
  - >> Mcu_Lld_SetRcu
  [Called By]
  - >> main

  Mcu_InitClock (Thumb, 134 bytes, Stack size 16 bytes, mcu.o(.mcal_text))
  [Stack]

  - Max Depth = 84
  - Call Chain = Mcu_InitClock ⇒ Mcu_Lld_InitClock ⇒ Mcu_Lld_SetClockSource ⇒ Mcu_Lld_SwitchSystemClock ⇒ Mcu_Lld_SetSystemClockSource
  [Calls]
  - >> Mcu_Lld_InitClock
  [Called By]
  - >> main

  Mcu_InitRamSection (Thumb, 120 bytes, Stack size 24 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_SetRamSection

  Mcu_SetMode (Thumb, 82 bytes, Stack size 16 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00
  - >> Mcu_Lld_SetMode
  - >> SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00

  Mcu_GetResetRawValue (Thumb, 22 bytes, Stack size 16 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_GetResetRawValue

  Mcu_180_GetCoreClockFrequency (Thumb, 78 bytes, Stack size 16 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_GetCoreClockFrequency

  Mcu_Lld_SystemReset (Thumb, 52 bytes, Stack size 4 bytes, mcu_lld.o(.mcal_text), UNUSED)

  Mcu_Lld_SetRcu (Thumb, 60 bytes, Stack size 4 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 4
  - Call Chain = Mcu_Lld_SetRcu
  [Called By]
  - >> Mcu_Init

  Mcu_Lld_SetRamSection (Thumb, 64 bytes, Stack size 12 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_InitRamSection

  Mcu_Lld_SetMode (Thumb, 10 bytes, Stack size 4 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_SetMode

  Mcu_Lld_SetClockSource (Thumb, 84 bytes, Stack size 16 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 52
  - Call Chain = Mcu_Lld_SetClockSource ⇒ Mcu_Lld_SwitchSystemClock ⇒ Mcu_Lld_SetSystemClockSource
  [Calls]
  - >> Mcu_Lld_SetPeripheralClock
  - >> Mcu_Lld_SetClockOut
  - >> Mcu_Lld_ClkOutDisable
  - >> Mcu_Lld_SetCmu
  - >> Mcu_Lld_SwitchSystemClock
  [Called By]
  - >> Mcu_Lld_InitClock

  Mcu_Lld_SetPeripheralClock (Thumb, 158 bytes, Stack size 20 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Mcu_Lld_SetPeripheralClock
  [Called By]
  - >> Mcu_Lld_SetClockSource

  Mcu_Lld_InitClock (Thumb, 166 bytes, Stack size 16 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 68
  - Call Chain = Mcu_Lld_InitClock ⇒ Mcu_Lld_SetClockSource ⇒ Mcu_Lld_SwitchSystemClock ⇒ Mcu_Lld_SetSystemClockSource
  [Calls]
  - >> Mcu_Lld_SetClockSource
  - >> Mcu_Lld_InitClockDivider
  - >> Mcu_Lld_EfmPrescaler
  - >> Mcu_Lld_InitFxosc
  - >> Mcu_Lld_InitFirc
  - >> Mcu_Lld_InitSirc
  - >> Mcu_Lld_DisableAllCmu
  - >> Mcu_Lld_SwitchSystemClock
  [Called By]
  - >> Mcu_InitClock

  Mcu_Lld_GetResetRawValue (Thumb, 32 bytes, Stack size 4 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_GetResetRawValue
  - >> Mcu_Lld_GetResetValue

  Mcu_Lld_GetResetValue (Thumb, 220 bytes, Stack size 24 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_GetResetRawValue
  [Called By]
  - >> Mcu_GetResetReason

  Mcu_Lld_GetCoreClockFrequency (Thumb, 106 bytes, Stack size 32 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_GetCoreDiv
  - >> Mcu_Lld_GetCoreClockSource
  [Called By]
  - >> Mcu_180_GetCoreClockFrequency

  Mcu_schm_read_msr (Thumb, 14 bytes, Stack size 4 bytes, schm_mcu.o(.mcal_text), UNUSED)
  [Called By]

  - >> SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00

  SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00 (Thumb, 64 bytes, Stack size 8 bytes, schm_mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_schm_read_msr
  [Called By]
  - >> Mcu_SetMode

  SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00 (Thumb, 52 bytes, Stack size 0 bytes, schm_mcu.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_SetMode

  Reset_Handler (Thumb, 90 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - ytm32b1mc0_startup_armc.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - ytm32b1mc0_startup_armc.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - ytm32b1mc0_startup_armc.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - ytm32b1mc0_startup_armc.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - ytm32b1mc0_startup_armc.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - ytm32b1mc0_startup_armc.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - ytm32b1mc0_startup_armc.o(RESET)

  DefaultISR (Thumb, 2 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text), UNUSED, KEPT)
  [Calls]

  - >> DefaultISR
  [Called By]
  - >> DefaultISR

  ACMP0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Calls]

  - >> ACMP0_IRQHandler
  [Called By]
  - >> ACMP0_IRQHandler
  [Address Reference Count : 1]
  - ytm32b1mc0_startup_armc.o(RESET)

  ADC0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  CAN0_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  CAN0_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  CAN0_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  CAN0_ORed_32_47_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  CAN0_ORed_48_63_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  CAN0_ORed_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  CAN0_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  CAN1_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  CAN1_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  CAN1_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  CAN1_ORed_32_47_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  CAN1_ORed_48_63_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  CAN1_ORed_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  CAN1_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  DMA0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  DMA1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  DMA2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  DMA3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  DMA_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  EFM_Ecc_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  EFM_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  EFM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  EMU_DB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  EMU_SB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  GPIOA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  GPIOB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  GPIOC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  GPIOD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  GPIOE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  HCU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  I2C0_Master_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  I2C0_Slave_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  I2C1_Master_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  MPWM0_Ch0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  MPWM0_Ch0_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  MPWM0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  MPWM0_Ch1_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  MPWM0_Ch2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  MPWM0_Ch2_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  MPWM0_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  MPWM0_Ch3_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  MPWM0_Ch4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  MPWM0_Ch4_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  MPWM0_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  MPWM0_Ch5_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  MPWM0_Ch6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  MPWM0_Ch6_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  MPWM0_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  MPWM0_Ch7_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  PCU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved16_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved17_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved18_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved19_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved20_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved21_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved22_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved23_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved24_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved25_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved26_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved27_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved28_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved29_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved30_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved31_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved32_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved33_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved34_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved35_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved36_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved37_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved38_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved39_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved40_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved41_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved42_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved43_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved44_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved45_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved46_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved47_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved48_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved49_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved50_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved51_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved52_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved53_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved54_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved55_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved56_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved57_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved58_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved59_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved60_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved61_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved62_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved63_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved64_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved65_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved66_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved67_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved68_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved69_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved70_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved71_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved72_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved73_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved74_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved75_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved76_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved77_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved78_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved79_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved80_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved81_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved82_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved83_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved84_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Reserved9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  SCU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  SPI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  TRNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  UART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  UART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  Wdg_Mld_Isr (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  eTMR0_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  eTMR0_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  eTMR0_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  eTMR0_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  eTMR0_Fault_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  eTMR0_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  eTMR1_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  eTMR1_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  eTMR1_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  eTMR1_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  eTMR1_Fault_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  eTMR1_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  lpTMR0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  pTMR_Ch0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  pTMR_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  pTMR_Ch2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  pTMR_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, ytm32b1mc0_startup_armc.o(.text))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __decompress (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl.o(.text), UNUSED)

  __decompress0 (Thumb, 58 bytes, Stack size unknown bytes, __dczerorl.o(.text), UNUSED)

  Det_ReportRuntimeError (Thumb, 94 bytes, Stack size 8 bytes, det.o(.text.Det_ReportRuntimeError))
  [Stack]

  - Max Depth = 8
  - Call Chain = Det_ReportRuntimeError
  [Called By]
  - >> Fls_Lld_TranslateReturnCode
  - >> Fls_Lld_MainFunction

  Det_ReportTransientFault (Thumb, 94 bytes, Stack size 8 bytes, det.o(.text.Det_ReportTransientFault))
  [Stack]

  - Max Depth = 8
  - Call Chain = Det_ReportTransientFault
  [Called By]
  - >> Fls_Lld_MainFunction
  - >> Fls_ExecuteJobWrite
  - >> Fls_ProcessJobDataTransfer
  - >> Fls_ExecuteJobErase

  Fls_Lld_TranslateReturnCode (Thumb, 134 bytes, Stack size 16 bytes, fls_lld.o(.text.Fls_Lld_TranslateReturnCode))
  [Stack]

  - Max Depth = 24
  - Call Chain = Fls_Lld_TranslateReturnCode ⇒ Det_ReportRuntimeError
  [Calls]
  - >> Det_ReportRuntimeError
  [Called By]
  - >> Fls_ExecuteJobRdBlankCheckComp
  - >> Fls_ExecuteJobErase

  SVC_Handler (Thumb, 4 bytes, Stack size 0 bytes, exceptions.o(.text.SVC_Handler))
  [Address Reference Count : 1]

  - ytm32b1mc0_startup_armc.o(RESET)

  main (Thumb, 1032 bytes, Stack size 24 bytes, main.o(.text.main))
  [Stack]

  - Max Depth = 264
  - Call Chain = main ⇒ Fls_MainFunction ⇒ Fls_ProcessRequestedJobs ⇒ Fls_DoJobDataTransfer ⇒ Fls_ProcessJobDataTransfer ⇒ Fls_ExecuteJobRdBlankCheckComp ⇒ Fls_Lld_ReadFlash ⇒ Fls_Lld_ReadUserPartition ⇒ Fls_Lld_ValidFlash ⇒ Fls_Lld_ValidDFlash
  [Calls]
  - >> Fls_BlankCheck
  - >> Fls_Compare
  - >> Fls_Read
  - >> Fls_Write
  - >> Fls_GetJobResult
  - >> Fls_GetStatus
  - >> Fls_MainFunction
  - >> Fls_Erase
  - >> Mcu_InitClock
  - >> Mcu_Init
  - >> Board_Init
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  Board_Init (Thumb, 16 bytes, Stack size 8 bytes, main.o(.text.Board_Init))
  [Stack]

  - Max Depth = 48
  - Call Chain = Board_Init ⇒ Fls_Init ⇒ Fls_Lld_Init ⇒ Fls_Lld_SetProtectReg
  [Calls]
  - >> Fls_Init
  [Called By]
  - >> main

  Fls_IsSectorStartAddrAligned (Thumb, 86 bytes, Stack size 16 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Fls_IsSectorStartAddrAligned ⇒ Fls_GetSectorIndexByAddr
  [Calls]
  - >> Fls_GetSectorIndexByAddr
  [Called By]
  - >> Fls_Erase

  Fls_IsSectorEndAddrAligned (Thumb, 92 bytes, Stack size 16 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Fls_IsSectorEndAddrAligned ⇒ Fls_GetSectorIndexByAddr
  [Calls]
  - >> Fls_GetSectorIndexByAddr
  [Called By]
  - >> Fls_Erase

  Fls_GetSectorIndexByAddr (Thumb, 138 bytes, Stack size 8 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Fls_GetSectorIndexByAddr
  [Called By]
  - >> Fls_IsAddrInRange
  - >> Fls_IsSectorAddrPageAligned
  - >> Fls_IsSectorEndAddrAligned
  - >> Fls_IsSectorStartAddrAligned
  - >> Fls_BlankCheck
  - >> Fls_Compare
  - >> Fls_Read
  - >> Fls_Write
  - >> Fls_Erase

  Fls_IsSectorAddrPageAligned (Thumb, 176 bytes, Stack size 16 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Fls_IsSectorAddrPageAligned ⇒ Fls_GetSectorIndexByAddr
  [Calls]
  - >> Fls_GetSectorIndexByAddr
  [Called By]
  - >> Fls_Write

  Fls_GetLldJobResult (Thumb, 12 bytes, Stack size 0 bytes, fls.o(.mcal_text))
  [Called By]

  - >> Fls_Cancel
  - >> Fls_MainFunction

  Fls_IsAddrInRange (Thumb, 138 bytes, Stack size 16 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Fls_IsAddrInRange ⇒ Fls_GetSectorIndexByAddr
  [Calls]
  - >> Fls_GetSectorIndexByAddr
  [Called By]
  - >> Fls_BlankCheck
  - >> Fls_Compare
  - >> Fls_Read

  Fls_ClrLldJobResult (Thumb, 24 bytes, Stack size 0 bytes, fls.o(.mcal_text))
  [Called By]

  - >> Fls_MainFunction

  Fls_ProcessRequestedJobs (Thumb, 106 bytes, Stack size 16 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 224
  - Call Chain = Fls_ProcessRequestedJobs ⇒ Fls_DoJobDataTransfer ⇒ Fls_ProcessJobDataTransfer ⇒ Fls_ExecuteJobRdBlankCheckComp ⇒ Fls_Lld_ReadFlash ⇒ Fls_Lld_ReadUserPartition ⇒ Fls_Lld_ValidFlash ⇒ Fls_Lld_ValidDFlash
  [Calls]
  - >> Fls_DoJobDataTransfer
  - >> Fls_ExecuteJobErase
  [Called By]
  - >> Fls_MainFunction

  Fls_MainFunctionCheckJobResult (Thumb, 136 bytes, Stack size 16 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Fls_MainFunctionCheckJobResult
  [Called By]
  - >> Fls_MainFunction

  Fls_ExecuteJobErase (Thumb, 458 bytes, Stack size 32 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 76
  - Call Chain = Fls_ExecuteJobErase ⇒ Fls_Lld_SectorErase ⇒ Fls_Lld_LoadCommandSync ⇒ Fls_Lld_CheckErrorFlag
  [Calls]
  - >> Fls_Lld_GetPhycSectorSize
  - >> Fls_Lld_TranslateReturnCode
  - >> Fls_Lld_SectorErase
  - >> Det_ReportTransientFault
  [Called By]
  - >> Fls_ProcessRequestedJobs

  Fls_DoJobDataTransfer (Thumb, 340 bytes, Stack size 48 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 208
  - Call Chain = Fls_DoJobDataTransfer ⇒ Fls_ProcessJobDataTransfer ⇒ Fls_ExecuteJobRdBlankCheckComp ⇒ Fls_Lld_ReadFlash ⇒ Fls_Lld_ReadUserPartition ⇒ Fls_Lld_ValidFlash ⇒ Fls_Lld_ValidDFlash
  [Calls]
  - >> Fls_ProcessJobDataTransfer
  - >> Fls_CalcSectorTransferLength
  - >> Fls_CalcMaxTransferAddrEnd
  [Called By]
  - >> Fls_ProcessRequestedJobs

  Fls_CalcMaxTransferAddrEnd (Thumb, 58 bytes, Stack size 8 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Fls_CalcMaxTransferAddrEnd
  [Called By]
  - >> Fls_DoJobDataTransfer

  Fls_CalcSectorTransferLength (Thumb, 202 bytes, Stack size 20 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Fls_CalcSectorTransferLength
  [Called By]
  - >> Fls_DoJobDataTransfer

  Fls_ProcessJobDataTransfer (Thumb, 278 bytes, Stack size 24 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 160
  - Call Chain = Fls_ProcessJobDataTransfer ⇒ Fls_ExecuteJobRdBlankCheckComp ⇒ Fls_Lld_ReadFlash ⇒ Fls_Lld_ReadUserPartition ⇒ Fls_Lld_ValidFlash ⇒ Fls_Lld_ValidDFlash
  [Calls]
  - >> Fls_ExecuteJobRdBlankCheckComp
  - >> Fls_ExecuteJobWrite
  - >> Det_ReportTransientFault
  [Called By]
  - >> Fls_DoJobDataTransfer

  Fls_ExecuteJobWrite (Thumb, 118 bytes, Stack size 24 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 88
  - Call Chain = Fls_ExecuteJobWrite ⇒ Fls_Lld_SectorWrite ⇒ Fls_Lld_WriteDataPage ⇒ Fls_Lld_JudgeSetAddr
  [Calls]
  - >> Fls_Lld_SectorWrite
  - >> Det_ReportTransientFault
  [Called By]
  - >> Fls_ProcessJobDataTransfer

  Fls_ExecuteJobRdBlankCheckComp (Thumb, 130 bytes, Stack size 32 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 136
  - Call Chain = Fls_ExecuteJobRdBlankCheckComp ⇒ Fls_Lld_ReadFlash ⇒ Fls_Lld_ReadUserPartition ⇒ Fls_Lld_ValidFlash ⇒ Fls_Lld_ValidDFlash
  [Calls]
  - >> Fls_Lld_CompareFlash
  - >> Fls_Lld_ReadFlash
  - >> Fls_Lld_TranslateReturnCode
  [Called By]
  - >> Fls_ProcessJobDataTransfer

  Fls_Lld_GetRecoverr (Thumb, 14 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Fls_Lld_GetOneBitEccErrFlag

  Fls_Lld_GetUnrecoverr (Thumb, 14 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Fls_Lld_GetTwoBitEccErrFlag

  Fls_Lld_ClearRecoverr (Thumb, 12 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Fls_Lld_ClearOneBitEccErrFlag

  Fls_Lld_ClearUnrecoverr (Thumb, 12 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Fls_Lld_ClearTwoBitEccErrFlag

  Fls_Lld_GetEccErrorAddrReg (Thumb, 10 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Fls_Lld_GetEccErrAddr

  Fls_Lld_CheckIdle (Thumb, 14 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text))
  [Called By]

  - >> Fls_Lld_GetCtrlStatus
  - >> Fls_Lld_LoadAESKey
  - >> Fls_Lld_SectorWrite
  - >> Fls_Lld_SectorErase
  - >> Fls_Lld_Cancel
  - >> Fls_Lld_Init

  Fls_Lld_ClearRegSTS (Thumb, 12 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text))
  [Called By]

  - >> Fls_Lld_WriteDataPage
  - >> Fls_Lld_LoadAESKey
  - >> Fls_Lld_SectorErase
  - >> Fls_Lld_Init

  Fls_Lld_SetProtectReg (Thumb, 28 bytes, Stack size 8 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Fls_Lld_SetProtectReg
  [Called By]
  - >> Fls_Lld_Init

  Fls_Lld_ValidFlash (Thumb, 54 bytes, Stack size 16 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Fls_Lld_ValidFlash ⇒ Fls_Lld_ValidDFlash
  [Calls]
  - >> Fls_Lld_ValidDFlash
  - >> Fls_Lld_ValidPFlash
  [Called By]
  - >> Fls_Lld_ReadUserPartition
  - >> Fls_Lld_CompareFlash
  - >> Fls_Lld_ReadFlash
  - >> Fls_Lld_SectorWrite
  - >> Fls_Lld_SectorErase

  Fls_Lld_EFMNopCommand (Thumb, 22 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text))
  [Called By]

  - >> Fls_Lld_LoadAESKey
  - >> Fls_Lld_SectorWrite
  - >> Fls_Lld_SectorErase

  ARM_MPU_Disable (Thumb, 46 bytes, Stack size 0 bytes, fls_lld.o(.text.ARM_MPU_Disable))
  [Called By]

  - >> Fls_Lld_WriteDataPage
  - >> Fls_Lld_SectorErase

  Fls_Lld_SetWE (Thumb, 24 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text))
  [Called By]

  - >> Fls_Lld_WriteDataPage
  - >> Fls_Lld_LoadNvrAddr
  - >> Fls_Lld_SectorErase

  Fls_Lld_ClearWE (Thumb, 24 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text))
  [Called By]

  - >> Fls_Lld_WriteDataPage
  - >> Fls_Lld_LoadNvrAddr
  - >> Fls_Lld_SectorErase

  Fls_Lld_JudgeSetAddr (Thumb, 76 bytes, Stack size 8 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Fls_Lld_JudgeSetAddr
  [Called By]
  - >> Fls_Lld_WriteDataPage
  - >> Fls_Lld_LoadNvrAddr
  - >> Fls_Lld_SectorErase

  ARM_MPU_Enable (Thumb, 52 bytes, Stack size 4 bytes, fls_lld.o(.text.ARM_MPU_Enable))
  [Stack]

  - Max Depth = 4
  - Call Chain = ARM_MPU_Enable
  [Called By]
  - >> Fls_Lld_WriteDataPage
  - >> Fls_Lld_SectorErase

  Fls_Lld_UnLockCMD (Thumb, 20 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text))
  [Called By]

  - >> Fls_Lld_SectorWrite
  - >> Fls_Lld_SectorErase

  Fls_Lld_LoadCommand (Thumb, 22 bytes, Stack size 4 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 4
  - Call Chain = Fls_Lld_LoadCommand
  [Called By]
  - >> Fls_Lld_SectorWrite
  - >> Fls_Lld_SectorErase

  Fls_Lld_LoadCommandSync (Thumb, 172 bytes, Stack size 24 bytes, fls_lld.o(.ramcode))
  [Stack]

  - Max Depth = 28
  - Call Chain = Fls_Lld_LoadCommandSync ⇒ Fls_Lld_CheckErrorFlag
  [Calls]
  - >> Fls_Lld_CheckErrorFlag (via Veneer)
  - >> Fls_Lld_CheckIdleInRam
  [Called By]
  - >> Fls_Lld_SectorWrite (via Veneer)
  - >> Fls_Lld_SectorErase (via Veneer)

  Fls_Lld_ValidPFlash (Thumb, 38 bytes, Stack size 8 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Fls_Lld_ValidPFlash
  [Called By]
  - >> Fls_Lld_AddrCheckPreWrite
  - >> Fls_Lld_ValidFlash
  - >> Fls_Lld_GetPhycSectorSize

  Fls_Lld_ValidDFlash (Thumb, 86 bytes, Stack size 8 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Fls_Lld_ValidDFlash
  [Called By]
  - >> Fls_Lld_AddrCheckPreWrite
  - >> Fls_Lld_ValidFlash

  Fls_Lld_CheckIdleInRam (Thumb, 14 bytes, Stack size 0 bytes, fls_lld.o(.ramcode))
  [Called By]

  - >> Fls_Lld_LoadAESCommand
  - >> Fls_Lld_LoadCommandSync

  Fls_Lld_CheckErrorFlag (Thumb, 42 bytes, Stack size 4 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 4
  - Call Chain = Fls_Lld_CheckErrorFlag
  [Called By]
  - >> Fls_Lld_GetCtrlStatus
  - >> Fls_Lld_LoadCommandSync (via Veneer)

  Fls_Lld_ReadUserPartition (Thumb, 322 bytes, Stack size 56 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 80
  - Call Chain = Fls_Lld_ReadUserPartition ⇒ Fls_Lld_ValidFlash ⇒ Fls_Lld_ValidDFlash
  [Calls]
  - >> Fls_Lld_ComputeReadSize
  - >> Fls_Lld_ValidFlash
  [Called By]
  - >> Fls_Lld_ReadFlash

  Fls_Lld_ValidNVRFlash (Thumb, 60 bytes, Stack size 8 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Fls_Lld_ValidNVRFlash
  [Called By]
  - >> Fls_Lld_ReadFlash

  Fls_Lld_LoadAESKey (Thumb, 102 bytes, Stack size 16 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Fls_Lld_LoadAESKey ⇒ Fls_Lld_LoadAESCommand
  [Calls]
  - >> SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_07
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_07
  - >> Fls_Lld_LoadAESCommand (via Veneer)
  - >> Fls_Lld_LoadNvrAddr
  - >> Fls_Lld_EFMNopCommand
  - >> Fls_Lld_ClearRegSTS
  - >> Fls_Lld_CheckIdle
  [Called By]
  - >> Fls_Lld_ReadFlash

  Fls_Lld_ComputeReadSize (Thumb, 102 bytes, Stack size 20 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Fls_Lld_ComputeReadSize
  [Called By]
  - >> Fls_Lld_BlankCheck
  - >> Fls_Lld_CompareCheck
  - >> Fls_Lld_ReadUserPartition

  Fls_Lld_LoadNvrAddr (Thumb, 38 bytes, Stack size 16 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Fls_Lld_LoadNvrAddr ⇒ Fls_Lld_JudgeSetAddr
  [Calls]
  - >> Fls_Lld_JudgeSetAddr
  - >> Fls_Lld_ClearWE
  - >> Fls_Lld_SetWE
  [Called By]
  - >> Fls_Lld_LoadAESKey

  Fls_Lld_LoadAESCommand (Thumb, 154 bytes, Stack size 24 bytes, fls_lld.o(.ramcode))
  [Stack]

  - Max Depth = 24
  - Call Chain = Fls_Lld_LoadAESCommand
  [Calls]
  - >> Fls_Lld_CheckIdleInRam
  [Called By]
  - >> Fls_Lld_LoadAESKey (via Veneer)

  Fls_Lld_CompareCheck (Thumb, 254 bytes, Stack size 48 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 68
  - Call Chain = Fls_Lld_CompareCheck ⇒ Fls_Lld_ComputeReadSize
  [Calls]
  - >> Fls_Lld_ComputeReadSize
  [Called By]
  - >> Fls_Lld_CompareFlash

  Fls_Lld_SectorEraseStatus (Thumb, 84 bytes, Stack size 16 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 36
  - Call Chain = Fls_Lld_SectorEraseStatus ⇒ Fls_Lld_GetCtrlStatus ⇒ Fls_Lld_CheckErrorFlag
  [Calls]
  - >> Fls_Lld_GetCtrlStatus
  [Called By]
  - >> Fls_Lld_MainFunction

  Fls_Lld_SectorWriteStatus (Thumb, 84 bytes, Stack size 16 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 36
  - Call Chain = Fls_Lld_SectorWriteStatus ⇒ Fls_Lld_GetCtrlStatus ⇒ Fls_Lld_CheckErrorFlag
  [Calls]
  - >> Fls_Lld_GetCtrlStatus
  [Called By]
  - >> Fls_Lld_MainFunction

  Fls_Lld_GetCtrlStatus (Thumb, 102 bytes, Stack size 16 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Fls_Lld_GetCtrlStatus ⇒ Fls_Lld_CheckErrorFlag
  [Calls]
  - >> Fls_Lld_ClearErrorFlag
  - >> Fls_Lld_CheckErrorFlag
  - >> Fls_Lld_CheckIdle
  [Called By]
  - >> Fls_Lld_SectorWriteStatus
  - >> Fls_Lld_SectorEraseStatus

  Fls_Lld_AddrCheckPreWrite (Thumb, 178 bytes, Stack size 24 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Fls_Lld_AddrCheckPreWrite ⇒ Fls_Lld_ValidDFlash
  [Calls]
  - >> Fls_Lld_ValidDFlash
  - >> Fls_Lld_ValidPFlash
  [Called By]
  - >> Fls_Lld_SectorWrite

  Fls_Lld_WriteDataPage (Thumb, 124 bytes, Stack size 24 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Fls_Lld_WriteDataPage ⇒ Fls_Lld_JudgeSetAddr
  [Calls]
  - >> ARM_MPU_Enable
  - >> Fls_Lld_JudgeSetAddr
  - >> Fls_Lld_ClearWE
  - >> Fls_Lld_SetWE
  - >> ARM_MPU_Disable
  - >> Fls_Lld_ClearRegSTS
  [Called By]
  - >> Fls_Lld_SectorWrite

  Fls_Lld_WriteRstCheck (Thumb, 70 bytes, Stack size 4 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 4
  - Call Chain = Fls_Lld_WriteRstCheck
  [Called By]
  - >> Fls_Lld_SectorWrite

  Fls_Lld_ClearErrorFlag (Thumb, 12 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text))
  [Called By]

  - >> Fls_Lld_GetCtrlStatus

  Mcu_Lld_SwitchSystemClock (Thumb, 120 bytes, Stack size 32 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 36
  - Call Chain = Mcu_Lld_SwitchSystemClock ⇒ Mcu_Lld_SetSystemClockSource
  [Calls]
  - >> Mcu_Lld_GetSystemClockStatus
  - >> Mcu_Lld_SetSystemClockSource
  [Called By]
  - >> Mcu_Lld_SetClockSource
  - >> Mcu_Lld_InitClock

  Mcu_Lld_SetCmu (Thumb, 292 bytes, Stack size 28 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 28
  - Call Chain = Mcu_Lld_SetCmu
  [Called By]
  - >> Mcu_Lld_SetClockSource

  Mcu_Lld_ClkOutDisable (Thumb, 18 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_SetClockSource

  Mcu_Lld_SetClockOut (Thumb, 50 bytes, Stack size 4 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 4
  - Call Chain = Mcu_Lld_SetClockOut
  [Called By]
  - >> Mcu_Lld_SetClockSource

  Mcu_Lld_SetSystemClockSource (Thumb, 30 bytes, Stack size 4 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 4
  - Call Chain = Mcu_Lld_SetSystemClockSource
  [Called By]
  - >> Mcu_Lld_SwitchSystemClock

  Mcu_Lld_GetSystemClockStatus (Thumb, 16 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_SwitchSystemClock

  Mcu_Lld_DisableAllCmu (Thumb, 18 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_InitClock

  Mcu_Lld_InitSirc (Thumb, 90 bytes, Stack size 12 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Mcu_Lld_InitSirc
  [Called By]
  - >> Mcu_Lld_InitClock

  Mcu_Lld_InitFirc (Thumb, 148 bytes, Stack size 32 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Mcu_Lld_InitFirc ⇒ Mcu_Lld_FircEnable
  [Calls]
  - >> Mcu_Lld_FircDisable
  - >> Mcu_Lld_GetClockStatus
  - >> Mcu_Lld_FircEnable
  [Called By]
  - >> Mcu_Lld_InitClock

  Mcu_Lld_InitFxosc (Thumb, 148 bytes, Stack size 32 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 52
  - Call Chain = Mcu_Lld_InitFxosc ⇒ Mcu_Lld_SetFxoscClock
  [Calls]
  - >> Mcu_Lld_FxoscDisable
  - >> Mcu_Lld_SetFxoscClock
  - >> Mcu_Lld_GetClockStatus
  [Called By]
  - >> Mcu_Lld_InitClock

  Mcu_Lld_EfmPrescaler (Thumb, 50 bytes, Stack size 8 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Mcu_Lld_EfmPrescaler
  [Called By]
  - >> Mcu_Lld_InitClock

  Mcu_Lld_InitClockDivider (Thumb, 144 bytes, Stack size 32 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 44
  - Call Chain = Mcu_Lld_InitClockDivider ⇒ Mcu_Lld_SetClockDivider
  [Calls]
  - >> Mcu_Lld_GetDividerStatus
  - >> Mcu_Lld_SetClockDivider
  [Called By]
  - >> Mcu_Lld_InitClock

  Mcu_Lld_FircEnable (Thumb, 72 bytes, Stack size 8 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Mcu_Lld_FircEnable
  [Called By]
  - >> Mcu_Lld_InitFirc

  Mcu_Lld_GetClockStatus (Thumb, 22 bytes, Stack size 4 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 4
  - Call Chain = Mcu_Lld_GetClockStatus
  [Called By]
  - >> Mcu_Lld_InitFxosc
  - >> Mcu_Lld_InitFirc

  Mcu_Lld_FircDisable (Thumb, 18 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_InitFirc

  Mcu_Lld_SetFxoscClock (Thumb, 120 bytes, Stack size 20 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Mcu_Lld_SetFxoscClock
  [Called By]
  - >> Mcu_Lld_InitFxosc

  Mcu_Lld_FxoscDisable (Thumb, 18 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_InitFxosc

  Mcu_Lld_SetClockDivider (Thumb, 62 bytes, Stack size 12 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 12
  - Call Chain = Mcu_Lld_SetClockDivider
  [Called By]
  - >> Mcu_Lld_InitClockDivider

  Mcu_Lld_GetDividerStatus (Thumb, 12 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_InitClockDivider

  Mcu_Lld_GetCoreClockSource (Thumb, 26 bytes, Stack size 4 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_Lld_GetCoreClockFrequency

  Mcu_Lld_GetCoreDiv (Thumb, 22 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_Lld_GetCoreClockFrequency

  ### Undefined Global Symbols