T0C78 002:813.229   SEGGER J-Link V7.92 Log File
T0C78 002:813.377   DLL Compiled: Aug 11 2023 08:33:59
T0C78 002:813.389   Logging started @ 2024-01-15 02:52
T0C78 002:813.395 - 10.216ms
T0C78 002:813.444 JLINK_SetWarnOutHandler(...)
T0C78 002:813.450 - 0.006ms
T0C78 002:813.462 JLINK_OpenEx(...)
T0C78 002:817.577   Firmware: J-Link V11 compiled Apr 27 2041 16:36:21
T0C78 002:817.937   Firmware: J-Link V11 compiled Apr 27 2041 16:36:21
T0C78 002:838.089   Hardware: V11.00
T0C78 002:838.107   S/N: 941000024
T0C78 002:838.111   OEM: SEGGER
T0C78 002:838.116   Feature(s): GDB, JFlash, FlashDL, RDI, FlashBP
T0C78 002:839.614   Bootloader: (Could not read)
T0C78 002:847.842   TELNET listener socket opened on port 19021
T0C78 002:852.830   WEBSRV WEBSRV_Init(): Starting webserver thread(s)
T0C78 002:852.931   WEBSRV Failed to put socket into listener state (port 19080)
T0C78 002:853.029   WEBSRV Webserver running on local port 19081
T0C78 002:853.157   Looking for J-Link GUI Server exe at: C:\Keil_v5\ARM\Segger\JLinkGUIServer.exe
T0C78 002:853.211   Looking for J-Link GUI Server exe at: C:\Program Files\SEGGER\JLink\JLinkGUIServer.exe
T0C78 002:853.234   Forking J-Link GUI Server: C:\Program Files\SEGGER\JLink\JLinkGUIServer.exe
T0C78 002:855.292   J-Link GUI Server info: "J-Link GUI server V7.92 "
T0C78 002:855.724 - 42.260ms returns "O.K."
T0C78 002:855.780 JLINK_GetEmuCaps()
T0C78 002:855.788 - 0.007ms returns 0xB9FF7BBF
T0C78 002:855.799 JLINK_TIF_GetAvailable(...)
T0C78 002:856.071 - 0.272ms
T0C78 002:856.099 JLINK_SetErrorOutHandler(...)
T0C78 002:856.103 - 0.004ms
T0C78 002:856.113 JLINK_ExecCommand("ProjectFile = "D:\YTM_MCU\YTM32B1ME0\03_MCAL\yt_mcal\Examples\YTM32B1MC0\Fls\YCT\Fls_Demo\KEIL\JLinkSettings.ini"", ...). 
T0C78 002:857.391 - 1.276ms returns 0x00
T0C78 002:857.428 JLINK_ExecCommand("Device = YTM32B1MC03", ...). 
T0C78 002:857.967   Flash bank @ 0x00000000: SFL: Parsing sectorization info from ELF file
T0C78 002:857.985     FlashDevice.SectorInfo[0]: .SectorSize = 0x00000200, .SectorStartAddr = 0x00000000
T0C78 002:857.994   OFL: Init() present @ offset 0x0000003D
T0C78 002:858.001   OFL: UnInit() present @ offset 0x000000C5
T0C78 002:858.012   OFL: EraseSector() present @ offset 0x0000011F
T0C78 002:858.020   OFL: ProgramPage() present @ offset 0x0000015B
T0C78 002:858.027   OFL: EraseChip() present @ offset 0x000000CB
T0C78 002:858.034   OFL: BlankCheck() N/A
T0C78 002:858.042   OFL: Verify() N/A
T0C78 002:858.049   OFL: SEGGER_FL_Erase() N/A
T0C78 002:858.056   OFL: SEGGER_OPEN_Erase() N/A
T0C78 002:858.071   OFL: SEGGER_FL_Program() N/A
T0C78 002:858.078   OFL: SEGGER_OPEN_Program() N/A
T0C78 002:858.085   OFL: SEGGER_FL_Read() N/A
T0C78 002:858.099   OFL: SEGGER_OPEN_Read() N/A
T0C78 002:858.106   OFL: SEGGER_FL_CalcCRC() N/A
T0C78 002:858.113   OFL: SEGGER_OPEN_CalcCRC() N/A
T0C78 002:858.120   OFL: SEGGER_FL_Start() N/A
T0C78 002:858.128   OFL: SEGGER_OPEN_Start() N/A
T0C78 002:858.137   OFL: SEGGER_FL_GetFlashInfo() N/A
T0C78 002:858.144   OFL: SEGGER_OPEN_GetFlashInfo() N/A
T0C78 002:858.152   OFL: SEGGER_FL_Verify() N/A
T0C78 002:858.159   OFL: SEGGER_FL_CheckBlank() N/A
T0C78 002:858.166   OFL: SEGGER_FL_Prepare() N/A
T0C78 002:858.173   OFL: SEGGER_FL_Restore() N/A
T0C78 002:858.180   OFL: SEGGER_FL_EraseChip() N/A
T0C78 002:858.188   OFL var <SEGGER_FL_GoIntEn>: N/A
T0C78 002:858.422   Flash bank @ 0x10001000: SFL: Parsing sectorization info from ELF file
T0C78 002:858.432     FlashDevice.SectorInfo[0]: .SectorSize = 0x00000200, .SectorStartAddr = 0x00000000
T0C78 002:858.441   OFL: Init() present @ offset 0x0000003D
T0C78 002:858.448   OFL: UnInit() present @ offset 0x000000C5
T0C78 002:858.456   OFL: EraseSector() present @ offset 0x000000ED
T0C78 002:858.464   OFL: ProgramPage() present @ offset 0x00000177
T0C78 002:858.471   OFL: EraseChip() present @ offset 0x00000129
T0C78 002:858.479   OFL: BlankCheck() N/A
T0C78 002:858.486   OFL: Verify() N/A
T0C78 002:858.493   OFL: SEGGER_FL_Erase() N/A
T0C78 002:858.500   OFL: SEGGER_OPEN_Erase() N/A
T0C78 002:858.553   OFL: SEGGER_FL_Program() N/A
T0C78 002:858.561   OFL: SEGGER_OPEN_Program() N/A
T0C78 002:858.571   OFL: SEGGER_FL_Read() N/A
T0C78 002:858.578   OFL: SEGGER_OPEN_Read() N/A
T0C78 002:858.585   OFL: SEGGER_FL_CalcCRC() N/A
T0C78 002:858.592   OFL: SEGGER_OPEN_CalcCRC() N/A
T0C78 002:858.601   OFL: SEGGER_FL_Start() N/A
T0C78 002:858.608   OFL: SEGGER_OPEN_Start() N/A
T0C78 002:858.618   OFL: SEGGER_FL_GetFlashInfo() N/A
T0C78 002:858.625   OFL: SEGGER_OPEN_GetFlashInfo() N/A
T0C78 002:858.633   OFL: SEGGER_FL_Verify() N/A
T0C78 002:858.640   OFL: SEGGER_FL_CheckBlank() N/A
T0C78 002:858.647   OFL: SEGGER_FL_Prepare() N/A
T0C78 002:858.655   OFL: SEGGER_FL_Restore() N/A
T0C78 002:858.665   OFL: SEGGER_FL_EraseChip() N/A
T0C78 002:858.674   OFL var <SEGGER_FL_GoIntEn>: N/A
T0C78 002:858.777   Flash bank @ 0x10001000: SFL: Parsing sectorization info from ELF file
T0C78 002:858.786     FlashDevice.SectorInfo[0]: .SectorSize = 0x00000200, .SectorStartAddr = 0x00000000
T0C78 002:858.794   OFL: Init() present @ offset 0x0000003D
T0C78 002:858.801   OFL: UnInit() present @ offset 0x000000C5
T0C78 002:858.807   OFL: EraseSector() present @ offset 0x000000ED
T0C78 002:858.815   OFL: ProgramPage() present @ offset 0x00000177
T0C78 002:858.822   OFL: EraseChip() present @ offset 0x00000129
T0C78 002:858.828   OFL: BlankCheck() N/A
T0C78 002:858.858   OFL: Verify() N/A
T0C78 002:858.865   OFL: SEGGER_FL_Erase() N/A
T0C78 002:858.872   OFL: SEGGER_OPEN_Erase() N/A
T0C78 002:858.880   OFL: SEGGER_FL_Program() N/A
T0C78 002:858.888   OFL: SEGGER_OPEN_Program() N/A
T0C78 002:858.902   OFL: SEGGER_FL_Read() N/A
T0C78 002:858.909   OFL: SEGGER_OPEN_Read() N/A
T0C78 002:858.917   OFL: SEGGER_FL_CalcCRC() N/A
T0C78 002:858.924   OFL: SEGGER_OPEN_CalcCRC() N/A
T0C78 002:858.931   OFL: SEGGER_FL_Start() N/A
T0C78 002:858.938   OFL: SEGGER_OPEN_Start() N/A
T0C78 002:858.945   OFL: SEGGER_FL_GetFlashInfo() N/A
T0C78 002:858.953   OFL: SEGGER_OPEN_GetFlashInfo() N/A
T0C78 002:858.960   OFL: SEGGER_FL_Verify() N/A
T0C78 002:858.972   OFL: SEGGER_FL_CheckBlank() N/A
T0C78 002:858.980   OFL: SEGGER_FL_Prepare() N/A
T0C78 002:858.987   OFL: SEGGER_FL_Restore() N/A
T0C78 002:858.994   OFL: SEGGER_FL_EraseChip() N/A
T0C78 002:859.002   OFL var <SEGGER_FL_GoIntEn>: N/A
T0C78 002:859.037   Device "YTM32B1MC03" selected.
T0C78 002:859.348 - 1.910ms returns 0x00
T0C78 002:859.364 JLINK_ExecCommand("DisableConnectionTimeout", ...). 
T0C78 002:859.373 - 0.001ms returns 0x01
T0C78 002:859.380 JLINK_GetHardwareVersion()
T0C78 002:859.386 - 0.006ms returns 110000
T0C78 002:859.392 JLINK_GetDLLVersion()
T0C78 002:859.397 - 0.004ms returns 79200
T0C78 002:859.402 JLINK_GetOEMString(...)
T0C78 002:859.408 JLINK_GetFirmwareString(...)
T0C78 002:859.414 - 0.006ms
T0C78 002:859.425 JLINK_GetDLLVersion()
T0C78 002:859.429 - 0.004ms returns 79200
T0C78 002:859.435 JLINK_GetCompileDateTime()
T0C78 002:859.440 - 0.004ms
T0C78 002:859.447 JLINK_GetFirmwareString(...)
T0C78 002:859.452 - 0.005ms
T0C78 002:859.458 JLINK_GetHardwareVersion()
T0C78 002:859.463 - 0.004ms returns 110000
T0C78 002:859.469 JLINK_GetSN()
T0C78 002:859.474 - 0.004ms returns 941000024
T0C78 002:859.480 JLINK_GetOEMString(...)
T0C78 002:859.488 JLINK_TIF_Select(JLINKARM_TIF_SWD)
T0C78 002:860.583 - 1.093ms returns 0x00
T0C78 002:860.641 JLINK_HasError()
T0C78 002:860.663 JLINK_SetSpeed(5000)
T0C78 002:860.863 - 0.199ms
T0C78 002:861.368 JLINK_HasError()
T0C78 002:861.387 JLINK_SetResetType(JLINKARM_RESET_TYPE_NORMAL)
T0C78 002:861.393 - 0.006ms returns JLINKARM_RESET_TYPE_NORMAL
T0C78 002:861.400 JLINK_Reset()
T0C78 002:866.043   Found SW-DP with ID 0x6BA02477
T0C78 002:869.385   DPIDR: 0x6BA02477
T0C78 002:869.405   CoreSight SoC-400 or earlier
T0C78 002:869.411   Scanning AP map to find all available APs
T0C78 002:871.066   AP[3]: Stopped AP scan as end of AP map has been reached
T0C78 002:871.081   AP[0]: AHB-AP (IDR: 0x84770001)
T0C78 002:871.087   AP[1]: JTAG-AP (IDR: 0x01680000)
T0C78 002:871.092   AP[2]: APB-AP (IDR: 0x54770002)
T0C78 002:871.101   Iterating through AP map to find AHB-AP to use
T0C78 002:871.709   AP[0]: Core found
T0C78 002:871.717   AP[0]: AHB-AP ROM base: 0xE00FF000
T0C78 002:871.963   CPUID register: 0x411FD210. Implementer code: 0x41 (ARM)
T0C78 002:871.971   Feature set: Mainline
T0C78 002:872.209   Cache: No cache
T0C78 002:872.216   Found Cortex-M33 r1p0, Little endian.
T0C78 002:872.593   -- Max. mem block: 0x00004038
T0C78 002:873.495   
  ***** Warning: 
T0C78 002:873.502   Cortex-M (ARMv8-M and later): The connected J-Link (S/N 941000024) uses an old firmware module that does not handle I/D-cache correctly. Proper debugging functionality cannot be guaranteed if cache is enabled
T0C78 002:873.513   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T0C78 002:873.812   CPU_ReadMem(4 bytes @ 0xE0002000)
T0C78 002:874.062   FPUnit: 4 code (BP) slots and 0 literal slots
T0C78 002:874.068   CPU_ReadMem(4 bytes @ 0xE000EDFC)
T0C78 002:874.319   CPU_ReadMem(4 bytes @ 0xE0001000)
T0C78 002:874.605   CPU_ReadMem(4 bytes @ 0xE0001000)
T0C78 002:874.997   CPU_ReadMem(4 bytes @ 0xE0001028)
T0C78 002:875.264   CPU_ReadMem(4 bytes @ 0xE0001038)
T0C78 002:875.599   CPU_WriteMem(4 bytes @ 0xE0001000)
T0C78 002:875.844   CPU_ReadMem(4 bytes @ 0xE000ED88)
T0C78 002:876.062   CPU_WriteMem(4 bytes @ 0xE000ED88)
T0C78 002:876.290   CPU_ReadMem(4 bytes @ 0xE000ED88)
T0C78 002:876.523   CPU_WriteMem(4 bytes @ 0xE000ED88)
T0C78 002:876.792   CPU_ReadMem(4 bytes @ 0xE000EFB8)
T0C78 002:877.042   Security extension: not implemented
T0C78 002:877.049   CoreSight components:
T0C78 002:877.055   ROMTbl[0] @ E00FF000
T0C78 002:877.060   CPU_ReadMem(64 bytes @ 0xE00FF000)
T0C78 002:877.519   CPU_ReadMem(32 bytes @ 0xE000EFE0)
T0C78 002:877.855   CPU_ReadMem(4 bytes @ 0xE000EFBC)
T0C78 002:878.061   CPU_ReadMem(4 bytes @ 0xE000EFCC)
T0C78 002:878.274   [0][0]: E000E000 CID B105900D PID 000BBD21 DEVARCH 47702A04 DEVTYPE 00 Cortex-M33
T0C78 002:878.280   CPU_ReadMem(32 bytes @ 0xE0001FE0)
T0C78 002:878.625   CPU_ReadMem(4 bytes @ 0xE0001FBC)
T0C78 002:878.935   CPU_ReadMem(4 bytes @ 0xE0001FCC)
T0C78 002:879.149   [0][1]: E0001000 CID B105900D PID 000BBD21 DEVARCH 47701A02 DEVTYPE 00 DWT
T0C78 002:879.155   CPU_ReadMem(32 bytes @ 0xE0002FE0)
T0C78 002:879.501   CPU_ReadMem(4 bytes @ 0xE0002FBC)
T0C78 002:879.811   CPU_ReadMem(4 bytes @ 0xE0002FCC)
T0C78 002:880.038   [0][2]: E0002000 CID B105900D PID 000BBD21 DEVARCH 47701A03 DEVTYPE 00 FPB
T0C78 002:880.045   SetupTarget() start
T0C78 002:880.050    J-Link Script File: Executing SetupTarget()
T0C78 002:880.078   CPU_ReadMem(8192 bytes @ 0x20000000)
T0C78 002:905.283   SetupTarget() end - Took 25.2ms
T0C78 002:905.616   CPU is running
T0C78 002:905.628   CPU_WriteMem(4 bytes @ 0xE000EDF0)
T0C78 002:906.169   CPU_ReadMem(4 bytes @ 0xE000ED44)
T0C78 002:906.590   CPU is running
T0C78 002:906.607   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T0C78 002:906.906   Reset: Halt core after reset via DEMCR.VC_CORERESET.
T0C78 002:907.392   Reset: Reset device via AIRCR.SYSRESETREQ.
T0C78 002:907.401   CPU is running
T0C78 002:907.407   CPU_WriteMem(4 bytes @ 0xE000ED0C)
T0C78 002:962.812   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T0C78 002:963.273   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T0C78 002:966.595   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T0C78 002:973.400   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T0C78 002:975.891   CPU_ReadMem(4 bytes @ 0xE000EE08)
T0C78 002:976.336   CPU_WriteMem(4 bytes @ 0xE0002000)
T0C78 002:976.764   CPU_ReadMem(4 bytes @ 0xE000EDFC)
T0C78 002:977.195   CPU_ReadMem(4 bytes @ 0xE0001000)
T0C78 002:977.522   CPU_ReadMem(4 bytes @ 0xE000EE08)
T0C78 002:977.819 - 116.418ms
T0C78 002:977.856 JLINK_GetId()
T0C78 002:978.081 - 0.225ms returns 0x6BA02477
T0C78 002:979.429 JLINK_GetFirmwareString(...)
T0C78 002:979.441 - 0.011ms
T0C78 003:816.672 JLINK_Close()
T0C78 004:935.061   CPU_ReadMem(4 bytes @ 0xE0001000)
T0C78 004:935.539   CPU_WriteMem(4 bytes @ 0xE0001004)
T0C78 004:937.468 - 1120.797ms
T0C78 004:937.488   
T0C78 004:937.501   Closed
