#

##

##

##

##

##

##

    µVision Build Log
    Tool Versions:
    IDE-Version: ¦ÌVision V5.36.0.0
    Copyright (C) 2021 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: run ma, QQ, LIC=PE7DL-0ZUMX-01NP1-C9RQ7-IMF3F-QU9I5

    Tool Versions:
    Toolchain:       MDK-ARM Plus  Version: 5.36.0.0
    Toolchain Path:  C:\Keil_v5\ARM\ARMCLANG\Bin
    C Compiler:      ArmClang.exe V6.16
    Assembler:       Armasm.exe V6.16
    Linker/Locator:  ArmLink.exe V6.16
    Library Manager: ArmAr.exe V6.16
    Hex Converter:   FromElf.exe V6.16
    CPU DLL:         SARMCM3.DLL V5.36.0.0
    Dialog DLL:      DCM.DLL V1.17.3.0
    Target DLL:      Segger\JL2CM3.dll V2.99.40.0
    Dialog DLL:      TCM.DLL V1.53.0.0

    Project:
    C:\Users\run\Desktop\flash_driver\YTM32B1HA0_Flash_Demo\KEIL\Flash_Demo.uvprojx
    Project File Date:  05/07/2024

    Output:
    *** Using Compiler 'V6.16', folder: 'C:\Keil_v5\ARM\ARMCLANG\Bin'
    Build target 'Flash_Demo'
    compiling RamInit1.c...
    compiling RamInit2.c...
    compiling clock_config.c...
    compiling main.c...
    compiling pin_mux.c...
    assembling startup.S...
    assembling RamInit0.S...
    compiling dma_config.c...
    compiling interrupt_config.c...
    compiling utility_print_config.c...
    assembling vector.S...
    compiling linflexd_uart_config.c...
    compiling vector_table_copy.c...
    compiling pins_port_hw_access.c...
    compiling secure_boot_YTM32B1HA0.c...
    compiling clock_YTM32B1Hx.c...
    compiling pins_driver.c...
    compiling system_YTM32B1HA0.c...
    compiling dma_irq.c...
    compiling interrupt_manager.c...
    compiling linflexd_uart_irq.c...
    compiling osif_baremetal.c...
    compiling dma_hw_access.c...
    compiling dma_driver.c...
    compiling printf.c...
    compiling linflexd_uart_driver.c...
    linking...
    .\Objects\Flash_Demo.axf: Warning: L6319W: Ignoring --keep command. Cannot find section *(.sb_config_group).
    ../board/yt_linker.scf(132): warning: L6329W: Pattern *(.ARM.exidx*) only matches removed unused sections.
    Program Size: Code=9508 RO-data=616 RW-data=1048 ZI-data=132240
    Finished: 0 information, 2 warning and 0 error messages.
    FromELF: creating hex file...
    After Build - User command #1: fromelf --bin --bincombined --output=Objects\Flash_Demo.bin .\Objects\Flash_Demo.axf
    After Build - User command #2: fromelf --m32 --m32combined --output=Objects\Flash_Demo.srec .\Objects\Flash_Demo.axf
    ".\Objects\Flash_Demo.axf" - 0 Error(s), 2 Warning(s).

    Software Packages used:

    Package Vendor: YTMicro
                    https://doc.ytmicro.com/keil/YTMicro.YTM32B1HA0_DFP.1.0.1.pack
                    YTMicro.YTM32B1HA0_DFP.1.0.1
                    Device Family Pack for YTM32B1HA0

    Collection of Component include folders:
      C:\Users\run\AppData\Local\Arm\Packs\YTMicro\YTM32B1HA0_DFP\1.0.1\Device\Include

    Collection of Component Files used:
    Build Time Elapsed:  00:00:02