# Static Call Graph for image .\Objects\Flash_Demo.axf

#<CALLGRAPH># ARM Linker, 6160001: Last Updated: Tue May 7 10:23:38 2024

### Maximum Stack Usage = 6272 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

Reset_Handler ⇒ main ⇒ Board_Init ⇒ CLOCK_SYS_UpdateConfiguration ⇒ CLOCK_SYS_SetConfiguration ⇒ CLOCK_DRV_Init ⇒ CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq

### Functions with no stack information

- RamInit0
- Reset_Handler

### Mutually Recursive functions

- DefaultISR ⇒ DefaultISR

  ### Function Pointers

  - ACMP0_IRQHandler from vector_table_copy.o(.text.ACMP0_IRQHandler) referenced from vector.o(.isr_vector)
  - ACMP1_IRQHandler from vector_table_copy.o(.text.ACMP1_IRQHandler) referenced from vector.o(.isr_vector)
  - ADC0_IRQHandler from vector_table_copy.o(.text.ADC0_IRQHandler) referenced from vector.o(.isr_vector)
  - ADC1_IRQHandler from vector_table_copy.o(.text.ADC1_IRQHandler) referenced from vector.o(.isr_vector)
  - BusFault_Handler from vector_table_copy.o(.text.BusFault_Handler) referenced from vector.o(.isr_vector)
  - CAN0_Error_IRQHandler from vector_table_copy.o(.text.CAN0_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_112_127_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_112_127_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_64_79_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_64_79_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_80_95_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_80_95_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_96_111_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_96_111_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_BusOff_Warning_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_BusOff_Warning_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN0_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_Error_IRQHandler from vector_table_copy.o(.text.CAN1_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_112_127_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_112_127_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_64_79_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_64_79_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_80_95_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_80_95_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_96_111_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_96_111_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_BusOff_Warning_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_BusOff_Warning_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN1_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_Error_IRQHandler from vector_table_copy.o(.text.CAN2_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_BusOff_Warning_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_BusOff_Warning_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN2_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_Error_IRQHandler from vector_table_copy.o(.text.CAN3_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_BusOff_Warning_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_BusOff_Warning_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN3_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_Error_IRQHandler from vector_table_copy.o(.text.CAN4_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_BusOff_Warning_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_BusOff_Warning_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN4_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_Error_IRQHandler from vector_table_copy.o(.text.CAN5_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN5_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN5_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_ORed_BusOff_Warning_IRQHandler from vector_table_copy.o(.text.CAN5_ORed_BusOff_Warning_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN5_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN6_Error_IRQHandler from vector_table_copy.o(.text.CAN6_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN6_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN6_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN6_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN6_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN6_ORed_BusOff_Warning_IRQHandler from vector_table_copy.o(.text.CAN6_ORed_BusOff_Warning_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN6_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN6_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN7_Error_IRQHandler from vector_table_copy.o(.text.CAN7_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN7_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN7_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN7_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN7_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN7_ORed_BusOff_Warning_IRQHandler from vector_table_copy.o(.text.CAN7_ORed_BusOff_Warning_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN7_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN7_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CMU_IRQHandler from vector_table_copy.o(.text.CMU_IRQHandler) referenced from vector.o(.isr_vector)
  - CORE_CTI_IRQHandler from vector_table_copy.o(.text.CORE_CTI_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA0_IRQHandler from dma_irq.o(.text.DMA0_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA10_IRQHandler from dma_irq.o(.text.DMA10_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA11_IRQHandler from dma_irq.o(.text.DMA11_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA12_IRQHandler from dma_irq.o(.text.DMA12_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA13_IRQHandler from dma_irq.o(.text.DMA13_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA14_IRQHandler from dma_irq.o(.text.DMA14_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA15_IRQHandler from dma_irq.o(.text.DMA15_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA16_IRQHandler from dma_irq.o(.text.DMA16_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA17_IRQHandler from dma_irq.o(.text.DMA17_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA18_IRQHandler from dma_irq.o(.text.DMA18_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA19_IRQHandler from dma_irq.o(.text.DMA19_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA1_IRQHandler from dma_irq.o(.text.DMA1_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA20_IRQHandler from dma_irq.o(.text.DMA20_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA21_IRQHandler from dma_irq.o(.text.DMA21_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA22_IRQHandler from dma_irq.o(.text.DMA22_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA23_IRQHandler from dma_irq.o(.text.DMA23_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA24_IRQHandler from dma_irq.o(.text.DMA24_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA25_IRQHandler from dma_irq.o(.text.DMA25_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA26_IRQHandler from dma_irq.o(.text.DMA26_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA27_IRQHandler from dma_irq.o(.text.DMA27_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA28_IRQHandler from dma_irq.o(.text.DMA28_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA29_IRQHandler from dma_irq.o(.text.DMA29_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA2_IRQHandler from dma_irq.o(.text.DMA2_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA30_IRQHandler from dma_irq.o(.text.DMA30_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA31_IRQHandler from dma_irq.o(.text.DMA31_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA3_IRQHandler from dma_irq.o(.text.DMA3_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA4_IRQHandler from dma_irq.o(.text.DMA4_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA5_IRQHandler from dma_irq.o(.text.DMA5_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA6_IRQHandler from dma_irq.o(.text.DMA6_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA7_IRQHandler from dma_irq.o(.text.DMA7_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA8_IRQHandler from dma_irq.o(.text.DMA8_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA9_IRQHandler from dma_irq.o(.text.DMA9_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA_Error_IRQHandler from dma_irq.o(.text.DMA_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - DebugMon_Handler from vector_table_copy.o(.text.DebugMon_Handler) referenced from vector.o(.isr_vector)
  - DefaultISR from vector_table_copy.o(.text.DefaultISR) referenced 26 times from vector.o(.isr_vector)
  - EFM_Ecc_IRQHandler from vector_table_copy.o(.text.EFM_Ecc_IRQHandler) referenced from vector.o(.isr_vector)
  - EFM_Error_IRQHandler from vector_table_copy.o(.text.EFM_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - EFM_IRQHandler from vector_table_copy.o(.text.EFM_IRQHandler) referenced from vector.o(.isr_vector)
  - EMU_IRQHandler from vector_table_copy.o(.text.EMU_IRQHandler) referenced from vector.o(.isr_vector)
  - ENET_ECC_IRQHandler from vector_table_copy.o(.text.ENET_ECC_IRQHandler) referenced from vector.o(.isr_vector)
  - ENET_IRQHandler from vector_table_copy.o(.text.ENET_IRQHandler) referenced from vector.o(.isr_vector)
  - ENET_RX_IRQHandler from vector_table_copy.o(.text.ENET_RX_IRQHandler) referenced from vector.o(.isr_vector)
  - ENET_TX_IRQHandler from vector_table_copy.o(.text.ENET_TX_IRQHandler) referenced from vector.o(.isr_vector)
  - FMU_Alarm_IRQHandler from vector_table_copy.o(.text.FMU_Alarm_IRQHandler) referenced from vector.o(.isr_vector)
  - FMU_MISC_IRQHandler from vector_table_copy.o(.text.FMU_MISC_IRQHandler) referenced from vector.o(.isr_vector)
  - FPU_IRQHandler from vector_table_copy.o(.text.FPU_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOA_IRQHandler from vector_table_copy.o(.text.GPIOA_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOB_IRQHandler from vector_table_copy.o(.text.GPIOB_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOC_IRQHandler from vector_table_copy.o(.text.GPIOC_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOD_IRQHandler from vector_table_copy.o(.text.GPIOD_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOE_IRQHandler from vector_table_copy.o(.text.GPIOE_IRQHandler) referenced from vector.o(.isr_vector)
  - HCU_IRQHandler from vector_table_copy.o(.text.HCU_IRQHandler) referenced from vector.o(.isr_vector)
  - HardFault_Handler from vector_table_copy.o(.text.HardFault_Handler) referenced from vector.o(.isr_vector)
  - I2C0_Master_Slave_IRQHandler from vector_table_copy.o(.text.I2C0_Master_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C1_Master_Slave_IRQHandler from vector_table_copy.o(.text.I2C1_Master_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C2_Master_Slave_IRQHandler from vector_table_copy.o(.text.I2C2_Master_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C3_Master_Slave_IRQHandler from vector_table_copy.o(.text.I2C3_Master_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C4_Master_Slave_IRQHandler from vector_table_copy.o(.text.I2C4_Master_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - INTM_IRQHandler from vector_table_copy.o(.text.INTM_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD0_IRQHandler from vector_table_copy.o(.text.LINFlexD0_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD0_UART_IRQHandler from linflexd_uart_irq.o(.text.LINFlexD0_UART_IRQHandler) referenced from linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)
  - LINFlexD1_IRQHandler from vector_table_copy.o(.text.LINFlexD1_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD1_UART_IRQHandler from linflexd_uart_irq.o(.text.LINFlexD1_UART_IRQHandler) referenced from linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)
  - LINFlexD2_IRQHandler from vector_table_copy.o(.text.LINFlexD2_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD2_UART_IRQHandler from linflexd_uart_irq.o(.text.LINFlexD2_UART_IRQHandler) referenced from linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)
  - LINFlexD3_IRQHandler from vector_table_copy.o(.text.LINFlexD3_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD3_UART_IRQHandler from linflexd_uart_irq.o(.text.LINFlexD3_UART_IRQHandler) referenced from linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)
  - LINFlexD4_IRQHandler from vector_table_copy.o(.text.LINFlexD4_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD4_UART_IRQHandler from linflexd_uart_irq.o(.text.LINFlexD4_UART_IRQHandler) referenced from linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)
  - LINFlexD5_IRQHandler from vector_table_copy.o(.text.LINFlexD5_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD5_UART_IRQHandler from linflexd_uart_irq.o(.text.LINFlexD5_UART_IRQHandler) referenced from linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)
  - LINFlexD6_IRQHandler from vector_table_copy.o(.text.LINFlexD6_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD7_IRQHandler from vector_table_copy.o(.text.LINFlexD7_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD8_IRQHandler from vector_table_copy.o(.text.LINFlexD8_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD9_IRQHandler from vector_table_copy.o(.text.LINFlexD9_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch0_Ch7_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch0_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch8_Ch15_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch8_Ch15_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM1_Ch0_Ch7_IRQHandler from vector_table_copy.o(.text.MPWM1_Ch0_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM1_Ch8_Ch15_IRQHandler from vector_table_copy.o(.text.MPWM1_Ch8_Ch15_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM2_Ch0_Ch7_IRQHandler from vector_table_copy.o(.text.MPWM2_Ch0_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM2_Ch8_Ch15_IRQHandler from vector_table_copy.o(.text.MPWM2_Ch8_Ch15_IRQHandler) referenced from vector.o(.isr_vector)
  - MemManage_Handler from vector_table_copy.o(.text.MemManage_Handler) referenced from vector.o(.isr_vector)
  - NMI_Handler from vector_table_copy.o(.text.NMI_Handler) referenced from vector.o(.isr_vector)
  - PCU_IRQHandler from vector_table_copy.o(.text.PCU_IRQHandler) referenced from vector.o(.isr_vector)
  - PTU0_IRQHandler from vector_table_copy.o(.text.PTU0_IRQHandler) referenced from vector.o(.isr_vector)
  - PTU1_IRQHandler from vector_table_copy.o(.text.PTU1_IRQHandler) referenced from vector.o(.isr_vector)
  - PendSV_Handler from vector_table_copy.o(.text.PendSV_Handler) referenced from vector.o(.isr_vector)
  - QSPI_IRQHandler from vector_table_copy.o(.text.QSPI_IRQHandler) referenced from vector.o(.isr_vector)
  - RTC_IRQHandler from vector_table_copy.o(.text.RTC_IRQHandler) referenced from vector.o(.isr_vector)
  - RTC_Seconds_IRQHandler from vector_table_copy.o(.text.RTC_Seconds_IRQHandler) referenced from vector.o(.isr_vector)
  - RamInit1 from raminit1.o(.text.RamInit1) referenced from startup.o(.text)
  - RamInit2 from raminit2.o(.text.RamInit2) referenced from startup.o(.text)
  - Reset_Handler from startup.o(.text) referenced from vector.o(.isr_vector)
  - SAI0_IRQHandler from vector_table_copy.o(.text.SAI0_IRQHandler) referenced from vector.o(.isr_vector)
  - SAI1_IRQHandler from vector_table_copy.o(.text.SAI1_IRQHandler) referenced from vector.o(.isr_vector)
  - SENT0_IRQHandler from vector_table_copy.o(.text.SENT0_IRQHandler) referenced from vector.o(.isr_vector)
  - SENT1_IRQHandler from vector_table_copy.o(.text.SENT1_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI0_IRQHandler from vector_table_copy.o(.text.SPI0_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI1_IRQHandler from vector_table_copy.o(.text.SPI1_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI2_IRQHandler from vector_table_copy.o(.text.SPI2_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI3_IRQHandler from vector_table_copy.o(.text.SPI3_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI4_IRQHandler from vector_table_copy.o(.text.SPI4_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI5_IRQHandler from vector_table_copy.o(.text.SPI5_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI6_IRQHandler from vector_table_copy.o(.text.SPI6_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI7_IRQHandler from vector_table_copy.o(.text.SPI7_IRQHandler) referenced from vector.o(.isr_vector)
  - SVC_Handler from vector_table_copy.o(.text.SVC_Handler) referenced from vector.o(.isr_vector)
  - SysTick_Handler from osif_baremetal.o(.text.SysTick_Handler) referenced from vector.o(.isr_vector)
  - SystemInit from system_ytm32b1ha0.o(.text.SystemInit) referenced from startup.o(.text)
  - TMR0_IRQHandler from vector_table_copy.o(.text.TMR0_IRQHandler) referenced from vector.o(.isr_vector)
  - TMR1_IRQHandler from vector_table_copy.o(.text.TMR1_IRQHandler) referenced from vector.o(.isr_vector)
  - TRNG_IRQHandler from vector_table_copy.o(.text.TRNG_IRQHandler) referenced from vector.o(.isr_vector)
  - UsageFault_Handler from vector_table_copy.o(.text.UsageFault_Handler) referenced from vector.o(.isr_vector)
  - VectorTableCopy from vector_table_copy.o(.text.VectorTableCopy) referenced from startup.o(.text)
  - WDG_IRQHandler from vector_table_copy.o(.text.WDG_IRQHandler) referenced from vector.o(.isr_vector)
  - WKU_IRQHandler from vector_table_copy.o(.text.WKU_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Fault_IRQHandler from vector_table_copy.o(.text.eTMR0_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR0_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Fault_IRQHandler from vector_table_copy.o(.text.eTMR1_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR1_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR2_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR2_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR2_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR2_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Fault_IRQHandler from vector_table_copy.o(.text.eTMR2_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR2_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR3_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR3_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR3_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR3_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Fault_IRQHandler from vector_table_copy.o(.text.eTMR3_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR3_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR4_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR4_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR4_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR4_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Fault_IRQHandler from vector_table_copy.o(.text.eTMR4_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR4_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR5_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR5_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR5_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR5_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Fault_IRQHandler from vector_table_copy.o(.text.eTMR5_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR5_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - lpTMR0_IRQHandler from vector_table_copy.o(.text.lpTMR0_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR0_Ch0_IRQHandler from vector_table_copy.o(.text.pTMR0_Ch0_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR0_Ch1_IRQHandler from vector_table_copy.o(.text.pTMR0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR0_Ch2_IRQHandler from vector_table_copy.o(.text.pTMR0_Ch2_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR0_Ch3_IRQHandler from vector_table_copy.o(.text.pTMR0_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR1_Ch0_IRQHandler from vector_table_copy.o(.text.pTMR1_Ch0_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR1_Ch1_IRQHandler from vector_table_copy.o(.text.pTMR1_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR1_Ch2_IRQHandler from vector_table_copy.o(.text.pTMR1_Ch2_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR1_Ch3_IRQHandler from vector_table_copy.o(.text.pTMR1_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR2_Ch0_IRQHandler from vector_table_copy.o(.text.pTMR2_Ch0_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR2_Ch1_IRQHandler from vector_table_copy.o(.text.pTMR2_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR2_Ch2_IRQHandler from vector_table_copy.o(.text.pTMR2_Ch2_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR2_Ch3_IRQHandler from vector_table_copy.o(.text.pTMR2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)

  ### Global Symbols

  RamInit0 (Thumb, 0 bytes, Stack size unknown bytes, raminit0.o(.text))
  [Called By]

  - >> Reset_Handler

  Reset_Handler (Thumb, 0 bytes, Stack size unknown bytes, startup.o(.text))
  [Stack]

  - Max Depth = 6272 + Unknown Stack Size
  - Call Chain = Reset_Handler ⇒ main ⇒ Board_Init ⇒ CLOCK_SYS_UpdateConfiguration ⇒ CLOCK_SYS_SetConfiguration ⇒ CLOCK_DRV_Init ⇒ CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> RamInit0
  - >> main
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> VectorTableCopy

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text))
  [Calls]

  - >> __aeabi_memset
  [Called By]
  - >> LINFlexD_UART_DRV_Init

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> RamInit1

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  ACMP0_IRQHandler (Thumb, 0 bytes, Stack size 8 bytes, vector_table_copy.o(.text.ACMP0_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = ACMP0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  ACMP1_IRQHandler (Thumb, 0 bytes, Stack size 8 bytes, vector_table_copy.o(.text.ACMP1_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = ACMP1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  ADC0_IRQHandler (Thumb, 0 bytes, Stack size 8 bytes, vector_table_copy.o(.text.ADC0_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  ADC1_IRQHandler (Thumb, 0 bytes, Stack size 8 bytes, vector_table_copy.o(.text.ADC1_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  BusFault_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.BusFault_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_112_127_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_112_127_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_32_47_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_32_47_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_48_63_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_48_63_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_64_79_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_64_79_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_80_95_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_80_95_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_96_111_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_96_111_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_BusOff_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_BusOff_Warning_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_112_127_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_112_127_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_32_47_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_32_47_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_48_63_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_48_63_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_64_79_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_64_79_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_80_95_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_80_95_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_96_111_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_96_111_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_BusOff_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_BusOff_Warning_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN2_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN2_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN2_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN2_ORed_32_47_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_32_47_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN2_ORed_48_63_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_48_63_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN2_ORed_BusOff_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_BusOff_Warning_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN2_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN3_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN3_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN3_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN3_ORed_32_47_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_32_47_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN3_ORed_48_63_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_48_63_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN3_ORed_BusOff_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_BusOff_Warning_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN3_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN4_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN4_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN4_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN4_ORed_32_47_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_32_47_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN4_ORed_48_63_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_48_63_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN4_ORed_BusOff_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_BusOff_Warning_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN4_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN5_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN5_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN5_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN5_ORed_BusOff_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_ORed_BusOff_Warning_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN5_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN6_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN6_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN6_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN6_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN6_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN6_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN6_ORed_BusOff_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN6_ORed_BusOff_Warning_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN6_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN6_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN7_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN7_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN7_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN7_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN7_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN7_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN7_ORed_BusOff_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN7_ORed_BusOff_Warning_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN7_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN7_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CLOCK_DRV_GetFreq (Thumb, 370 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.CLOCK_DRV_GetFreq))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> CLOCK_DRV_GetPllFreq
  - >> SCU_GetSysClkSrc
  - >> SCU_GetSysClkDiv
  - >> SCU_GetSlowBusClkDiv
  - >> SCU_GetFastBusClkDiv
  [Called By]
  - >> CLOCK_SYS_GetFreq

  CLOCK_DRV_GetPllFreq (Thumb, 68 bytes, Stack size 16 bytes, clock_ytm32b1hx.o(.text.CLOCK_DRV_GetPllFreq))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_DRV_GetPllFreq
  [Calls]
  - >> SCU_GetPllRefClkDiv
  - >> SCU_GetPllRefClk
  - >> SCU_GetPllLock
  - >> SCU_GetPllFeedBackDiv
  [Called By]
  - >> CLOCK_DRV_GetFreq
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_DRV_Init (Thumb, 24 bytes, Stack size 8 bytes, clock_ytm32b1hx.o(.text.CLOCK_DRV_Init))
  [Stack]

  - Max Depth = 56
  - Call Chain = CLOCK_DRV_Init ⇒ CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> CLOCK_SYS_SetScuConfiguration
  - >> CLOCK_SYS_SetIpcConfiguration
  [Called By]
  - >> CLOCK_SYS_SetConfiguration

  CLOCK_SYS_GetFreq (Thumb, 8 bytes, Stack size 8 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_GetFreq))
  [Stack]

  - Max Depth = 24
  - Call Chain = CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> CLOCK_DRV_GetFreq
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration
  - >> LINFlexD_UART_DRV_Init
  - >> LINFlexD_UART_DRV_SetBaudRate

  CLOCK_SYS_Init (Thumb, 56 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_Init))
  [Called By]

  - >> Board_Init

  CLOCK_SYS_SetConfiguration (Thumb, 8 bytes, Stack size 8 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_SetConfiguration))
  [Stack]

  - Max Depth = 64
  - Call Chain = CLOCK_SYS_SetConfiguration ⇒ CLOCK_DRV_Init ⇒ CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> CLOCK_DRV_Init
  [Called By]
  - >> CLOCK_SYS_UpdateConfiguration

  CLOCK_SYS_UpdateConfiguration (Thumb, 352 bytes, Stack size 40 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_UpdateConfiguration))
  [Stack]

  - Max Depth = 104
  - Call Chain = CLOCK_SYS_UpdateConfiguration ⇒ CLOCK_SYS_SetConfiguration ⇒ CLOCK_DRV_Init ⇒ CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> CLOCK_SYS_SetConfiguration
  - >> INT_SYS_EnableIRQGlobal
  - >> INT_SYS_DisableIRQGlobal
  [Called By]
  - >> Board_Init

  CMU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CMU_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CORE_CTI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CORE_CTI_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA0_IRQHandler (Thumb, 10 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA0_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA0_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA10_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA10_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA10_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA11_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA11_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA11_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA12_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA12_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA12_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA13_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA13_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA13_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA14_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA14_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA14_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA15_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA15_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA15_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA16_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA16_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA16_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA17_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA17_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA17_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA18_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA18_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA18_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA19_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA19_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA19_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA1_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA1_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA1_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA20_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA20_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA20_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA21_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA21_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA21_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA22_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA22_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA22_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA23_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA23_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA23_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA24_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA24_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA24_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA25_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA25_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA25_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA26_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA26_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA26_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA27_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA27_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA27_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA28_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA28_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA28_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA29_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA29_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA29_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA2_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA2_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA2_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA30_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA30_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA30_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA31_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA31_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA31_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA3_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA3_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA3_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA4_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA4_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA4_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA5_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA5_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA5_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA6_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA6_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA6_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA7_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA7_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA7_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA8_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA8_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA8_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA9_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA9_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA9_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA_CTSSetTriggerCount (Thumb, 70 bytes, Stack size 0 bytes, dma_hw_access.o(.text.DMA_CTSSetTriggerCount))
  [Called By]

  - >> DMA_DRV_SetTriggerLoopIterationCount

  DMA_DRV_ErrorIRQHandler (Thumb, 74 bytes, Stack size 16 bytes, dma_driver.o(.text.DMA_DRV_ErrorIRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA_DRV_ErrorIRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_ClearIntStatus
  - >> DMA_ClearErrorIntStatusFlag
  - >> DMA_SetDmaRequestCmd
  [Called By]
  - >> DMA_Error_IRQHandler

  DMA_DRV_GetDmaRegBaseAddr (Thumb, 8 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_DRV_GetDmaRegBaseAddr))
  [Called By]

  - >> DMA_Error_IRQHandler

  DMA_DRV_IRQHandler (Thumb, 38 bytes, Stack size 8 bytes, dma_driver.o(.text.DMA_DRV_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_ClearIntStatus
  [Called By]
  - >> DMA9_IRQHandler
  - >> DMA8_IRQHandler
  - >> DMA7_IRQHandler
  - >> DMA6_IRQHandler
  - >> DMA5_IRQHandler
  - >> DMA4_IRQHandler
  - >> DMA3_IRQHandler
  - >> DMA31_IRQHandler
  - >> DMA30_IRQHandler
  - >> DMA2_IRQHandler
  - >> DMA29_IRQHandler
  - >> DMA28_IRQHandler
  - >> DMA27_IRQHandler
  - >> DMA26_IRQHandler
  - >> DMA25_IRQHandler
  - >> DMA24_IRQHandler
  - >> DMA23_IRQHandler
  - >> DMA22_IRQHandler
  - >> DMA21_IRQHandler
  - >> DMA20_IRQHandler
  - >> DMA1_IRQHandler
  - >> DMA19_IRQHandler
  - >> DMA18_IRQHandler
  - >> DMA17_IRQHandler
  - >> DMA16_IRQHandler
  - >> DMA15_IRQHandler
  - >> DMA14_IRQHandler
  - >> DMA13_IRQHandler
  - >> DMA12_IRQHandler
  - >> DMA11_IRQHandler
  - >> DMA10_IRQHandler
  - >> DMA0_IRQHandler

  DMA_DRV_SetDestAddr (Thumb, 20 bytes, Stack size 8 bytes, dma_driver.o(.text.DMA_DRV_SetDestAddr))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_DRV_SetDestAddr
  [Calls]
  - >> DMA_CTSSetDestAddr
  [Called By]
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingDma

  DMA_DRV_SetTriggerLoopIterationCount (Thumb, 20 bytes, Stack size 8 bytes, dma_driver.o(.text.DMA_DRV_SetTriggerLoopIterationCount))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_DRV_SetTriggerLoopIterationCount
  [Calls]
  - >> DMA_CTSSetTriggerCount
  [Called By]
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingDma

  DMA_DRV_StartChannel (Thumb, 22 bytes, Stack size 8 bytes, dma_driver.o(.text.DMA_DRV_StartChannel))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_DRV_StartChannel
  [Calls]
  - >> DMA_SetDmaRequestCmd
  [Called By]
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingDma

  DMA_DRV_StopChannel (Thumb, 22 bytes, Stack size 8 bytes, dma_driver.o(.text.DMA_DRV_StopChannel))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_DRV_StopChannel
  [Calls]
  - >> DMA_SetDmaRequestCmd
  [Called By]
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingDma

  DMA_Error_IRQHandler (Thumb, 46 bytes, Stack size 16 bytes, dma_irq.o(.text.DMA_Error_IRQHandler))
  [Stack]

  - Max Depth = 48
  - Call Chain = DMA_Error_IRQHandler ⇒ DMA_DRV_ErrorIRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_ErrorIRQHandler
  - >> DMA_GetErrorIntStatusFlag
  - >> DMA_DRV_GetDmaRegBaseAddr
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA_SetDmaRequestCmd (Thumb, 22 bytes, Stack size 0 bytes, dma_hw_access.o(.text.DMA_SetDmaRequestCmd))
  [Called By]

  - >> DMA_DRV_ErrorIRQHandler
  - >> DMA_DRV_StopChannel
  - >> DMA_DRV_StartChannel

  DebugMon_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DebugMon_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DefaultISR (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DefaultISR))
  [Calls]

  - >> DefaultISR
  [Called By]
  - >> DefaultISR
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  EFM_Ecc_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_Ecc_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  EFM_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  EFM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  EMU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EMU_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  ENET_ECC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ENET_ECC_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  ENET_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ENET_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  ENET_RX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ENET_RX_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  ENET_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ENET_TX_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  FMU_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.FMU_Alarm_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  FMU_MISC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.FMU_MISC_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.FPU_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOA_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOC_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOD_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOE_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  HCU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.HCU_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  HardFault_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.HardFault_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  I2C0_Master_Slave_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C0_Master_Slave_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  I2C1_Master_Slave_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C1_Master_Slave_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  I2C2_Master_Slave_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C2_Master_Slave_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  I2C3_Master_Slave_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C3_Master_Slave_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  I2C4_Master_Slave_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C4_Master_Slave_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  INTM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.INTM_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  INT_SYS_DisableIRQGlobal (Thumb, 18 bytes, Stack size 0 bytes, interrupt_manager.o(.text.INT_SYS_DisableIRQGlobal))
  [Called By]

  - >> CLOCK_SYS_UpdateConfiguration
  - >> osif_DisableIrqGlobal

  INT_SYS_EnableIRQ (Thumb, 8 bytes, Stack size 8 bytes, interrupt_manager.o(.text.INT_SYS_EnableIRQ))
  [Stack]

  - Max Depth = 8
  - Call Chain = INT_SYS_EnableIRQ
  [Calls]
  - >> __NVIC_EnableIRQ
  [Called By]
  - >> LINFlexD_UART_DRV_Init

  INT_SYS_EnableIRQGlobal (Thumb, 28 bytes, Stack size 0 bytes, interrupt_manager.o(.text.INT_SYS_EnableIRQGlobal))
  [Called By]

  - >> CLOCK_SYS_UpdateConfiguration
  - >> osif_EnableIrqGlobal

  INT_SYS_InstallHandler (Thumb, 128 bytes, Stack size 16 bytes, interrupt_manager.o(.text.INT_SYS_InstallHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = INT_SYS_InstallHandler
  [Called By]
  - >> LINFlexD_UART_DRV_Init

  LINFlexD0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD0_UART_IRQHandler (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_irq.o(.text.LINFlexD0_UART_IRQHandler))
  [Stack]

  - Max Depth = 64
  - Call Chain = LINFlexD0_UART_IRQHandler ⇒ LINFlexD_UART_DRV_IRQHandler ⇒ LINFlexD_UART_DRV_TxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> LINFlexD_UART_DRV_IRQHandler
  [Address Reference Count : 1]
  - linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)

  LINFlexD1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD1_UART_IRQHandler (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_irq.o(.text.LINFlexD1_UART_IRQHandler))
  [Stack]

  - Max Depth = 64
  - Call Chain = LINFlexD1_UART_IRQHandler ⇒ LINFlexD_UART_DRV_IRQHandler ⇒ LINFlexD_UART_DRV_TxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> LINFlexD_UART_DRV_IRQHandler
  [Address Reference Count : 1]
  - linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)

  LINFlexD2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD2_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD2_UART_IRQHandler (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_irq.o(.text.LINFlexD2_UART_IRQHandler))
  [Stack]

  - Max Depth = 64
  - Call Chain = LINFlexD2_UART_IRQHandler ⇒ LINFlexD_UART_DRV_IRQHandler ⇒ LINFlexD_UART_DRV_TxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> LINFlexD_UART_DRV_IRQHandler
  [Address Reference Count : 1]
  - linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)

  LINFlexD3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD3_UART_IRQHandler (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_irq.o(.text.LINFlexD3_UART_IRQHandler))
  [Stack]

  - Max Depth = 64
  - Call Chain = LINFlexD3_UART_IRQHandler ⇒ LINFlexD_UART_DRV_IRQHandler ⇒ LINFlexD_UART_DRV_TxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> LINFlexD_UART_DRV_IRQHandler
  [Address Reference Count : 1]
  - linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)

  LINFlexD4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD4_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD4_UART_IRQHandler (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_irq.o(.text.LINFlexD4_UART_IRQHandler))
  [Stack]

  - Max Depth = 64
  - Call Chain = LINFlexD4_UART_IRQHandler ⇒ LINFlexD_UART_DRV_IRQHandler ⇒ LINFlexD_UART_DRV_TxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> LINFlexD_UART_DRV_IRQHandler
  [Address Reference Count : 1]
  - linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)

  LINFlexD5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD5_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD5_UART_IRQHandler (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_irq.o(.text.LINFlexD5_UART_IRQHandler))
  [Stack]

  - Max Depth = 64
  - Call Chain = LINFlexD5_UART_IRQHandler ⇒ LINFlexD_UART_DRV_IRQHandler ⇒ LINFlexD_UART_DRV_TxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> LINFlexD_UART_DRV_IRQHandler
  [Address Reference Count : 1]
  - linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)

  LINFlexD6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD6_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD7_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD8_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD9_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD_UART_DRV_ErrIRQHandler (Thumb, 124 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_ErrIRQHandler))
  [Stack]

  - Max Depth = 48
  - Call Chain = LINFlexD_UART_DRV_ErrIRQHandler ⇒ LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts ⇒ OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingDma
  - >> LINFlexD_GetStatusFlag
  - >> LINFlexD_ClearStatusFlag
  [Called By]
  - >> LINFlexD_UART_DRV_IRQHandler

  LINFlexD_UART_DRV_IRQHandler (Thumb, 120 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_IRQHandler))
  [Stack]

  - Max Depth = 64
  - Call Chain = LINFlexD_UART_DRV_IRQHandler ⇒ LINFlexD_UART_DRV_TxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> LINFlexD_UART_DRV_TxIRQHandler
  - >> LINFlexD_UART_DRV_RxTOHandler
  - >> LINFlexD_UART_DRV_RxIRQHandler
  - >> LINFlexD_UART_DRV_ErrIRQHandler
  - >> LINFlexD_IsInterruptEnabled
  - >> LINFlexD_GetStatusFlag
  [Called By]
  - >> LINFlexD5_UART_IRQHandler
  - >> LINFlexD4_UART_IRQHandler
  - >> LINFlexD3_UART_IRQHandler
  - >> LINFlexD2_UART_IRQHandler
  - >> LINFlexD1_UART_IRQHandler
  - >> LINFlexD0_UART_IRQHandler

  LINFlexD_UART_DRV_Init (Thumb, 336 bytes, Stack size 32 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = LINFlexD_UART_DRV_Init ⇒ LINFlexD_UART_DRV_SetBaudRate ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> INT_SYS_InstallHandler
  - >> INT_SYS_EnableIRQ
  - >> CLOCK_SYS_GetFreq
  - >> __aeabi_memclr
  - >> OSIF_SemaCreate
  - >> LINFlexD_UART_DRV_SetBaudRate
  - >> LINFlexD_SetUartWordLength
  - >> LINFlexD_SetTxStopBitsCount
  - >> LINFlexD_SetTxMode
  - >> LINFlexD_SetTxDataFieldLength
  - >> LINFlexD_SetRxStopBitsCount
  - >> LINFlexD_SetRxMode
  - >> LINFlexD_SetRxDataFieldLength
  - >> LINFlexD_SetParityType
  - >> LINFlexD_SetParityControl
  - >> LINFlexD_SetMonitorIdleState
  - >> LINFlexD_SetMode
  - >> LINFlexD_SetInterruptMode
  - >> LINFlexD_SetDisableTimeout
  - >> LINFlexD_GetLinState
  - >> LINFlexD_EnterNormalMode
  - >> LINFlexD_EnterInitMode
  [Called By]
  - >> UTILITY_PRINT_Init

  LINFlexD_UART_DRV_RxIRQHandler (Thumb, 130 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_RxIRQHandler))
  [Stack]

  - Max Depth = 48
  - Call Chain = LINFlexD_UART_DRV_RxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts ⇒ OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> LINFlexD_UART_DRV_GetData
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts
  - >> LINFlexD_SetInterruptMode
  - >> LINFlexD_ClearStatusFlag
  [Called By]
  - >> LINFlexD_UART_DRV_IRQHandler

  LINFlexD_UART_DRV_RxTOHandler (Thumb, 70 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_RxTOHandler))
  [Stack]

  - Max Depth = 48
  - Call Chain = LINFlexD_UART_DRV_RxTOHandler ⇒ LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts ⇒ OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts
  - >> LINFlexD_ClearStatusFlag
  [Called By]
  - >> LINFlexD_UART_DRV_IRQHandler

  LINFlexD_UART_DRV_SendDataPolling (Thumb, 156 bytes, Stack size 24 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_SendDataPolling))
  [Stack]

  - Max Depth = 40
  - Call Chain = LINFlexD_UART_DRV_SendDataPolling ⇒ LINFlexD_UART_DRV_PutData
  [Calls]
  - >> LINFlexD_UART_DRV_PutData
  - >> LINFlexD_SetTransmitterState
  - >> LINFlexD_GetStatusFlag
  - >> LINFlexD_ClearStatusFlag
  [Called By]
  - >> printf_char

  LINFlexD_UART_DRV_SetBaudRate (Thumb, 210 bytes, Stack size 24 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_SetBaudRate))
  [Stack]

  - Max Depth = 48
  - Call Chain = LINFlexD_UART_DRV_SetBaudRate ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> CLOCK_SYS_GetFreq
  - >> LINFlexD_SetIntegerBaudRate
  - >> LINFlexD_SetFractionalBaudRate
  - >> LINFlexD_GetLinState
  - >> LINFlexD_EnterNormalMode
  - >> LINFlexD_EnterInitMode
  [Called By]
  - >> LINFlexD_UART_DRV_Init

  LINFlexD_UART_DRV_TxIRQHandler (Thumb, 100 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_TxIRQHandler))
  [Stack]

  - Max Depth = 48
  - Call Chain = LINFlexD_UART_DRV_TxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> LINFlexD_UART_DRV_PutData
  - >> LINFlexD_UART_DRV_CompleteSendUsingInterrupts
  - >> LINFlexD_ClearStatusFlag
  [Called By]
  - >> LINFlexD_UART_DRV_IRQHandler

  MPWM0_Ch0_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch0_Ch7_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM0_Ch8_Ch15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch8_Ch15_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM1_Ch0_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM1_Ch0_Ch7_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM1_Ch8_Ch15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM1_Ch8_Ch15_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM2_Ch0_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM2_Ch0_Ch7_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM2_Ch8_Ch15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM2_Ch8_Ch15_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MemManage_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MemManage_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  NMI_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.NMI_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  OSIF_SemaCreate (Thumb, 20 bytes, Stack size 0 bytes, osif_baremetal.o(.text.OSIF_SemaCreate))
  [Stack]

  - Max Depth = 8
  - Call Chain = OSIF_SemaCreate ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> osif_EnableIrqGlobal
  - >> osif_DisableIrqGlobal
  [Called By]
  - >> LINFlexD_UART_DRV_Init

  OSIF_SemaPost (Thumb, 34 bytes, Stack size 8 bytes, osif_baremetal.o(.text.OSIF_SemaPost))
  [Stack]

  - Max Depth = 16
  - Call Chain = OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> osif_EnableIrqGlobal
  - >> osif_DisableIrqGlobal
  [Called By]
  - >> LINFlexD_UART_DRV_CompleteSendUsingInterrupts
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingDma

  PCU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.PCU_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  PINS_DRV_Init (Thumb, 26 bytes, Stack size 16 bytes, pins_driver.o(.text.PINS_DRV_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = PINS_DRV_Init ⇒ PINS_Init ⇒ PINS_GPIO_WritePin
  [Calls]
  - >> PINS_Init
  [Called By]
  - >> Board_Init

  PINS_Init (Thumb, 264 bytes, Stack size 16 bytes, pins_port_hw_access.o(.text.PINS_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = PINS_Init ⇒ PINS_GPIO_WritePin
  [Calls]
  - >> PINS_GPIO_WritePin
  - >> PINS_ConfigDigitalFilter
  [Called By]
  - >> PINS_DRV_Init

  PRINTF (Thumb, 216 bytes, Stack size 32 bytes, printf.o(.text.PRINTF))
  [Stack]

  - Max Depth = 104
  - Call Chain = PRINTF ⇒ printf_dec ⇒ printf_char ⇒ LINFlexD_UART_DRV_SendDataPolling ⇒ LINFlexD_UART_DRV_PutData
  [Calls]
  - >> printf_char
  - >> printf_str
  - >> printf_hex
  - >> printf_dec
  [Called By]
  - >> main

  PTU0_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.PTU0_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = PTU0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  PTU1_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.PTU1_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = PTU1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  PendSV_Handler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.PendSV_Handler))
  [Stack]

  - Max Depth = 32
  - Call Chain = PendSV_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  QSPI_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.QSPI_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = QSPI_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.RTC_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = RTC_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  RTC_Seconds_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.RTC_Seconds_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = RTC_Seconds_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  RamInit1 (Thumb, 248 bytes, Stack size 32 bytes, raminit1.o(.text.RamInit1))
  [Stack]

  - Max Depth = 32
  - Call Chain = RamInit1
  [Calls]
  - >> __aeabi_memclr4
  [Address Reference Count : 1]
  - startup.o(.text)

  RamInit2 (Thumb, 2 bytes, Stack size 0 bytes, raminit2.o(.text.RamInit2))
  [Address Reference Count : 1]

  - startup.o(.text)

  SAI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SAI0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SAI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SAI1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SENT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SENT0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SENT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SENT1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI2_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI4_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI5_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI6_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI7_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SVC_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SVC_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SysTick_Handler (Thumb, 8 bytes, Stack size 0 bytes, osif_baremetal.o(.text.SysTick_Handler))
  [Calls]

  - >> osif_Tick
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SystemInit (Thumb, 60 bytes, Stack size 0 bytes, system_ytm32b1ha0.o(.text.SystemInit))
  [Address Reference Count : 1]

  - startup.o(.text)

  TMR0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.TMR0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  TMR1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.TMR1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  TRNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.TRNG_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  UTILITY_PRINT_Init (Thumb, 26 bytes, Stack size 0 bytes, utility_print_config.o(.text.UTILITY_PRINT_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = UTILITY_PRINT_Init ⇒ LINFlexD_UART_DRV_Init ⇒ LINFlexD_UART_DRV_SetBaudRate ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> LINFlexD_UART_DRV_Init
  [Called By]
  - >> Board_Init

  UsageFault_Handler (Thumb, 0 bytes, Stack size 8 bytes, vector_table_copy.o(.text.UsageFault_Handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = UsageFault_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  VectorTableCopy (Thumb, 74 bytes, Stack size 8 bytes, vector_table_copy.o(.text.VectorTableCopy))
  [Stack]

  - Max Depth = 8
  - Call Chain = VectorTableCopy
  [Calls]
  - >> __aeabi_memcpy4
  [Address Reference Count : 1]
  - startup.o(.text)

  WDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.WDG_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  WKU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.WKU_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR0_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR0_Ch0_Ch1_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR0_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR0_Ch2_Ch3_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR0_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR0_Ch4_Ch5_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR0_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR0_Ch6_Ch7_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR0_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Fault_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR0_Fault_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR0_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR0_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR0_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR1_Ch0_Ch1_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR1_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR1_Ch2_Ch3_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR1_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR1_Ch4_Ch5_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR1_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR1_Ch6_Ch7_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR1_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Fault_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR1_Fault_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR1_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR1_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR1_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR2_Ch0_Ch1_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR2_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR2_Ch2_Ch3_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR2_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR2_Ch4_Ch5_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR2_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR2_Ch6_Ch7_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR2_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Fault_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR2_Fault_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR2_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR2_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR2_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR3_Ch0_Ch1_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR3_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR3_Ch2_Ch3_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR3_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR3_Ch4_Ch5_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR3_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR3_Ch6_Ch7_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR3_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Fault_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR3_Fault_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR3_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR3_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR3_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR4_Ch0_Ch1_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR4_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR4_Ch2_Ch3_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR4_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR4_Ch4_Ch5_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR4_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR4_Ch6_Ch7_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR4_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Fault_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR4_Fault_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR4_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR4_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR4_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR5_Ch0_Ch1_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR5_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR5_Ch2_Ch3_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR5_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR5_Ch4_Ch5_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR5_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR5_Ch6_Ch7_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR5_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Fault_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR5_Fault_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR5_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.eTMR5_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = eTMR5_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  lpTMR0_IRQHandler (Thumb, 0 bytes, Stack size 6160 bytes, vector_table_copy.o(.text.lpTMR0_IRQHandler))
  [Stack]

  - Max Depth = 6160
  - Call Chain = lpTMR0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  main (Thumb, 400 bytes, Stack size 6160 bytes, main.o(.text.main))
  [Stack]

  - Max Depth = 6272
  - Call Chain = main ⇒ Board_Init ⇒ CLOCK_SYS_UpdateConfiguration ⇒ CLOCK_SYS_SetConfiguration ⇒ CLOCK_DRV_Init ⇒ CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> PRINTF
  - >> Board_Init
  [Called By]
  - >> Reset_Handler

  pTMR0_Ch0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR0_Ch0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR0_Ch1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR0_Ch2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR0_Ch2_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR0_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR0_Ch3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR1_Ch0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR1_Ch0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR1_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR1_Ch1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR1_Ch2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR1_Ch2_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR1_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR1_Ch3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR2_Ch0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR2_Ch0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR2_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR2_Ch1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR2_Ch2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR2_Ch2_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR2_Ch3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  printf_char (Thumb, 24 bytes, Stack size 0 bytes, utility_print_config.o(.text.printf_char))
  [Stack]

  - Max Depth = 40
  - Call Chain = printf_char ⇒ LINFlexD_UART_DRV_SendDataPolling ⇒ LINFlexD_UART_DRV_PutData
  [Calls]
  - >> LINFlexD_UART_DRV_SendDataPolling
  [Called By]
  - >> PRINTF
  - >> printf_str
  - >> printf_hex
  - >> printf_dec

  ### Local Symbols

  Board_Init (Thumb, 54 bytes, Stack size 8 bytes, main.o(.text.Board_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = Board_Init ⇒ CLOCK_SYS_UpdateConfiguration ⇒ CLOCK_SYS_SetConfiguration ⇒ CLOCK_DRV_Init ⇒ CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> UTILITY_PRINT_Init
  - >> PINS_DRV_Init
  - >> CLOCK_SYS_UpdateConfiguration
  - >> CLOCK_SYS_Init
  [Called By]
  - >> main

  CLOCK_SCU_WaitDividerStable (Thumb, 32 bytes, Stack size 8 bytes, clock_ytm32b1hx.o(.text.CLOCK_SCU_WaitDividerStable))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLOCK_SCU_WaitDividerStable
  [Calls]
  - >> SCU_GetDividerStable
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SCU_WaitFXOSCValid (Thumb, 32 bytes, Stack size 8 bytes, clock_ytm32b1hx.o(.text.CLOCK_SCU_WaitFXOSCValid))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLOCK_SCU_WaitFXOSCValid
  [Calls]
  - >> SCU_GetFXOSCValid
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SCU_WaitPllLock (Thumb, 32 bytes, Stack size 8 bytes, clock_ytm32b1hx.o(.text.CLOCK_SCU_WaitPllLock))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLOCK_SCU_WaitPllLock
  [Calls]
  - >> SCU_GetPllLock
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_ConfigureSystemClock (Thumb, 38 bytes, Stack size 16 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_ConfigureSystemClock))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_SYS_ConfigureSystemClock
  [Calls]
  - >> SCU_SetSysClkSrc
  - >> SCU_GetSysClkSrc
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_SetCmuChannelConfiguration (Thumb, 58 bytes, Stack size 16 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_SetCmuChannelConfiguration))
  [Stack]

  - Max Depth = 24
  - Call Chain = CLOCK_SYS_SetCmuChannelConfiguration ⇒ SCU_SetCmuChResetEnable
  [Calls]
  - >> SCU_SetCmuChResetEnable
  - >> SCU_SetCmuChRefClock
  - >> SCU_SetCmuChEnable
  - >> SCU_SetCmuChCompLow
  - >> SCU_SetCmuChCompHigh
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_SetDefaultCmuChannelConfiguration (Thumb, 86 bytes, Stack size 16 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_SetDefaultCmuChannelConfiguration))
  [Stack]

  - Max Depth = 24
  - Call Chain = CLOCK_SYS_SetDefaultCmuChannelConfiguration ⇒ SCU_SetCmuChResetEnable
  [Calls]
  - >> SCU_SetCmuChResetEnable
  - >> SCU_SetCmuChRefClock
  - >> SCU_SetCmuChEnable
  - >> SCU_SetCmuChCompLow
  - >> SCU_SetCmuChCompHigh
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_SetIpcConfiguration (Thumb, 60 bytes, Stack size 16 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_SetIpcConfiguration))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_SYS_SetIpcConfiguration
  [Calls]
  - >> IPC_SetPeripheralClockControl
  - >> IPC_SetClockMode
  [Called By]
  - >> CLOCK_DRV_Init

  CLOCK_SYS_SetScuConfiguration (Thumb, 522 bytes, Stack size 24 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_SetScuConfiguration))
  [Stack]

  - Max Depth = 48
  - Call Chain = CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> CLOCK_SYS_GetFreq
  - >> CLOCK_DRV_GetPllFreq
  - >> SCU_SxoscStandbyEnable
  - >> SCU_SxoscPowerDownEnable
  - >> SCU_SxoscDeepSleepEnable
  - >> SCU_SircStandbyEnable
  - >> SCU_SircPowerDownEnable
  - >> SCU_SircDeepSleepEnable
  - >> SCU_SetSysClkDiv
  - >> SCU_SetSxoscGain
  - >> SCU_SetSxoscBypassMode
  - >> SCU_SetSlowBusClkDiv
  - >> SCU_SetPllRefClkDiv
  - >> SCU_SetPllRefClk
  - >> SCU_SetPllFeedBackDiv
  - >> SCU_SetFxoscGain
  - >> SCU_SetFxoscComp
  - >> SCU_SetFxoscBypassMode
  - >> SCU_SetFastBusClkDiv
  - >> SCU_SetClkOutSrc
  - >> SCU_SetClkOutDiv
  - >> SCU_GetSxoscEnableFlag
  - >> SCU_FircDeepSleepEnable
  - >> SCU_EnableSxosc
  - >> SCU_EnablePll
  - >> SCU_EnableFxosc
  - >> SCU_EnableFirc
  - >> CLOCK_SYS_SetDefaultCmuChannelConfiguration
  - >> CLOCK_SYS_SetCmuChannelConfiguration
  - >> CLOCK_SYS_ConfigureSystemClock
  - >> CLOCK_SCU_WaitPllLock
  - >> CLOCK_SCU_WaitFXOSCValid
  - >> CLOCK_SCU_WaitDividerStable
  [Called By]
  - >> CLOCK_DRV_Init

  IPC_SetClockMode (Thumb, 34 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.IPC_SetClockMode))
  [Called By]

  - >> CLOCK_SYS_SetIpcConfiguration

  IPC_SetPeripheralClockControl (Thumb, 38 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.IPC_SetPeripheralClockControl))
  [Called By]

  - >> CLOCK_SYS_SetIpcConfiguration

  SCU_EnableFirc (Thumb, 18 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_EnableFirc))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_EnableFxosc (Thumb, 18 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_EnableFxosc))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_EnablePll (Thumb, 18 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_EnablePll))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_EnableSxosc (Thumb, 18 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_EnableSxosc))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_FircDeepSleepEnable (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_FircDeepSleepEnable))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_GetDividerStable (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetDividerStable))
  [Called By]

  - >> CLOCK_SCU_WaitDividerStable

  SCU_GetFXOSCValid (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetFXOSCValid))
  [Called By]

  - >> CLOCK_SCU_WaitFXOSCValid

  SCU_GetFastBusClkDiv (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetFastBusClkDiv))
  [Called By]

  - >> CLOCK_DRV_GetFreq

  SCU_GetPllFeedBackDiv (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetPllFeedBackDiv))
  [Called By]

  - >> CLOCK_DRV_GetPllFreq

  SCU_GetPllLock (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetPllLock))
  [Called By]

  - >> CLOCK_DRV_GetPllFreq
  - >> CLOCK_SCU_WaitPllLock

  SCU_GetPllRefClk (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetPllRefClk))
  [Called By]

  - >> CLOCK_DRV_GetPllFreq

  SCU_GetPllRefClkDiv (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetPllRefClkDiv))
  [Called By]

  - >> CLOCK_DRV_GetPllFreq

  SCU_GetSlowBusClkDiv (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetSlowBusClkDiv))
  [Called By]

  - >> CLOCK_DRV_GetFreq

  SCU_GetSxoscEnableFlag (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetSxoscEnableFlag))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_GetSysClkDiv (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetSysClkDiv))
  [Called By]

  - >> CLOCK_DRV_GetFreq

  SCU_GetSysClkSrc (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetSysClkSrc))
  [Called By]

  - >> CLOCK_DRV_GetFreq
  - >> CLOCK_SYS_ConfigureSystemClock

  SCU_SetClkOutDiv (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetClkOutDiv))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetClkOutSrc (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetClkOutSrc))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetCmuChCompHigh (Thumb, 12 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetCmuChCompHigh))
  [Called By]

  - >> CLOCK_SYS_SetDefaultCmuChannelConfiguration
  - >> CLOCK_SYS_SetCmuChannelConfiguration

  SCU_SetCmuChCompLow (Thumb, 12 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetCmuChCompLow))
  [Called By]

  - >> CLOCK_SYS_SetDefaultCmuChannelConfiguration
  - >> CLOCK_SYS_SetCmuChannelConfiguration

  SCU_SetCmuChEnable (Thumb, 38 bytes, Stack size 8 bytes, clock_ytm32b1hx.o(.text.SCU_SetCmuChEnable))
  [Stack]

  - Max Depth = 8
  - Call Chain = SCU_SetCmuChEnable
  [Called By]
  - >> CLOCK_SYS_SetDefaultCmuChannelConfiguration
  - >> CLOCK_SYS_SetCmuChannelConfiguration

  SCU_SetCmuChRefClock (Thumb, 40 bytes, Stack size 8 bytes, clock_ytm32b1hx.o(.text.SCU_SetCmuChRefClock))
  [Stack]

  - Max Depth = 8
  - Call Chain = SCU_SetCmuChRefClock
  [Called By]
  - >> CLOCK_SYS_SetDefaultCmuChannelConfiguration
  - >> CLOCK_SYS_SetCmuChannelConfiguration

  SCU_SetCmuChResetEnable (Thumb, 40 bytes, Stack size 8 bytes, clock_ytm32b1hx.o(.text.SCU_SetCmuChResetEnable))
  [Stack]

  - Max Depth = 8
  - Call Chain = SCU_SetCmuChResetEnable
  [Called By]
  - >> CLOCK_SYS_SetDefaultCmuChannelConfiguration
  - >> CLOCK_SYS_SetCmuChannelConfiguration

  SCU_SetFastBusClkDiv (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetFastBusClkDiv))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetFxoscBypassMode (Thumb, 22 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetFxoscBypassMode))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetFxoscComp (Thumb, 24 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetFxoscComp))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetFxoscGain (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetFxoscGain))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetPllFeedBackDiv (Thumb, 26 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetPllFeedBackDiv))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetPllRefClk (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetPllRefClk))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetPllRefClkDiv (Thumb, 26 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetPllRefClkDiv))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetSlowBusClkDiv (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetSlowBusClkDiv))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetSxoscBypassMode (Thumb, 22 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetSxoscBypassMode))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetSxoscGain (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetSxoscGain))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetSysClkDiv (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetSysClkDiv))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetSysClkSrc (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetSysClkSrc))
  [Called By]

  - >> CLOCK_SYS_ConfigureSystemClock

  SCU_SircDeepSleepEnable (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SircDeepSleepEnable))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SircPowerDownEnable (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SircPowerDownEnable))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SircStandbyEnable (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SircStandbyEnable))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SxoscDeepSleepEnable (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SxoscDeepSleepEnable))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SxoscPowerDownEnable (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SxoscPowerDownEnable))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SxoscStandbyEnable (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SxoscStandbyEnable))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  PINS_ConfigDigitalFilter (Thumb, 32 bytes, Stack size 0 bytes, pins_port_hw_access.o(.text.PINS_ConfigDigitalFilter))
  [Called By]

  - >> PINS_Init

  PINS_GPIO_WritePin (Thumb, 28 bytes, Stack size 8 bytes, pins_port_hw_access.o(.text.PINS_GPIO_WritePin))
  [Stack]

  - Max Depth = 8
  - Call Chain = PINS_GPIO_WritePin
  [Called By]
  - >> PINS_Init

  __NVIC_EnableIRQ (Thumb, 32 bytes, Stack size 0 bytes, interrupt_manager.o(.text.__NVIC_EnableIRQ))
  [Called By]

  - >> INT_SYS_EnableIRQ

  DMA_CTSSetDestAddr (Thumb, 10 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_CTSSetDestAddr))
  [Called By]

  - >> DMA_DRV_SetDestAddr

  DMA_ClearDoneStatusFlag (Thumb, 10 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_ClearDoneStatusFlag))
  [Called By]

  - >> DMA_DRV_ClearIntStatus

  DMA_ClearErrorIntStatusFlag (Thumb, 10 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_ClearErrorIntStatusFlag))
  [Called By]

  - >> DMA_DRV_ErrorIRQHandler

  DMA_ClearIntStatusFlag (Thumb, 10 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_ClearIntStatusFlag))
  [Called By]

  - >> DMA_DRV_ClearIntStatus

  DMA_DRV_ClearIntStatus (Thumb, 30 bytes, Stack size 16 bytes, dma_driver.o(.text.DMA_DRV_ClearIntStatus))
  [Stack]

  - Max Depth = 16
  - Call Chain = DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_ClearIntStatusFlag
  - >> DMA_ClearDoneStatusFlag
  [Called By]
  - >> DMA_DRV_ErrorIRQHandler
  - >> DMA_DRV_IRQHandler

  DMA_GetErrorIntStatusFlag (Thumb, 4 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA_GetErrorIntStatusFlag))
  [Called By]

  - >> DMA_Error_IRQHandler

  LINFlexD_ClearStatusFlag (Thumb, 4 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_ClearStatusFlag))
  [Called By]

  - >> LINFlexD_UART_DRV_SendDataPolling
  - >> LINFlexD_UART_DRV_TxIRQHandler
  - >> LINFlexD_UART_DRV_RxTOHandler
  - >> LINFlexD_UART_DRV_RxIRQHandler
  - >> LINFlexD_UART_DRV_ErrIRQHandler

  LINFlexD_EnterInitMode (Thumb, 12 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_EnterInitMode))
  [Called By]

  - >> LINFlexD_UART_DRV_Init
  - >> LINFlexD_UART_DRV_SetBaudRate

  LINFlexD_EnterNormalMode (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_EnterNormalMode))
  [Called By]

  - >> LINFlexD_UART_DRV_Init
  - >> LINFlexD_UART_DRV_SetBaudRate

  LINFlexD_GetLinState (Thumb, 8 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_GetLinState))
  [Called By]

  - >> LINFlexD_UART_DRV_Init
  - >> LINFlexD_UART_DRV_SetBaudRate

  LINFlexD_GetRxDataBuffer1Byte (Thumb, 6 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_GetRxDataBuffer1Byte))
  [Called By]

  - >> LINFlexD_UART_DRV_GetData

  LINFlexD_GetRxDataBuffer2Bytes (Thumb, 4 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_GetRxDataBuffer2Bytes))
  [Called By]

  - >> LINFlexD_UART_DRV_GetData

  LINFlexD_GetStatusFlag (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_GetStatusFlag))
  [Called By]

  - >> LINFlexD_UART_DRV_SendDataPolling
  - >> LINFlexD_UART_DRV_IRQHandler
  - >> LINFlexD_UART_DRV_ErrIRQHandler

  LINFlexD_IsInterruptEnabled (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_IsInterruptEnabled))
  [Called By]

  - >> LINFlexD_UART_DRV_IRQHandler

  LINFlexD_SetDisableTimeout (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetDisableTimeout))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetFractionalBaudRate (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetFractionalBaudRate))
  [Called By]

  - >> LINFlexD_UART_DRV_SetBaudRate

  LINFlexD_SetIntegerBaudRate (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetIntegerBaudRate))
  [Called By]

  - >> LINFlexD_UART_DRV_SetBaudRate

  LINFlexD_SetInterruptMode (Thumb, 20 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetInterruptMode))
  [Called By]

  - >> LINFlexD_UART_DRV_Init
  - >> LINFlexD_UART_DRV_RxIRQHandler
  - >> LINFlexD_UART_DRV_CompleteSendUsingInterrupts
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts

  LINFlexD_SetMode (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetMode))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetMonitorIdleState (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetMonitorIdleState))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetParityControl (Thumb, 14 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetParityControl))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetParityType (Thumb, 26 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetParityType))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetReceiverState (Thumb, 14 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetReceiverState))
  [Called By]

  - >> LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingDma

  LINFlexD_SetRxDataFieldLength (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetRxDataFieldLength))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetRxMode (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetRxMode))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetRxStopBitsCount (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetRxStopBitsCount))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetTransmitterState (Thumb, 14 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetTransmitterState))
  [Called By]

  - >> LINFlexD_UART_DRV_SendDataPolling
  - >> LINFlexD_UART_DRV_CompleteSendUsingInterrupts

  LINFlexD_SetTxDataBuffer1Byte (Thumb, 6 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetTxDataBuffer1Byte))
  [Called By]

  - >> LINFlexD_UART_DRV_PutData

  LINFlexD_SetTxDataBuffer2Bytes (Thumb, 4 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetTxDataBuffer2Bytes))
  [Called By]

  - >> LINFlexD_UART_DRV_PutData

  LINFlexD_SetTxDataFieldLength (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetTxDataFieldLength))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetTxMode (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetTxMode))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetTxStopBitsCount (Thumb, 14 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetTxStopBitsCount))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetUartWordLength (Thumb, 26 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetUartWordLength))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_UART_DRV_CompleteReceiveUsingDma (Thumb, 146 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_CompleteReceiveUsingDma))
  [Stack]

  - Max Depth = 32
  - Call Chain = LINFlexD_UART_DRV_CompleteReceiveUsingDma ⇒ OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> OSIF_SemaPost
  - >> LINFlexD_SetReceiverState
  - >> DMA_DRV_StopChannel
  - >> DMA_DRV_StartChannel
  - >> DMA_DRV_SetTriggerLoopIterationCount
  - >> DMA_DRV_SetDestAddr
  [Called By]
  - >> LINFlexD_UART_DRV_ErrIRQHandler

  LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts (Thumb, 74 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts))
  [Stack]

  - Max Depth = 32
  - Call Chain = LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts ⇒ OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> OSIF_SemaPost
  - >> LINFlexD_SetReceiverState
  - >> LINFlexD_SetInterruptMode
  [Called By]
  - >> LINFlexD_UART_DRV_RxTOHandler
  - >> LINFlexD_UART_DRV_RxIRQHandler
  - >> LINFlexD_UART_DRV_ErrIRQHandler

  LINFlexD_UART_DRV_CompleteSendUsingInterrupts (Thumb, 74 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_CompleteSendUsingInterrupts))
  [Stack]

  - Max Depth = 32
  - Call Chain = LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> OSIF_SemaPost
  - >> LINFlexD_SetTransmitterState
  - >> LINFlexD_SetInterruptMode
  [Called By]
  - >> LINFlexD_UART_DRV_TxIRQHandler

  LINFlexD_UART_DRV_GetData (Thumb, 108 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_GetData))
  [Stack]

  - Max Depth = 16
  - Call Chain = LINFlexD_UART_DRV_GetData
  [Calls]
  - >> LINFlexD_GetRxDataBuffer2Bytes
  - >> LINFlexD_GetRxDataBuffer1Byte
  [Called By]
  - >> LINFlexD_UART_DRV_RxIRQHandler

  LINFlexD_UART_DRV_PutData (Thumb, 114 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_PutData))
  [Stack]

  - Max Depth = 16
  - Call Chain = LINFlexD_UART_DRV_PutData
  [Calls]
  - >> LINFlexD_SetTxDataBuffer2Bytes
  - >> LINFlexD_SetTxDataBuffer1Byte
  [Called By]
  - >> LINFlexD_UART_DRV_SendDataPolling
  - >> LINFlexD_UART_DRV_TxIRQHandler

  osif_DisableIrqGlobal (Thumb, 8 bytes, Stack size 8 bytes, osif_baremetal.o(.text.osif_DisableIrqGlobal))
  [Stack]

  - Max Depth = 8
  - Call Chain = osif_DisableIrqGlobal
  [Calls]
  - >> INT_SYS_DisableIRQGlobal
  [Called By]
  - >> OSIF_SemaPost
  - >> OSIF_SemaCreate

  osif_EnableIrqGlobal (Thumb, 8 bytes, Stack size 8 bytes, osif_baremetal.o(.text.osif_EnableIrqGlobal))
  [Stack]

  - Max Depth = 8
  - Call Chain = osif_EnableIrqGlobal
  [Calls]
  - >> INT_SYS_EnableIRQGlobal
  [Called By]
  - >> OSIF_SemaPost
  - >> OSIF_SemaCreate

  osif_Tick (Thumb, 16 bytes, Stack size 0 bytes, osif_baremetal.o(.text.osif_Tick))
  [Called By]

  - >> SysTick_Handler

  printf_dec (Thumb, 76 bytes, Stack size 32 bytes, printf.o(.text.printf_dec))
  [Stack]

  - Max Depth = 72
  - Call Chain = printf_dec ⇒ printf_char ⇒ LINFlexD_UART_DRV_SendDataPolling ⇒ LINFlexD_UART_DRV_PutData
  [Calls]
  - >> printf_char
  [Called By]
  - >> PRINTF

  printf_hex (Thumb, 68 bytes, Stack size 24 bytes, printf.o(.text.printf_hex))
  [Stack]

  - Max Depth = 64
  - Call Chain = printf_hex ⇒ printf_char ⇒ LINFlexD_UART_DRV_SendDataPolling ⇒ LINFlexD_UART_DRV_PutData
  [Calls]
  - >> printf_char
  [Called By]
  - >> PRINTF

  printf_str (Thumb, 32 bytes, Stack size 8 bytes, printf.o(.text.printf_str))
  [Stack]

  - Max Depth = 48
  - Call Chain = printf_str ⇒ printf_char ⇒ LINFlexD_UART_DRV_SendDataPolling ⇒ LINFlexD_UART_DRV_PutData
  [Calls]
  - >> printf_char
  [Called By]
  - >> PRINTF

  ### Undefined Global Symbols