/**
@defgroup clock_manager_ytm32b1hx Clock Manager ytm32b1hx
@brief This module covers the device-specific clock_manager functionality implemented for YTM32B1Hx SOC.
@ingroup clock_manager
<p>
The support for YTM32B1Hx consist in the following items:
- Clock names enumeration
<b> clock_names_t </b> is an enumeration which contains all clock names which are relevant for YTM32B1Hx.
- Submodule configuration structures
   
- Submodule configuration functions
The following function <b> CLOCK_SYS_SetConfiguration </b> was implemented for YTM32B1Hx:

## Hardware background ##

Features of clock_manager module include the following clock sources:
    - 4 - 40 MHz fast external oscillator (SOSC)
    - 48 MHz Fast Internal RC oscillator (FIRC)
    - 8 MHz Slow Internal RC oscillator (SIRC)
    - 128 kHz Low Power Oscillator (LPO)

## How to use the CLOCK_MANAGER driver in your application ##

In order to be able to use the clock_manager in your application,
<b>CLOCK_DRV_Init</b> function has to be called. The same function is called
when another configuration is loaded and clock configuration is updated.

## Code Example ##

This is an example for switching between two configurations:

@code
  CLOCK_SYS_Init(g_clockManConfigsArr,
                 CLOCK_MANAGER_CONFIG_CNT,
                 g_clockManCallbacksArr,
                 CLOCK_MANAGER_CALLBACK_CNT);

  CLOCK_SYS_UpdateConfiguration(0, CLOCK_MANAGER_POLICY_FORCIBLE);
  CLOCK_SYS_UpdateConfiguration(1, CLOCK_MANAGER_POLICY_FORCIBLE);
@endcode

## Notes ##

Current implementation assumes that the clock configurations are valid and are applied in a valid sequence.
Mainly this means that the configuration doesn't reinitialize the clock used as the system clock.

The S32DS do not support generate Callbacks configuration. It's alway empty.

## Integration guideline ##

### Compilation units ###

The following files need to be compiled in the project:
\verbatim
${SDK_PATH}\platform\drivers\src\clock\YTM32B1Hx\clock_YTM32B1Hx.c
\endverbatim

### Include path ###

The following paths need to be added to the include path of the toolchain:
\verbatim
${SDK_PATH}\platform\drivers\inc\
${SDK_PATH}\platform\drivers\src\clock\
${SDK_PATH}\platform\drivers\src\clock\YTM32B1Hx\
\endverbatim

### Compile symbols ###

No special symbols are required for this component

### Dependencies ###

\ref interrupt_manager
</p>
*/
