# Static Call Graph for image .\Objects\Fls_Demo.axf

#<CALLGRAPH># ARM Linker, 6180002: Last Updated: Thu Apr 11 10:36:46 2024

### Maximum Stack Usage = 80 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

Reset_Handler ⇒ main ⇒ Mcu_InitClock ⇒ Mcu_Lld_InitClock ⇒ Mcu_Lld_SetClockSource

### Functions with no stack information

- RamInit0
- Reset_Handler

### Mutually Recursive functions

- ACMP0_IRQHandler ⇒ ACMP0_IRQHandler
- ACMP1_IRQHandler ⇒ ACMP1_IRQHandler
- ADC0_IRQHandler ⇒ ADC0_IRQHandler
- ADC1_IRQHandler ⇒ ADC1_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- CAN0_Error_IRQHandler ⇒ CAN0_Error_IRQHandler
- CAN0_ORed_0_15_MB_IRQHandler ⇒ CAN0_ORed_0_15_MB_IRQHandler
- CAN0_ORed_112_127_MB_IRQHandler ⇒ CAN0_ORed_112_127_MB_IRQHandler
- CAN0_ORed_16_31_MB_IRQHandler ⇒ CAN0_ORed_16_31_MB_IRQHandler
- CAN0_ORed_32_47_MB_IRQHandler ⇒ CAN0_ORed_32_47_MB_IRQHandler
- CAN0_ORed_48_63_MB_IRQHandler ⇒ CAN0_ORed_48_63_MB_IRQHandler
- CAN0_ORed_64_79_MB_IRQHandler ⇒ CAN0_ORed_64_79_MB_IRQHandler
- CAN0_ORed_80_95_MB_IRQHandler ⇒ CAN0_ORed_80_95_MB_IRQHandler
- CAN0_ORed_96_111_MB_IRQHandler ⇒ CAN0_ORed_96_111_MB_IRQHandler
- CAN0_ORed_IRQHandler ⇒ CAN0_ORed_IRQHandler
- CAN0_Wake_Up_IRQHandler ⇒ CAN0_Wake_Up_IRQHandler
- CAN1_Error_IRQHandler ⇒ CAN1_Error_IRQHandler
- CAN1_ORed_0_15_MB_IRQHandler ⇒ CAN1_ORed_0_15_MB_IRQHandler
- CAN1_ORed_112_127_MB_IRQHandler ⇒ CAN1_ORed_112_127_MB_IRQHandler
- CAN1_ORed_16_31_MB_IRQHandler ⇒ CAN1_ORed_16_31_MB_IRQHandler
- CAN1_ORed_32_47_MB_IRQHandler ⇒ CAN1_ORed_32_47_MB_IRQHandler
- CAN1_ORed_48_63_MB_IRQHandler ⇒ CAN1_ORed_48_63_MB_IRQHandler
- CAN1_ORed_64_79_MB_IRQHandler ⇒ CAN1_ORed_64_79_MB_IRQHandler
- CAN1_ORed_80_95_MB_IRQHandler ⇒ CAN1_ORed_80_95_MB_IRQHandler
- CAN1_ORed_96_111_MB_IRQHandler ⇒ CAN1_ORed_96_111_MB_IRQHandler
- CAN1_ORed_IRQHandler ⇒ CAN1_ORed_IRQHandler
- CAN1_Wake_Up_IRQHandler ⇒ CAN1_Wake_Up_IRQHandler
- CAN2_Error_IRQHandler ⇒ CAN2_Error_IRQHandler
- CAN2_ORed_0_15_MB_IRQHandler ⇒ CAN2_ORed_0_15_MB_IRQHandler
- CAN2_ORed_16_31_MB_IRQHandler ⇒ CAN2_ORed_16_31_MB_IRQHandler
- CAN2_ORed_32_47_MB_IRQHandler ⇒ CAN2_ORed_32_47_MB_IRQHandler
- CAN2_ORed_48_63_MB_IRQHandler ⇒ CAN2_ORed_48_63_MB_IRQHandler
- CAN2_ORed_IRQHandler ⇒ CAN2_ORed_IRQHandler
- CAN2_Wake_Up_IRQHandler ⇒ CAN2_Wake_Up_IRQHandler
- CAN3_Error_IRQHandler ⇒ CAN3_Error_IRQHandler
- CAN3_ORed_0_15_MB_IRQHandler ⇒ CAN3_ORed_0_15_MB_IRQHandler
- CAN3_ORed_16_31_MB_IRQHandler ⇒ CAN3_ORed_16_31_MB_IRQHandler
- CAN3_ORed_32_47_MB_IRQHandler ⇒ CAN3_ORed_32_47_MB_IRQHandler
- CAN3_ORed_48_63_MB_IRQHandler ⇒ CAN3_ORed_48_63_MB_IRQHandler
- CAN3_ORed_IRQHandler ⇒ CAN3_ORed_IRQHandler
- CAN3_Wake_Up_IRQHandler ⇒ CAN3_Wake_Up_IRQHandler
- CAN4_Error_IRQHandler ⇒ CAN4_Error_IRQHandler
- CAN4_ORed_0_15_MB_IRQHandler ⇒ CAN4_ORed_0_15_MB_IRQHandler
- CAN4_ORed_16_31_MB_IRQHandler ⇒ CAN4_ORed_16_31_MB_IRQHandler
- CAN4_ORed_32_47_MB_IRQHandler ⇒ CAN4_ORed_32_47_MB_IRQHandler
- CAN4_ORed_48_63_MB_IRQHandler ⇒ CAN4_ORed_48_63_MB_IRQHandler
- CAN4_ORed_IRQHandler ⇒ CAN4_ORed_IRQHandler
- CAN4_Wake_Up_IRQHandler ⇒ CAN4_Wake_Up_IRQHandler
- CAN5_Error_IRQHandler ⇒ CAN5_Error_IRQHandler
- CAN5_ORed_0_15_MB_IRQHandler ⇒ CAN5_ORed_0_15_MB_IRQHandler
- CAN5_ORed_16_31_MB_IRQHandler ⇒ CAN5_ORed_16_31_MB_IRQHandler
- CAN5_ORed_IRQHandler ⇒ CAN5_ORed_IRQHandler
- CAN5_Wake_Up_IRQHandler ⇒ CAN5_Wake_Up_IRQHandler
- CAN6_Error_IRQHandler ⇒ CAN6_Error_IRQHandler
- CAN6_ORed_0_15_MB_IRQHandler ⇒ CAN6_ORed_0_15_MB_IRQHandler
- CAN6_ORed_16_31_MB_IRQHandler ⇒ CAN6_ORed_16_31_MB_IRQHandler
- CAN6_ORed_IRQHandler ⇒ CAN6_ORed_IRQHandler
- CAN6_Wake_Up_IRQHandler ⇒ CAN6_Wake_Up_IRQHandler
- CAN7_Error_IRQHandler ⇒ CAN7_Error_IRQHandler
- CAN7_ORed_0_15_MB_IRQHandler ⇒ CAN7_ORed_0_15_MB_IRQHandler
- CAN7_ORed_16_31_MB_IRQHandler ⇒ CAN7_ORed_16_31_MB_IRQHandler
- CAN7_ORed_IRQHandler ⇒ CAN7_ORed_IRQHandler
- CAN7_Wake_Up_IRQHandler ⇒ CAN7_Wake_Up_IRQHandler
- CORE_CTI_IRQHandler ⇒ CORE_CTI_IRQHandler
- DMA0_IRQHandler ⇒ DMA0_IRQHandler
- DMA10_IRQHandler ⇒ DMA10_IRQHandler
- DMA11_IRQHandler ⇒ DMA11_IRQHandler
- DMA12_IRQHandler ⇒ DMA12_IRQHandler
- DMA13_IRQHandler ⇒ DMA13_IRQHandler
- DMA14_IRQHandler ⇒ DMA14_IRQHandler
- DMA15_IRQHandler ⇒ DMA15_IRQHandler
- DMA16_IRQHandler ⇒ DMA16_IRQHandler
- DMA17_IRQHandler ⇒ DMA17_IRQHandler
- DMA18_IRQHandler ⇒ DMA18_IRQHandler
- DMA19_IRQHandler ⇒ DMA19_IRQHandler
- DMA1_IRQHandler ⇒ DMA1_IRQHandler
- DMA20_IRQHandler ⇒ DMA20_IRQHandler
- DMA21_IRQHandler ⇒ DMA21_IRQHandler
- DMA22_IRQHandler ⇒ DMA22_IRQHandler
- DMA23_IRQHandler ⇒ DMA23_IRQHandler
- DMA24_IRQHandler ⇒ DMA24_IRQHandler
- DMA25_IRQHandler ⇒ DMA25_IRQHandler
- DMA26_IRQHandler ⇒ DMA26_IRQHandler
- DMA27_IRQHandler ⇒ DMA27_IRQHandler
- DMA28_IRQHandler ⇒ DMA28_IRQHandler
- DMA29_IRQHandler ⇒ DMA29_IRQHandler
- DMA2_IRQHandler ⇒ DMA2_IRQHandler
- DMA30_IRQHandler ⇒ DMA30_IRQHandler
- DMA31_IRQHandler ⇒ DMA31_IRQHandler
- DMA3_IRQHandler ⇒ DMA3_IRQHandler
- DMA4_IRQHandler ⇒ DMA4_IRQHandler
- DMA5_IRQHandler ⇒ DMA5_IRQHandler
- DMA6_IRQHandler ⇒ DMA6_IRQHandler
- DMA7_IRQHandler ⇒ DMA7_IRQHandler
- DMA8_IRQHandler ⇒ DMA8_IRQHandler
- DMA9_IRQHandler ⇒ DMA9_IRQHandler
- DMA_Error_IRQHandler ⇒ DMA_Error_IRQHandler
- DebugMon_Handler ⇒ DebugMon_Handler
- DefaultISR ⇒ DefaultISR
- EFM_Ecc_IRQHandler ⇒ EFM_Ecc_IRQHandler
- EFM_Error_IRQHandler ⇒ EFM_Error_IRQHandler
- EFM_IRQHandler ⇒ EFM_IRQHandler
- EMU_IRQHandler ⇒ EMU_IRQHandler
- ENET_ECC_IRQHandler ⇒ ENET_ECC_IRQHandler
- ENET_IRQHandler ⇒ ENET_IRQHandler
- ENET_RX_IRQHandler ⇒ ENET_RX_IRQHandler
- ENET_TX_IRQHandler ⇒ ENET_TX_IRQHandler
- FMU_Alarm_IRQHandler ⇒ FMU_Alarm_IRQHandler
- FMU_MISC_IRQHandler ⇒ FMU_MISC_IRQHandler
- FPU_IRQHandler ⇒ FPU_IRQHandler
- GPIOA_IRQHandler ⇒ GPIOA_IRQHandler
- GPIOB_IRQHandler ⇒ GPIOB_IRQHandler
- GPIOC_IRQHandler ⇒ GPIOC_IRQHandler
- GPIOD_IRQHandler ⇒ GPIOD_IRQHandler
- GPIOE_IRQHandler ⇒ GPIOE_IRQHandler
- HCU_IRQHandler ⇒ HCU_IRQHandler
- HardFault_Handler ⇒ HardFault_Handler
- I2C0_Master_Slave_IRQHandler ⇒ I2C0_Master_Slave_IRQHandler
- I2C1_Master_Slave_IRQHandler ⇒ I2C1_Master_Slave_IRQHandler
- I2C2_Master_Slave_IRQHandler ⇒ I2C2_Master_Slave_IRQHandler
- I2C3_Master_Slave_IRQHandler ⇒ I2C3_Master_Slave_IRQHandler
- I2C4_Master_Slave_IRQHandler ⇒ I2C4_Master_Slave_IRQHandler
- INTM_IRQHandler ⇒ INTM_IRQHandler
- LINFlexD0_IRQHandler ⇒ LINFlexD0_IRQHandler
- LINFlexD1_IRQHandler ⇒ LINFlexD1_IRQHandler
- LINFlexD2_IRQHandler ⇒ LINFlexD2_IRQHandler
- LINFlexD3_IRQHandler ⇒ LINFlexD3_IRQHandler
- LINFlexD4_IRQHandler ⇒ LINFlexD4_IRQHandler
- LINFlexD5_IRQHandler ⇒ LINFlexD5_IRQHandler
- LINFlexD6_IRQHandler ⇒ LINFlexD6_IRQHandler
- LINFlexD7_IRQHandler ⇒ LINFlexD7_IRQHandler
- LINFlexD8_IRQHandler ⇒ LINFlexD8_IRQHandler
- LINFlexD9_IRQHandler ⇒ LINFlexD9_IRQHandler
- MPWM0_Ch0_Ch7_IRQHandler ⇒ MPWM0_Ch0_Ch7_IRQHandler
- MPWM0_Ch8_Ch15_IRQHandler ⇒ MPWM0_Ch8_Ch15_IRQHandler
- MPWM1_Ch0_Ch7_IRQHandler ⇒ MPWM1_Ch0_Ch7_IRQHandler
- MPWM1_Ch8_Ch15_IRQHandler ⇒ MPWM1_Ch8_Ch15_IRQHandler
- MPWM2_Ch0_Ch7_IRQHandler ⇒ MPWM2_Ch0_Ch7_IRQHandler
- MPWM2_Ch8_Ch15_IRQHandler ⇒ MPWM2_Ch8_Ch15_IRQHandler
- MemManage_Handler ⇒ MemManage_Handler
- NMI_Handler ⇒ NMI_Handler
- PCU_IRQHandler ⇒ PCU_IRQHandler
- PTU0_IRQHandler ⇒ PTU0_IRQHandler
- PTU1_IRQHandler ⇒ PTU1_IRQHandler
- PendSV_Handler ⇒ PendSV_Handler
- QSPI_IRQHandler ⇒ QSPI_IRQHandler
- RTC_IRQHandler ⇒ RTC_IRQHandler
- RTC_Seconds_IRQHandler ⇒ RTC_Seconds_IRQHandler
- SAI0_IRQHandler ⇒ SAI0_IRQHandler
- SAI1_IRQHandler ⇒ SAI1_IRQHandler
- SCU_IRQHandler ⇒ SCU_IRQHandler
- SENT0_IRQHandler ⇒ SENT0_IRQHandler
- SENT1_IRQHandler ⇒ SENT1_IRQHandler
- SPI0_IRQHandler ⇒ SPI0_IRQHandler
- SPI1_IRQHandler ⇒ SPI1_IRQHandler
- SPI2_IRQHandler ⇒ SPI2_IRQHandler
- SPI3_IRQHandler ⇒ SPI3_IRQHandler
- SPI4_IRQHandler ⇒ SPI4_IRQHandler
- SPI5_IRQHandler ⇒ SPI5_IRQHandler
- SPI6_IRQHandler ⇒ SPI6_IRQHandler
- SPI7_IRQHandler ⇒ SPI7_IRQHandler
- SVC_Handler ⇒ SVC_Handler
- SysTick_Handler ⇒ SysTick_Handler
- TMR0_IRQHandler ⇒ TMR0_IRQHandler
- TMR1_IRQHandler ⇒ TMR1_IRQHandler
- TRNG_IRQHandler ⇒ TRNG_IRQHandler
- UsageFault_Handler ⇒ UsageFault_Handler
- WKU_IRQHandler ⇒ WKU_IRQHandler
- Wdg_Lld_Isr ⇒ Wdg_Lld_Isr
- eTMR0_Ch0_Ch1_IRQHandler ⇒ eTMR0_Ch0_Ch1_IRQHandler
- eTMR0_Ch2_Ch3_IRQHandler ⇒ eTMR0_Ch2_Ch3_IRQHandler
- eTMR0_Ch4_Ch5_IRQHandler ⇒ eTMR0_Ch4_Ch5_IRQHandler
- eTMR0_Ch6_Ch7_IRQHandler ⇒ eTMR0_Ch6_Ch7_IRQHandler
- eTMR0_Fault_IRQHandler ⇒ eTMR0_Fault_IRQHandler
- eTMR0_Ovf_IRQHandler ⇒ eTMR0_Ovf_IRQHandler
- eTMR1_Ch0_Ch1_IRQHandler ⇒ eTMR1_Ch0_Ch1_IRQHandler
- eTMR1_Ch2_Ch3_IRQHandler ⇒ eTMR1_Ch2_Ch3_IRQHandler
- eTMR1_Ch4_Ch5_IRQHandler ⇒ eTMR1_Ch4_Ch5_IRQHandler
- eTMR1_Ch6_Ch7_IRQHandler ⇒ eTMR1_Ch6_Ch7_IRQHandler
- eTMR1_Fault_IRQHandler ⇒ eTMR1_Fault_IRQHandler
- eTMR1_Ovf_IRQHandler ⇒ eTMR1_Ovf_IRQHandler
- eTMR2_Ch0_Ch1_IRQHandler ⇒ eTMR2_Ch0_Ch1_IRQHandler
- eTMR2_Ch2_Ch3_IRQHandler ⇒ eTMR2_Ch2_Ch3_IRQHandler
- eTMR2_Ch4_Ch5_IRQHandler ⇒ eTMR2_Ch4_Ch5_IRQHandler
- eTMR2_Ch6_Ch7_IRQHandler ⇒ eTMR2_Ch6_Ch7_IRQHandler
- eTMR2_Fault_IRQHandler ⇒ eTMR2_Fault_IRQHandler
- eTMR2_Ovf_IRQHandler ⇒ eTMR2_Ovf_IRQHandler
- eTMR3_Ch0_Ch1_IRQHandler ⇒ eTMR3_Ch0_Ch1_IRQHandler
- eTMR3_Ch2_Ch3_IRQHandler ⇒ eTMR3_Ch2_Ch3_IRQHandler
- eTMR3_Ch4_Ch5_IRQHandler ⇒ eTMR3_Ch4_Ch5_IRQHandler
- eTMR3_Ch6_Ch7_IRQHandler ⇒ eTMR3_Ch6_Ch7_IRQHandler
- eTMR3_Fault_IRQHandler ⇒ eTMR3_Fault_IRQHandler
- eTMR3_Ovf_IRQHandler ⇒ eTMR3_Ovf_IRQHandler
- eTMR4_Ch0_Ch1_IRQHandler ⇒ eTMR4_Ch0_Ch1_IRQHandler
- eTMR4_Ch2_Ch3_IRQHandler ⇒ eTMR4_Ch2_Ch3_IRQHandler
- eTMR4_Ch4_Ch5_IRQHandler ⇒ eTMR4_Ch4_Ch5_IRQHandler
- eTMR4_Ch6_Ch7_IRQHandler ⇒ eTMR4_Ch6_Ch7_IRQHandler
- eTMR4_Fault_IRQHandler ⇒ eTMR4_Fault_IRQHandler
- eTMR4_Ovf_IRQHandler ⇒ eTMR4_Ovf_IRQHandler
- eTMR5_Ch0_Ch1_IRQHandler ⇒ eTMR5_Ch0_Ch1_IRQHandler
- eTMR5_Ch2_Ch3_IRQHandler ⇒ eTMR5_Ch2_Ch3_IRQHandler
- eTMR5_Ch4_Ch5_IRQHandler ⇒ eTMR5_Ch4_Ch5_IRQHandler
- eTMR5_Ch6_Ch7_IRQHandler ⇒ eTMR5_Ch6_Ch7_IRQHandler
- eTMR5_Fault_IRQHandler ⇒ eTMR5_Fault_IRQHandler
- eTMR5_Ovf_IRQHandler ⇒ eTMR5_Ovf_IRQHandler
- lpTMR0_IRQHandler ⇒ lpTMR0_IRQHandler
- pTMR0_Ch0_IRQHandler ⇒ pTMR0_Ch0_IRQHandler
- pTMR0_Ch1_IRQHandler ⇒ pTMR0_Ch1_IRQHandler
- pTMR0_Ch2_IRQHandler ⇒ pTMR0_Ch2_IRQHandler
- pTMR0_Ch3_IRQHandler ⇒ pTMR0_Ch3_IRQHandler
- pTMR1_Ch0_IRQHandler ⇒ pTMR1_Ch0_IRQHandler
- pTMR1_Ch1_IRQHandler ⇒ pTMR1_Ch1_IRQHandler
- pTMR1_Ch2_IRQHandler ⇒ pTMR1_Ch2_IRQHandler
- pTMR1_Ch3_IRQHandler ⇒ pTMR1_Ch3_IRQHandler
- pTMR2_Ch0_IRQHandler ⇒ pTMR2_Ch0_IRQHandler
- pTMR2_Ch1_IRQHandler ⇒ pTMR2_Ch1_IRQHandler
- pTMR2_Ch2_IRQHandler ⇒ pTMR2_Ch2_IRQHandler
- pTMR2_Ch3_IRQHandler ⇒ pTMR2_Ch3_IRQHandler

  ### Function Pointers

  - ACMP0_IRQHandler from vector_table_copy.o(.text.ACMP0_IRQHandler) referenced from vector.o(.isr_vector)
  - ACMP1_IRQHandler from vector_table_copy.o(.text.ACMP1_IRQHandler) referenced from vector.o(.isr_vector)
  - ADC0_IRQHandler from vector_table_copy.o(.text.ADC0_IRQHandler) referenced from vector.o(.isr_vector)
  - ADC1_IRQHandler from vector_table_copy.o(.text.ADC1_IRQHandler) referenced from vector.o(.isr_vector)
  - BusFault_Handler from vector_table_copy.o(.text.BusFault_Handler) referenced from vector.o(.isr_vector)
  - CAN0_Error_IRQHandler from vector_table_copy.o(.text.CAN0_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_112_127_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_112_127_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_64_79_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_64_79_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_80_95_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_80_95_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_96_111_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_96_111_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN0_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_Error_IRQHandler from vector_table_copy.o(.text.CAN1_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_112_127_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_112_127_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_64_79_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_64_79_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_80_95_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_80_95_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_96_111_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_96_111_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN1_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_Error_IRQHandler from vector_table_copy.o(.text.CAN2_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN2_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_Error_IRQHandler from vector_table_copy.o(.text.CAN3_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN3_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_Error_IRQHandler from vector_table_copy.o(.text.CAN4_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN4_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_Error_IRQHandler from vector_table_copy.o(.text.CAN5_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN5_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN5_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_ORed_IRQHandler from vector_table_copy.o(.text.CAN5_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN5_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN6_Error_IRQHandler from vector_table_copy.o(.text.CAN6_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN6_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN6_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN6_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN6_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN6_ORed_IRQHandler from vector_table_copy.o(.text.CAN6_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN6_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN6_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN7_Error_IRQHandler from vector_table_copy.o(.text.CAN7_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN7_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN7_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN7_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN7_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN7_ORed_IRQHandler from vector_table_copy.o(.text.CAN7_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN7_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN7_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CORE_CTI_IRQHandler from vector_table_copy.o(.text.CORE_CTI_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA0_IRQHandler from vector_table_copy.o(.text.DMA0_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA10_IRQHandler from vector_table_copy.o(.text.DMA10_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA11_IRQHandler from vector_table_copy.o(.text.DMA11_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA12_IRQHandler from vector_table_copy.o(.text.DMA12_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA13_IRQHandler from vector_table_copy.o(.text.DMA13_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA14_IRQHandler from vector_table_copy.o(.text.DMA14_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA15_IRQHandler from vector_table_copy.o(.text.DMA15_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA16_IRQHandler from vector_table_copy.o(.text.DMA16_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA17_IRQHandler from vector_table_copy.o(.text.DMA17_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA18_IRQHandler from vector_table_copy.o(.text.DMA18_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA19_IRQHandler from vector_table_copy.o(.text.DMA19_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA1_IRQHandler from vector_table_copy.o(.text.DMA1_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA20_IRQHandler from vector_table_copy.o(.text.DMA20_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA21_IRQHandler from vector_table_copy.o(.text.DMA21_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA22_IRQHandler from vector_table_copy.o(.text.DMA22_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA23_IRQHandler from vector_table_copy.o(.text.DMA23_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA24_IRQHandler from vector_table_copy.o(.text.DMA24_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA25_IRQHandler from vector_table_copy.o(.text.DMA25_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA26_IRQHandler from vector_table_copy.o(.text.DMA26_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA27_IRQHandler from vector_table_copy.o(.text.DMA27_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA28_IRQHandler from vector_table_copy.o(.text.DMA28_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA29_IRQHandler from vector_table_copy.o(.text.DMA29_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA2_IRQHandler from vector_table_copy.o(.text.DMA2_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA30_IRQHandler from vector_table_copy.o(.text.DMA30_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA31_IRQHandler from vector_table_copy.o(.text.DMA31_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA3_IRQHandler from vector_table_copy.o(.text.DMA3_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA4_IRQHandler from vector_table_copy.o(.text.DMA4_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA5_IRQHandler from vector_table_copy.o(.text.DMA5_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA6_IRQHandler from vector_table_copy.o(.text.DMA6_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA7_IRQHandler from vector_table_copy.o(.text.DMA7_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA8_IRQHandler from vector_table_copy.o(.text.DMA8_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA9_IRQHandler from vector_table_copy.o(.text.DMA9_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA_Error_IRQHandler from vector_table_copy.o(.text.DMA_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - DebugMon_Handler from vector_table_copy.o(.text.DebugMon_Handler) referenced from vector.o(.isr_vector)
  - DefaultISR from vector_table_copy.o(.text.DefaultISR) referenced 26 times from vector.o(.isr_vector)
  - EFM_Ecc_IRQHandler from vector_table_copy.o(.text.EFM_Ecc_IRQHandler) referenced from vector.o(.isr_vector)
  - EFM_Error_IRQHandler from vector_table_copy.o(.text.EFM_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - EFM_IRQHandler from vector_table_copy.o(.text.EFM_IRQHandler) referenced from vector.o(.isr_vector)
  - EMU_IRQHandler from vector_table_copy.o(.text.EMU_IRQHandler) referenced from vector.o(.isr_vector)
  - ENET_ECC_IRQHandler from vector_table_copy.o(.text.ENET_ECC_IRQHandler) referenced from vector.o(.isr_vector)
  - ENET_IRQHandler from vector_table_copy.o(.text.ENET_IRQHandler) referenced from vector.o(.isr_vector)
  - ENET_RX_IRQHandler from vector_table_copy.o(.text.ENET_RX_IRQHandler) referenced from vector.o(.isr_vector)
  - ENET_TX_IRQHandler from vector_table_copy.o(.text.ENET_TX_IRQHandler) referenced from vector.o(.isr_vector)
  - FMU_Alarm_IRQHandler from vector_table_copy.o(.text.FMU_Alarm_IRQHandler) referenced from vector.o(.isr_vector)
  - FMU_MISC_IRQHandler from vector_table_copy.o(.text.FMU_MISC_IRQHandler) referenced from vector.o(.isr_vector)
  - FPU_IRQHandler from vector_table_copy.o(.text.FPU_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOA_IRQHandler from vector_table_copy.o(.text.GPIOA_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOB_IRQHandler from vector_table_copy.o(.text.GPIOB_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOC_IRQHandler from vector_table_copy.o(.text.GPIOC_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOD_IRQHandler from vector_table_copy.o(.text.GPIOD_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOE_IRQHandler from vector_table_copy.o(.text.GPIOE_IRQHandler) referenced from vector.o(.isr_vector)
  - HCU_IRQHandler from vector_table_copy.o(.text.HCU_IRQHandler) referenced from vector.o(.isr_vector)
  - HardFault_Handler from vector_table_copy.o(.text.HardFault_Handler) referenced from vector.o(.isr_vector)
  - I2C0_Master_Slave_IRQHandler from vector_table_copy.o(.text.I2C0_Master_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C1_Master_Slave_IRQHandler from vector_table_copy.o(.text.I2C1_Master_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C2_Master_Slave_IRQHandler from vector_table_copy.o(.text.I2C2_Master_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C3_Master_Slave_IRQHandler from vector_table_copy.o(.text.I2C3_Master_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C4_Master_Slave_IRQHandler from vector_table_copy.o(.text.I2C4_Master_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - INTM_IRQHandler from vector_table_copy.o(.text.INTM_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD0_IRQHandler from vector_table_copy.o(.text.LINFlexD0_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD1_IRQHandler from vector_table_copy.o(.text.LINFlexD1_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD2_IRQHandler from vector_table_copy.o(.text.LINFlexD2_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD3_IRQHandler from vector_table_copy.o(.text.LINFlexD3_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD4_IRQHandler from vector_table_copy.o(.text.LINFlexD4_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD5_IRQHandler from vector_table_copy.o(.text.LINFlexD5_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD6_IRQHandler from vector_table_copy.o(.text.LINFlexD6_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD7_IRQHandler from vector_table_copy.o(.text.LINFlexD7_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD8_IRQHandler from vector_table_copy.o(.text.LINFlexD8_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD9_IRQHandler from vector_table_copy.o(.text.LINFlexD9_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch0_Ch7_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch0_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch8_Ch15_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch8_Ch15_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM1_Ch0_Ch7_IRQHandler from vector_table_copy.o(.text.MPWM1_Ch0_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM1_Ch8_Ch15_IRQHandler from vector_table_copy.o(.text.MPWM1_Ch8_Ch15_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM2_Ch0_Ch7_IRQHandler from vector_table_copy.o(.text.MPWM2_Ch0_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM2_Ch8_Ch15_IRQHandler from vector_table_copy.o(.text.MPWM2_Ch8_Ch15_IRQHandler) referenced from vector.o(.isr_vector)
  - MemManage_Handler from vector_table_copy.o(.text.MemManage_Handler) referenced from vector.o(.isr_vector)
  - NMI_Handler from vector_table_copy.o(.text.NMI_Handler) referenced from vector.o(.isr_vector)
  - PCU_IRQHandler from vector_table_copy.o(.text.PCU_IRQHandler) referenced from vector.o(.isr_vector)
  - PTU0_IRQHandler from vector_table_copy.o(.text.PTU0_IRQHandler) referenced from vector.o(.isr_vector)
  - PTU1_IRQHandler from vector_table_copy.o(.text.PTU1_IRQHandler) referenced from vector.o(.isr_vector)
  - PendSV_Handler from vector_table_copy.o(.text.PendSV_Handler) referenced from vector.o(.isr_vector)
  - QSPI_IRQHandler from vector_table_copy.o(.text.QSPI_IRQHandler) referenced from vector.o(.isr_vector)
  - RTC_IRQHandler from vector_table_copy.o(.text.RTC_IRQHandler) referenced from vector.o(.isr_vector)
  - RTC_Seconds_IRQHandler from vector_table_copy.o(.text.RTC_Seconds_IRQHandler) referenced from vector.o(.isr_vector)
  - RamInit1 from raminit1.o(.text.RamInit1) referenced from startup.o(.text)
  - RamInit2 from raminit2.o(.text.RamInit2) referenced from startup.o(.text)
  - Reset_Handler from startup.o(.text) referenced from vector.o(.isr_vector)
  - SAI0_IRQHandler from vector_table_copy.o(.text.SAI0_IRQHandler) referenced from vector.o(.isr_vector)
  - SAI1_IRQHandler from vector_table_copy.o(.text.SAI1_IRQHandler) referenced from vector.o(.isr_vector)
  - SCU_IRQHandler from vector_table_copy.o(.text.SCU_IRQHandler) referenced from vector.o(.isr_vector)
  - SENT0_IRQHandler from vector_table_copy.o(.text.SENT0_IRQHandler) referenced from vector.o(.isr_vector)
  - SENT1_IRQHandler from vector_table_copy.o(.text.SENT1_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI0_IRQHandler from vector_table_copy.o(.text.SPI0_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI1_IRQHandler from vector_table_copy.o(.text.SPI1_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI2_IRQHandler from vector_table_copy.o(.text.SPI2_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI3_IRQHandler from vector_table_copy.o(.text.SPI3_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI4_IRQHandler from vector_table_copy.o(.text.SPI4_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI5_IRQHandler from vector_table_copy.o(.text.SPI5_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI6_IRQHandler from vector_table_copy.o(.text.SPI6_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI7_IRQHandler from vector_table_copy.o(.text.SPI7_IRQHandler) referenced from vector.o(.isr_vector)
  - SVC_Handler from vector_table_copy.o(.text.SVC_Handler) referenced from vector.o(.isr_vector)
  - SysTick_Handler from vector_table_copy.o(.text.SysTick_Handler) referenced from vector.o(.isr_vector)
  - SystemInit from system.o(.text.SystemInit) referenced from startup.o(.text)
  - TMR0_IRQHandler from vector_table_copy.o(.text.TMR0_IRQHandler) referenced from vector.o(.isr_vector)
  - TMR1_IRQHandler from vector_table_copy.o(.text.TMR1_IRQHandler) referenced from vector.o(.isr_vector)
  - TRNG_IRQHandler from vector_table_copy.o(.text.TRNG_IRQHandler) referenced from vector.o(.isr_vector)
  - UsageFault_Handler from vector_table_copy.o(.text.UsageFault_Handler) referenced from vector.o(.isr_vector)
  - VectorTableCopy from vector_table_copy.o(.text.VectorTableCopy) referenced from startup.o(.text)
  - WKU_IRQHandler from vector_table_copy.o(.text.WKU_IRQHandler) referenced from vector.o(.isr_vector)
  - Wdg_Lld_Isr from vector_table_copy.o(.text.Wdg_Lld_Isr) referenced from vector.o(.isr_vector)
  - eTMR0_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Fault_IRQHandler from vector_table_copy.o(.text.eTMR0_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR0_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Fault_IRQHandler from vector_table_copy.o(.text.eTMR1_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR1_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR2_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR2_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR2_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR2_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Fault_IRQHandler from vector_table_copy.o(.text.eTMR2_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR2_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR3_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR3_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR3_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR3_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Fault_IRQHandler from vector_table_copy.o(.text.eTMR3_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR3_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR4_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR4_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR4_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR4_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Fault_IRQHandler from vector_table_copy.o(.text.eTMR4_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR4_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR5_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR5_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR5_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR5_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Fault_IRQHandler from vector_table_copy.o(.text.eTMR5_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR5_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - lpTMR0_IRQHandler from vector_table_copy.o(.text.lpTMR0_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR0_Ch0_IRQHandler from vector_table_copy.o(.text.pTMR0_Ch0_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR0_Ch1_IRQHandler from vector_table_copy.o(.text.pTMR0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR0_Ch2_IRQHandler from vector_table_copy.o(.text.pTMR0_Ch2_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR0_Ch3_IRQHandler from vector_table_copy.o(.text.pTMR0_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR1_Ch0_IRQHandler from vector_table_copy.o(.text.pTMR1_Ch0_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR1_Ch1_IRQHandler from vector_table_copy.o(.text.pTMR1_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR1_Ch2_IRQHandler from vector_table_copy.o(.text.pTMR1_Ch2_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR1_Ch3_IRQHandler from vector_table_copy.o(.text.pTMR1_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR2_Ch0_IRQHandler from vector_table_copy.o(.text.pTMR2_Ch0_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR2_Ch1_IRQHandler from vector_table_copy.o(.text.pTMR2_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR2_Ch2_IRQHandler from vector_table_copy.o(.text.pTMR2_Ch2_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR2_Ch3_IRQHandler from vector_table_copy.o(.text.pTMR2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)

  ### Global Symbols

  RamInit0 (Thumb, 0 bytes, Stack size unknown bytes, raminit0.o(.text))
  [Called By]

  - >> Reset_Handler

  Reset_Handler (Thumb, 0 bytes, Stack size unknown bytes, startup.o(.text))
  [Stack]

  - Max Depth = 80 + Unknown Stack Size
  - Call Chain = Reset_Handler ⇒ main ⇒ Mcu_InitClock ⇒ Mcu_Lld_InitClock ⇒ Mcu_Lld_SetClockSource
  [Calls]
  - >> RamInit0
  - >> main
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> VectorTableCopy

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> RamInit1

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  ACMP0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ACMP0_IRQHandler))
  [Calls]

  - >> ACMP0_IRQHandler
  [Called By]
  - >> ACMP0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  ACMP1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ACMP1_IRQHandler))
  [Calls]

  - >> ACMP1_IRQHandler
  [Called By]
  - >> ACMP1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  ADC0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ADC0_IRQHandler))
  [Calls]

  - >> ADC0_IRQHandler
  [Called By]
  - >> ADC0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  ADC1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ADC1_IRQHandler))
  [Calls]

  - >> ADC1_IRQHandler
  [Called By]
  - >> ADC1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_Error_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_Error_IRQHandler))
  [Calls]

  - >> CAN0_Error_IRQHandler
  [Called By]
  - >> CAN0_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_0_15_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_0_15_MB_IRQHandler))
  [Calls]

  - >> CAN0_ORed_0_15_MB_IRQHandler
  [Called By]
  - >> CAN0_ORed_0_15_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_112_127_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_112_127_MB_IRQHandler))
  [Calls]

  - >> CAN0_ORed_112_127_MB_IRQHandler
  [Called By]
  - >> CAN0_ORed_112_127_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_16_31_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_16_31_MB_IRQHandler))
  [Calls]

  - >> CAN0_ORed_16_31_MB_IRQHandler
  [Called By]
  - >> CAN0_ORed_16_31_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_32_47_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_32_47_MB_IRQHandler))
  [Calls]

  - >> CAN0_ORed_32_47_MB_IRQHandler
  [Called By]
  - >> CAN0_ORed_32_47_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_48_63_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_48_63_MB_IRQHandler))
  [Calls]

  - >> CAN0_ORed_48_63_MB_IRQHandler
  [Called By]
  - >> CAN0_ORed_48_63_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_64_79_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_64_79_MB_IRQHandler))
  [Calls]

  - >> CAN0_ORed_64_79_MB_IRQHandler
  [Called By]
  - >> CAN0_ORed_64_79_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_80_95_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_80_95_MB_IRQHandler))
  [Calls]

  - >> CAN0_ORed_80_95_MB_IRQHandler
  [Called By]
  - >> CAN0_ORed_80_95_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_96_111_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_96_111_MB_IRQHandler))
  [Calls]

  - >> CAN0_ORed_96_111_MB_IRQHandler
  [Called By]
  - >> CAN0_ORed_96_111_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_IRQHandler))
  [Calls]

  - >> CAN0_ORed_IRQHandler
  [Called By]
  - >> CAN0_ORed_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_Wake_Up_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_Wake_Up_IRQHandler))
  [Calls]

  - >> CAN0_Wake_Up_IRQHandler
  [Called By]
  - >> CAN0_Wake_Up_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_Error_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_Error_IRQHandler))
  [Calls]

  - >> CAN1_Error_IRQHandler
  [Called By]
  - >> CAN1_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_0_15_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_0_15_MB_IRQHandler))
  [Calls]

  - >> CAN1_ORed_0_15_MB_IRQHandler
  [Called By]
  - >> CAN1_ORed_0_15_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_112_127_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_112_127_MB_IRQHandler))
  [Calls]

  - >> CAN1_ORed_112_127_MB_IRQHandler
  [Called By]
  - >> CAN1_ORed_112_127_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_16_31_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_16_31_MB_IRQHandler))
  [Calls]

  - >> CAN1_ORed_16_31_MB_IRQHandler
  [Called By]
  - >> CAN1_ORed_16_31_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_32_47_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_32_47_MB_IRQHandler))
  [Calls]

  - >> CAN1_ORed_32_47_MB_IRQHandler
  [Called By]
  - >> CAN1_ORed_32_47_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_48_63_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_48_63_MB_IRQHandler))
  [Calls]

  - >> CAN1_ORed_48_63_MB_IRQHandler
  [Called By]
  - >> CAN1_ORed_48_63_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_64_79_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_64_79_MB_IRQHandler))
  [Calls]

  - >> CAN1_ORed_64_79_MB_IRQHandler
  [Called By]
  - >> CAN1_ORed_64_79_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_80_95_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_80_95_MB_IRQHandler))
  [Calls]

  - >> CAN1_ORed_80_95_MB_IRQHandler
  [Called By]
  - >> CAN1_ORed_80_95_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_96_111_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_96_111_MB_IRQHandler))
  [Calls]

  - >> CAN1_ORed_96_111_MB_IRQHandler
  [Called By]
  - >> CAN1_ORed_96_111_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_IRQHandler))
  [Calls]

  - >> CAN1_ORed_IRQHandler
  [Called By]
  - >> CAN1_ORed_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_Wake_Up_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_Wake_Up_IRQHandler))
  [Calls]

  - >> CAN1_Wake_Up_IRQHandler
  [Called By]
  - >> CAN1_Wake_Up_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN2_Error_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_Error_IRQHandler))
  [Calls]

  - >> CAN2_Error_IRQHandler
  [Called By]
  - >> CAN2_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN2_ORed_0_15_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_0_15_MB_IRQHandler))
  [Calls]

  - >> CAN2_ORed_0_15_MB_IRQHandler
  [Called By]
  - >> CAN2_ORed_0_15_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN2_ORed_16_31_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_16_31_MB_IRQHandler))
  [Calls]

  - >> CAN2_ORed_16_31_MB_IRQHandler
  [Called By]
  - >> CAN2_ORed_16_31_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN2_ORed_32_47_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_32_47_MB_IRQHandler))
  [Calls]

  - >> CAN2_ORed_32_47_MB_IRQHandler
  [Called By]
  - >> CAN2_ORed_32_47_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN2_ORed_48_63_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_48_63_MB_IRQHandler))
  [Calls]

  - >> CAN2_ORed_48_63_MB_IRQHandler
  [Called By]
  - >> CAN2_ORed_48_63_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN2_ORed_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_IRQHandler))
  [Calls]

  - >> CAN2_ORed_IRQHandler
  [Called By]
  - >> CAN2_ORed_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN2_Wake_Up_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_Wake_Up_IRQHandler))
  [Calls]

  - >> CAN2_Wake_Up_IRQHandler
  [Called By]
  - >> CAN2_Wake_Up_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN3_Error_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_Error_IRQHandler))
  [Calls]

  - >> CAN3_Error_IRQHandler
  [Called By]
  - >> CAN3_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN3_ORed_0_15_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_0_15_MB_IRQHandler))
  [Calls]

  - >> CAN3_ORed_0_15_MB_IRQHandler
  [Called By]
  - >> CAN3_ORed_0_15_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN3_ORed_16_31_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_16_31_MB_IRQHandler))
  [Calls]

  - >> CAN3_ORed_16_31_MB_IRQHandler
  [Called By]
  - >> CAN3_ORed_16_31_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN3_ORed_32_47_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_32_47_MB_IRQHandler))
  [Calls]

  - >> CAN3_ORed_32_47_MB_IRQHandler
  [Called By]
  - >> CAN3_ORed_32_47_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN3_ORed_48_63_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_48_63_MB_IRQHandler))
  [Calls]

  - >> CAN3_ORed_48_63_MB_IRQHandler
  [Called By]
  - >> CAN3_ORed_48_63_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN3_ORed_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_IRQHandler))
  [Calls]

  - >> CAN3_ORed_IRQHandler
  [Called By]
  - >> CAN3_ORed_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN3_Wake_Up_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_Wake_Up_IRQHandler))
  [Calls]

  - >> CAN3_Wake_Up_IRQHandler
  [Called By]
  - >> CAN3_Wake_Up_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN4_Error_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_Error_IRQHandler))
  [Calls]

  - >> CAN4_Error_IRQHandler
  [Called By]
  - >> CAN4_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN4_ORed_0_15_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_0_15_MB_IRQHandler))
  [Calls]

  - >> CAN4_ORed_0_15_MB_IRQHandler
  [Called By]
  - >> CAN4_ORed_0_15_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN4_ORed_16_31_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_16_31_MB_IRQHandler))
  [Calls]

  - >> CAN4_ORed_16_31_MB_IRQHandler
  [Called By]
  - >> CAN4_ORed_16_31_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN4_ORed_32_47_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_32_47_MB_IRQHandler))
  [Calls]

  - >> CAN4_ORed_32_47_MB_IRQHandler
  [Called By]
  - >> CAN4_ORed_32_47_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN4_ORed_48_63_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_48_63_MB_IRQHandler))
  [Calls]

  - >> CAN4_ORed_48_63_MB_IRQHandler
  [Called By]
  - >> CAN4_ORed_48_63_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN4_ORed_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_IRQHandler))
  [Calls]

  - >> CAN4_ORed_IRQHandler
  [Called By]
  - >> CAN4_ORed_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN4_Wake_Up_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_Wake_Up_IRQHandler))
  [Calls]

  - >> CAN4_Wake_Up_IRQHandler
  [Called By]
  - >> CAN4_Wake_Up_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN5_Error_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_Error_IRQHandler))
  [Calls]

  - >> CAN5_Error_IRQHandler
  [Called By]
  - >> CAN5_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN5_ORed_0_15_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_ORed_0_15_MB_IRQHandler))
  [Calls]

  - >> CAN5_ORed_0_15_MB_IRQHandler
  [Called By]
  - >> CAN5_ORed_0_15_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN5_ORed_16_31_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_ORed_16_31_MB_IRQHandler))
  [Calls]

  - >> CAN5_ORed_16_31_MB_IRQHandler
  [Called By]
  - >> CAN5_ORed_16_31_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN5_ORed_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_ORed_IRQHandler))
  [Calls]

  - >> CAN5_ORed_IRQHandler
  [Called By]
  - >> CAN5_ORed_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN5_Wake_Up_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_Wake_Up_IRQHandler))
  [Calls]

  - >> CAN5_Wake_Up_IRQHandler
  [Called By]
  - >> CAN5_Wake_Up_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN6_Error_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN6_Error_IRQHandler))
  [Calls]

  - >> CAN6_Error_IRQHandler
  [Called By]
  - >> CAN6_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN6_ORed_0_15_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN6_ORed_0_15_MB_IRQHandler))
  [Calls]

  - >> CAN6_ORed_0_15_MB_IRQHandler
  [Called By]
  - >> CAN6_ORed_0_15_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN6_ORed_16_31_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN6_ORed_16_31_MB_IRQHandler))
  [Calls]

  - >> CAN6_ORed_16_31_MB_IRQHandler
  [Called By]
  - >> CAN6_ORed_16_31_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN6_ORed_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN6_ORed_IRQHandler))
  [Calls]

  - >> CAN6_ORed_IRQHandler
  [Called By]
  - >> CAN6_ORed_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN6_Wake_Up_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN6_Wake_Up_IRQHandler))
  [Calls]

  - >> CAN6_Wake_Up_IRQHandler
  [Called By]
  - >> CAN6_Wake_Up_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN7_Error_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN7_Error_IRQHandler))
  [Calls]

  - >> CAN7_Error_IRQHandler
  [Called By]
  - >> CAN7_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN7_ORed_0_15_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN7_ORed_0_15_MB_IRQHandler))
  [Calls]

  - >> CAN7_ORed_0_15_MB_IRQHandler
  [Called By]
  - >> CAN7_ORed_0_15_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN7_ORed_16_31_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN7_ORed_16_31_MB_IRQHandler))
  [Calls]

  - >> CAN7_ORed_16_31_MB_IRQHandler
  [Called By]
  - >> CAN7_ORed_16_31_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN7_ORed_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN7_ORed_IRQHandler))
  [Calls]

  - >> CAN7_ORed_IRQHandler
  [Called By]
  - >> CAN7_ORed_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN7_Wake_Up_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN7_Wake_Up_IRQHandler))
  [Calls]

  - >> CAN7_Wake_Up_IRQHandler
  [Called By]
  - >> CAN7_Wake_Up_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CORE_CTI_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CORE_CTI_IRQHandler))
  [Calls]

  - >> CORE_CTI_IRQHandler
  [Called By]
  - >> CORE_CTI_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA0_IRQHandler))
  [Calls]

  - >> DMA0_IRQHandler
  [Called By]
  - >> DMA0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA10_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA10_IRQHandler))
  [Calls]

  - >> DMA10_IRQHandler
  [Called By]
  - >> DMA10_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA11_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA11_IRQHandler))
  [Calls]

  - >> DMA11_IRQHandler
  [Called By]
  - >> DMA11_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA12_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA12_IRQHandler))
  [Calls]

  - >> DMA12_IRQHandler
  [Called By]
  - >> DMA12_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA13_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA13_IRQHandler))
  [Calls]

  - >> DMA13_IRQHandler
  [Called By]
  - >> DMA13_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA14_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA14_IRQHandler))
  [Calls]

  - >> DMA14_IRQHandler
  [Called By]
  - >> DMA14_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA15_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA15_IRQHandler))
  [Calls]

  - >> DMA15_IRQHandler
  [Called By]
  - >> DMA15_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA16_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA16_IRQHandler))
  [Calls]

  - >> DMA16_IRQHandler
  [Called By]
  - >> DMA16_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA17_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA17_IRQHandler))
  [Calls]

  - >> DMA17_IRQHandler
  [Called By]
  - >> DMA17_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA18_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA18_IRQHandler))
  [Calls]

  - >> DMA18_IRQHandler
  [Called By]
  - >> DMA18_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA19_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA19_IRQHandler))
  [Calls]

  - >> DMA19_IRQHandler
  [Called By]
  - >> DMA19_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA1_IRQHandler))
  [Calls]

  - >> DMA1_IRQHandler
  [Called By]
  - >> DMA1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA20_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA20_IRQHandler))
  [Calls]

  - >> DMA20_IRQHandler
  [Called By]
  - >> DMA20_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA21_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA21_IRQHandler))
  [Calls]

  - >> DMA21_IRQHandler
  [Called By]
  - >> DMA21_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA22_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA22_IRQHandler))
  [Calls]

  - >> DMA22_IRQHandler
  [Called By]
  - >> DMA22_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA23_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA23_IRQHandler))
  [Calls]

  - >> DMA23_IRQHandler
  [Called By]
  - >> DMA23_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA24_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA24_IRQHandler))
  [Calls]

  - >> DMA24_IRQHandler
  [Called By]
  - >> DMA24_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA25_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA25_IRQHandler))
  [Calls]

  - >> DMA25_IRQHandler
  [Called By]
  - >> DMA25_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA26_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA26_IRQHandler))
  [Calls]

  - >> DMA26_IRQHandler
  [Called By]
  - >> DMA26_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA27_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA27_IRQHandler))
  [Calls]

  - >> DMA27_IRQHandler
  [Called By]
  - >> DMA27_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA28_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA28_IRQHandler))
  [Calls]

  - >> DMA28_IRQHandler
  [Called By]
  - >> DMA28_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA29_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA29_IRQHandler))
  [Calls]

  - >> DMA29_IRQHandler
  [Called By]
  - >> DMA29_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA2_IRQHandler))
  [Calls]

  - >> DMA2_IRQHandler
  [Called By]
  - >> DMA2_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA30_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA30_IRQHandler))
  [Calls]

  - >> DMA30_IRQHandler
  [Called By]
  - >> DMA30_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA31_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA31_IRQHandler))
  [Calls]

  - >> DMA31_IRQHandler
  [Called By]
  - >> DMA31_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA3_IRQHandler))
  [Calls]

  - >> DMA3_IRQHandler
  [Called By]
  - >> DMA3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA4_IRQHandler))
  [Calls]

  - >> DMA4_IRQHandler
  [Called By]
  - >> DMA4_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA5_IRQHandler))
  [Calls]

  - >> DMA5_IRQHandler
  [Called By]
  - >> DMA5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA6_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA6_IRQHandler))
  [Calls]

  - >> DMA6_IRQHandler
  [Called By]
  - >> DMA6_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA7_IRQHandler))
  [Calls]

  - >> DMA7_IRQHandler
  [Called By]
  - >> DMA7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA8_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA8_IRQHandler))
  [Calls]

  - >> DMA8_IRQHandler
  [Called By]
  - >> DMA8_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA9_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA9_IRQHandler))
  [Calls]

  - >> DMA9_IRQHandler
  [Called By]
  - >> DMA9_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA_Error_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA_Error_IRQHandler))
  [Calls]

  - >> DMA_Error_IRQHandler
  [Called By]
  - >> DMA_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DebugMon_Handler))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DefaultISR (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DefaultISR))
  [Calls]

  - >> DefaultISR
  [Called By]
  - >> DefaultISR
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  Det_ReportError (Thumb, 38 bytes, Stack size 0 bytes, det.o(.text.Det_ReportError))
  [Called By]

  - >> Fls_Cancel
  - >> Mcu_GetResetRawValue
  - >> Mcu_SetMode
  - >> Mcu_InitRamSection
  - >> Mcu_GetResetReason
  - >> Fls_BlankCheck
  - >> Fls_GetJobResult
  - >> Fls_Compare
  - >> Fls_Read
  - >> Fls_Write
  - >> Fls_Erase
  - >> Fls_Init
  - >> Mcu_DistributePllClock
  - >> Mcu_GetPllStatus
  - >> Mcu_InitClock
  - >> Mcu_Init

  Det_ReportRuntimeError (Thumb, 38 bytes, Stack size 0 bytes, det.o(.text.Det_ReportRuntimeError))
  [Called By]

  - >> Fls_Lld_TranslateReturnCode
  - >> Fls_Lld_MainFunction

  Det_ReportTransientFault (Thumb, 38 bytes, Stack size 0 bytes, det.o(.text.Det_ReportTransientFault))
  [Called By]

  - >> Fls_Lld_MainFunction
  - >> Fls_DoJobDataTransfer
  - >> Fls_MainFunction

  EFM_Ecc_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_Ecc_IRQHandler))
  [Calls]

  - >> EFM_Ecc_IRQHandler
  [Called By]
  - >> EFM_Ecc_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  EFM_Error_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_Error_IRQHandler))
  [Calls]

  - >> EFM_Error_IRQHandler
  [Called By]
  - >> EFM_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  EFM_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_IRQHandler))
  [Calls]

  - >> EFM_IRQHandler
  [Called By]
  - >> EFM_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  EMU_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EMU_IRQHandler))
  [Calls]

  - >> EMU_IRQHandler
  [Called By]
  - >> EMU_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  ENET_ECC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ENET_ECC_IRQHandler))
  [Calls]

  - >> ENET_ECC_IRQHandler
  [Called By]
  - >> ENET_ECC_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  ENET_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ENET_IRQHandler))
  [Calls]

  - >> ENET_IRQHandler
  [Called By]
  - >> ENET_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  ENET_RX_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ENET_RX_IRQHandler))
  [Calls]

  - >> ENET_RX_IRQHandler
  [Called By]
  - >> ENET_RX_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  ENET_TX_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ENET_TX_IRQHandler))
  [Calls]

  - >> ENET_TX_IRQHandler
  [Called By]
  - >> ENET_TX_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  FMU_Alarm_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.FMU_Alarm_IRQHandler))
  [Calls]

  - >> FMU_Alarm_IRQHandler
  [Called By]
  - >> FMU_Alarm_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  FMU_MISC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.FMU_MISC_IRQHandler))
  [Calls]

  - >> FMU_MISC_IRQHandler
  [Called By]
  - >> FMU_MISC_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  FPU_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.FPU_IRQHandler))
  [Calls]

  - >> FPU_IRQHandler
  [Called By]
  - >> FPU_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  Fls_Lld_TranslateReturnCode (Thumb, 88 bytes, Stack size 8 bytes, fls_lld.o(.text.Fls_Lld_TranslateReturnCode))
  [Stack]

  - Max Depth = 8
  - Call Chain = Fls_Lld_TranslateReturnCode
  [Calls]
  - >> Det_ReportRuntimeError
  [Called By]
  - >> Fls_DoJobDataTransfer
  - >> Fls_MainFunction

  GPIOA_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOA_IRQHandler))
  [Calls]

  - >> GPIOA_IRQHandler
  [Called By]
  - >> GPIOA_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  GPIOB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOB_IRQHandler))
  [Calls]

  - >> GPIOB_IRQHandler
  [Called By]
  - >> GPIOB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  GPIOC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOC_IRQHandler))
  [Calls]

  - >> GPIOC_IRQHandler
  [Called By]
  - >> GPIOC_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  GPIOD_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOD_IRQHandler))
  [Calls]

  - >> GPIOD_IRQHandler
  [Called By]
  - >> GPIOD_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  GPIOE_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOE_IRQHandler))
  [Calls]

  - >> GPIOE_IRQHandler
  [Called By]
  - >> GPIOE_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  HCU_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.HCU_IRQHandler))
  [Calls]

  - >> HCU_IRQHandler
  [Called By]
  - >> HCU_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  I2C0_Master_Slave_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C0_Master_Slave_IRQHandler))
  [Calls]

  - >> I2C0_Master_Slave_IRQHandler
  [Called By]
  - >> I2C0_Master_Slave_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  I2C1_Master_Slave_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C1_Master_Slave_IRQHandler))
  [Calls]

  - >> I2C1_Master_Slave_IRQHandler
  [Called By]
  - >> I2C1_Master_Slave_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  I2C2_Master_Slave_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C2_Master_Slave_IRQHandler))
  [Calls]

  - >> I2C2_Master_Slave_IRQHandler
  [Called By]
  - >> I2C2_Master_Slave_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  I2C3_Master_Slave_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C3_Master_Slave_IRQHandler))
  [Calls]

  - >> I2C3_Master_Slave_IRQHandler
  [Called By]
  - >> I2C3_Master_Slave_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  I2C4_Master_Slave_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C4_Master_Slave_IRQHandler))
  [Calls]

  - >> I2C4_Master_Slave_IRQHandler
  [Called By]
  - >> I2C4_Master_Slave_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  INTM_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.INTM_IRQHandler))
  [Calls]

  - >> INTM_IRQHandler
  [Called By]
  - >> INTM_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  LINFlexD0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD0_IRQHandler))
  [Calls]

  - >> LINFlexD0_IRQHandler
  [Called By]
  - >> LINFlexD0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  LINFlexD1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD1_IRQHandler))
  [Calls]

  - >> LINFlexD1_IRQHandler
  [Called By]
  - >> LINFlexD1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  LINFlexD2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD2_IRQHandler))
  [Calls]

  - >> LINFlexD2_IRQHandler
  [Called By]
  - >> LINFlexD2_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  LINFlexD3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD3_IRQHandler))
  [Calls]

  - >> LINFlexD3_IRQHandler
  [Called By]
  - >> LINFlexD3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  LINFlexD4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD4_IRQHandler))
  [Calls]

  - >> LINFlexD4_IRQHandler
  [Called By]
  - >> LINFlexD4_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  LINFlexD5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD5_IRQHandler))
  [Calls]

  - >> LINFlexD5_IRQHandler
  [Called By]
  - >> LINFlexD5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  LINFlexD6_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD6_IRQHandler))
  [Calls]

  - >> LINFlexD6_IRQHandler
  [Called By]
  - >> LINFlexD6_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  LINFlexD7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD7_IRQHandler))
  [Calls]

  - >> LINFlexD7_IRQHandler
  [Called By]
  - >> LINFlexD7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  LINFlexD8_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD8_IRQHandler))
  [Calls]

  - >> LINFlexD8_IRQHandler
  [Called By]
  - >> LINFlexD8_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  LINFlexD9_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD9_IRQHandler))
  [Calls]

  - >> LINFlexD9_IRQHandler
  [Called By]
  - >> LINFlexD9_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM0_Ch0_Ch7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch0_Ch7_IRQHandler))
  [Calls]

  - >> MPWM0_Ch0_Ch7_IRQHandler
  [Called By]
  - >> MPWM0_Ch0_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM0_Ch8_Ch15_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch8_Ch15_IRQHandler))
  [Calls]

  - >> MPWM0_Ch8_Ch15_IRQHandler
  [Called By]
  - >> MPWM0_Ch8_Ch15_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM1_Ch0_Ch7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM1_Ch0_Ch7_IRQHandler))
  [Calls]

  - >> MPWM1_Ch0_Ch7_IRQHandler
  [Called By]
  - >> MPWM1_Ch0_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM1_Ch8_Ch15_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM1_Ch8_Ch15_IRQHandler))
  [Calls]

  - >> MPWM1_Ch8_Ch15_IRQHandler
  [Called By]
  - >> MPWM1_Ch8_Ch15_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM2_Ch0_Ch7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM2_Ch0_Ch7_IRQHandler))
  [Calls]

  - >> MPWM2_Ch0_Ch7_IRQHandler
  [Called By]
  - >> MPWM2_Ch0_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM2_Ch8_Ch15_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM2_Ch8_Ch15_IRQHandler))
  [Calls]

  - >> MPWM2_Ch8_Ch15_IRQHandler
  [Called By]
  - >> MPWM2_Ch8_Ch15_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.NMI_Handler))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  PCU_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.PCU_IRQHandler))
  [Calls]

  - >> PCU_IRQHandler
  [Called By]
  - >> PCU_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  PTU0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.PTU0_IRQHandler))
  [Calls]

  - >> PTU0_IRQHandler
  [Called By]
  - >> PTU0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  PTU1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.PTU1_IRQHandler))
  [Calls]

  - >> PTU1_IRQHandler
  [Called By]
  - >> PTU1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.PendSV_Handler))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  QSPI_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.QSPI_IRQHandler))
  [Calls]

  - >> QSPI_IRQHandler
  [Called By]
  - >> QSPI_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  RTC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.RTC_IRQHandler))
  [Calls]

  - >> RTC_IRQHandler
  [Called By]
  - >> RTC_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  RTC_Seconds_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.RTC_Seconds_IRQHandler))
  [Calls]

  - >> RTC_Seconds_IRQHandler
  [Called By]
  - >> RTC_Seconds_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  RamInit1 (Thumb, 482 bytes, Stack size 48 bytes, raminit1.o(.text.RamInit1))
  [Stack]

  - Max Depth = 48
  - Call Chain = RamInit1
  [Calls]
  - >> __aeabi_memclr4
  [Address Reference Count : 1]
  - startup.o(.text)

  RamInit2 (Thumb, 2 bytes, Stack size 0 bytes, raminit2.o(.text.RamInit2))
  [Address Reference Count : 1]

  - startup.o(.text)

  SAI0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SAI0_IRQHandler))
  [Calls]

  - >> SAI0_IRQHandler
  [Called By]
  - >> SAI0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SAI1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SAI1_IRQHandler))
  [Calls]

  - >> SAI1_IRQHandler
  [Called By]
  - >> SAI1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SCU_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SCU_IRQHandler))
  [Calls]

  - >> SCU_IRQHandler
  [Called By]
  - >> SCU_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SENT0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SENT0_IRQHandler))
  [Calls]

  - >> SENT0_IRQHandler
  [Called By]
  - >> SENT0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SENT1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SENT1_IRQHandler))
  [Calls]

  - >> SENT1_IRQHandler
  [Called By]
  - >> SENT1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SPI0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI0_IRQHandler))
  [Calls]

  - >> SPI0_IRQHandler
  [Called By]
  - >> SPI0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SPI1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI1_IRQHandler))
  [Calls]

  - >> SPI1_IRQHandler
  [Called By]
  - >> SPI1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SPI2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI2_IRQHandler))
  [Calls]

  - >> SPI2_IRQHandler
  [Called By]
  - >> SPI2_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SPI3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI3_IRQHandler))
  [Calls]

  - >> SPI3_IRQHandler
  [Called By]
  - >> SPI3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SPI4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI4_IRQHandler))
  [Calls]

  - >> SPI4_IRQHandler
  [Called By]
  - >> SPI4_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SPI5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI5_IRQHandler))
  [Calls]

  - >> SPI5_IRQHandler
  [Called By]
  - >> SPI5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SPI6_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI6_IRQHandler))
  [Calls]

  - >> SPI6_IRQHandler
  [Called By]
  - >> SPI6_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SPI7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI7_IRQHandler))
  [Calls]

  - >> SPI7_IRQHandler
  [Called By]
  - >> SPI7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SVC_Handler))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SysTick_Handler))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SystemInit (Thumb, 358 bytes, Stack size 48 bytes, system.o(.text.SystemInit))
  [Stack]

  - Max Depth = 68
  - Call Chain = SystemInit ⇒ Mpu_Lld_M7_Init
  [Calls]
  - >> Mpu_Lld_M7_Init
  [Address Reference Count : 1]
  - startup.o(.text)

  TMR0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.TMR0_IRQHandler))
  [Calls]

  - >> TMR0_IRQHandler
  [Called By]
  - >> TMR0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  TMR1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.TMR1_IRQHandler))
  [Calls]

  - >> TMR1_IRQHandler
  [Called By]
  - >> TMR1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  TRNG_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.TRNG_IRQHandler))
  [Calls]

  - >> TRNG_IRQHandler
  [Called By]
  - >> TRNG_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  VectorTableCopy (Thumb, 76 bytes, Stack size 8 bytes, vector_table_copy.o(.text.VectorTableCopy))
  [Stack]

  - Max Depth = 8
  - Call Chain = VectorTableCopy
  [Calls]
  - >> __aeabi_memcpy4
  - >> Sys_GetCoreID
  [Address Reference Count : 1]
  - startup.o(.text)

  WKU_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.WKU_IRQHandler))
  [Calls]

  - >> WKU_IRQHandler
  [Called By]
  - >> WKU_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  Wdg_Lld_Isr (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.Wdg_Lld_Isr))
  [Calls]

  - >> Wdg_Lld_Isr
  [Called By]
  - >> Wdg_Lld_Isr
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ch0_Ch1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ch0_Ch1_IRQHandler))
  [Calls]

  - >> eTMR0_Ch0_Ch1_IRQHandler
  [Called By]
  - >> eTMR0_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ch2_Ch3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ch2_Ch3_IRQHandler))
  [Calls]

  - >> eTMR0_Ch2_Ch3_IRQHandler
  [Called By]
  - >> eTMR0_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ch4_Ch5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ch4_Ch5_IRQHandler))
  [Calls]

  - >> eTMR0_Ch4_Ch5_IRQHandler
  [Called By]
  - >> eTMR0_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ch6_Ch7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ch6_Ch7_IRQHandler))
  [Calls]

  - >> eTMR0_Ch6_Ch7_IRQHandler
  [Called By]
  - >> eTMR0_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Fault_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Fault_IRQHandler))
  [Calls]

  - >> eTMR0_Fault_IRQHandler
  [Called By]
  - >> eTMR0_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ovf_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ovf_IRQHandler))
  [Calls]

  - >> eTMR0_Ovf_IRQHandler
  [Called By]
  - >> eTMR0_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ch0_Ch1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ch0_Ch1_IRQHandler))
  [Calls]

  - >> eTMR1_Ch0_Ch1_IRQHandler
  [Called By]
  - >> eTMR1_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ch2_Ch3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ch2_Ch3_IRQHandler))
  [Calls]

  - >> eTMR1_Ch2_Ch3_IRQHandler
  [Called By]
  - >> eTMR1_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ch4_Ch5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ch4_Ch5_IRQHandler))
  [Calls]

  - >> eTMR1_Ch4_Ch5_IRQHandler
  [Called By]
  - >> eTMR1_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ch6_Ch7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ch6_Ch7_IRQHandler))
  [Calls]

  - >> eTMR1_Ch6_Ch7_IRQHandler
  [Called By]
  - >> eTMR1_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Fault_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Fault_IRQHandler))
  [Calls]

  - >> eTMR1_Fault_IRQHandler
  [Called By]
  - >> eTMR1_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ovf_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ovf_IRQHandler))
  [Calls]

  - >> eTMR1_Ovf_IRQHandler
  [Called By]
  - >> eTMR1_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ch0_Ch1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR2_Ch0_Ch1_IRQHandler))
  [Calls]

  - >> eTMR2_Ch0_Ch1_IRQHandler
  [Called By]
  - >> eTMR2_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ch2_Ch3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR2_Ch2_Ch3_IRQHandler))
  [Calls]

  - >> eTMR2_Ch2_Ch3_IRQHandler
  [Called By]
  - >> eTMR2_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ch4_Ch5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR2_Ch4_Ch5_IRQHandler))
  [Calls]

  - >> eTMR2_Ch4_Ch5_IRQHandler
  [Called By]
  - >> eTMR2_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ch6_Ch7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR2_Ch6_Ch7_IRQHandler))
  [Calls]

  - >> eTMR2_Ch6_Ch7_IRQHandler
  [Called By]
  - >> eTMR2_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Fault_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR2_Fault_IRQHandler))
  [Calls]

  - >> eTMR2_Fault_IRQHandler
  [Called By]
  - >> eTMR2_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ovf_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR2_Ovf_IRQHandler))
  [Calls]

  - >> eTMR2_Ovf_IRQHandler
  [Called By]
  - >> eTMR2_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ch0_Ch1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR3_Ch0_Ch1_IRQHandler))
  [Calls]

  - >> eTMR3_Ch0_Ch1_IRQHandler
  [Called By]
  - >> eTMR3_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ch2_Ch3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR3_Ch2_Ch3_IRQHandler))
  [Calls]

  - >> eTMR3_Ch2_Ch3_IRQHandler
  [Called By]
  - >> eTMR3_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ch4_Ch5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR3_Ch4_Ch5_IRQHandler))
  [Calls]

  - >> eTMR3_Ch4_Ch5_IRQHandler
  [Called By]
  - >> eTMR3_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ch6_Ch7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR3_Ch6_Ch7_IRQHandler))
  [Calls]

  - >> eTMR3_Ch6_Ch7_IRQHandler
  [Called By]
  - >> eTMR3_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Fault_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR3_Fault_IRQHandler))
  [Calls]

  - >> eTMR3_Fault_IRQHandler
  [Called By]
  - >> eTMR3_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ovf_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR3_Ovf_IRQHandler))
  [Calls]

  - >> eTMR3_Ovf_IRQHandler
  [Called By]
  - >> eTMR3_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ch0_Ch1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR4_Ch0_Ch1_IRQHandler))
  [Calls]

  - >> eTMR4_Ch0_Ch1_IRQHandler
  [Called By]
  - >> eTMR4_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ch2_Ch3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR4_Ch2_Ch3_IRQHandler))
  [Calls]

  - >> eTMR4_Ch2_Ch3_IRQHandler
  [Called By]
  - >> eTMR4_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ch4_Ch5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR4_Ch4_Ch5_IRQHandler))
  [Calls]

  - >> eTMR4_Ch4_Ch5_IRQHandler
  [Called By]
  - >> eTMR4_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ch6_Ch7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR4_Ch6_Ch7_IRQHandler))
  [Calls]

  - >> eTMR4_Ch6_Ch7_IRQHandler
  [Called By]
  - >> eTMR4_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Fault_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR4_Fault_IRQHandler))
  [Calls]

  - >> eTMR4_Fault_IRQHandler
  [Called By]
  - >> eTMR4_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ovf_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR4_Ovf_IRQHandler))
  [Calls]

  - >> eTMR4_Ovf_IRQHandler
  [Called By]
  - >> eTMR4_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ch0_Ch1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR5_Ch0_Ch1_IRQHandler))
  [Calls]

  - >> eTMR5_Ch0_Ch1_IRQHandler
  [Called By]
  - >> eTMR5_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ch2_Ch3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR5_Ch2_Ch3_IRQHandler))
  [Calls]

  - >> eTMR5_Ch2_Ch3_IRQHandler
  [Called By]
  - >> eTMR5_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ch4_Ch5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR5_Ch4_Ch5_IRQHandler))
  [Calls]

  - >> eTMR5_Ch4_Ch5_IRQHandler
  [Called By]
  - >> eTMR5_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ch6_Ch7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR5_Ch6_Ch7_IRQHandler))
  [Calls]

  - >> eTMR5_Ch6_Ch7_IRQHandler
  [Called By]
  - >> eTMR5_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Fault_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR5_Fault_IRQHandler))
  [Calls]

  - >> eTMR5_Fault_IRQHandler
  [Called By]
  - >> eTMR5_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ovf_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR5_Ovf_IRQHandler))
  [Calls]

  - >> eTMR5_Ovf_IRQHandler
  [Called By]
  - >> eTMR5_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  lpTMR0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.lpTMR0_IRQHandler))
  [Calls]

  - >> lpTMR0_IRQHandler
  [Called By]
  - >> lpTMR0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  main (Thumb, 918 bytes, Stack size 0 bytes, main.o(.text.main))
  [Stack]

  - Max Depth = 80
  - Call Chain = main ⇒ Mcu_InitClock ⇒ Mcu_Lld_InitClock ⇒ Mcu_Lld_SetClockSource
  [Calls]
  - >> Fls_BlankCheck
  - >> Fls_GetJobResult
  - >> Fls_Compare
  - >> Fls_Read
  - >> Fls_Write
  - >> Fls_GetStatus
  - >> Fls_MainFunction
  - >> Fls_Erase
  - >> Fls_Init
  - >> Mcu_DistributePllClock
  - >> Mcu_GetPllStatus
  - >> Mcu_InitClock
  - >> Mcu_Init
  [Called By]
  - >> Reset_Handler

  pTMR0_Ch0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR0_Ch0_IRQHandler))
  [Calls]

  - >> pTMR0_Ch0_IRQHandler
  [Called By]
  - >> pTMR0_Ch0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  pTMR0_Ch1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR0_Ch1_IRQHandler))
  [Calls]

  - >> pTMR0_Ch1_IRQHandler
  [Called By]
  - >> pTMR0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  pTMR0_Ch2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR0_Ch2_IRQHandler))
  [Calls]

  - >> pTMR0_Ch2_IRQHandler
  [Called By]
  - >> pTMR0_Ch2_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  pTMR0_Ch3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR0_Ch3_IRQHandler))
  [Calls]

  - >> pTMR0_Ch3_IRQHandler
  [Called By]
  - >> pTMR0_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  pTMR1_Ch0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR1_Ch0_IRQHandler))
  [Calls]

  - >> pTMR1_Ch0_IRQHandler
  [Called By]
  - >> pTMR1_Ch0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  pTMR1_Ch1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR1_Ch1_IRQHandler))
  [Calls]

  - >> pTMR1_Ch1_IRQHandler
  [Called By]
  - >> pTMR1_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  pTMR1_Ch2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR1_Ch2_IRQHandler))
  [Calls]

  - >> pTMR1_Ch2_IRQHandler
  [Called By]
  - >> pTMR1_Ch2_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  pTMR1_Ch3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR1_Ch3_IRQHandler))
  [Calls]

  - >> pTMR1_Ch3_IRQHandler
  [Called By]
  - >> pTMR1_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  pTMR2_Ch0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR2_Ch0_IRQHandler))
  [Calls]

  - >> pTMR2_Ch0_IRQHandler
  [Called By]
  - >> pTMR2_Ch0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  pTMR2_Ch1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR2_Ch1_IRQHandler))
  [Calls]

  - >> pTMR2_Ch1_IRQHandler
  [Called By]
  - >> pTMR2_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  pTMR2_Ch2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR2_Ch2_IRQHandler))
  [Calls]

  - >> pTMR2_Ch2_IRQHandler
  [Called By]
  - >> pTMR2_Ch2_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  pTMR2_Ch3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR2_Ch3_IRQHandler))
  [Calls]

  - >> pTMR2_Ch3_IRQHandler
  [Called By]
  - >> pTMR2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  Sys_GetCoreID (Thumb, 4 bytes, Stack size 0 bytes, osif.o(.mcal_text))
  [Called By]

  - >> VectorTableCopy

  Mpu_Lld_M7_Init (Thumb, 398 bytes, Stack size 20 bytes, mpu_lld_m7.o(.mcal_text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Mpu_Lld_M7_Init
  [Called By]
  - >> SystemInit

  Mcu_DistributePllClock (Thumb, 58 bytes, Stack size 8 bytes, mcu.o(.mcal_text))
  [Stack]

  - Max Depth = 52
  - Call Chain = Mcu_DistributePllClock ⇒ Mcu_Lld_SetClockSource
  [Calls]
  - >> Mcu_Lld_SetClockSource
  - >> Mcu_Lld_GetPllStatus
  - >> Det_ReportError
  [Called By]
  - >> main

  Mcu_GetPllStatus (Thumb, 40 bytes, Stack size 8 bytes, mcu.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Mcu_GetPllStatus
  [Calls]
  - >> Mcu_Lld_GetPllStatus
  - >> Det_ReportError
  [Called By]
  - >> main

  Mcu_GetResetReason (Thumb, 40 bytes, Stack size 8 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_GetResetValue
  - >> Det_ReportError

  Mcu_Init (Thumb, 78 bytes, Stack size 16 bytes, mcu.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Mcu_Init ⇒ Mcu_Lld_SetPcu
  [Calls]
  - >> Mcu_Lld_SetPcu
  - >> Mcu_Lld_SetRcu
  - >> Det_ReportError
  [Called By]
  - >> main

  Mcu_InitClock (Thumb, 72 bytes, Stack size 8 bytes, mcu.o(.mcal_text))
  [Stack]

  - Max Depth = 80
  - Call Chain = Mcu_InitClock ⇒ Mcu_Lld_InitClock ⇒ Mcu_Lld_SetClockSource
  [Calls]
  - >> Mcu_Lld_InitClock
  - >> Det_ReportError
  [Called By]
  - >> main

  Mcu_InitRamSection (Thumb, 78 bytes, Stack size 8 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_SetRamSection
  - >> Det_ReportError

  Mcu_SetMode (Thumb, 80 bytes, Stack size 16 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00
  - >> Mcu_Lld_SetMode
  - >> SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00
  - >> Det_ReportError

  Mcu_GetResetRawValue (Thumb, 42 bytes, Stack size 8 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_GetResetRawValue
  - >> Det_ReportError

  Mcu_180_GetCoreClockFrequency (Thumb, 32 bytes, Stack size 0 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_GetCoreClockFrequency

  Mcu_Lld_SetCmuChannel2 (Thumb, 16 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)

  Mcu_Lld_GetPllStatus (Thumb, 16 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_DistributePllClock
  - >> Mcu_GetPllStatus

  Mcu_Lld_SystemReset (Thumb, 36 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)

  Mcu_Lld_SetRcu (Thumb, 52 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Init

  Mcu_Lld_SetRamSection (Thumb, 76 bytes, Stack size 8 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_InitRamSection

  Mcu_Lld_SetMode (Thumb, 238 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_SetMode

  Mcu_Lld_SetClockSource (Thumb, 1450 bytes, Stack size 44 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 44
  - Call Chain = Mcu_Lld_SetClockSource
  [Called By]
  - >> Mcu_Lld_InitClock
  - >> Mcu_DistributePllClock

  Mcu_Lld_SetPeripheralClock (Thumb, 482 bytes, Stack size 24 bytes, mcu_lld.o(.mcal_text), UNUSED)

  Mcu_Lld_InitClock (Thumb, 968 bytes, Stack size 28 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 72
  - Call Chain = Mcu_Lld_InitClock ⇒ Mcu_Lld_SetClockSource
  [Calls]
  - >> Mcu_Lld_SetClockSource
  [Called By]
  - >> Mcu_InitClock

  Mcu_Lld_GetResetRawValue (Thumb, 24 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_GetResetRawValue

  Mcu_Lld_GetResetValue (Thumb, 184 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_GetResetReason

  Mcu_Lld_GetPllClockFrequency (Thumb, 74 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)

  Mcu_Lld_GetCoreClockFrequency (Thumb, 134 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_180_GetCoreClockFrequency

  Mcu_Lld_SetPcu (Thumb, 90 bytes, Stack size 8 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Mcu_Lld_SetPcu
  [Called By]
  - >> Mcu_Init

  Mcu_schm_read_msr (Thumb, 6 bytes, Stack size 0 bytes, schm_mcu.o(.mcal_text), UNUSED)

  SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00 (Thumb, 44 bytes, Stack size 0 bytes, schm_mcu.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_SetMode

  SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00 (Thumb, 34 bytes, Stack size 0 bytes, schm_mcu.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_SetMode

  Fls_Init (Thumb, 110 bytes, Stack size 8 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Fls_Init
  [Calls]
  - >> Fls_Lld_Init
  - >> Det_ReportError
  [Called By]
  - >> main

  Fls_Erase (Thumb, 402 bytes, Stack size 24 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Fls_Erase
  [Calls]
  - >> SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_02
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_02
  - >> Det_ReportError
  [Called By]
  - >> main

  Fls_Write (Thumb, 470 bytes, Stack size 32 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Fls_Write
  [Calls]
  - >> SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_03
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_03
  - >> Det_ReportError
  [Called By]
  - >> main

  Fls_Cancel (Thumb, 112 bytes, Stack size 16 bytes, fls.o(.mcal_text), UNUSED)
  [Calls]

  - >> Fls_Lld_Cancel
  - >> Det_ReportError

  Fls_GetStatus (Thumb, 26 bytes, Stack size 0 bytes, fls.o(.mcal_text))
  [Called By]

  - >> main

  Fls_GetJobResult (Thumb, 36 bytes, Stack size 8 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Fls_GetJobResult
  [Calls]
  - >> Det_ReportError
  [Called By]
  - >> main

  Fls_Read (Thumb, 430 bytes, Stack size 32 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Fls_Read
  [Calls]
  - >> SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_06
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_06
  - >> Det_ReportError
  [Called By]
  - >> main

  Fls_MainFunction (Thumb, 288 bytes, Stack size 24 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 64
  - Call Chain = Fls_MainFunction ⇒ Fls_Lld_SectorErase ⇒ Fls_Lld_LoadCommandSync
  [Calls]
  - >> Fls_Lld_GetPhycSectorSize
  - >> Fls_Lld_TranslateReturnCode
  - >> Fls_Lld_SectorErase
  - >> Fls_Lld_MainFunction
  - >> Det_ReportTransientFault
  [Called By]
  - >> main

  Fls_Compare (Thumb, 390 bytes, Stack size 32 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Fls_Compare
  [Calls]
  - >> SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_04
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_04
  - >> Det_ReportError
  [Called By]
  - >> main

  Fls_BlankCheck (Thumb, 388 bytes, Stack size 24 bytes, fls.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Fls_BlankCheck
  [Calls]
  - >> SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_05
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_05
  - >> Det_ReportError
  [Called By]
  - >> main

  Fls_Lld_GetOneBitEccErrFlag (Thumb, 14 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text), UNUSED)

  Fls_Lld_GetTwoBitEccErrFlag (Thumb, 14 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text), UNUSED)

  Fls_Lld_ClearOneBitEccErrFlag (Thumb, 12 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text), UNUSED)

  Fls_Lld_ClearTwoBitEccErrFlag (Thumb, 12 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text), UNUSED)

  Fls_Lld_GetEccErrAddr (Thumb, 10 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text), UNUSED)

  Fls_Lld_Init (Thumb, 118 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text))
  [Called By]

  - >> Fls_Init

  Fls_Lld_SectorErase (Thumb, 544 bytes, Stack size 24 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Fls_Lld_SectorErase ⇒ Fls_Lld_LoadCommandSync
  [Calls]
  - >> SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_00
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_00
  - >> Fls_Lld_LoadCommandSync (via Veneer)
  [Called By]
  - >> Fls_MainFunction

  Fls_Lld_ReadFlash (Thumb, 522 bytes, Stack size 16 bytes, fls_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_07
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_07
  - >> Fls_Lld_LoadAESCommand (via Veneer)
  [Called By]
  - >> Fls_DoJobDataTransfer

  Fls_Lld_CompareFlash (Thumb, 376 bytes, Stack size 16 bytes, fls_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Fls_DoJobDataTransfer

  Fls_Lld_MainFunction (Thumb, 770 bytes, Stack size 8 bytes, fls_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Fls_Lld_MainFunction
  [Calls]
  - >> Det_ReportTransientFault
  - >> Det_ReportRuntimeError
  [Called By]
  - >> Fls_MainFunction

  Fls_Lld_SectorWrite (Thumb, 612 bytes, Stack size 32 bytes, fls_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_01
  - >> SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_01
  - >> Fls_Lld_LoadCommandSync (via Veneer)
  [Called By]
  - >> Fls_DoJobDataTransfer

  Fls_Lld_Cancel (Thumb, 82 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Fls_Cancel

  Fls_Lld_GetPhycSectorSize (Thumb, 18 bytes, Stack size 0 bytes, fls_lld.o(.mcal_text))
  [Called By]

  - >> Fls_MainFunction

  Fls_schm_read_msr (Thumb, 6 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text), UNUSED)

  SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_00 (Thumb, 44 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_Lld_SectorErase

  SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_00 (Thumb, 34 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_Lld_SectorErase

  SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_01 (Thumb, 44 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text), UNUSED)
  [Called By]

  - >> Fls_Lld_SectorWrite

  SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_01 (Thumb, 34 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text), UNUSED)
  [Called By]

  - >> Fls_Lld_SectorWrite

  SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_02 (Thumb, 44 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_Erase

  SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_02 (Thumb, 34 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_Erase

  SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_03 (Thumb, 44 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_Write

  SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_03 (Thumb, 34 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_Write

  SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_04 (Thumb, 44 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_Compare

  SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_04 (Thumb, 34 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_Compare

  SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_05 (Thumb, 44 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_BlankCheck

  SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_05 (Thumb, 34 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_BlankCheck

  SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_06 (Thumb, 44 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_Read

  SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_06 (Thumb, 34 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text))
  [Called By]

  - >> Fls_Read

  SchM_Enter_Fls_FLS_EXCLUSIVE_AREA_07 (Thumb, 44 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text), UNUSED)
  [Called By]

  - >> Fls_Lld_ReadFlash

  SchM_Exit_Fls_FLS_EXCLUSIVE_AREA_07 (Thumb, 34 bytes, Stack size 0 bytes, schm_fls.o(.mcal_text), UNUSED)
  [Called By]

  - >> Fls_Lld_ReadFlash

  ### Local Symbols

  Fls_DoJobDataTransfer (Thumb, 446 bytes, Stack size 40 bytes, fls.o(.mcal_text), UNUSED)
  [Calls]

  - >> Fls_Lld_CompareFlash
  - >> Fls_Lld_ReadFlash
  - >> Fls_Lld_SectorWrite
  - >> Fls_Lld_TranslateReturnCode
  - >> Det_ReportTransientFault

  Fls_Lld_LoadCommandSync (Thumb, 74 bytes, Stack size 16 bytes, fls_lld.o(.ramcode))
  [Stack]

  - Max Depth = 16
  - Call Chain = Fls_Lld_LoadCommandSync
  [Calls]
  - >> Fls_Lld_CheckIdleInRam
  [Called By]
  - >> Fls_Lld_SectorWrite (via Veneer)
  - >> Fls_Lld_SectorErase (via Veneer)

  Fls_Lld_CheckIdleInRam (Thumb, 14 bytes, Stack size 0 bytes, fls_lld.o(.ramcode))
  [Called By]

  - >> Fls_Lld_LoadAESCommand
  - >> Fls_Lld_LoadCommandSync

  Fls_Lld_LoadAESCommand (Thumb, 70 bytes, Stack size 16 bytes, fls_lld.o(.ramcode), UNUSED)
  [Calls]

  - >> Fls_Lld_CheckIdleInRam
  [Called By]
  - >> Fls_Lld_ReadFlash (via Veneer)

  ### Undefined Global Symbols