C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:48: * Function Name : LIN_DRV_ProcessParity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:51: * is making parity bits, then from input value of ID, the function returns PID.
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:54: * Implements    : LIN_DRV_ProcessParity_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:56:uint8_t LIN_DRV_ProcessParity(uint8_t PID,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:62:    parity = (uint8_t) (((0xFFU & (BIT(PID, 0U) ^ BIT(PID, 1U) ^ BIT(PID, 2U) ^ BIT(PID, 4U))) << 6U) | /*PRQA S 2986*/
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:63:                        ((0xFFU ^ (BIT(PID, 1U) ^ BIT(PID, 3U) ^ BIT(PID, 4U) ^ BIT(PID, 5U))) << 7U)); /*PRQA S 2986*/
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:69:        if ((PID & 0xC0U) != parity)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:78:            retVal = (uint8_t) (PID & 0x3FU);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:84:        /* Return PID in case of making parity bits */
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:85:        retVal = (uint8_t) (PID | parity);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:93: * Function Name : LIN_DRV_MakeChecksumByte
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:94: * Description   : Makes the checksum byte for a frame. For PID of identifiers,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:95: * if PID is 0x3C (ID 0x3C) or 0x7D (ID 0x3D) or 0xFE (ID 0x3E) or 0xBF (ID 0x3F)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:96: * apply classic checksum and apply enhanced checksum for other PID.
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:97: * In case user want to calculate classic checksum please set PID to zero.
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:99: * Implements    : LIN_DRV_MakeChecksumByte_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:101:uint8_t LIN_DRV_MakeChecksumByte(const uint8_t *buffer,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:103:                                 uint8_t PID)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:106:    uint16_t checksum = 0U;
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:109:    /* For PID is 0x3C (ID 0x3C) or 0x7D (ID 0x3D) or 0xFE (ID 0x3E) or 0xBF (ID 0x3F)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:110:     * apply classic checksum and apply enhanced checksum for other PID */
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:111:    if ((0x3CU != PID) && (0x7DU != PID) && (0xFEU != PID) && (0xBFU != PID))
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:113:        /* For PID other than 0x3C, 0x7D, 0xFE and 0xBF: Add PID in checksum calculation */
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:114:        checksum = PID;
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:117:        /* For 0x3C, 0x7D, 0xFE and 0xBF: Do not add PID in checksum calculation */
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:118:        checksum = 0U;
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:124:        checksum += *temp;
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:127:        if (checksum > 0xFFU)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:129:            checksum -= 0xFFU;
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:133:    /* Return reversed checksum */
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_common.c:134:    return (uint8_t) (~checksum);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:27: * Function Name : LIN_DRV_Init
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:35: * lin_user_config_t parameters and how to call the LIN_DRV_Init function
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:41: *    linUserConfig.timerGetTimeIntervalCallback = (lin_timer_get_time_interval_t) l_ifc_timerGetTimeIntervalCallbackHandler
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:43: *    LIN_DRV_Init(instance, (lin_user_config_t *) &linUserConfig, (lin_state_t *) &linState)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:45: * Implements    : LIN_DRV_Init_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:47:status_t LIN_DRV_Init(uint32_t instance,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:62: * Function Name : LIN_DRV_Deinit
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:66: * Implements    : LIN_DRV_Deinit_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:68:void LIN_DRV_Deinit(uint32_t instance)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:77: * Function Name : LIN_DRV_GetDefaultConfig
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:81: * Implements    : LIN_DRV_GetDefaultConfig_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:83:void LIN_DRV_GetDefaultConfig(bool isMaster,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:93: * Function Name : LIN_DRV_InstallCallback
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:94: * Description   : This function installs the callback function that is used for LIN_DRV_IRQHandler.
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:97: * Implements    : LIN_DRV_InstallCallback_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:99:lin_callback_t LIN_DRV_InstallCallback(uint32_t instance,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:113: * Function Name : LIN_DRV_SendFrameDataBlocking
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:115: * blocking method. This function will calculate the checksum byte and send it with the
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:116: * frame data. Blocking means that the function does not return until the transmission is
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:123: * Implements    : LIN_DRV_SendFrameDataBlocking_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:125:status_t LIN_DRV_SendFrameDataBlocking(uint32_t instance,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:133:    retVal = LIN_UART_DRV_SendFrameDataBlocking(instance, txBuff, txSize, timeoutMSec);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:141: * Function Name : LIN_DRV_SendFrameData
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:143: * non-blocking method. This function will calculate the checksum byte and send it with the
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:144: * frame data. The function will return immediately after calling this function. If txSize
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:148: * Implements    : LIN_DRV_SendFrameData_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:150:status_t LIN_DRV_SendFrameData(uint32_t instance,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:157:    retVal = LIN_UART_DRV_SendFrameData(instance, txBuff, txSize);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:165: * Function Name : LIN_DRV_GetTransmitStatus
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:173: * Implements    : LIN_DRV_GetTransmitStatus_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:175:status_t LIN_DRV_GetTransmitStatus(uint32_t instance,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:189: * Function Name : LIN_DRV_ReceiveFrameDataBlocking
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:193: * handler LIN_UART_DRV_IRQHandler will check the checksum byte. If the checksum
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:194: * is correct, it will receive the frame data. If the checksum is incorrect, this
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:200: * Implements    : LIN_DRV_ReceiveFrameDataBlocking_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:202:status_t LIN_DRV_ReceiveFrameDataBlocking(uint32_t instance,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:218: * Function Name : LIN_DRV_ReceiveFrameData
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:220: * non-blocking method. This function will check the checksum byte. If the checksum is
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:221: * correct, it will receive it with the frame data.
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:224: * The interrupt handler LIN_UART_DRV_IRQHandler will check the checksum byte. If the
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:225: * checksum is correct, it will receive the frame data. If the checksum is incorrect, this
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:230: * Implements    : LIN_DRV_ReceiveFrameData_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:232:status_t LIN_DRV_ReceiveFrameData(uint32_t instance,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:247: * Function Name : LIN_DRV_AbortTransferData
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:252: * Implements    : LIN_DRV_AbortTransferData_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:254:status_t LIN_DRV_AbortTransferData(uint32_t instance)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:267: * Function Name : LIN_DRV_GetReceiveStatus
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:275: * Implements    : LIN_DRV_GetReceiveStatus_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:277:status_t LIN_DRV_GetReceiveStatus(uint32_t instance,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:291: * Function Name : LIN_DRV_GoToSleepMode
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:295: * Implements    : LIN_DRV_GoToSleepMode_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:297:status_t LIN_DRV_GoToSleepMode(uint32_t instance)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:310: * Function Name : LIN_DRV_GotoIdleState
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:311: * Description   : This function puts current node to Idle state.
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:313: * Implements    : LIN_DRV_GoToIdleState_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:315:status_t LIN_DRV_GotoIdleState(uint32_t instance)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:320:    retVal = LIN_UART_DRV_GotoIdleState(instance);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:328: * Function Name : LIN_DRV_SendWakeupSignal
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:331: * Implements    : LIN_DRV_SendWakeupSignal_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:333:status_t LIN_DRV_SendWakeupSignal(uint32_t instance)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:346: * Function Name : LIN_DRV_GetCurrentNodeState
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:349: * Implements    : LIN_DRV_GetCurrentNodeState_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:351:lin_node_state_t LIN_DRV_GetCurrentNodeState(uint32_t instance)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:364: * Function Name : LIN_DRV_TimeoutService
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:365: * Description   : This is callback function for Timer Interrupt Handler.
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:367: * with period of 500 micro seconds. In timer IRQ handler, call this function.
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:369: * Implements    : LIN_DRV_TimeoutService_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:371:void LIN_DRV_TimeoutService(uint32_t instance)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:380: * Function Name : LIN_DRV_SetTimeoutCounter
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:382: * LIN_DRV_TimeoutService
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:384: * Implements    : LIN_DRV_SetTimeoutCounter_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:386:void LIN_DRV_SetTimeoutCounter(uint32_t instance,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:396: * Function Name : LIN_DRV_MasterSendHeader
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:404: * Implements    : LIN_DRV_MasterSendHeader_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:406:status_t LIN_DRV_MasterSendHeader(uint32_t instance,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:420: * Function Name : LIN_DRV_EnableIRQ
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:423: * Implements    : LIN_DRV_EnableIRQ_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:425:status_t LIN_DRV_EnableIRQ(uint32_t instance)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:438: * Function Name : LIN_DRV_DisableIRQ
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:441: * Implements    : LIN_DRV_DisableIRQ_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:443:status_t LIN_DRV_DisableIRQ(uint32_t instance)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:456: * Function Name : LIN_DRV_IRQHandler
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:457: * Description   : Interrupt handler for LIN Hardware Interface.
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:461: * Implements    : LIN_DRV_IRQHandler_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:463:void LIN_DRV_IRQHandler(uint32_t instance)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:466:    LIN_UART_DRV_IRQHandler(instance);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:472: * Function Name : LIN_DRV_AutoBaudCapture
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:479: * Implements    : LIN_DRV_AutoBaudCapture_Activity
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_driver.c:481:status_t LIN_DRV_AutoBaudCapture(uint32_t instance)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:29:static void LIN_UART0_RxTx_IRQHandler(void)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:31:    LIN_DRV_IRQHandler(0U);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:35:static void LIN_UART0_ERR_IRQHandler(void)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:37:    LIN_DRV_IRQHandler(0U);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:43:static void LIN_UART1_RxTx_IRQHandler(void)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:45:    LIN_DRV_IRQHandler(1U);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:49:static void LIN_UART1_ERR_IRQHandler(void)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:51:    LIN_DRV_IRQHandler(1U);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:57:static void LIN_UART2_RxTx_IRQHandler(void)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:59:    LIN_DRV_IRQHandler(2U);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:63:static void LIN_UART2_ERR_IRQHandler(void)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:65:    LIN_DRV_IRQHandler(2U);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:71:static void LIN_UART3_RxTx_IRQHandler(void)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:73:    LIN_DRV_IRQHandler(3U);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:77:static void LIN_UART3_ERR_IRQHandler(void)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:79:    LIN_DRV_IRQHandler(3U);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:85:static void LIN_UART4_RxTx_IRQHandler(void)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:87:    LIN_DRV_IRQHandler(4U);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:91:static void LIN_UART4_ERR_IRQHandler(void)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:93:    LIN_DRV_IRQHandler(4U);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:99:static void LIN_UART5_RxTx_IRQHandler(void)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:101:    LIN_DRV_IRQHandler(5U);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:105:static void LIN_UART5_ERR_IRQHandler(void)
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:107:    LIN_DRV_IRQHandler(5U);
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:115:        LIN_UART0_RxTx_IRQHandler,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:118:        LIN_UART1_RxTx_IRQHandler,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:121:        LIN_UART2_RxTx_IRQHandler,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:124:        LIN_UART3_RxTx_IRQHandler,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:127:        LIN_UART4_RxTx_IRQHandler,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:130:        LIN_UART5_RxTx_IRQHandler,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:138:    LIN_UART0_ERR_IRQHandler,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:141:    LIN_UART1_ERR_IRQHandler,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:144:    LIN_UART2_ERR_IRQHandler,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:147:    LIN_UART3_ERR_IRQHandler,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:150:    LIN_UART4_ERR_IRQHandler,
C:\Users\Administrator\Desktop\Code\My_Project\2.MC03\demo\SDK_DEMO\Test_MC03_SDK_LIN_SLAVE\platform\drivers\src\lin\lin_irq.c:153:    LIN_UART5_ERR_IRQHandler,
