# Static Call Graph for image .\Objects\MC03_MCAL_Project.axf

#<CALLGRAPH># ARM Linker, 6140101: Last Updated: Mon Jul 6 11:19:03 2026

### Maximum Stack Usage = 104 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

Reset_Handler ⇒ main ⇒ Board_Init ⇒ Port_Init ⇒ Port_Lld_Init ⇒ Port_Lld_InitMode ⇒ Port_Lld_InitGPIOMode

### Functions with no stack information

- RamInit0
- Reset_Handler

### Mutually Recursive functions

- DefaultISR ⇒ DefaultISR

  ### Function Pointers

  - ACMP0_IRQHandler from vector_table_copy.o(.text.ACMP0_IRQHandler) referenced from vector.o(.isr_vector)
  - ADC0_IRQHandler from vector_table_copy.o(.text.ADC0_IRQHandler) referenced from vector.o(.isr_vector)
  - BusFault_Handler from vector_table_copy.o(.text.BusFault_Handler) referenced from vector.o(.isr_vector)
  - CAN0_Error_IRQHandler from vector_table_copy.o(.text.CAN0_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN0_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_Error_IRQHandler from vector_table_copy.o(.text.CAN1_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN1_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA0_IRQHandler from vector_table_copy.o(.text.DMA0_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA1_IRQHandler from vector_table_copy.o(.text.DMA1_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA2_IRQHandler from vector_table_copy.o(.text.DMA2_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA3_IRQHandler from vector_table_copy.o(.text.DMA3_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA_Error_IRQHandler from vector_table_copy.o(.text.DMA_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - DebugMon_Handler from vector_table_copy.o(.text.DebugMon_Handler) referenced from vector.o(.isr_vector)
  - DefaultISR from vector_table_copy.o(.text.DefaultISR) referenced 85 times from vector.o(.isr_vector)
  - EFM_Ecc_IRQHandler from vector_table_copy.o(.text.EFM_Ecc_IRQHandler) referenced from vector.o(.isr_vector)
  - EFM_Error_IRQHandler from vector_table_copy.o(.text.EFM_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - EFM_IRQHandler from vector_table_copy.o(.text.EFM_IRQHandler) referenced from vector.o(.isr_vector)
  - EMU_DB_IRQHandler from vector_table_copy.o(.text.EMU_DB_IRQHandler) referenced from vector.o(.isr_vector)
  - EMU_SB_IRQHandler from vector_table_copy.o(.text.EMU_SB_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOA_IRQHandler from vector_table_copy.o(.text.GPIOA_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOB_IRQHandler from vector_table_copy.o(.text.GPIOB_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOC_IRQHandler from vector_table_copy.o(.text.GPIOC_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOD_IRQHandler from vector_table_copy.o(.text.GPIOD_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOE_IRQHandler from vector_table_copy.o(.text.GPIOE_IRQHandler) referenced from vector.o(.isr_vector)
  - Gpt_Notification_Ptmr from lin_pbcfg.o(.mcal_text) referenced from gpt_pbcfg.o(.mcal_const_cfg)
  - HCU_IRQHandler from vector_table_copy.o(.text.HCU_IRQHandler) referenced from vector.o(.isr_vector)
  - HardFault_Handler from vector_table_copy.o(.text.HardFault_Handler) referenced from vector.o(.isr_vector)
  - I2C0_Master_IRQHandler from vector_table_copy.o(.text.I2C0_Master_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C0_Slave_IRQHandler from vector_table_copy.o(.text.I2C0_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C1_Master_IRQHandler from vector_table_copy.o(.text.I2C1_Master_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch0_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch0_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch0_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch0_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch1_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch1_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch1_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch2_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch2_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch2_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch2_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch3_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch3_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch3_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch4_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch4_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch4_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch4_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch5_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch5_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch5_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch6_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch6_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch6_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch6_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch7_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch7_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch7_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - MemManage_Handler from vector_table_copy.o(.text.MemManage_Handler) referenced from vector.o(.isr_vector)
  - NMI_Handler from vector_table_copy.o(.text.NMI_Handler) referenced from vector.o(.isr_vector)
  - PCU_IRQHandler from vector_table_copy.o(.text.PCU_IRQHandler) referenced from vector.o(.isr_vector)
  - PendSV_Handler from vector_table_copy.o(.text.PendSV_Handler) referenced from vector.o(.isr_vector)
  - RamInit1 from raminit1.o(.text.RamInit1) referenced from startup.o(.text)
  - RamInit2 from raminit2.o(.text.RamInit2) referenced from startup.o(.text)
  - Reset_Handler from startup.o(.text) referenced from vector.o(.isr_vector)
  - SCU_IRQHandler from vector_table_copy.o(.text.SCU_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI0_IRQHandler from vector_table_copy.o(.text.SPI0_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI1_IRQHandler from vector_table_copy.o(.text.SPI1_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI2_IRQHandler from vector_table_copy.o(.text.SPI2_IRQHandler) referenced from vector.o(.isr_vector)
  - SVC_Handler from vector_table_copy.o(.text.SVC_Handler) referenced from vector.o(.isr_vector)
  - SysTick_Handler from vector_table_copy.o(.text.SysTick_Handler) referenced from vector.o(.isr_vector)
  - SystemInit from system.o(.text.SystemInit) referenced from startup.o(.text)
  - TRNG_IRQHandler from vector_table_copy.o(.text.TRNG_IRQHandler) referenced from vector.o(.isr_vector)
  - UART0_IRQHandler from lin_lld_uart.o(.mcal_text) referenced from vector.o(.isr_vector)
  - UART1_IRQHandler from vector_table_copy.o(.text.UART1_IRQHandler) referenced from vector.o(.isr_vector)
  - UART2_IRQHandler from vector_table_copy.o(.text.UART2_IRQHandler) referenced from vector.o(.isr_vector)
  - UsageFault_Handler from vector_table_copy.o(.text.UsageFault_Handler) referenced from vector.o(.isr_vector)
  - VectorTableCopy from vector_table_copy.o(.text.VectorTableCopy) referenced from startup.o(.text)
  - Wdg_Mld_Isr from vector_table_copy.o(.text.Wdg_Mld_Isr) referenced from vector.o(.isr_vector)
  - eTMR0_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Fault_IRQHandler from vector_table_copy.o(.text.eTMR0_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR0_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Fault_IRQHandler from vector_table_copy.o(.text.eTMR1_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR1_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - lpTMR0_IRQHandler from vector_table_copy.o(.text.lpTMR0_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR_Ch0_IRQHandler from gpt_lld_ptmr_irq.o(.mcal_text) referenced from vector.o(.isr_vector)
  - pTMR_Ch1_IRQHandler from vector_table_copy.o(.text.pTMR_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR_Ch2_IRQHandler from vector_table_copy.o(.text.pTMR_Ch2_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR_Ch3_IRQHandler from vector_table_copy.o(.text.pTMR_Ch3_IRQHandler) referenced from vector.o(.isr_vector)

  ### Global Symbols

  RamInit0 (Thumb, 0 bytes, Stack size unknown bytes, raminit0.o(.text))
  [Called By]

  - >> Reset_Handler

  Reset_Handler (Thumb, 0 bytes, Stack size unknown bytes, startup.o(.text))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = Reset_Handler ⇒ main ⇒ Board_Init ⇒ Port_Init ⇒ Port_Lld_Init ⇒ Port_Lld_InitMode ⇒ Port_Lld_InitGPIOMode
  [Calls]
  - >> RamInit0
  - >> main
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> VectorTableCopy

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> RamInit1

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  ACMP0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ACMP0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  ADC0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ADC0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  BusFault_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.BusFault_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_32_47_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_32_47_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_48_63_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_48_63_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_32_47_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_32_47_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_48_63_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_48_63_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA2_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DMA_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DebugMon_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DebugMon_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DefaultISR (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DefaultISR))
  [Calls]

  - >> DefaultISR
  [Called By]
  - >> DefaultISR
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  Det_ReportError (Thumb, 60 bytes, Stack size 0 bytes, det.o(.text.Det_ReportError))
  [Called By]

  - >> Port_Init
  - >> Platform_Init
  - >> Lin_WakeupInternal
  - >> Lin_Init
  - >> Port_SetPinMode
  - >> Port_SetPinDirection
  - >> Port_RefreshPortDirection
  - >> Platform_SetIrqPriority
  - >> Platform_SetIrq
  - >> Platform_InstallIrqHandler
  - >> Platform_GetIrqPriority
  - >> Lin_Wakeup
  - >> Lin_GoToSleepInternal
  - >> Lin_DeInit
  - >> Lin_CheckWakeup

  EFM_Ecc_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_Ecc_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  EFM_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  EFM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  EMU_DB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EMU_DB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  EMU_SB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EMU_SB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  EcuM_CheckWakeup (Thumb, 8 bytes, Stack size 0 bytes, ecum.o(.text.EcuM_CheckWakeup))
  [Calls]

  - >> WkuInterruptCallback
  [Called By]
  - >> Lin_Lld_Uart_CheckWakeup
  - >> Lin_Lld_Uart_LocIntWuRsp

  EcuM_SetWakeupEvent (Thumb, 2 bytes, Stack size 0 bytes, ecum.o(.text.EcuM_SetWakeupEvent), UNUSED)
  [Called By]

  - >> Lin_CheckWakeup

  GPIOA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOA_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOC_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOD_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOE_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  HCU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.HCU_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  HardFault_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.HardFault_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  I2C0_Master_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C0_Master_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  I2C0_Slave_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C0_Slave_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  I2C1_Master_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C1_Master_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LinIf_HeaderIndication (Thumb, 98 bytes, Stack size 0 bytes, main.o(.text.LinIf_HeaderIndication))
  [Called By]

  - >> Lin_Lld_Uart_LocSlaveRxOk

  LinIf_LinErrorIndication (Thumb, 26 bytes, Stack size 0 bytes, main.o(.text.LinIf_LinErrorIndication))
  [Called By]

  - >> Lin_Lld_Uart_TimerTickCbk
  - >> Lin_Lld_Uart_LocSlaveRxOk
  - >> Lin_Lld_Uart_LocIntRxRsp
  - >> Lin_Lld_Uart_LocIntOvrRsp

  LinIf_RxIndication (Thumb, 46 bytes, Stack size 0 bytes, main.o(.text.LinIf_RxIndication))
  [Called By]

  - >> Lin_Lld_Uart_LocSlaveRxOk

  LinIf_TxConfirmation (Thumb, 14 bytes, Stack size 0 bytes, main.o(.text.LinIf_TxConfirmation))
  [Called By]

  - >> Lin_Lld_Uart_LocSlaveRxOk

  LinIf_WakeupConfirmation (Thumb, 2 bytes, Stack size 0 bytes, linif.o(.text.LinIf_WakeupConfirmation), UNUSED)
  [Called By]

  - >> Lin_CheckWakeup

  MPWM0_Ch0_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.MPWM0_Ch0_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = MPWM0_Ch0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM0_Ch0_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.MPWM0_Ch0_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = MPWM0_Ch0_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.MPWM0_Ch1_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = MPWM0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM0_Ch1_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.MPWM0_Ch1_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = MPWM0_Ch1_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM0_Ch2_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.MPWM0_Ch2_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = MPWM0_Ch2_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM0_Ch2_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.MPWM0_Ch2_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = MPWM0_Ch2_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM0_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.MPWM0_Ch3_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = MPWM0_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM0_Ch3_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.MPWM0_Ch3_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = MPWM0_Ch3_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM0_Ch4_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.MPWM0_Ch4_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = MPWM0_Ch4_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM0_Ch4_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.MPWM0_Ch4_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = MPWM0_Ch4_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM0_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.MPWM0_Ch5_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = MPWM0_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM0_Ch5_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.MPWM0_Ch5_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = MPWM0_Ch5_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM0_Ch6_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.MPWM0_Ch6_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = MPWM0_Ch6_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM0_Ch6_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.MPWM0_Ch6_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = MPWM0_Ch6_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM0_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.MPWM0_Ch7_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = MPWM0_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MPWM0_Ch7_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.MPWM0_Ch7_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = MPWM0_Ch7_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MemManage_Handler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.MemManage_Handler))
  [Stack]

  - Max Depth = 32
  - Call Chain = MemManage_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  NMI_Handler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.NMI_Handler))
  [Stack]

  - Max Depth = 32
  - Call Chain = NMI_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  PCU_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.PCU_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = PCU_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  PendSV_Handler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.PendSV_Handler))
  [Stack]

  - Max Depth = 32
  - Call Chain = PendSV_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  RamInit1 (Thumb, 268 bytes, Stack size 32 bytes, raminit1.o(.text.RamInit1))
  [Stack]

  - Max Depth = 32
  - Call Chain = RamInit1
  [Calls]
  - >> IsPOR
  - >> __aeabi_memclr4
  [Address Reference Count : 1]
  - startup.o(.text)

  RamInit2 (Thumb, 2 bytes, Stack size 0 bytes, raminit2.o(.text.RamInit2))
  [Address Reference Count : 1]

  - startup.o(.text)

  SCU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SCU_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI2_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SVC_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SVC_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SysTick_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SysTick_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SystemInit (Thumb, 58 bytes, Stack size 0 bytes, system.o(.text.SystemInit))
  [Stack]

  - Max Depth = 32
  - Call Chain = SystemInit ⇒ Mpu_Lld_M33_Init ⇒ ARM_MPU_SetMemAttr ⇒ ARM_MPU_SetMemAttrEx
  [Calls]
  - >> Mpu_Lld_M33_Init
  [Address Reference Count : 1]
  - startup.o(.text)

  TRNG_IRQHandler (Thumb, 0 bytes, Stack size 8 bytes, vector_table_copy.o(.text.TRNG_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = TRNG_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  UART1_IRQHandler (Thumb, 0 bytes, Stack size 8 bytes, vector_table_copy.o(.text.UART1_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  UART2_IRQHandler (Thumb, 0 bytes, Stack size 8 bytes, vector_table_copy.o(.text.UART2_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART2_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  UsageFault_Handler (Thumb, 0 bytes, Stack size 8 bytes, vector_table_copy.o(.text.UsageFault_Handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = UsageFault_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  VectorTableCopy (Thumb, 76 bytes, Stack size 8 bytes, vector_table_copy.o(.text.VectorTableCopy))
  [Stack]

  - Max Depth = 8
  - Call Chain = VectorTableCopy
  [Calls]
  - >> Sys_GetCoreID
  - >> __aeabi_memcpy4
  [Address Reference Count : 1]
  - startup.o(.text)

  Wdg_Mld_Isr (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.Wdg_Mld_Isr))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  WkuInterruptCallback (Thumb, 2 bytes, Stack size 0 bytes, ecum.o(.text.WkuInterruptCallback))
  [Called By]

  - >> EcuM_CheckWakeup

  eTMR0_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ch0_Ch1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR0_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ch2_Ch3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR0_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ch4_Ch5_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR0_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ch6_Ch7_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR0_Fault_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Fault_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR0_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ovf_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR1_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ch0_Ch1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR1_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ch2_Ch3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR1_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ch4_Ch5_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR1_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ch6_Ch7_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR1_Fault_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Fault_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR1_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ovf_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  lpTMR0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.lpTMR0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  main (Thumb, 78 bytes, Stack size 0 bytes, main.o(.text.main))
  [Stack]

  - Max Depth = 104
  - Call Chain = main ⇒ Board_Init ⇒ Port_Init ⇒ Port_Lld_Init ⇒ Port_Lld_InitMode ⇒ Port_Lld_InitGPIOMode
  [Calls]
  - >> Lin_WakeupInternal
  - >> Board_Init
  [Called By]
  - >> Reset_Handler

  pTMR_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR_Ch1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR_Ch2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR_Ch2_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR_Ch3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  Gpt_Notification_Ptmr (Thumb, 8 bytes, Stack size 8 bytes, lin_pbcfg.o(.mcal_text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Gpt_Notification_Ptmr ⇒ Lin_Lld_Uart_TimerTickCbk ⇒ Lin_Lld_Uart_LocGoToSleep ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_05
  [Calls]
  - >> Lin_Lld_Uart_TimerTickCbk
  [Address Reference Count : 1]
  - gpt_pbcfg.o(.mcal_const_cfg)

  Port_Init (Thumb, 46 bytes, Stack size 8 bytes, port.o(.mcal_text))
  [Stack]

  - Max Depth = 96
  - Call Chain = Port_Init ⇒ Port_Lld_Init ⇒ Port_Lld_InitMode ⇒ Port_Lld_InitGPIOMode
  [Calls]
  - >> Port_Lld_Init
  - >> Det_ReportError
  [Called By]
  - >> Board_Init

  Port_RefreshPortDirection (Thumb, 44 bytes, Stack size 8 bytes, port.o(.mcal_text), UNUSED)
  [Calls]

  - >> Port_Lld_RefreshPortDirection
  - >> Det_ReportError

  Port_SetPinDirection (Thumb, 106 bytes, Stack size 16 bytes, port.o(.mcal_text), UNUSED)
  [Calls]

  - >> Port_Lld_SetPinDirection
  - >> Port_Lld_IsPinDireChangeable
  - >> Det_ReportError

  Port_SetPinMode (Thumb, 124 bytes, Stack size 16 bytes, port.o(.mcal_text), UNUSED)
  [Calls]

  - >> Port_Lld_SetPinMode
  - >> Port_Lld_IsPinModeChangeable
  - >> Det_ReportError

  Port_Lld_Init (Thumb, 116 bytes, Stack size 40 bytes, port_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 88
  - Call Chain = Port_Lld_Init ⇒ Port_Lld_InitMode ⇒ Port_Lld_InitGPIOMode
  [Calls]
  - >> Port_Lld_InitPull
  - >> Port_Lld_InitMode
  [Called By]
  - >> Port_Init

  Port_Lld_RefreshPortDirection (Thumb, 158 bytes, Stack size 40 bytes, port_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_Port_PORT_EXCLUSIVE_AREA_02
  - >> SchM_Enter_Port_PORT_EXCLUSIVE_AREA_02
  [Called By]
  - >> Port_RefreshPortDirection

  Port_Lld_IsPinDireChangeable (Thumb, 72 bytes, Stack size 8 bytes, port_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Port_SetPinDirection

  Port_Lld_IsPinModeChangeable (Thumb, 72 bytes, Stack size 8 bytes, port_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Port_SetPinMode

  Port_Lld_SetPinDirection (Thumb, 84 bytes, Stack size 24 bytes, port_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_Port_PORT_EXCLUSIVE_AREA_00
  - >> SchM_Enter_Port_PORT_EXCLUSIVE_AREA_00
  [Called By]
  - >> Port_SetPinDirection

  Port_Lld_SetPinMode (Thumb, 40 bytes, Stack size 16 bytes, port_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_Port_PORT_EXCLUSIVE_AREA_01
  - >> SchM_Enter_Port_PORT_EXCLUSIVE_AREA_01
  [Called By]
  - >> Port_SetPinMode

  SchM_Port_ReadMsr (Thumb, 6 bytes, Stack size 0 bytes, schm_port.o(.mcal_text), UNUSED)
  [Called By]

  - >> SchM_Enter_Port_PORT_EXCLUSIVE_AREA_02
  - >> SchM_Enter_Port_PORT_EXCLUSIVE_AREA_01
  - >> SchM_Enter_Port_PORT_EXCLUSIVE_AREA_00

  SchM_Enter_Port_PORT_EXCLUSIVE_AREA_00 (Thumb, 44 bytes, Stack size 8 bytes, schm_port.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Port_ReadMsr
  [Called By]
  - >> Port_Lld_SetPinDirection

  SchM_Exit_Port_PORT_EXCLUSIVE_AREA_00 (Thumb, 40 bytes, Stack size 0 bytes, schm_port.o(.mcal_text), UNUSED)
  [Called By]

  - >> Port_Lld_SetPinDirection

  SchM_Enter_Port_PORT_EXCLUSIVE_AREA_01 (Thumb, 44 bytes, Stack size 8 bytes, schm_port.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Port_ReadMsr
  [Called By]
  - >> Port_Lld_SetPinMode

  SchM_Exit_Port_PORT_EXCLUSIVE_AREA_01 (Thumb, 40 bytes, Stack size 0 bytes, schm_port.o(.mcal_text), UNUSED)
  [Called By]

  - >> Port_Lld_SetPinMode

  SchM_Enter_Port_PORT_EXCLUSIVE_AREA_02 (Thumb, 44 bytes, Stack size 8 bytes, schm_port.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Port_ReadMsr
  [Called By]
  - >> Port_Lld_RefreshPortDirection

  SchM_Exit_Port_PORT_EXCLUSIVE_AREA_02 (Thumb, 40 bytes, Stack size 0 bytes, schm_port.o(.mcal_text), UNUSED)
  [Called By]

  - >> Port_Lld_RefreshPortDirection

  IntCtrl_Lld_Init (Thumb, 118 bytes, Stack size 16 bytes, intctrl_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> IntCtrl_Lld_SetPriority
  - >> IntCtrl_Lld_EnableIrq
  - >> IntCtrl_Lld_DisableIrq
  - >> IntCtrl_Lld_ClearPending
  - >> DevAssert

  IntCtrl_Lld_ClearPending (Thumb, 8 bytes, Stack size 8 bytes, intctrl_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> IntCtrl_Lld_ClrPendingPrivileged
  [Called By]
  - >> IntCtrl_Lld_Init

  IntCtrl_Lld_SetPriority (Thumb, 8 bytes, Stack size 8 bytes, intctrl_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = IntCtrl_Lld_SetPriority ⇒ IntCtrl_Lld_SetPriPrivileged
  [Calls]
  - >> IntCtrl_Lld_SetPriPrivileged
  [Called By]
  - >> Platform_Mld_SetIrqPriority
  - >> Platform_Mld_InitIntCtrl
  - >> IntCtrl_Lld_Init

  IntCtrl_Lld_EnableIrq (Thumb, 8 bytes, Stack size 8 bytes, intctrl_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IntCtrl_Lld_EnableIrq ⇒ IntCtrl_Lld_EnableIrqPrivileged
  [Calls]
  - >> IntCtrl_Lld_EnableIrqPrivileged
  [Called By]
  - >> Platform_Mld_SetIrq
  - >> Platform_Mld_InitIntCtrl
  - >> IntCtrl_Lld_Init

  IntCtrl_Lld_DisableIrq (Thumb, 8 bytes, Stack size 8 bytes, intctrl_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IntCtrl_Lld_DisableIrq ⇒ IntCtrl_Lld_DisableIrqPrivileged
  [Calls]
  - >> IntCtrl_Lld_DisableIrqPrivileged
  [Called By]
  - >> Platform_Mld_SetIrq
  - >> Platform_Mld_InitIntCtrl
  - >> IntCtrl_Lld_Init

  IntCtrl_Lld_InstallHandler (Thumb, 8 bytes, Stack size 8 bytes, intctrl_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> IntCtrl_Lld_InstIsrPrivileged
  [Called By]
  - >> Platform_Mld_InstallIrqHandler

  IntCtrl_Lld_GetPriority (Thumb, 8 bytes, Stack size 8 bytes, intctrl_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> IntCtrl_Lld_GetPriPrivileged
  [Called By]
  - >> Platform_Mld_GetIrqPriority

  Sys_GetCoreID (Thumb, 4 bytes, Stack size 0 bytes, osif.o(.mcal_text))
  [Called By]

  - >> VectorTableCopy
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_31
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_30
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_29
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_28
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_27
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_26
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_25
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_24
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_23
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_22
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_21
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_20
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_19
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_18
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_17
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_16
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_15
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_14
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_13
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_12
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_11
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_10
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_09
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_08
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_07
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_06
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_05
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_04
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_03
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_02
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_01
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_00
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_31
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_30
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_29
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_28
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_27
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_26
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_25
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_24
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_23
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_22
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_21
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_20
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_19
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_18
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_17
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_16
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_15
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_14
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_13
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_12
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_11
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_10
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_09
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_08
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_07
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_06
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_05
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_04
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_03
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_02
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_01
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_00

  Platform_Mld_Init (Thumb, 20 bytes, Stack size 8 bytes, platform_mld.o(.mcal_text))
  [Stack]

  - Max Depth = 48
  - Call Chain = Platform_Mld_Init ⇒ Platform_Mld_InitIntCtrl ⇒ IntCtrl_Lld_SetPriority ⇒ IntCtrl_Lld_SetPriPrivileged
  [Calls]
  - >> Platform_Mld_InitIntCtrl
  [Called By]
  - >> Platform_Init

  Platform_Init (Thumb, 36 bytes, Stack size 8 bytes, platform.o(.mcal_text))
  [Stack]

  - Max Depth = 56
  - Call Chain = Platform_Init ⇒ Platform_Mld_Init ⇒ Platform_Mld_InitIntCtrl ⇒ IntCtrl_Lld_SetPriority ⇒ IntCtrl_Lld_SetPriPrivileged
  [Calls]
  - >> Det_ReportError
  - >> Platform_Mld_Init
  [Called By]
  - >> Board_Init

  Platform_SetIrq (Thumb, 32 bytes, Stack size 8 bytes, platform.o(.mcal_text), UNUSED)
  [Calls]

  - >> Det_ReportError
  - >> Platform_Mld_SetIrq

  Platform_SetIrqPriority (Thumb, 36 bytes, Stack size 8 bytes, platform.o(.mcal_text), UNUSED)
  [Calls]

  - >> Det_ReportError
  - >> Platform_Mld_SetIrqPriority

  Platform_GetIrqPriority (Thumb, 60 bytes, Stack size 8 bytes, platform.o(.mcal_text), UNUSED)
  [Calls]

  - >> Det_ReportError
  - >> Platform_Mld_GetIrqPriority

  Platform_InstallIrqHandler (Thumb, 60 bytes, Stack size 8 bytes, platform.o(.mcal_text), UNUSED)
  [Calls]

  - >> Det_ReportError
  - >> Platform_Mld_InstallIrqHandler

  Mpu_Lld_M33_Init (Thumb, 136 bytes, Stack size 16 bytes, mpu_lld_m33.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Mpu_Lld_M33_Init ⇒ ARM_MPU_SetMemAttr ⇒ ARM_MPU_SetMemAttrEx
  [Calls]
  - >> ARM_MPU_SetRegion
  - >> ARM_MPU_SetMemAttr
  - >> ARM_MPU_Enable
  - >> ARM_MPU_Disable
  - >> ARM_MPU_ClrRegion
  [Called By]
  - >> SystemInit

  Mcu_GetPllStatus (Thumb, 4 bytes, Stack size 0 bytes, mcu.o(.mcal_text), UNUSED)

  Mcu_GetResetReason (Thumb, 24 bytes, Stack size 8 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_GetResetValue

  Mcu_Init (Thumb, 52 bytes, Stack size 16 bytes, mcu.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Mcu_Init ⇒ Mcu_Lld_SetPcu
  [Calls]
  - >> Mcu_Lld_SetRcu
  - >> Mcu_Lld_SetPcu
  [Called By]
  - >> Board_Init

  Mcu_InitClock (Thumb, 74 bytes, Stack size 8 bytes, mcu.o(.mcal_text))
  [Stack]

  - Max Depth = 64
  - Call Chain = Mcu_InitClock ⇒ Mcu_Lld_InitClock ⇒ Mcu_Lld_InitFxosc ⇒ Mcu_Lld_SetFxoscClock
  [Calls]
  - >> Mcu_Lld_InitClock
  [Called By]
  - >> Board_Init

  Mcu_InitRamSection (Thumb, 54 bytes, Stack size 8 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_SetRamSection

  Mcu_SetMode (Thumb, 58 bytes, Stack size 16 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00
  - >> SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00
  - >> Mcu_Lld_SetMode

  Mcu_GetResetRawValue (Thumb, 8 bytes, Stack size 8 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_GetResetRawValue

  Mcu_180_GetCoreClockFrequency (Thumb, 56 bytes, Stack size 8 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_GetCoreClockFrequency

  Mcu_Lld_SystemReset (Thumb, 36 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)

  Mcu_Lld_SetRcu (Thumb, 56 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Init

  Mcu_Lld_SetRamSection (Thumb, 34 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_InitRamSection

  Mcu_Lld_SetMode (Thumb, 154 bytes, Stack size 16 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_DisableAllCmu
  [Called By]
  - >> Mcu_SetMode

  Mcu_Lld_SetClockSource (Thumb, 50 bytes, Stack size 16 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 36
  - Call Chain = Mcu_Lld_SetClockSource ⇒ Mcu_Lld_SetCmu
  [Calls]
  - >> Mcu_Lld_SwitchSystemClock
  - >> Mcu_Lld_SetCmu
  - >> Mcu_Lld_SetClockOut
  - >> Mcu_Lld_ClkOutDisable
  [Called By]
  - >> Mcu_Lld_InitClock

  Mcu_Lld_SetPeripheralClock (Thumb, 100 bytes, Stack size 20 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Mcu_Lld_SetPeripheralClock
  [Called By]
  - >> Mcu_Lld_InitClock

  Mcu_Lld_InitClock (Thumb, 90 bytes, Stack size 16 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 56
  - Call Chain = Mcu_Lld_InitClock ⇒ Mcu_Lld_InitFxosc ⇒ Mcu_Lld_SetFxoscClock
  [Calls]
  - >> Mcu_Lld_SetPeripheralClock
  - >> Mcu_Lld_SetClockSource
  - >> Mcu_Lld_SwitchSystemClock
  - >> Mcu_Lld_InitSirc
  - >> Mcu_Lld_InitFxosc
  - >> Mcu_Lld_InitFirc
  - >> Mcu_Lld_InitClockDivider
  - >> Mcu_Lld_EfmPrescaler
  - >> Mcu_Lld_DisableAllCmu
  [Called By]
  - >> Mcu_InitClock

  Mcu_Lld_GetResetRawValue (Thumb, 24 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_Lld_GetResetValue
  - >> Mcu_GetResetRawValue

  Mcu_Lld_GetResetValue (Thumb, 148 bytes, Stack size 8 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_GetResetRawValue
  [Called By]
  - >> Mcu_GetResetReason

  Mcu_Lld_GetCoreClockFrequency (Thumb, 54 bytes, Stack size 8 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_GetCoreDiv
  - >> Mcu_Lld_GetCoreClockSource
  [Called By]
  - >> Mcu_180_GetCoreClockFrequency

  Mcu_Lld_SetPcu (Thumb, 136 bytes, Stack size 16 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Mcu_Lld_SetPcu
  [Called By]
  - >> Mcu_Init

  SchM_Mcu_ReadMsr (Thumb, 6 bytes, Stack size 0 bytes, schm_mcu.o(.mcal_text), UNUSED)
  [Called By]

  - >> SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00

  SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00 (Thumb, 44 bytes, Stack size 8 bytes, schm_mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Mcu_ReadMsr
  [Called By]
  - >> Mcu_SetMode

  SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00 (Thumb, 40 bytes, Stack size 0 bytes, schm_mcu.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_SetMode

  SchM_Lin_ReadMsr (Thumb, 6 bytes, Stack size 0 bytes, schm_lin.o(.mcal_text))
  [Called By]

  - >> SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_06
  - >> SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_05
  - >> SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_04
  - >> SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_03
  - >> SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_02
  - >> SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_01
  - >> SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00

  SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00 (Thumb, 44 bytes, Stack size 8 bytes, schm_lin.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00
  [Calls]
  - >> SchM_Lin_ReadMsr
  [Called By]
  - >> Lin_Lld_Uart_LocEnableLbkDtc

  SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_00 (Thumb, 40 bytes, Stack size 0 bytes, schm_lin.o(.mcal_text))
  [Called By]

  - >> Lin_Lld_Uart_LocEnableLbkDtc

  SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_01 (Thumb, 44 bytes, Stack size 8 bytes, schm_lin.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_01
  [Calls]
  - >> SchM_Lin_ReadMsr
  [Called By]
  - >> Lin_Lld_Uart_InitChannel

  SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_01 (Thumb, 40 bytes, Stack size 0 bytes, schm_lin.o(.mcal_text))
  [Called By]

  - >> Lin_Lld_Uart_InitChannel

  SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_02 (Thumb, 44 bytes, Stack size 8 bytes, schm_lin.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_02
  [Calls]
  - >> SchM_Lin_ReadMsr
  [Called By]
  - >> Lin_Lld_Uart_LocIntLbkRsp

  SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_02 (Thumb, 40 bytes, Stack size 0 bytes, schm_lin.o(.mcal_text))
  [Called By]

  - >> Lin_Lld_Uart_LocIntLbkRsp

  SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_03 (Thumb, 44 bytes, Stack size 8 bytes, schm_lin.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Lin_ReadMsr
  [Called By]
  - >> Lin_Lld_Uart_Wakeup

  SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_03 (Thumb, 40 bytes, Stack size 0 bytes, schm_lin.o(.mcal_text), UNUSED)
  [Called By]

  - >> Lin_Lld_Uart_Wakeup

  SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_04 (Thumb, 44 bytes, Stack size 8 bytes, schm_lin.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Lin_ReadMsr

  SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_04 (Thumb, 40 bytes, Stack size 0 bytes, schm_lin.o(.mcal_text), UNUSED)

  SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_05 (Thumb, 44 bytes, Stack size 8 bytes, schm_lin.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_05
  [Calls]
  - >> SchM_Lin_ReadMsr
  [Called By]
  - >> Lin_Lld_Uart_LocGoToSleep

  SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_05 (Thumb, 40 bytes, Stack size 0 bytes, schm_lin.o(.mcal_text))
  [Called By]

  - >> Lin_Lld_Uart_LocGoToSleep

  SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_06 (Thumb, 44 bytes, Stack size 8 bytes, schm_lin.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Lin_ReadMsr
  [Called By]
  - >> Lin_Lld_Uart_SendGoToSleep

  SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_06 (Thumb, 40 bytes, Stack size 0 bytes, schm_lin.o(.mcal_text), UNUSED)
  [Called By]

  - >> Lin_Lld_Uart_SendGoToSleep

  Lin_CheckWakeup (Thumb, 118 bytes, Stack size 16 bytes, lin.o(.mcal_text), UNUSED)
  [Calls]

  - >> EcuM_SetWakeupEvent
  - >> Det_ReportError
  - >> Lin_Mld_CheckWakeup
  - >> LinIf_WakeupConfirmation

  Lin_GoToSleepInternal (Thumb, 100 bytes, Stack size 16 bytes, lin.o(.mcal_text), UNUSED)
  [Calls]

  - >> Det_ReportError
  - >> Lin_Mld_GoToSleepInternal

  Lin_Init (Thumb, 156 bytes, Stack size 16 bytes, lin.o(.mcal_text))
  [Stack]

  - Max Depth = 72
  - Call Chain = Lin_Init ⇒ Gpt_StopTimer ⇒ Gpt_Mld_StopTimer ⇒ Gpt_Lld_Ptmr_StopChannel ⇒ SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_10
  [Calls]
  - >> Det_ReportError
  - >> Lin_Mld_SetInstMap
  - >> Lin_Mld_InitChannel
  - >> Gpt_StopTimer
  - >> Gpt_StartTimer
  - >> Gpt_EnableNotification
  [Called By]
  - >> Board_Init

  Lin_DeInit (Thumb, 86 bytes, Stack size 24 bytes, lin.o(.mcal_text), UNUSED)
  [Calls]

  - >> Det_ReportError
  - >> Lin_Mld_DeInitChannel
  - >> Gpt_StopTimer

  Lin_Wakeup (Thumb, 88 bytes, Stack size 8 bytes, lin.o(.mcal_text), UNUSED)
  [Calls]

  - >> Det_ReportError
  - >> Lin_Mld_Wakeup

  Lin_WakeupInternal (Thumb, 88 bytes, Stack size 8 bytes, lin.o(.mcal_text))
  [Stack]

  - Max Depth = 48
  - Call Chain = Lin_WakeupInternal ⇒ Lin_Mld_WakeupInternal ⇒ Lin_Lld_Uart_WakeupInternal ⇒ Lin_Lld_Uart_LocWakeup ⇒ Lin_Lld_Uart_LocEnableLbkDtc ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00
  [Calls]
  - >> Det_ReportError
  - >> Lin_Mld_WakeupInternal
  [Called By]
  - >> main

  Lin_Mld_SetInstMap (Thumb, 8 bytes, Stack size 8 bytes, lin_mld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Lin_Mld_SetInstMap
  [Calls]
  - >> Lin_Lld_Uart_SetInstMap
  [Called By]
  - >> Lin_Init

  Lin_Mld_InitChannel (Thumb, 8 bytes, Stack size 8 bytes, lin_mld.o(.mcal_text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Lin_Mld_InitChannel ⇒ Lin_Lld_Uart_InitChannel ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_01
  [Calls]
  - >> Lin_Lld_Uart_InitChannel
  [Called By]
  - >> Lin_Init

  Lin_Mld_DeInitChannel (Thumb, 8 bytes, Stack size 8 bytes, lin_mld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Lin_Lld_Uart_DeInitChannel
  [Called By]
  - >> Lin_DeInit

  Lin_Mld_Wakeup (Thumb, 8 bytes, Stack size 8 bytes, lin_mld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Lin_Lld_Uart_Wakeup
  [Called By]
  - >> Lin_Wakeup

  Lin_Mld_WakeupInternal (Thumb, 8 bytes, Stack size 8 bytes, lin_mld.o(.mcal_text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Lin_Mld_WakeupInternal ⇒ Lin_Lld_Uart_WakeupInternal ⇒ Lin_Lld_Uart_LocWakeup ⇒ Lin_Lld_Uart_LocEnableLbkDtc ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00
  [Calls]
  - >> Lin_Lld_Uart_WakeupInternal
  [Called By]
  - >> Lin_WakeupInternal

  Lin_Mld_CheckWakeup (Thumb, 8 bytes, Stack size 8 bytes, lin_mld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Lin_Lld_Uart_CheckWakeup
  [Called By]
  - >> Lin_CheckWakeup

  Lin_Mld_GoToSleepInternal (Thumb, 8 bytes, Stack size 8 bytes, lin_mld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Lin_Lld_Uart_GoToSleepInternal
  [Called By]
  - >> Lin_GoToSleepInternal

  Lin_Lld_Uart_LocWakeup (Thumb, 84 bytes, Stack size 8 bytes, lin_lld_uart.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Lin_Lld_Uart_LocWakeup ⇒ Lin_Lld_Uart_LocEnableLbkDtc ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00
  [Calls]
  - >> Lin_Lld_Uart_LocEnableLbkDtc
  [Called By]
  - >> Lin_Lld_Uart_WakeupInternal
  - >> Lin_Lld_Uart_Wakeup
  - >> Lin_Lld_Uart_GoToSleepInternal
  - >> Lin_Lld_Uart_SendGoToSleep

  Lin_Lld_Uart_TimerTickCbk (Thumb, 230 bytes, Stack size 8 bytes, lin_lld_uart.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Lin_Lld_Uart_TimerTickCbk ⇒ Lin_Lld_Uart_LocGoToSleep ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_05
  [Calls]
  - >> LinIf_LinErrorIndication
  - >> Lin_Lld_Uart_LocGoToSleep
  - >> Lin_Lld_Uart_LocEnableLbkDtc
  [Called By]
  - >> Gpt_Notification_Ptmr

  Lin_Lld_Uart_SetInstMap (Thumb, 12 bytes, Stack size 0 bytes, lin_lld_uart.o(.mcal_text))
  [Called By]

  - >> Lin_Mld_SetInstMap

  Lin_Lld_Uart_InitChannel (Thumb, 272 bytes, Stack size 24 bytes, lin_lld_uart.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Lin_Lld_Uart_InitChannel ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_01
  [Calls]
  - >> SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_01
  - >> SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_01
  - >> Lin_Lld_Uart_LocGetWakeupByte
  [Called By]
  - >> Lin_Mld_InitChannel

  Lin_Lld_Uart_DeInitChannel (Thumb, 50 bytes, Stack size 0 bytes, lin_lld_uart.o(.mcal_text), UNUSED)
  [Called By]

  - >> Lin_Mld_DeInitChannel

  Lin_Lld_Uart_SendGoToSleep (Thumb, 236 bytes, Stack size 24 bytes, lin_lld_uart.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_06
  - >> SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_06
  - >> Lin_Lld_Uart_LocWakeup
  - >> Lin_Lld_Uart_LocTransmittionAbort
  - >> Lin_Lld_Uart_LocStopToTicks
  - >> Lin_Lld_Uart_LocStartToTicks
  - >> Lin_Lld_Uart_LocGetChecksumByte
  - >> Lin_Lld_Uart_LocEnableLbkDtc

  Lin_Lld_Uart_GoToSleepInternal (Thumb, 74 bytes, Stack size 16 bytes, lin_lld_uart.o(.mcal_text), UNUSED)
  [Calls]

  - >> Lin_Lld_Uart_LocWakeup
  - >> Lin_Lld_Uart_LocTransmittionAbort
  - >> Lin_Lld_Uart_LocStopToTicks
  - >> Lin_Lld_Uart_LocGoToSleep
  [Called By]
  - >> Lin_Mld_GoToSleepInternal

  Lin_Lld_Uart_Wakeup (Thumb, 172 bytes, Stack size 16 bytes, lin_lld_uart.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_03
  - >> SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_03
  - >> Lin_Lld_Uart_LocWakeup
  - >> Lin_Lld_Uart_LocTransmittionAbort
  - >> Lin_Lld_Uart_LocStopToTicks
  [Called By]
  - >> Lin_Mld_Wakeup

  Lin_Lld_Uart_WakeupInternal (Thumb, 46 bytes, Stack size 8 bytes, lin_lld_uart.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Lin_Lld_Uart_WakeupInternal ⇒ Lin_Lld_Uart_LocWakeup ⇒ Lin_Lld_Uart_LocEnableLbkDtc ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00
  [Calls]
  - >> Lin_Lld_Uart_LocWakeup
  [Called By]
  - >> Lin_Mld_WakeupInternal

  Lin_Lld_Uart_CheckWakeup (Thumb, 158 bytes, Stack size 16 bytes, lin_lld_uart.o(.mcal_text), UNUSED)
  [Calls]

  - >> EcuM_CheckWakeup
  - >> Lin_Lld_Uart_LocEnableLbkDtc
  [Called By]
  - >> Lin_Mld_CheckWakeup

  Lin_Lld_Uart_GetTxHeaderComands (Thumb, 12 bytes, Stack size 0 bytes, lin_lld_uart.o(.mcal_text), UNUSED)

  Lin_Lld_Uart_GetFrameErrStates (Thumb, 12 bytes, Stack size 0 bytes, lin_lld_uart.o(.mcal_text), UNUSED)

  Lin_Lld_Uart_GetFrameStates (Thumb, 12 bytes, Stack size 0 bytes, lin_lld_uart.o(.mcal_text), UNUSED)

  Lin_Lld_Uart_GetRxEmptyState (Thumb, 18 bytes, Stack size 0 bytes, lin_lld_uart.o(.mcal_text), UNUSED)

  Lin_Lld_Uart_LocGetRxFlag (Thumb, 8 bytes, Stack size 0 bytes, lin_lld_uart.o(.mcal_text), UNUSED)
  [Called By]

  - >> Lin_Lld_Uart_LocReadSentData

  Lin_Lld_Uart_LocReadSentData (Thumb, 42 bytes, Stack size 16 bytes, lin_lld_uart.o(.mcal_text), UNUSED)
  [Calls]

  - >> Lin_Lld_Uart_LocGetRxFlag

  Lin_Lld_Uart_LocMasterRxOk (Thumb, 732 bytes, Stack size 24 bytes, lin_lld_uart.o(.mcal_text))
  [Stack]

  - Max Depth = 48
  - Call Chain = Lin_Lld_Uart_LocMasterRxOk ⇒ Lin_Lld_Uart_LocGoToSleep ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_05
  [Calls]
  - >> Lin_Lld_Uart_LocStopToTicks
  - >> Lin_Lld_Uart_LocStartToTicks
  - >> Lin_Lld_Uart_LocGoToSleep
  - >> Lin_Lld_Uart_LocGetChecksumByte
  [Called By]
  - >> Lin_Lld_Uart_LocIntRxRsp

  Lin_Lld_Uart_LocSlaveRxOk (Thumb, 702 bytes, Stack size 32 bytes, lin_lld_uart.o(.mcal_text))
  [Stack]

  - Max Depth = 48
  - Call Chain = Lin_Lld_Uart_LocSlaveRxOk ⇒ Lin_Lld_Uart_LocEnableLbkDtc ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00
  [Calls]
  - >> LinIf_TxConfirmation
  - >> LinIf_RxIndication
  - >> LinIf_LinErrorIndication
  - >> LinIf_HeaderIndication
  - >> Lin_Lld_Uart_LocStopToTicks
  - >> Lin_Lld_Uart_LocStartToTicks
  - >> Lin_Lld_Uart_LocGetChecksumByte
  - >> Lin_Lld_Uart_LocEnableLbkDtc
  [Called By]
  - >> Lin_Lld_Uart_LocIntRxRsp

  Lin_Lld_Uart_LocIntWuRsp (Thumb, 152 bytes, Stack size 16 bytes, lin_lld_uart.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Lin_Lld_Uart_LocIntWuRsp ⇒ Lin_Lld_Uart_LocEnableLbkDtc ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00
  [Calls]
  - >> EcuM_CheckWakeup
  - >> Lin_Lld_Uart_LocEnableLbkDtc
  [Called By]
  - >> Lin_Lld_Uart_LocIntHandler

  Lin_Lld_Uart_LocIntLbkRsp (Thumb, 104 bytes, Stack size 16 bytes, lin_lld_uart.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Lin_Lld_Uart_LocIntLbkRsp ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_02
  [Calls]
  - >> SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_02
  - >> SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_02
  - >> Lin_Lld_Uart_LocStopToTicks
  - >> Lin_Lld_Uart_LocStartToTicks
  [Called By]
  - >> Lin_Lld_Uart_LocIntHandler

  Lin_Lld_Uart_LocIntRxRsp (Thumb, 262 bytes, Stack size 16 bytes, lin_lld_uart.o(.mcal_text))
  [Stack]

  - Max Depth = 64
  - Call Chain = Lin_Lld_Uart_LocIntRxRsp ⇒ Lin_Lld_Uart_LocSlaveRxOk ⇒ Lin_Lld_Uart_LocEnableLbkDtc ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00
  [Calls]
  - >> LinIf_LinErrorIndication
  - >> Lin_Lld_Uart_LocSlaveRxOk
  - >> Lin_Lld_Uart_LocMasterRxOk
  - >> Lin_Lld_Uart_LocGoToSleep
  - >> Lin_Lld_Uart_LocEnableLbkDtc
  [Called By]
  - >> Lin_Lld_Uart_LocIntHandler

  Lin_Lld_Uart_LocIntOvrRsp (Thumb, 76 bytes, Stack size 16 bytes, lin_lld_uart.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Lin_Lld_Uart_LocIntOvrRsp ⇒ Lin_Lld_Uart_LocEnableLbkDtc ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00
  [Calls]
  - >> LinIf_LinErrorIndication
  - >> Lin_Lld_Uart_LocEnableLbkDtc
  [Called By]
  - >> Lin_Lld_Uart_LocIntHandler

  Lin_Lld_Uart_LocIntHandler (Thumb, 124 bytes, Stack size 16 bytes, lin_lld_uart.o(.mcal_text))
  [Stack]

  - Max Depth = 80
  - Call Chain = Lin_Lld_Uart_LocIntHandler ⇒ Lin_Lld_Uart_LocIntRxRsp ⇒ Lin_Lld_Uart_LocSlaveRxOk ⇒ Lin_Lld_Uart_LocEnableLbkDtc ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00
  [Calls]
  - >> Lin_Lld_Uart_LocIntWuRsp
  - >> Lin_Lld_Uart_LocIntRxRsp
  - >> Lin_Lld_Uart_LocIntOvrRsp
  - >> Lin_Lld_Uart_LocIntLbkRsp
  [Called By]
  - >> UART0_IRQHandler

  UART0_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, lin_lld_uart.o(.mcal_text))
  [Stack]

  - Max Depth = 88
  - Call Chain = UART0_IRQHandler ⇒ Lin_Lld_Uart_LocIntHandler ⇒ Lin_Lld_Uart_LocIntRxRsp ⇒ Lin_Lld_Uart_LocSlaveRxOk ⇒ Lin_Lld_Uart_LocEnableLbkDtc ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00
  [Calls]
  - >> Lin_Lld_Uart_LocIntHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SchM_Gpt_ReadMsr (Thumb, 6 bytes, Stack size 0 bytes, schm_gpt.o(.mcal_text))
  [Called By]

  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_31
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_30
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_29
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_28
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_27
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_26
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_25
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_24
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_23
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_22
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_21
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_20
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_19
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_18
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_17
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_16
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_15
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_14
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_13
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_12
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_11
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_10
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_09
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_08
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_07
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_06
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_05
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_04
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_03
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_02
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_01
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_00

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_00 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_00 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_01 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_01 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_02 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_02 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_03 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_03 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_04 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_04 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_05 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_05 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_06 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_06 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_07 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_07
  [Calls]
  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr
  [Called By]
  - >> Gpt_Lld_Ptmr_InitInstance

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_07 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_07
  [Calls]
  - >> Sys_GetCoreID
  [Called By]
  - >> Gpt_Lld_Ptmr_InitInstance

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_08 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr
  [Called By]
  - >> Gpt_Lld_Ptmr_InitChannel

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_08 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  [Called By]
  - >> Gpt_Lld_Ptmr_InitChannel

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_09 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_09
  [Calls]
  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr
  [Called By]
  - >> Gpt_Lld_Ptmr_StartChannel

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_09 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_09
  [Calls]
  - >> Sys_GetCoreID
  [Called By]
  - >> Gpt_Lld_Ptmr_StartChannel

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_10 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_10
  [Calls]
  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr
  [Called By]
  - >> Gpt_Lld_Ptmr_StopChannel

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_10 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_10
  [Calls]
  - >> Sys_GetCoreID
  [Called By]
  - >> Gpt_Lld_Ptmr_StopChannel

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_11 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_11
  [Calls]
  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr
  [Called By]
  - >> Gpt_Lld_Ptmr_ChannelIrqProcess

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_11 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_11
  [Calls]
  - >> Sys_GetCoreID
  [Called By]
  - >> Gpt_Lld_Ptmr_ChannelIrqProcess

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_12 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_12
  [Calls]
  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr
  [Called By]
  - >> Gpt_Lld_Ptmr_EnableNotification

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_12 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_12
  [Calls]
  - >> Sys_GetCoreID
  [Called By]
  - >> Gpt_Lld_Ptmr_EnableNotification

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_13 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr
  [Called By]
  - >> Gpt_Lld_Ptmr_DisNotification

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_13 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  [Called By]
  - >> Gpt_Lld_Ptmr_DisNotification

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_14 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_14 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_15 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_15 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_16 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_16 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_17 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_17 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_18 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_18 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_19 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_19 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_20 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_20 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_21 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_21 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_22 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_22 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_23 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_23 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_24 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_24 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_25 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_25 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_26 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_26 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_27 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_27 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_28 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_28 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_29 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_29 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_30 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_30 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_31 (Thumb, 60 bytes, Stack size 16 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID
  - >> SchM_Gpt_ReadMsr

  SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_31 (Thumb, 54 bytes, Stack size 8 bytes, schm_gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Sys_GetCoreID

  Gpt_Init (Thumb, 84 bytes, Stack size 24 bytes, gpt.o(.mcal_text))
  [Stack]

  - Max Depth = 64
  - Call Chain = Gpt_Init ⇒ Gpt_Mld_InitInstances ⇒ Gpt_Lld_Ptmr_InitInstance ⇒ SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_07
  [Calls]
  - >> Gpt_Mld_InitInstances
  - >> Gpt_Mld_Init
  [Called By]
  - >> Board_Init

  Gpt_DeInit (Thumb, 50 bytes, Stack size 16 bytes, gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Gpt_Mld_DeInit

  Gpt_DisableNotification (Thumb, 68 bytes, Stack size 16 bytes, gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Gpt_Mld_DisableNotification
  - >> Gpt_Mld_CheckChannel

  Gpt_EnableNotification (Thumb, 68 bytes, Stack size 16 bytes, gpt.o(.mcal_text))
  [Stack]

  - Max Depth = 56
  - Call Chain = Gpt_EnableNotification ⇒ Gpt_Mld_EnableNotification ⇒ Gpt_Lld_Ptmr_EnableNotification ⇒ SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_12
  [Calls]
  - >> Gpt_Mld_EnableNotification
  - >> Gpt_Mld_CheckChannel
  [Called By]
  - >> Lin_Init

  Gpt_GetTimeElapsed (Thumb, 64 bytes, Stack size 16 bytes, gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Gpt_Mld_GetTimeElapsed
  - >> Gpt_Mld_CheckChannel

  Gpt_GetTimeRemaining (Thumb, 64 bytes, Stack size 16 bytes, gpt.o(.mcal_text), UNUSED)
  [Calls]

  - >> Gpt_Mld_GetTimeRemaining
  - >> Gpt_Mld_CheckChannel

  Gpt_StartTimer (Thumb, 100 bytes, Stack size 16 bytes, gpt.o(.mcal_text))
  [Stack]

  - Max Depth = 56
  - Call Chain = Gpt_StartTimer ⇒ Gpt_Mld_StartTimer ⇒ Gpt_Lld_Ptmr_StartChannel ⇒ SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_09
  [Calls]
  - >> Gpt_Mld_StartTimer
  - >> Gpt_Mld_GetChannelState
  - >> Gpt_Mld_CheckChannel
  [Called By]
  - >> Lin_Init

  Gpt_StopTimer (Thumb, 62 bytes, Stack size 16 bytes, gpt.o(.mcal_text))
  [Stack]

  - Max Depth = 56
  - Call Chain = Gpt_StopTimer ⇒ Gpt_Mld_StopTimer ⇒ Gpt_Lld_Ptmr_StopChannel ⇒ SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_10
  [Calls]
  - >> Gpt_Mld_StopTimer
  - >> Gpt_Mld_CheckChannel
  [Called By]
  - >> Lin_Init
  - >> Lin_DeInit

  Gpt_Mld_InitInstances (Thumb, 52 bytes, Stack size 16 bytes, gpt_mld.o(.mcal_text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Gpt_Mld_InitInstances ⇒ Gpt_Lld_Ptmr_InitInstance ⇒ SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_07
  [Calls]
  - >> Gpt_Lld_Ptmr_InitInstance
  [Called By]
  - >> Gpt_Init

  Gpt_Mld_Init (Thumb, 22 bytes, Stack size 16 bytes, gpt_mld.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Gpt_Mld_Init
  [Called By]
  - >> Gpt_Init

  Gpt_Mld_DeInit (Thumb, 106 bytes, Stack size 16 bytes, gpt_mld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Gpt_Lld_Ptmr_DeInitInstance
  - >> Gpt_Lld_Ptmr_DeInitChannel
  [Called By]
  - >> Gpt_DeInit

  Gpt_Mld_StartTimer (Thumb, 24 bytes, Stack size 8 bytes, gpt_mld.o(.mcal_text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Gpt_Mld_StartTimer ⇒ Gpt_Lld_Ptmr_StartChannel ⇒ SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_09
  [Calls]
  - >> Gpt_Lld_Ptmr_StartChannel
  [Called By]
  - >> Gpt_StartTimer

  Gpt_Mld_StopTimer (Thumb, 34 bytes, Stack size 8 bytes, gpt_mld.o(.mcal_text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Gpt_Mld_StopTimer ⇒ Gpt_Lld_Ptmr_StopChannel ⇒ SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_10
  [Calls]
  - >> Gpt_Lld_Ptmr_StopChannel
  - >> Gpt_Lld_Ptmr_GetTimerState
  [Called By]
  - >> Gpt_StopTimer

  Gpt_Mld_CheckChannel (Thumb, 12 bytes, Stack size 0 bytes, gpt_mld.o(.mcal_text))
  [Called By]

  - >> Gpt_StopTimer
  - >> Gpt_StartTimer
  - >> Gpt_EnableNotification
  - >> Gpt_GetTimeRemaining
  - >> Gpt_GetTimeElapsed
  - >> Gpt_DisableNotification

  Gpt_Mld_GetChannelState (Thumb, 24 bytes, Stack size 8 bytes, gpt_mld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Gpt_Mld_GetChannelState
  [Calls]
  - >> Gpt_Lld_Ptmr_GetTimerState
  [Called By]
  - >> Gpt_StartTimer

  Gpt_Mld_EnableNotification (Thumb, 36 bytes, Stack size 8 bytes, gpt_mld.o(.mcal_text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Gpt_Mld_EnableNotification ⇒ Gpt_Lld_Ptmr_EnableNotification ⇒ SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_12
  [Calls]
  - >> Gpt_Lld_Ptmr_EnableNotification
  [Called By]
  - >> Gpt_EnableNotification

  Gpt_Mld_DisableNotification (Thumb, 36 bytes, Stack size 8 bytes, gpt_mld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Gpt_Lld_Ptmr_DisNotification
  [Called By]
  - >> Gpt_DisableNotification

  Gpt_Mld_GetTimeElapsed (Thumb, 24 bytes, Stack size 8 bytes, gpt_mld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Gpt_Lld_Ptmr_GetChTimeElapsed
  [Called By]
  - >> Gpt_GetTimeElapsed

  Gpt_Mld_GetTimeRemaining (Thumb, 24 bytes, Stack size 8 bytes, gpt_mld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Gpt_Lld_Ptmr_GetChTimeRemaining
  [Called By]
  - >> Gpt_GetTimeRemaining

  Gpt_Lld_Ptmr_InitInstance (Thumb, 62 bytes, Stack size 8 bytes, gpt_lld_ptmr.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Gpt_Lld_Ptmr_InitInstance ⇒ SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_07
  [Calls]
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_07
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_07
  [Called By]
  - >> Gpt_Mld_InitInstances

  Gpt_Lld_Ptmr_InitChannel (Thumb, 92 bytes, Stack size 16 bytes, gpt_lld_ptmr.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_08
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_08
  [Called By]
  - >> Gpt_Mld_PtmrChannelInit

  Gpt_Lld_Ptmr_DeInitInstance (Thumb, 14 bytes, Stack size 0 bytes, gpt_lld_ptmr.o(.mcal_text), UNUSED)
  [Called By]

  - >> Gpt_Mld_DeInit

  Gpt_Lld_Ptmr_DeInitChannel (Thumb, 74 bytes, Stack size 8 bytes, gpt_lld_ptmr.o(.mcal_text), UNUSED)
  [Called By]

  - >> Gpt_Mld_DeInit

  Gpt_Lld_Ptmr_StartChannel (Thumb, 98 bytes, Stack size 16 bytes, gpt_lld_ptmr.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Gpt_Lld_Ptmr_StartChannel ⇒ SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_09
  [Calls]
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_09
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_09
  [Called By]
  - >> Gpt_Mld_StartTimer

  Gpt_Lld_Ptmr_StopChannel (Thumb, 78 bytes, Stack size 16 bytes, gpt_lld_ptmr.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Gpt_Lld_Ptmr_StopChannel ⇒ SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_10
  [Calls]
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_10
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_10
  [Called By]
  - >> Gpt_Mld_StopTimer

  Gpt_Lld_Ptmr_ChannelIrqProcess (Thumb, 116 bytes, Stack size 16 bytes, gpt_lld_ptmr.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Gpt_Lld_Ptmr_ChannelIrqProcess ⇒ SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_11
  [Calls]
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_11
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_11
  [Called By]
  - >> pTMR_Ch0_IRQHandler

  Gpt_Lld_Ptmr_GetChTimeElapsed (Thumb, 90 bytes, Stack size 16 bytes, gpt_lld_ptmr.o(.mcal_text), UNUSED)
  [Called By]

  - >> Gpt_Mld_GetTimeElapsed

  Gpt_Lld_Ptmr_GetChTimeRemaining (Thumb, 82 bytes, Stack size 16 bytes, gpt_lld_ptmr.o(.mcal_text), UNUSED)
  [Called By]

  - >> Gpt_Mld_GetTimeRemaining

  Gpt_Lld_Ptmr_GetTimerState (Thumb, 26 bytes, Stack size 0 bytes, gpt_lld_ptmr.o(.mcal_text))
  [Called By]

  - >> Gpt_Mld_StopTimer
  - >> Gpt_Mld_GetChannelState

  Gpt_Lld_Ptmr_EnableNotification (Thumb, 62 bytes, Stack size 16 bytes, gpt_lld_ptmr.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Gpt_Lld_Ptmr_EnableNotification ⇒ SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_12
  [Calls]
  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_12
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_12
  [Called By]
  - >> Gpt_Mld_EnableNotification

  Gpt_Lld_Ptmr_DisNotification (Thumb, 78 bytes, Stack size 16 bytes, gpt_lld_ptmr.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_Gpt_GPT_EXCLUSIVE_AREA_13
  - >> SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_13
  [Called By]
  - >> Gpt_Mld_DisableNotification

  Gpt_Lld_Ptmr_GetInstanceCfg (Thumb, 32 bytes, Stack size 4 bytes, gpt_lld_ptmr.o(.mcal_text), UNUSED)

  Gpt_Lld_Ptmr_GetChannelCfg (Thumb, 42 bytes, Stack size 0 bytes, gpt_lld_ptmr.o(.mcal_text), UNUSED)

  pTMR_Ch0_IRQHandler (Thumb, 12 bytes, Stack size 8 bytes, gpt_lld_ptmr_irq.o(.mcal_text))
  [Stack]

  - Max Depth = 40
  - Call Chain = pTMR_Ch0_IRQHandler ⇒ Gpt_Lld_Ptmr_ChannelIrqProcess ⇒ SchM_Enter_Gpt_GPT_EXCLUSIVE_AREA_11
  [Calls]
  - >> Gpt_Lld_Ptmr_ChannelIrqProcess
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  ### Local Symbols

  Board_Init (Thumb, 64 bytes, Stack size 8 bytes, main.o(.text.Board_Init))
  [Stack]

  - Max Depth = 104
  - Call Chain = Board_Init ⇒ Port_Init ⇒ Port_Lld_Init ⇒ Port_Lld_InitMode ⇒ Port_Lld_InitGPIOMode
  [Calls]
  - >> Port_Init
  - >> Platform_Init
  - >> Mcu_InitClock
  - >> Mcu_Init
  - >> Lin_Init
  - >> Gpt_Init
  [Called By]
  - >> main

  IsPOR (Thumb, 16 bytes, Stack size 0 bytes, raminit1.o(.text.IsPOR))
  [Called By]

  - >> RamInit1

  Port_Lld_InitGPIOMode (Thumb, 222 bytes, Stack size 24 bytes, port_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Port_Lld_InitGPIOMode
  [Called By]
  - >> Port_Lld_InitMode

  Port_Lld_InitMode (Thumb, 128 bytes, Stack size 24 bytes, port_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 48
  - Call Chain = Port_Lld_InitMode ⇒ Port_Lld_InitGPIOMode
  [Calls]
  - >> Port_Lld_InitGPIOMode
  [Called By]
  - >> Port_Lld_Init

  Port_Lld_InitPull (Thumb, 58 bytes, Stack size 0 bytes, port_lld.o(.mcal_text))
  [Called By]

  - >> Port_Lld_Init

  DevAssert (Thumb, 12 bytes, Stack size 0 bytes, intctrl_lld.o(.text.DevAssert))
  [Called By]

  - >> IntCtrl_Lld_Init
  - >> IntCtrl_Lld_SetPriPrivileged
  - >> IntCtrl_Lld_InstIsrPrivileged
  - >> IntCtrl_Lld_GetPriPrivileged
  - >> IntCtrl_Lld_EnableIrqPrivileged
  - >> IntCtrl_Lld_DisableIrqPrivileged
  - >> IntCtrl_Lld_ClrPendingPrivileged

  IntCtrl_Lld_ClrPendingPrivileged (Thumb, 36 bytes, Stack size 8 bytes, intctrl_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> __NVIC_ClearPendingIRQ
  - >> DevAssert
  [Called By]
  - >> IntCtrl_Lld_ClearPending

  IntCtrl_Lld_DisableIrqPrivileged (Thumb, 36 bytes, Stack size 8 bytes, intctrl_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IntCtrl_Lld_DisableIrqPrivileged
  [Calls]
  - >> __NVIC_DisableIRQ
  - >> DevAssert
  [Called By]
  - >> IntCtrl_Lld_DisableIrq

  IntCtrl_Lld_EnableIrqPrivileged (Thumb, 36 bytes, Stack size 8 bytes, intctrl_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = IntCtrl_Lld_EnableIrqPrivileged
  [Calls]
  - >> __NVIC_EnableIRQ
  - >> DevAssert
  [Called By]
  - >> IntCtrl_Lld_EnableIrq

  IntCtrl_Lld_GetPriPrivileged (Thumb, 38 bytes, Stack size 8 bytes, intctrl_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> __NVIC_GetPriority
  - >> DevAssert
  [Called By]
  - >> IntCtrl_Lld_GetPriority

  IntCtrl_Lld_InstIsrPrivileged (Thumb, 102 bytes, Stack size 24 bytes, intctrl_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> DevAssert
  [Called By]
  - >> IntCtrl_Lld_InstallHandler

  IntCtrl_Lld_SetPriPrivileged (Thumb, 54 bytes, Stack size 16 bytes, intctrl_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = IntCtrl_Lld_SetPriPrivileged
  [Calls]
  - >> __NVIC_SetPriority
  - >> DevAssert
  [Called By]
  - >> IntCtrl_Lld_SetPriority

  __NVIC_ClearPendingIRQ (Thumb, 32 bytes, Stack size 0 bytes, intctrl_lld.o(.text.__NVIC_ClearPendingIRQ), UNUSED)
  [Called By]

  - >> IntCtrl_Lld_ClrPendingPrivileged

  __NVIC_DisableIRQ (Thumb, 40 bytes, Stack size 0 bytes, intctrl_lld.o(.text.__NVIC_DisableIRQ))
  [Called By]

  - >> IntCtrl_Lld_DisableIrqPrivileged

  __NVIC_EnableIRQ (Thumb, 32 bytes, Stack size 0 bytes, intctrl_lld.o(.text.__NVIC_EnableIRQ))
  [Called By]

  - >> IntCtrl_Lld_EnableIrqPrivileged

  __NVIC_GetPriority (Thumb, 34 bytes, Stack size 0 bytes, intctrl_lld.o(.text.__NVIC_GetPriority), UNUSED)
  [Called By]

  - >> IntCtrl_Lld_GetPriPrivileged

  __NVIC_SetPriority (Thumb, 34 bytes, Stack size 0 bytes, intctrl_lld.o(.text.__NVIC_SetPriority))
  [Called By]

  - >> IntCtrl_Lld_SetPriPrivileged

  Platform_Mld_InitIntCtrl (Thumb, 70 bytes, Stack size 16 bytes, platform_mld.o(.mcal_text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Platform_Mld_InitIntCtrl ⇒ IntCtrl_Lld_SetPriority ⇒ IntCtrl_Lld_SetPriPrivileged
  [Calls]
  - >> IntCtrl_Lld_SetPriority
  - >> IntCtrl_Lld_EnableIrq
  - >> IntCtrl_Lld_DisableIrq
  [Called By]
  - >> Platform_Mld_Init

  Platform_Mld_GetIrqPriority (Thumb, 8 bytes, Stack size 8 bytes, platform.o(.mcal_text), UNUSED)
  [Calls]

  - >> IntCtrl_Lld_GetPriority
  [Called By]
  - >> Platform_GetIrqPriority

  Platform_Mld_InstallIrqHandler (Thumb, 8 bytes, Stack size 8 bytes, platform.o(.mcal_text), UNUSED)
  [Calls]

  - >> IntCtrl_Lld_InstallHandler
  [Called By]
  - >> Platform_InstallIrqHandler

  Platform_Mld_SetIrq (Thumb, 18 bytes, Stack size 8 bytes, platform.o(.mcal_text), UNUSED)
  [Calls]

  - >> IntCtrl_Lld_EnableIrq
  - >> IntCtrl_Lld_DisableIrq
  [Called By]
  - >> Platform_SetIrq

  Platform_Mld_SetIrqPriority (Thumb, 8 bytes, Stack size 8 bytes, platform.o(.mcal_text), UNUSED)
  [Calls]

  - >> IntCtrl_Lld_SetPriority
  [Called By]
  - >> Platform_SetIrqPriority

  ARM_MPU_ClrRegion (Thumb, 8 bytes, Stack size 0 bytes, mpu_lld_m33.o(.text.ARM_MPU_ClrRegion))
  [Calls]

  - >> ARM_MPU_ClrRegionEx
  [Called By]
  - >> Mpu_Lld_M33_Init

  ARM_MPU_ClrRegionEx (Thumb, 16 bytes, Stack size 0 bytes, mpu_lld_m33.o(.text.ARM_MPU_ClrRegionEx))
  [Called By]

  - >> ARM_MPU_ClrRegion

  ARM_MPU_Disable (Thumb, 38 bytes, Stack size 0 bytes, mpu_lld_m33.o(.text.ARM_MPU_Disable))
  [Called By]

  - >> Mpu_Lld_M33_Init

  ARM_MPU_Enable (Thumb, 36 bytes, Stack size 0 bytes, mpu_lld_m33.o(.text.ARM_MPU_Enable))
  [Called By]

  - >> Mpu_Lld_M33_Init

  ARM_MPU_SetMemAttr (Thumb, 8 bytes, Stack size 8 bytes, mpu_lld_m33.o(.text.ARM_MPU_SetMemAttr))
  [Stack]

  - Max Depth = 16
  - Call Chain = ARM_MPU_SetMemAttr ⇒ ARM_MPU_SetMemAttrEx
  [Calls]
  - >> ARM_MPU_SetMemAttrEx
  [Called By]
  - >> Mpu_Lld_M33_Init

  ARM_MPU_SetMemAttrEx (Thumb, 56 bytes, Stack size 8 bytes, mpu_lld_m33.o(.text.ARM_MPU_SetMemAttrEx))
  [Stack]

  - Max Depth = 8
  - Call Chain = ARM_MPU_SetMemAttrEx
  [Called By]
  - >> ARM_MPU_SetMemAttr

  ARM_MPU_SetRegion (Thumb, 8 bytes, Stack size 8 bytes, mpu_lld_m33.o(.text.ARM_MPU_SetRegion))
  [Stack]

  - Max Depth = 8
  - Call Chain = ARM_MPU_SetRegion
  [Calls]
  - >> ARM_MPU_SetRegionEx
  [Called By]
  - >> Mpu_Lld_M33_Init

  ARM_MPU_SetRegionEx (Thumb, 16 bytes, Stack size 0 bytes, mpu_lld_m33.o(.text.ARM_MPU_SetRegionEx))
  [Called By]

  - >> ARM_MPU_SetRegion

  Mcu_Lld_ClkOutDisable (Thumb, 18 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_SetClockSource

  Mcu_Lld_DisableAllCmu (Thumb, 18 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_SetMode
  - >> Mcu_Lld_InitClock

  Mcu_Lld_EfmPrescaler (Thumb, 42 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_InitClock

  Mcu_Lld_FircDisable (Thumb, 18 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_InitFirc

  Mcu_Lld_FircEnable (Thumb, 38 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_InitFirc

  Mcu_Lld_FxoscDisable (Thumb, 18 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_InitFxosc

  Mcu_Lld_GetClockStatus (Thumb, 14 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_InitFxosc
  - >> Mcu_Lld_InitFirc

  Mcu_Lld_GetCoreClockSource (Thumb, 16 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_Lld_GetCoreClockFrequency

  Mcu_Lld_GetCoreDiv (Thumb, 18 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_Lld_GetCoreClockFrequency

  Mcu_Lld_GetDividerStatus (Thumb, 12 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_InitClockDivider

  Mcu_Lld_GetSystemClockStatus (Thumb, 16 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_SwitchSystemClock

  Mcu_Lld_InitClockDivider (Thumb, 114 bytes, Stack size 24 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Mcu_Lld_InitClockDivider ⇒ Mcu_Lld_SetClockDivider
  [Calls]
  - >> Mcu_Lld_SetClockDivider
  - >> Mcu_Lld_GetDividerStatus
  [Called By]
  - >> Mcu_Lld_InitClock

  Mcu_Lld_InitFirc (Thumb, 78 bytes, Stack size 16 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Mcu_Lld_InitFirc
  [Calls]
  - >> Mcu_Lld_GetClockStatus
  - >> Mcu_Lld_FircEnable
  - >> Mcu_Lld_FircDisable
  [Called By]
  - >> Mcu_Lld_InitClock

  Mcu_Lld_InitFxosc (Thumb, 142 bytes, Stack size 32 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Mcu_Lld_InitFxosc ⇒ Mcu_Lld_SetFxoscClock
  [Calls]
  - >> Mcu_Lld_SetFxoscGain
  - >> Mcu_Lld_SetFxoscClock
  - >> Mcu_Lld_GetClockStatus
  - >> Mcu_Lld_FxoscDisable
  [Called By]
  - >> Mcu_Lld_InitClock

  Mcu_Lld_InitSirc (Thumb, 44 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_InitClock

  Mcu_Lld_SetClockDivider (Thumb, 52 bytes, Stack size 8 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Mcu_Lld_SetClockDivider
  [Called By]
  - >> Mcu_Lld_InitClockDivider

  Mcu_Lld_SetClockOut (Thumb, 40 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_SetClockSource

  Mcu_Lld_SetCmu (Thumb, 112 bytes, Stack size 20 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Mcu_Lld_SetCmu
  [Called By]
  - >> Mcu_Lld_SetClockSource

  Mcu_Lld_SetFxoscClock (Thumb, 84 bytes, Stack size 8 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Mcu_Lld_SetFxoscClock
  [Called By]
  - >> Mcu_Lld_InitFxosc

  Mcu_Lld_SetFxoscGain (Thumb, 18 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_InitFxosc

  Mcu_Lld_SetSystemClockSource (Thumb, 18 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Lld_SwitchSystemClock

  Mcu_Lld_SwitchSystemClock (Thumb, 56 bytes, Stack size 16 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Mcu_Lld_SwitchSystemClock
  [Calls]
  - >> Mcu_Lld_SetSystemClockSource
  - >> Mcu_Lld_GetSystemClockStatus
  [Called By]
  - >> Mcu_Lld_SetClockSource
  - >> Mcu_Lld_InitClock

  Lin_Lld_Uart_LocEnableLbkDtc (Thumb, 28 bytes, Stack size 8 bytes, lin_lld_uart.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Lin_Lld_Uart_LocEnableLbkDtc ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00
  [Calls]
  - >> SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_00
  - >> SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_00
  [Called By]
  - >> Lin_Lld_Uart_TimerTickCbk
  - >> Lin_Lld_Uart_CheckWakeup
  - >> Lin_Lld_Uart_SendGoToSleep
  - >> Lin_Lld_Uart_LocWakeup
  - >> Lin_Lld_Uart_LocSlaveRxOk
  - >> Lin_Lld_Uart_LocIntWuRsp
  - >> Lin_Lld_Uart_LocIntRxRsp
  - >> Lin_Lld_Uart_LocIntOvrRsp

  Lin_Lld_Uart_LocGetChecksumByte (Thumb, 70 bytes, Stack size 0 bytes, lin_lld_uart.o(.mcal_text))
  [Called By]

  - >> Lin_Lld_Uart_SendGoToSleep
  - >> Lin_Lld_Uart_LocSlaveRxOk
  - >> Lin_Lld_Uart_LocMasterRxOk

  Lin_Lld_Uart_LocGetWakeupByte (Thumb, 36 bytes, Stack size 0 bytes, lin_lld_uart.o(.mcal_text))
  [Called By]

  - >> Lin_Lld_Uart_InitChannel

  Lin_Lld_Uart_LocGoToSleep (Thumb, 126 bytes, Stack size 16 bytes, lin_lld_uart.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Lin_Lld_Uart_LocGoToSleep ⇒ SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_05
  [Calls]
  - >> SchM_Exit_Lin_LIN_EXCLUSIVE_AREA_05
  - >> SchM_Enter_Lin_LIN_EXCLUSIVE_AREA_05
  - >> Lin_Lld_Uart_LocStopToTicks
  [Called By]
  - >> Lin_Lld_Uart_TimerTickCbk
  - >> Lin_Lld_Uart_GoToSleepInternal
  - >> Lin_Lld_Uart_LocMasterRxOk
  - >> Lin_Lld_Uart_LocIntRxRsp

  Lin_Lld_Uart_LocStartToTicks (Thumb, 180 bytes, Stack size 0 bytes, lin_lld_uart.o(.mcal_text))
  [Called By]

  - >> Lin_Lld_Uart_SendGoToSleep
  - >> Lin_Lld_Uart_LocSlaveRxOk
  - >> Lin_Lld_Uart_LocMasterRxOk
  - >> Lin_Lld_Uart_LocIntLbkRsp

  Lin_Lld_Uart_LocStopToTicks (Thumb, 26 bytes, Stack size 0 bytes, lin_lld_uart.o(.mcal_text))
  [Called By]

  - >> Lin_Lld_Uart_Wakeup
  - >> Lin_Lld_Uart_GoToSleepInternal
  - >> Lin_Lld_Uart_SendGoToSleep
  - >> Lin_Lld_Uart_LocSlaveRxOk
  - >> Lin_Lld_Uart_LocMasterRxOk
  - >> Lin_Lld_Uart_LocIntLbkRsp
  - >> Lin_Lld_Uart_LocGoToSleep

  Lin_Lld_Uart_LocTransmittionAbort (Thumb, 46 bytes, Stack size 16 bytes, lin_lld_uart.o(.mcal_text), UNUSED)
  [Calls]

  - >> Lin_Lld_Uart_LocTxIdleState
  [Called By]
  - >> Lin_Lld_Uart_Wakeup
  - >> Lin_Lld_Uart_GoToSleepInternal
  - >> Lin_Lld_Uart_SendGoToSleep

  Lin_Lld_Uart_LocTxIdleState (Thumb, 10 bytes, Stack size 0 bytes, lin_lld_uart.o(.mcal_text), UNUSED)
  [Called By]

  - >> Lin_Lld_Uart_LocTransmittionAbort

  Gpt_Mld_PtmrChannelInit (Thumb, 30 bytes, Stack size 8 bytes, gpt_mld.o(.mcal_text), UNUSED)
  [Calls]

  - >> Gpt_Lld_Ptmr_InitChannel

  ### Undefined Global Symbols