# Static Call Graph for image .\Objects\Adc_Demo.axf

#<CALLGRAPH># ARM Linker, 6220000: Last Updated: Thu Aug 6 10:18:15 2026

### Maximum Stack Usage = 224 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

ADC0_Group2CallBack ⇒ Adc_ReadGroup ⇒ Adc_HandleHwReloadAfterRead ⇒ Adc_Lld_StartConversion ⇒ CddDma_SetLogicChannelTransfer ⇒ Dma_Lld_SetChannelTransfer

### Functions with no stack information

- RamInit0
- Reset_Handler

### Mutually Recursive functions

- ACMP0_IRQHandler ⇒ ACMP0_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- CAN0_Error_IRQHandler ⇒ CAN0_Error_IRQHandler
- CAN0_ORed_0_15_MB_IRQHandler ⇒ CAN0_ORed_0_15_MB_IRQHandler
- CAN0_ORed_16_31_MB_IRQHandler ⇒ CAN0_ORed_16_31_MB_IRQHandler
- CAN0_ORed_32_47_MB_IRQHandler ⇒ CAN0_ORed_32_47_MB_IRQHandler
- CAN0_ORed_48_63_MB_IRQHandler ⇒ CAN0_ORed_48_63_MB_IRQHandler
- CAN0_ORed_IRQHandler ⇒ CAN0_ORed_IRQHandler
- CAN0_Wake_Up_IRQHandler ⇒ CAN0_Wake_Up_IRQHandler
- CAN1_Error_IRQHandler ⇒ CAN1_Error_IRQHandler
- CAN1_ORed_0_15_MB_IRQHandler ⇒ CAN1_ORed_0_15_MB_IRQHandler
- CAN1_ORed_16_31_MB_IRQHandler ⇒ CAN1_ORed_16_31_MB_IRQHandler
- CAN1_ORed_32_47_MB_IRQHandler ⇒ CAN1_ORed_32_47_MB_IRQHandler
- CAN1_ORed_48_63_MB_IRQHandler ⇒ CAN1_ORed_48_63_MB_IRQHandler
- CAN1_ORed_IRQHandler ⇒ CAN1_ORed_IRQHandler
- CAN1_Wake_Up_IRQHandler ⇒ CAN1_Wake_Up_IRQHandler
- CAN2_Error_IRQHandler ⇒ CAN2_Error_IRQHandler
- CAN2_ORed_0_15_MB_IRQHandler ⇒ CAN2_ORed_0_15_MB_IRQHandler
- CAN2_ORed_16_31_MB_IRQHandler ⇒ CAN2_ORed_16_31_MB_IRQHandler
- CAN2_ORed_32_47_MB_IRQHandler ⇒ CAN2_ORed_32_47_MB_IRQHandler
- CAN2_ORed_48_63_MB_IRQHandler ⇒ CAN2_ORed_48_63_MB_IRQHandler
- CAN2_ORed_IRQHandler ⇒ CAN2_ORed_IRQHandler
- CAN2_Wake_Up_IRQHandler ⇒ CAN2_Wake_Up_IRQHandler
- CAN3_Error_IRQHandler ⇒ CAN3_Error_IRQHandler
- CAN3_ORed_0_15_MB_IRQHandler ⇒ CAN3_ORed_0_15_MB_IRQHandler
- CAN3_ORed_16_31_MB_IRQHandler ⇒ CAN3_ORed_16_31_MB_IRQHandler
- CAN3_ORed_IRQHandler ⇒ CAN3_ORed_IRQHandler
- CAN3_Wake_Up_IRQHandler ⇒ CAN3_Wake_Up_IRQHandler
- CAN4_Error_IRQHandler ⇒ CAN4_Error_IRQHandler
- CAN4_ORed_0_15_MB_IRQHandler ⇒ CAN4_ORed_0_15_MB_IRQHandler
- CAN4_ORed_16_31_MB_IRQHandler ⇒ CAN4_ORed_16_31_MB_IRQHandler
- CAN4_ORed_IRQHandler ⇒ CAN4_ORed_IRQHandler
- CAN4_Wake_Up_IRQHandler ⇒ CAN4_Wake_Up_IRQHandler
- CAN5_Error_IRQHandler ⇒ CAN5_Error_IRQHandler
- CAN5_ORed_0_15_MB_IRQHandler ⇒ CAN5_ORed_0_15_MB_IRQHandler
- CAN5_ORed_16_31_MB_IRQHandler ⇒ CAN5_ORed_16_31_MB_IRQHandler
- CAN5_ORed_IRQHandler ⇒ CAN5_ORed_IRQHandler
- CAN5_Wake_Up_IRQHandler ⇒ CAN5_Wake_Up_IRQHandler
- DebugMon_Handler ⇒ DebugMon_Handler
- DefaultISR ⇒ DefaultISR
- EFM_Ecc_IRQHandler ⇒ EFM_Ecc_IRQHandler
- EFM_Error_IRQHandler ⇒ EFM_Error_IRQHandler
- EFM_IRQHandler ⇒ EFM_IRQHandler
- EMU_SB_IRQHandler ⇒ EMU_SB_IRQHandler
- FPU_IRQHandler ⇒ FPU_IRQHandler
- GPIOA_IRQHandler ⇒ GPIOA_IRQHandler
- GPIOB_IRQHandler ⇒ GPIOB_IRQHandler
- GPIOC_IRQHandler ⇒ GPIOC_IRQHandler
- GPIOD_IRQHandler ⇒ GPIOD_IRQHandler
- GPIOE_IRQHandler ⇒ GPIOE_IRQHandler
- HCU_IRQHandler ⇒ HCU_IRQHandler
- HardFault_Handler ⇒ HardFault_Handler
- I2C0_Master_IRQHandler ⇒ I2C0_Master_IRQHandler
- I2C0_Slave_IRQHandler ⇒ I2C0_Slave_IRQHandler
- I2C1_Master_IRQHandler ⇒ I2C1_Master_IRQHandler
- I2C1_Slave_IRQHandler ⇒ I2C1_Slave_IRQHandler
- I2C2_Master_IRQHandler ⇒ I2C2_Master_IRQHandler
- I2C2_Slave_IRQHandler ⇒ I2C2_Slave_IRQHandler
- INTM_IRQHandler ⇒ INTM_IRQHandler
- LINFlexD0_IRQHandler ⇒ LINFlexD0_IRQHandler
- LINFlexD1_IRQHandler ⇒ LINFlexD1_IRQHandler
- LINFlexD2_IRQHandler ⇒ LINFlexD2_IRQHandler
- LINFlexD3_IRQHandler ⇒ LINFlexD3_IRQHandler
- LINFlexD4_IRQHandler ⇒ LINFlexD4_IRQHandler
- LINFlexD5_IRQHandler ⇒ LINFlexD5_IRQHandler
- MemManage_Handler ⇒ MemManage_Handler
- NMI_Handler ⇒ NMI_Handler
- PCU_IRQHandler ⇒ PCU_IRQHandler
- PTU0_IRQHandler ⇒ PTU0_IRQHandler
- PTU1_IRQHandler ⇒ PTU1_IRQHandler
- PendSV_Handler ⇒ PendSV_Handler
- RCU_IRQHandler ⇒ RCU_IRQHandler
- RTC_IRQHandler ⇒ RTC_IRQHandler
- RTC_Seconds_IRQHandler ⇒ RTC_Seconds_IRQHandler
- SCU_IRQHandler ⇒ SCU_IRQHandler
- SPI0_IRQHandler ⇒ SPI0_IRQHandler
- SPI1_IRQHandler ⇒ SPI1_IRQHandler
- SPI2_IRQHandler ⇒ SPI2_IRQHandler
- SPI3_IRQHandler ⇒ SPI3_IRQHandler
- SPI4_IRQHandler ⇒ SPI4_IRQHandler
- SPI5_IRQHandler ⇒ SPI5_IRQHandler
- SVC_Handler ⇒ SVC_Handler
- SysTick_Handler ⇒ SysTick_Handler
- TMR0_Ch0_IRQHandler ⇒ TMR0_Ch0_IRQHandler
- TMR0_Ch1_IRQHandler ⇒ TMR0_Ch1_IRQHandler
- TMR0_Ch2_IRQHandler ⇒ TMR0_Ch2_IRQHandler
- TMR0_Ch3_IRQHandler ⇒ TMR0_Ch3_IRQHandler
- TRNG_IRQHandler ⇒ TRNG_IRQHandler
- UsageFault_Handler ⇒ UsageFault_Handler
- WKU_IRQHandler ⇒ WKU_IRQHandler
- Wdg_Mld_Isr ⇒ Wdg_Mld_Isr
- eTMR0_Ch0_Ch1_IRQHandler ⇒ eTMR0_Ch0_Ch1_IRQHandler
- eTMR0_Ch2_Ch3_IRQHandler ⇒ eTMR0_Ch2_Ch3_IRQHandler
- eTMR0_Ch4_Ch5_IRQHandler ⇒ eTMR0_Ch4_Ch5_IRQHandler
- eTMR0_Ch6_Ch7_IRQHandler ⇒ eTMR0_Ch6_Ch7_IRQHandler
- eTMR0_Fault_IRQHandler ⇒ eTMR0_Fault_IRQHandler
- eTMR0_Ovf_IRQHandler ⇒ eTMR0_Ovf_IRQHandler
- eTMR1_Ch0_Ch1_IRQHandler ⇒ eTMR1_Ch0_Ch1_IRQHandler
- eTMR1_Ch2_Ch3_IRQHandler ⇒ eTMR1_Ch2_Ch3_IRQHandler
- eTMR1_Ch4_Ch5_IRQHandler ⇒ eTMR1_Ch4_Ch5_IRQHandler
- eTMR1_Ch6_Ch7_IRQHandler ⇒ eTMR1_Ch6_Ch7_IRQHandler
- eTMR1_Fault_IRQHandler ⇒ eTMR1_Fault_IRQHandler
- eTMR1_Ovf_IRQHandler ⇒ eTMR1_Ovf_IRQHandler
- eTMR2_Ch0_Ch1_IRQHandler ⇒ eTMR2_Ch0_Ch1_IRQHandler
- eTMR2_Ch2_Ch3_IRQHandler ⇒ eTMR2_Ch2_Ch3_IRQHandler
- eTMR2_Ch4_Ch5_IRQHandler ⇒ eTMR2_Ch4_Ch5_IRQHandler
- eTMR2_Ch6_Ch7_IRQHandler ⇒ eTMR2_Ch6_Ch7_IRQHandler
- eTMR2_Fault_IRQHandler ⇒ eTMR2_Fault_IRQHandler
- eTMR2_Ovf_IRQHandler ⇒ eTMR2_Ovf_IRQHandler
- eTMR3_Ch0_Ch1_IRQHandler ⇒ eTMR3_Ch0_Ch1_IRQHandler
- eTMR3_Ch2_Ch3_IRQHandler ⇒ eTMR3_Ch2_Ch3_IRQHandler
- eTMR3_Ch4_Ch5_IRQHandler ⇒ eTMR3_Ch4_Ch5_IRQHandler
- eTMR3_Ch6_Ch7_IRQHandler ⇒ eTMR3_Ch6_Ch7_IRQHandler
- eTMR3_Fault_IRQHandler ⇒ eTMR3_Fault_IRQHandler
- eTMR3_Ovf_IRQHandler ⇒ eTMR3_Ovf_IRQHandler
- eTMR4_Ch0_Ch1_IRQHandler ⇒ eTMR4_Ch0_Ch1_IRQHandler
- eTMR4_Ch2_Ch3_IRQHandler ⇒ eTMR4_Ch2_Ch3_IRQHandler
- eTMR4_Ch4_Ch5_IRQHandler ⇒ eTMR4_Ch4_Ch5_IRQHandler
- eTMR4_Ch6_Ch7_IRQHandler ⇒ eTMR4_Ch6_Ch7_IRQHandler
- eTMR4_Fault_IRQHandler ⇒ eTMR4_Fault_IRQHandler
- eTMR4_Ovf_IRQHandler ⇒ eTMR4_Ovf_IRQHandler
- eTMR5_Ch0_Ch1_IRQHandler ⇒ eTMR5_Ch0_Ch1_IRQHandler
- eTMR5_Ch2_Ch3_IRQHandler ⇒ eTMR5_Ch2_Ch3_IRQHandler
- eTMR5_Ch4_Ch5_IRQHandler ⇒ eTMR5_Ch4_Ch5_IRQHandler
- eTMR5_Ch6_Ch7_IRQHandler ⇒ eTMR5_Ch6_Ch7_IRQHandler
- eTMR5_Fault_IRQHandler ⇒ eTMR5_Fault_IRQHandler
- eTMR5_Ovf_IRQHandler ⇒ eTMR5_Ovf_IRQHandler
- lpTMR0_IRQHandler ⇒ lpTMR0_IRQHandler
- pTMR_Ch0_IRQHandler ⇒ pTMR_Ch0_IRQHandler
- pTMR_Ch1_IRQHandler ⇒ pTMR_Ch1_IRQHandler
- pTMR_Ch2_IRQHandler ⇒ pTMR_Ch2_IRQHandler
- pTMR_Ch3_IRQHandler ⇒ pTMR_Ch3_IRQHandler

  ### Function Pointers

  - ACMP0_IRQHandler from vector_table_copy.o(.text.ACMP0_IRQHandler) referenced from vector.o(.isr_vector)
  - ADC0_Group2CallBack from main.o(.text.ADC0_Group2CallBack) referenced from adc_pbcfg.o(.mcal_const_cfg)
  - ADC0_Group3CallBack from main.o(.text.ADC0_Group3CallBack) referenced from adc_pbcfg.o(.mcal_const_cfg)
  - ADC0_IRQHandler from adc_irq.o(.mcal_text) referenced from vector.o(.isr_vector)
  - ADC1_Group0CallBack from main.o(.text.ADC1_Group0CallBack) referenced from adc_pbcfg.o(.mcal_const_cfg)
  - ADC1_Group1CallBack from main.o(.text.ADC1_Group1CallBack) referenced from adc_pbcfg.o(.mcal_const_cfg)
  - ADC1_IRQHandler from adc_irq.o(.mcal_text) referenced from vector.o(.isr_vector)
  - Adc_Lld_DmaTransEndNotification from adc_lld.o(.mcal_text) referenced 2 times from adc_lld.o(.mcal_text)
  - BusFault_Handler from vector_table_copy.o(.text.BusFault_Handler) referenced from vector.o(.isr_vector)
  - CAN0_Error_IRQHandler from vector_table_copy.o(.text.CAN0_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN0_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_Error_IRQHandler from vector_table_copy.o(.text.CAN1_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN1_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_Error_IRQHandler from vector_table_copy.o(.text.CAN2_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN2_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_Error_IRQHandler from vector_table_copy.o(.text.CAN3_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN3_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_Error_IRQHandler from vector_table_copy.o(.text.CAN4_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN4_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_Error_IRQHandler from vector_table_copy.o(.text.CAN5_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN5_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN5_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_ORed_IRQHandler from vector_table_copy.o(.text.CAN5_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN5_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA0_IRQHandler from cdddma_lld.o(.mcal_text) referenced from vector.o(.isr_vector)
  - DMA10_IRQHandler from cdddma_lld.o(.mcal_text) referenced from vector.o(.isr_vector)
  - DMA11_IRQHandler from cdddma_lld.o(.mcal_text) referenced from vector.o(.isr_vector)
  - DMA12_IRQHandler from cdddma_lld.o(.mcal_text) referenced from vector.o(.isr_vector)
  - DMA13_IRQHandler from cdddma_lld.o(.mcal_text) referenced from vector.o(.isr_vector)
  - DMA14_IRQHandler from cdddma_lld.o(.mcal_text) referenced from vector.o(.isr_vector)
  - DMA15_IRQHandler from cdddma_lld.o(.mcal_text) referenced from vector.o(.isr_vector)
  - DMA1_IRQHandler from cdddma_lld.o(.mcal_text) referenced from vector.o(.isr_vector)
  - DMA2_IRQHandler from cdddma_lld.o(.mcal_text) referenced from vector.o(.isr_vector)
  - DMA3_IRQHandler from cdddma_lld.o(.mcal_text) referenced from vector.o(.isr_vector)
  - DMA4_IRQHandler from cdddma_lld.o(.mcal_text) referenced from vector.o(.isr_vector)
  - DMA5_IRQHandler from cdddma_lld.o(.mcal_text) referenced from vector.o(.isr_vector)
  - DMA6_IRQHandler from cdddma_lld.o(.mcal_text) referenced from vector.o(.isr_vector)
  - DMA7_IRQHandler from cdddma_lld.o(.mcal_text) referenced from vector.o(.isr_vector)
  - DMA8_IRQHandler from cdddma_lld.o(.mcal_text) referenced from vector.o(.isr_vector)
  - DMA9_IRQHandler from cdddma_lld.o(.mcal_text) referenced from vector.o(.isr_vector)
  - DMA_Error_IRQHandler from cdddma_lld.o(.mcal_text) referenced from vector.o(.isr_vector)
  - DebugMon_Handler from vector_table_copy.o(.text.DebugMon_Handler) referenced from vector.o(.isr_vector)
  - DefaultISR from vector_table_copy.o(.text.DefaultISR) referenced 55 times from vector.o(.isr_vector)
  - EFM_Ecc_IRQHandler from vector_table_copy.o(.text.EFM_Ecc_IRQHandler) referenced from vector.o(.isr_vector)
  - EFM_Error_IRQHandler from vector_table_copy.o(.text.EFM_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - EFM_IRQHandler from vector_table_copy.o(.text.EFM_IRQHandler) referenced from vector.o(.isr_vector)
  - EMU_SB_IRQHandler from vector_table_copy.o(.text.EMU_SB_IRQHandler) referenced from vector.o(.isr_vector)
  - FPU_IRQHandler from vector_table_copy.o(.text.FPU_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOA_IRQHandler from vector_table_copy.o(.text.GPIOA_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOB_IRQHandler from vector_table_copy.o(.text.GPIOB_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOC_IRQHandler from vector_table_copy.o(.text.GPIOC_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOD_IRQHandler from vector_table_copy.o(.text.GPIOD_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOE_IRQHandler from vector_table_copy.o(.text.GPIOE_IRQHandler) referenced from vector.o(.isr_vector)
  - HCU_IRQHandler from vector_table_copy.o(.text.HCU_IRQHandler) referenced from vector.o(.isr_vector)
  - HardFault_Handler from vector_table_copy.o(.text.HardFault_Handler) referenced from vector.o(.isr_vector)
  - I2C0_Master_IRQHandler from vector_table_copy.o(.text.I2C0_Master_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C0_Slave_IRQHandler from vector_table_copy.o(.text.I2C0_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C1_Master_IRQHandler from vector_table_copy.o(.text.I2C1_Master_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C1_Slave_IRQHandler from vector_table_copy.o(.text.I2C1_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C2_Master_IRQHandler from vector_table_copy.o(.text.I2C2_Master_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C2_Slave_IRQHandler from vector_table_copy.o(.text.I2C2_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - INTM_IRQHandler from vector_table_copy.o(.text.INTM_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD0_IRQHandler from vector_table_copy.o(.text.LINFlexD0_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD1_IRQHandler from vector_table_copy.o(.text.LINFlexD1_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD2_IRQHandler from vector_table_copy.o(.text.LINFlexD2_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD3_IRQHandler from vector_table_copy.o(.text.LINFlexD3_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD4_IRQHandler from vector_table_copy.o(.text.LINFlexD4_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD5_IRQHandler from vector_table_copy.o(.text.LINFlexD5_IRQHandler) referenced from vector.o(.isr_vector)
  - MemManage_Handler from vector_table_copy.o(.text.MemManage_Handler) referenced from vector.o(.isr_vector)
  - NMI_Handler from vector_table_copy.o(.text.NMI_Handler) referenced from vector.o(.isr_vector)
  - PCU_IRQHandler from vector_table_copy.o(.text.PCU_IRQHandler) referenced from vector.o(.isr_vector)
  - PTU0_IRQHandler from vector_table_copy.o(.text.PTU0_IRQHandler) referenced from vector.o(.isr_vector)
  - PTU1_IRQHandler from vector_table_copy.o(.text.PTU1_IRQHandler) referenced from vector.o(.isr_vector)
  - PendSV_Handler from vector_table_copy.o(.text.PendSV_Handler) referenced from vector.o(.isr_vector)
  - RCU_IRQHandler from vector_table_copy.o(.text.RCU_IRQHandler) referenced from vector.o(.isr_vector)
  - RTC_IRQHandler from vector_table_copy.o(.text.RTC_IRQHandler) referenced from vector.o(.isr_vector)
  - RTC_Seconds_IRQHandler from vector_table_copy.o(.text.RTC_Seconds_IRQHandler) referenced from vector.o(.isr_vector)
  - RamInit1 from raminit1.o(.text.RamInit1) referenced from startup.o(.text)
  - RamInit2 from raminit2.o(.text.RamInit2) referenced from startup.o(.text)
  - Reset_Handler from startup.o(.text) referenced from vector.o(.isr_vector)
  - SCU_IRQHandler from vector_table_copy.o(.text.SCU_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI0_IRQHandler from vector_table_copy.o(.text.SPI0_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI1_IRQHandler from vector_table_copy.o(.text.SPI1_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI2_IRQHandler from vector_table_copy.o(.text.SPI2_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI3_IRQHandler from vector_table_copy.o(.text.SPI3_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI4_IRQHandler from vector_table_copy.o(.text.SPI4_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI5_IRQHandler from vector_table_copy.o(.text.SPI5_IRQHandler) referenced from vector.o(.isr_vector)
  - SVC_Handler from vector_table_copy.o(.text.SVC_Handler) referenced from vector.o(.isr_vector)
  - SysTick_Handler from vector_table_copy.o(.text.SysTick_Handler) referenced from vector.o(.isr_vector)
  - SystemInit from system.o(.text.SystemInit) referenced from startup.o(.text)
  - TMR0_Ch0_IRQHandler from vector_table_copy.o(.text.TMR0_Ch0_IRQHandler) referenced from vector.o(.isr_vector)
  - TMR0_Ch1_IRQHandler from vector_table_copy.o(.text.TMR0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - TMR0_Ch2_IRQHandler from vector_table_copy.o(.text.TMR0_Ch2_IRQHandler) referenced from vector.o(.isr_vector)
  - TMR0_Ch3_IRQHandler from vector_table_copy.o(.text.TMR0_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - TRNG_IRQHandler from vector_table_copy.o(.text.TRNG_IRQHandler) referenced from vector.o(.isr_vector)
  - UsageFault_Handler from vector_table_copy.o(.text.UsageFault_Handler) referenced from vector.o(.isr_vector)
  - VectorTableCopy from vector_table_copy.o(.text.VectorTableCopy) referenced from startup.o(.text)
  - WKU_IRQHandler from vector_table_copy.o(.text.WKU_IRQHandler) referenced from vector.o(.isr_vector)
  - Wdg_Mld_Isr from vector_table_copy.o(.text.Wdg_Mld_Isr) referenced from vector.o(.isr_vector)
  - eTMR0_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Fault_IRQHandler from vector_table_copy.o(.text.eTMR0_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR0_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Fault_IRQHandler from vector_table_copy.o(.text.eTMR1_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR1_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR2_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR2_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR2_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR2_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Fault_IRQHandler from vector_table_copy.o(.text.eTMR2_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR2_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR3_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR3_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR3_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR3_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Fault_IRQHandler from vector_table_copy.o(.text.eTMR3_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR3_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR4_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR4_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR4_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR4_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Fault_IRQHandler from vector_table_copy.o(.text.eTMR4_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR4_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR5_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR5_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR5_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR5_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Fault_IRQHandler from vector_table_copy.o(.text.eTMR5_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR5_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - lpTMR0_IRQHandler from vector_table_copy.o(.text.lpTMR0_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR_Ch0_IRQHandler from vector_table_copy.o(.text.pTMR_Ch0_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR_Ch1_IRQHandler from vector_table_copy.o(.text.pTMR_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR_Ch2_IRQHandler from vector_table_copy.o(.text.pTMR_Ch2_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR_Ch3_IRQHandler from vector_table_copy.o(.text.pTMR_Ch3_IRQHandler) referenced from vector.o(.isr_vector)

  ### Global Symbols

  RamInit0 (Thumb, 0 bytes, Stack size unknown bytes, raminit0.o(.text))
  [Called By]

  - >> Reset_Handler

  Reset_Handler (Thumb, 0 bytes, Stack size unknown bytes, startup.o(.text))
  [Stack]

  - Max Depth = 216 + Unknown Stack Size
  - Call Chain = Reset_Handler ⇒ main ⇒ Adc_GetStreamLastPointer ⇒ Adc_HandleHwReloadAfterRead ⇒ Adc_Lld_StartConversion ⇒ CddDma_SetLogicChannelTransfer ⇒ Dma_Lld_SetChannelTransfer
  [Calls]
  - >> RamInit0
  - >> main
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> VectorTableCopy

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> RamInit1

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  ACMP0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ACMP0_IRQHandler))
  [Calls]

  - >> ACMP0_IRQHandler
  [Called By]
  - >> ACMP0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  ADC0_Group2CallBack (Thumb, 74 bytes, Stack size 8 bytes, main.o(.text.ADC0_Group2CallBack))
  [Stack]

  - Max Depth = 224
  - Call Chain = ADC0_Group2CallBack ⇒ Adc_ReadGroup ⇒ Adc_HandleHwReloadAfterRead ⇒ Adc_Lld_StartConversion ⇒ CddDma_SetLogicChannelTransfer ⇒ Dma_Lld_SetChannelTransfer
  [Calls]
  - >> Adc_ReadGroup
  - >> Adc_GetGroupStatus
  [Address Reference Count : 1]
  - adc_pbcfg.o(.mcal_const_cfg)

  ADC0_Group3CallBack (Thumb, 16 bytes, Stack size 0 bytes, main.o(.text.ADC0_Group3CallBack))
  [Address Reference Count : 1]

  - adc_pbcfg.o(.mcal_const_cfg)

  ADC1_Group0CallBack (Thumb, 16 bytes, Stack size 0 bytes, main.o(.text.ADC1_Group0CallBack))
  [Address Reference Count : 1]

  - adc_pbcfg.o(.mcal_const_cfg)

  ADC1_Group1CallBack (Thumb, 16 bytes, Stack size 0 bytes, main.o(.text.ADC1_Group1CallBack))
  [Address Reference Count : 1]

  - adc_pbcfg.o(.mcal_const_cfg)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_Error_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_Error_IRQHandler))
  [Calls]

  - >> CAN0_Error_IRQHandler
  [Called By]
  - >> CAN0_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_0_15_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_0_15_MB_IRQHandler))
  [Calls]

  - >> CAN0_ORed_0_15_MB_IRQHandler
  [Called By]
  - >> CAN0_ORed_0_15_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_16_31_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_16_31_MB_IRQHandler))
  [Calls]

  - >> CAN0_ORed_16_31_MB_IRQHandler
  [Called By]
  - >> CAN0_ORed_16_31_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_32_47_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_32_47_MB_IRQHandler))
  [Calls]

  - >> CAN0_ORed_32_47_MB_IRQHandler
  [Called By]
  - >> CAN0_ORed_32_47_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_48_63_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_48_63_MB_IRQHandler))
  [Calls]

  - >> CAN0_ORed_48_63_MB_IRQHandler
  [Called By]
  - >> CAN0_ORed_48_63_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_IRQHandler))
  [Calls]

  - >> CAN0_ORed_IRQHandler
  [Called By]
  - >> CAN0_ORed_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_Wake_Up_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_Wake_Up_IRQHandler))
  [Calls]

  - >> CAN0_Wake_Up_IRQHandler
  [Called By]
  - >> CAN0_Wake_Up_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_Error_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_Error_IRQHandler))
  [Calls]

  - >> CAN1_Error_IRQHandler
  [Called By]
  - >> CAN1_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_0_15_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_0_15_MB_IRQHandler))
  [Calls]

  - >> CAN1_ORed_0_15_MB_IRQHandler
  [Called By]
  - >> CAN1_ORed_0_15_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_16_31_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_16_31_MB_IRQHandler))
  [Calls]

  - >> CAN1_ORed_16_31_MB_IRQHandler
  [Called By]
  - >> CAN1_ORed_16_31_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_32_47_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_32_47_MB_IRQHandler))
  [Calls]

  - >> CAN1_ORed_32_47_MB_IRQHandler
  [Called By]
  - >> CAN1_ORed_32_47_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_48_63_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_48_63_MB_IRQHandler))
  [Calls]

  - >> CAN1_ORed_48_63_MB_IRQHandler
  [Called By]
  - >> CAN1_ORed_48_63_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_IRQHandler))
  [Calls]

  - >> CAN1_ORed_IRQHandler
  [Called By]
  - >> CAN1_ORed_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_Wake_Up_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_Wake_Up_IRQHandler))
  [Calls]

  - >> CAN1_Wake_Up_IRQHandler
  [Called By]
  - >> CAN1_Wake_Up_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN2_Error_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_Error_IRQHandler))
  [Calls]

  - >> CAN2_Error_IRQHandler
  [Called By]
  - >> CAN2_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN2_ORed_0_15_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_0_15_MB_IRQHandler))
  [Calls]

  - >> CAN2_ORed_0_15_MB_IRQHandler
  [Called By]
  - >> CAN2_ORed_0_15_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN2_ORed_16_31_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_16_31_MB_IRQHandler))
  [Calls]

  - >> CAN2_ORed_16_31_MB_IRQHandler
  [Called By]
  - >> CAN2_ORed_16_31_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN2_ORed_32_47_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_32_47_MB_IRQHandler))
  [Calls]

  - >> CAN2_ORed_32_47_MB_IRQHandler
  [Called By]
  - >> CAN2_ORed_32_47_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN2_ORed_48_63_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_48_63_MB_IRQHandler))
  [Calls]

  - >> CAN2_ORed_48_63_MB_IRQHandler
  [Called By]
  - >> CAN2_ORed_48_63_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN2_ORed_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_IRQHandler))
  [Calls]

  - >> CAN2_ORed_IRQHandler
  [Called By]
  - >> CAN2_ORed_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN2_Wake_Up_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_Wake_Up_IRQHandler))
  [Calls]

  - >> CAN2_Wake_Up_IRQHandler
  [Called By]
  - >> CAN2_Wake_Up_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN3_Error_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_Error_IRQHandler))
  [Calls]

  - >> CAN3_Error_IRQHandler
  [Called By]
  - >> CAN3_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN3_ORed_0_15_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_0_15_MB_IRQHandler))
  [Calls]

  - >> CAN3_ORed_0_15_MB_IRQHandler
  [Called By]
  - >> CAN3_ORed_0_15_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN3_ORed_16_31_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_16_31_MB_IRQHandler))
  [Calls]

  - >> CAN3_ORed_16_31_MB_IRQHandler
  [Called By]
  - >> CAN3_ORed_16_31_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN3_ORed_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_IRQHandler))
  [Calls]

  - >> CAN3_ORed_IRQHandler
  [Called By]
  - >> CAN3_ORed_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN3_Wake_Up_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_Wake_Up_IRQHandler))
  [Calls]

  - >> CAN3_Wake_Up_IRQHandler
  [Called By]
  - >> CAN3_Wake_Up_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN4_Error_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_Error_IRQHandler))
  [Calls]

  - >> CAN4_Error_IRQHandler
  [Called By]
  - >> CAN4_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN4_ORed_0_15_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_0_15_MB_IRQHandler))
  [Calls]

  - >> CAN4_ORed_0_15_MB_IRQHandler
  [Called By]
  - >> CAN4_ORed_0_15_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN4_ORed_16_31_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_16_31_MB_IRQHandler))
  [Calls]

  - >> CAN4_ORed_16_31_MB_IRQHandler
  [Called By]
  - >> CAN4_ORed_16_31_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN4_ORed_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_IRQHandler))
  [Calls]

  - >> CAN4_ORed_IRQHandler
  [Called By]
  - >> CAN4_ORed_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN4_Wake_Up_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_Wake_Up_IRQHandler))
  [Calls]

  - >> CAN4_Wake_Up_IRQHandler
  [Called By]
  - >> CAN4_Wake_Up_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN5_Error_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_Error_IRQHandler))
  [Calls]

  - >> CAN5_Error_IRQHandler
  [Called By]
  - >> CAN5_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN5_ORed_0_15_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_ORed_0_15_MB_IRQHandler))
  [Calls]

  - >> CAN5_ORed_0_15_MB_IRQHandler
  [Called By]
  - >> CAN5_ORed_0_15_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN5_ORed_16_31_MB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_ORed_16_31_MB_IRQHandler))
  [Calls]

  - >> CAN5_ORed_16_31_MB_IRQHandler
  [Called By]
  - >> CAN5_ORed_16_31_MB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN5_ORed_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_ORed_IRQHandler))
  [Calls]

  - >> CAN5_ORed_IRQHandler
  [Called By]
  - >> CAN5_ORed_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN5_Wake_Up_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_Wake_Up_IRQHandler))
  [Calls]

  - >> CAN5_Wake_Up_IRQHandler
  [Called By]
  - >> CAN5_Wake_Up_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DebugMon_Handler))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DefaultISR (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DefaultISR))
  [Calls]

  - >> DefaultISR
  [Called By]
  - >> DefaultISR
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  Det_ReportError (Thumb, 60 bytes, Stack size 0 bytes, det.o(.text.Det_ReportError))
  [Called By]

  - >> Platform_InstallIrqHandler
  - >> Platform_GetIrqPriority
  - >> Platform_SetIrqPriority
  - >> Platform_SetIrq
  - >> Port_SetPinMode
  - >> Port_SetPinDirection
  - >> Port_RefreshPortDirection
  - >> Adc_StopGroupConversion
  - >> Adc_DisableGroupNotification
  - >> Adc_DeInit
  - >> Adc_GetStreamLastPointer
  - >> Adc_StartGroupConversion
  - >> Adc_EnableGroupNotification
  - >> Adc_SetupResultBuffer
  - >> Adc_Init
  - >> Platform_Init
  - >> Port_Init
  - >> Adc_ReadGroup
  - >> Adc_GetGroupStatus

  Det_ReportRuntimeError (Thumb, 60 bytes, Stack size 0 bytes, det.o(.text.Det_ReportRuntimeError))
  [Called By]

  - >> Adc_DeInit
  - >> Adc_StartGroupConversion
  - >> Adc_SetupResultBuffer
  - >> Adc_ReadGroup

  EFM_Ecc_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_Ecc_IRQHandler))
  [Calls]

  - >> EFM_Ecc_IRQHandler
  [Called By]
  - >> EFM_Ecc_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  EFM_Error_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_Error_IRQHandler))
  [Calls]

  - >> EFM_Error_IRQHandler
  [Called By]
  - >> EFM_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  EFM_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_IRQHandler))
  [Calls]

  - >> EFM_IRQHandler
  [Called By]
  - >> EFM_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  EMU_SB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EMU_SB_IRQHandler))
  [Calls]

  - >> EMU_SB_IRQHandler
  [Called By]
  - >> EMU_SB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  FPU_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.FPU_IRQHandler))
  [Calls]

  - >> FPU_IRQHandler
  [Called By]
  - >> FPU_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  GPIOA_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOA_IRQHandler))
  [Calls]

  - >> GPIOA_IRQHandler
  [Called By]
  - >> GPIOA_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  GPIOB_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOB_IRQHandler))
  [Calls]

  - >> GPIOB_IRQHandler
  [Called By]
  - >> GPIOB_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  GPIOC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOC_IRQHandler))
  [Calls]

  - >> GPIOC_IRQHandler
  [Called By]
  - >> GPIOC_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  GPIOD_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOD_IRQHandler))
  [Calls]

  - >> GPIOD_IRQHandler
  [Called By]
  - >> GPIOD_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  GPIOE_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOE_IRQHandler))
  [Calls]

  - >> GPIOE_IRQHandler
  [Called By]
  - >> GPIOE_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  HCU_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.HCU_IRQHandler))
  [Calls]

  - >> HCU_IRQHandler
  [Called By]
  - >> HCU_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  I2C0_Master_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C0_Master_IRQHandler))
  [Calls]

  - >> I2C0_Master_IRQHandler
  [Called By]
  - >> I2C0_Master_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  I2C0_Slave_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C0_Slave_IRQHandler))
  [Calls]

  - >> I2C0_Slave_IRQHandler
  [Called By]
  - >> I2C0_Slave_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  I2C1_Master_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C1_Master_IRQHandler))
  [Calls]

  - >> I2C1_Master_IRQHandler
  [Called By]
  - >> I2C1_Master_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  I2C1_Slave_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C1_Slave_IRQHandler))
  [Calls]

  - >> I2C1_Slave_IRQHandler
  [Called By]
  - >> I2C1_Slave_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  I2C2_Master_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C2_Master_IRQHandler))
  [Calls]

  - >> I2C2_Master_IRQHandler
  [Called By]
  - >> I2C2_Master_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  I2C2_Slave_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C2_Slave_IRQHandler))
  [Calls]

  - >> I2C2_Slave_IRQHandler
  [Called By]
  - >> I2C2_Slave_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  INTM_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.INTM_IRQHandler))
  [Calls]

  - >> INTM_IRQHandler
  [Called By]
  - >> INTM_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  LINFlexD0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD0_IRQHandler))
  [Calls]

  - >> LINFlexD0_IRQHandler
  [Called By]
  - >> LINFlexD0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  LINFlexD1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD1_IRQHandler))
  [Calls]

  - >> LINFlexD1_IRQHandler
  [Called By]
  - >> LINFlexD1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  LINFlexD2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD2_IRQHandler))
  [Calls]

  - >> LINFlexD2_IRQHandler
  [Called By]
  - >> LINFlexD2_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  LINFlexD3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD3_IRQHandler))
  [Calls]

  - >> LINFlexD3_IRQHandler
  [Called By]
  - >> LINFlexD3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  LINFlexD4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD4_IRQHandler))
  [Calls]

  - >> LINFlexD4_IRQHandler
  [Called By]
  - >> LINFlexD4_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  LINFlexD5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD5_IRQHandler))
  [Calls]

  - >> LINFlexD5_IRQHandler
  [Called By]
  - >> LINFlexD5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.NMI_Handler))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  PCU_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.PCU_IRQHandler))
  [Calls]

  - >> PCU_IRQHandler
  [Called By]
  - >> PCU_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  PTU0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.PTU0_IRQHandler))
  [Calls]

  - >> PTU0_IRQHandler
  [Called By]
  - >> PTU0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  PTU1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.PTU1_IRQHandler))
  [Calls]

  - >> PTU1_IRQHandler
  [Called By]
  - >> PTU1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.PendSV_Handler))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  RCU_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.RCU_IRQHandler))
  [Calls]

  - >> RCU_IRQHandler
  [Called By]
  - >> RCU_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  RTC_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.RTC_IRQHandler))
  [Calls]

  - >> RTC_IRQHandler
  [Called By]
  - >> RTC_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  RTC_Seconds_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.RTC_Seconds_IRQHandler))
  [Calls]

  - >> RTC_Seconds_IRQHandler
  [Called By]
  - >> RTC_Seconds_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  RamInit1 (Thumb, 324 bytes, Stack size 40 bytes, raminit1.o(.text.RamInit1))
  [Stack]

  - Max Depth = 40
  - Call Chain = RamInit1
  [Calls]
  - >> __aeabi_memclr4
  [Address Reference Count : 1]
  - startup.o(.text)

  RamInit2 (Thumb, 2 bytes, Stack size 0 bytes, raminit2.o(.text.RamInit2))
  [Address Reference Count : 1]

  - startup.o(.text)

  SCU_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SCU_IRQHandler))
  [Calls]

  - >> SCU_IRQHandler
  [Called By]
  - >> SCU_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SPI0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI0_IRQHandler))
  [Calls]

  - >> SPI0_IRQHandler
  [Called By]
  - >> SPI0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SPI1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI1_IRQHandler))
  [Calls]

  - >> SPI1_IRQHandler
  [Called By]
  - >> SPI1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SPI2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI2_IRQHandler))
  [Calls]

  - >> SPI2_IRQHandler
  [Called By]
  - >> SPI2_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SPI3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI3_IRQHandler))
  [Calls]

  - >> SPI3_IRQHandler
  [Called By]
  - >> SPI3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SPI4_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI4_IRQHandler))
  [Calls]

  - >> SPI4_IRQHandler
  [Called By]
  - >> SPI4_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SPI5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI5_IRQHandler))
  [Calls]

  - >> SPI5_IRQHandler
  [Called By]
  - >> SPI5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SVC_Handler))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SysTick_Handler))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SystemInit (Thumb, 60 bytes, Stack size 0 bytes, system.o(.text.SystemInit))
  [Address Reference Count : 1]

  - startup.o(.text)

  TMR0_Ch0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.TMR0_Ch0_IRQHandler))
  [Calls]

  - >> TMR0_Ch0_IRQHandler
  [Called By]
  - >> TMR0_Ch0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  TMR0_Ch1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.TMR0_Ch1_IRQHandler))
  [Calls]

  - >> TMR0_Ch1_IRQHandler
  [Called By]
  - >> TMR0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  TMR0_Ch2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.TMR0_Ch2_IRQHandler))
  [Calls]

  - >> TMR0_Ch2_IRQHandler
  [Called By]
  - >> TMR0_Ch2_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  TMR0_Ch3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.TMR0_Ch3_IRQHandler))
  [Calls]

  - >> TMR0_Ch3_IRQHandler
  [Called By]
  - >> TMR0_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  TRNG_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.TRNG_IRQHandler))
  [Calls]

  - >> TRNG_IRQHandler
  [Called By]
  - >> TRNG_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  VectorTableCopy (Thumb, 70 bytes, Stack size 8 bytes, vector_table_copy.o(.text.VectorTableCopy))
  [Stack]

  - Max Depth = 8
  - Call Chain = VectorTableCopy
  [Calls]
  - >> __aeabi_memcpy4
  - >> Sys_GetCoreID
  [Address Reference Count : 1]
  - startup.o(.text)

  WKU_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.WKU_IRQHandler))
  [Calls]

  - >> WKU_IRQHandler
  [Called By]
  - >> WKU_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  Wdg_Mld_Isr (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.Wdg_Mld_Isr))
  [Calls]

  - >> Wdg_Mld_Isr
  [Called By]
  - >> Wdg_Mld_Isr
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ch0_Ch1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ch0_Ch1_IRQHandler))
  [Calls]

  - >> eTMR0_Ch0_Ch1_IRQHandler
  [Called By]
  - >> eTMR0_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ch2_Ch3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ch2_Ch3_IRQHandler))
  [Calls]

  - >> eTMR0_Ch2_Ch3_IRQHandler
  [Called By]
  - >> eTMR0_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ch4_Ch5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ch4_Ch5_IRQHandler))
  [Calls]

  - >> eTMR0_Ch4_Ch5_IRQHandler
  [Called By]
  - >> eTMR0_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ch6_Ch7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ch6_Ch7_IRQHandler))
  [Calls]

  - >> eTMR0_Ch6_Ch7_IRQHandler
  [Called By]
  - >> eTMR0_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Fault_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Fault_IRQHandler))
  [Calls]

  - >> eTMR0_Fault_IRQHandler
  [Called By]
  - >> eTMR0_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ovf_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ovf_IRQHandler))
  [Calls]

  - >> eTMR0_Ovf_IRQHandler
  [Called By]
  - >> eTMR0_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ch0_Ch1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ch0_Ch1_IRQHandler))
  [Calls]

  - >> eTMR1_Ch0_Ch1_IRQHandler
  [Called By]
  - >> eTMR1_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ch2_Ch3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ch2_Ch3_IRQHandler))
  [Calls]

  - >> eTMR1_Ch2_Ch3_IRQHandler
  [Called By]
  - >> eTMR1_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ch4_Ch5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ch4_Ch5_IRQHandler))
  [Calls]

  - >> eTMR1_Ch4_Ch5_IRQHandler
  [Called By]
  - >> eTMR1_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ch6_Ch7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ch6_Ch7_IRQHandler))
  [Calls]

  - >> eTMR1_Ch6_Ch7_IRQHandler
  [Called By]
  - >> eTMR1_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Fault_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Fault_IRQHandler))
  [Calls]

  - >> eTMR1_Fault_IRQHandler
  [Called By]
  - >> eTMR1_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ovf_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ovf_IRQHandler))
  [Calls]

  - >> eTMR1_Ovf_IRQHandler
  [Called By]
  - >> eTMR1_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ch0_Ch1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR2_Ch0_Ch1_IRQHandler))
  [Calls]

  - >> eTMR2_Ch0_Ch1_IRQHandler
  [Called By]
  - >> eTMR2_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ch2_Ch3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR2_Ch2_Ch3_IRQHandler))
  [Calls]

  - >> eTMR2_Ch2_Ch3_IRQHandler
  [Called By]
  - >> eTMR2_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ch4_Ch5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR2_Ch4_Ch5_IRQHandler))
  [Calls]

  - >> eTMR2_Ch4_Ch5_IRQHandler
  [Called By]
  - >> eTMR2_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ch6_Ch7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR2_Ch6_Ch7_IRQHandler))
  [Calls]

  - >> eTMR2_Ch6_Ch7_IRQHandler
  [Called By]
  - >> eTMR2_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Fault_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR2_Fault_IRQHandler))
  [Calls]

  - >> eTMR2_Fault_IRQHandler
  [Called By]
  - >> eTMR2_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ovf_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR2_Ovf_IRQHandler))
  [Calls]

  - >> eTMR2_Ovf_IRQHandler
  [Called By]
  - >> eTMR2_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ch0_Ch1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR3_Ch0_Ch1_IRQHandler))
  [Calls]

  - >> eTMR3_Ch0_Ch1_IRQHandler
  [Called By]
  - >> eTMR3_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ch2_Ch3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR3_Ch2_Ch3_IRQHandler))
  [Calls]

  - >> eTMR3_Ch2_Ch3_IRQHandler
  [Called By]
  - >> eTMR3_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ch4_Ch5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR3_Ch4_Ch5_IRQHandler))
  [Calls]

  - >> eTMR3_Ch4_Ch5_IRQHandler
  [Called By]
  - >> eTMR3_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ch6_Ch7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR3_Ch6_Ch7_IRQHandler))
  [Calls]

  - >> eTMR3_Ch6_Ch7_IRQHandler
  [Called By]
  - >> eTMR3_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Fault_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR3_Fault_IRQHandler))
  [Calls]

  - >> eTMR3_Fault_IRQHandler
  [Called By]
  - >> eTMR3_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ovf_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR3_Ovf_IRQHandler))
  [Calls]

  - >> eTMR3_Ovf_IRQHandler
  [Called By]
  - >> eTMR3_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ch0_Ch1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR4_Ch0_Ch1_IRQHandler))
  [Calls]

  - >> eTMR4_Ch0_Ch1_IRQHandler
  [Called By]
  - >> eTMR4_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ch2_Ch3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR4_Ch2_Ch3_IRQHandler))
  [Calls]

  - >> eTMR4_Ch2_Ch3_IRQHandler
  [Called By]
  - >> eTMR4_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ch4_Ch5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR4_Ch4_Ch5_IRQHandler))
  [Calls]

  - >> eTMR4_Ch4_Ch5_IRQHandler
  [Called By]
  - >> eTMR4_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ch6_Ch7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR4_Ch6_Ch7_IRQHandler))
  [Calls]

  - >> eTMR4_Ch6_Ch7_IRQHandler
  [Called By]
  - >> eTMR4_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Fault_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR4_Fault_IRQHandler))
  [Calls]

  - >> eTMR4_Fault_IRQHandler
  [Called By]
  - >> eTMR4_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ovf_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR4_Ovf_IRQHandler))
  [Calls]

  - >> eTMR4_Ovf_IRQHandler
  [Called By]
  - >> eTMR4_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ch0_Ch1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR5_Ch0_Ch1_IRQHandler))
  [Calls]

  - >> eTMR5_Ch0_Ch1_IRQHandler
  [Called By]
  - >> eTMR5_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ch2_Ch3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR5_Ch2_Ch3_IRQHandler))
  [Calls]

  - >> eTMR5_Ch2_Ch3_IRQHandler
  [Called By]
  - >> eTMR5_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ch4_Ch5_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR5_Ch4_Ch5_IRQHandler))
  [Calls]

  - >> eTMR5_Ch4_Ch5_IRQHandler
  [Called By]
  - >> eTMR5_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ch6_Ch7_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR5_Ch6_Ch7_IRQHandler))
  [Calls]

  - >> eTMR5_Ch6_Ch7_IRQHandler
  [Called By]
  - >> eTMR5_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Fault_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR5_Fault_IRQHandler))
  [Calls]

  - >> eTMR5_Fault_IRQHandler
  [Called By]
  - >> eTMR5_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ovf_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR5_Ovf_IRQHandler))
  [Calls]

  - >> eTMR5_Ovf_IRQHandler
  [Called By]
  - >> eTMR5_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  lpTMR0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.lpTMR0_IRQHandler))
  [Calls]

  - >> lpTMR0_IRQHandler
  [Called By]
  - >> lpTMR0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  main (Thumb, 718 bytes, Stack size 0 bytes, main.o(.text.main))
  [Stack]

  - Max Depth = 216
  - Call Chain = main ⇒ Adc_GetStreamLastPointer ⇒ Adc_HandleHwReloadAfterRead ⇒ Adc_Lld_StartConversion ⇒ CddDma_SetLogicChannelTransfer ⇒ Dma_Lld_SetChannelTransfer
  [Calls]
  - >> Adc_GetStreamLastPointer
  - >> Dio_FlipChannel
  - >> Adc_StartGroupConversion
  - >> Adc_EnableGroupNotification
  - >> Adc_SetupResultBuffer
  - >> Adc_Init
  - >> CddDma_Init
  - >> Platform_Init
  - >> Port_Init
  - >> Mcu_DistributePllClock
  - >> Mcu_GetPllStatus
  - >> Mcu_InitClock
  - >> Mcu_Init
  - >> Adc_ReadGroup
  - >> Adc_GetGroupStatus
  [Called By]
  - >> Reset_Handler

  pTMR_Ch0_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR_Ch0_IRQHandler))
  [Calls]

  - >> pTMR_Ch0_IRQHandler
  [Called By]
  - >> pTMR_Ch0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  pTMR_Ch1_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR_Ch1_IRQHandler))
  [Calls]

  - >> pTMR_Ch1_IRQHandler
  [Called By]
  - >> pTMR_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  pTMR_Ch2_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR_Ch2_IRQHandler))
  [Calls]

  - >> pTMR_Ch2_IRQHandler
  [Called By]
  - >> pTMR_Ch2_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  pTMR_Ch3_IRQHandler (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR_Ch3_IRQHandler))
  [Calls]

  - >> pTMR_Ch3_IRQHandler
  [Called By]
  - >> pTMR_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  Mcu_DistributePllClock (Thumb, 32 bytes, Stack size 8 bytes, mcu.o(.mcal_text))
  [Stack]

  - Max Depth = 48
  - Call Chain = Mcu_DistributePllClock ⇒ Mcu_Lld_SetClockSource
  [Calls]
  - >> Mcu_Lld_SetClockSource
  - >> Mcu_Lld_GetPllStatus
  [Called By]
  - >> main

  Mcu_GetPllStatus (Thumb, 22 bytes, Stack size 0 bytes, mcu.o(.mcal_text))
  [Calls]

  - >> Mcu_Lld_GetPllStatus
  [Called By]
  - >> main

  Mcu_GetResetReason (Thumb, 22 bytes, Stack size 0 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_GetResetValue

  Mcu_Init (Thumb, 52 bytes, Stack size 16 bytes, mcu.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Mcu_Init
  [Calls]
  - >> Mcu_Lld_SetPcu
  - >> Mcu_Lld_SetRcu
  [Called By]
  - >> main

  Mcu_InitClock (Thumb, 66 bytes, Stack size 0 bytes, mcu.o(.mcal_text))
  [Stack]

  - Max Depth = 68
  - Call Chain = Mcu_InitClock ⇒ Mcu_Lld_InitClock ⇒ Mcu_Lld_SetClockSource
  [Calls]
  - >> Mcu_Lld_InitClock
  [Called By]
  - >> main

  Mcu_InitRamSection (Thumb, 54 bytes, Stack size 8 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_SetRamSection

  Mcu_SetMode (Thumb, 62 bytes, Stack size 16 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00
  - >> Mcu_Lld_SetMode
  - >> SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00

  Mcu_GetResetRawValue (Thumb, 4 bytes, Stack size 0 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_GetResetRawValue

  Mcu_180_GetCoreClockFrequency (Thumb, 48 bytes, Stack size 0 bytes, mcu.o(.mcal_text), UNUSED)
  [Calls]

  - >> Mcu_Lld_GetCoreClockFrequency

  Mcu_Lld_SetCmuChannel2 (Thumb, 18 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)

  Mcu_Lld_GetPllStatus (Thumb, 22 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_DistributePllClock
  - >> Mcu_GetPllStatus

  Mcu_Lld_SystemReset (Thumb, 36 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)

  Mcu_Lld_SetRcu (Thumb, 54 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Init

  Mcu_Lld_SetRamSection (Thumb, 34 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_InitRamSection

  Mcu_Lld_SetMode (Thumb, 216 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_SetMode

  Mcu_Lld_SetClockSource (Thumb, 254 bytes, Stack size 40 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Mcu_Lld_SetClockSource
  [Called By]
  - >> Mcu_Lld_InitClock
  - >> Mcu_DistributePllClock

  Mcu_Lld_SetPeripheralClock (Thumb, 108 bytes, Stack size 20 bytes, mcu_lld.o(.mcal_text), UNUSED)

  Mcu_Lld_InitClock (Thumb, 888 bytes, Stack size 28 bytes, mcu_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 68
  - Call Chain = Mcu_Lld_InitClock ⇒ Mcu_Lld_SetClockSource
  [Calls]
  - >> Mcu_Lld_SetClockSource
  [Called By]
  - >> Mcu_InitClock

  Mcu_Lld_GetResetRawValue (Thumb, 24 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_GetResetRawValue

  Mcu_Lld_GetResetValue (Thumb, 158 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_GetResetReason

  Mcu_Lld_GetPllClockFrequency (Thumb, 78 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)

  Mcu_Lld_GetCoreClockFrequency (Thumb, 124 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_180_GetCoreClockFrequency

  Mcu_Lld_SetPcu (Thumb, 62 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
  [Called By]

  - >> Mcu_Init

  SchM_Mcu_ReadMsr (Thumb, 6 bytes, Stack size 0 bytes, schm_mcu.o(.mcal_text), UNUSED)

  SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00 (Thumb, 42 bytes, Stack size 0 bytes, schm_mcu.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_SetMode

  SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00 (Thumb, 40 bytes, Stack size 0 bytes, schm_mcu.o(.mcal_text), UNUSED)
  [Called By]

  - >> Mcu_SetMode

  Adc_DeInit (Thumb, 226 bytes, Stack size 40 bytes, adc.o(.mcal_text), UNUSED)
  [Calls]

  - >> Det_ReportRuntimeError
  - >> Det_ReportError
  - >> Adc_Lld_DeinitHwUnit

  Adc_DisableGroupNotification (Thumb, 194 bytes, Stack size 16 bytes, adc.o(.mcal_text), UNUSED)
  [Calls]

  - >> Adc_Lld_GroupIndexCheck
  - >> Det_ReportError

  Adc_EnableGroupNotification (Thumb, 194 bytes, Stack size 16 bytes, adc.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Adc_EnableGroupNotification ⇒ Adc_Lld_GroupIndexCheck
  [Calls]
  - >> Adc_Lld_GroupIndexCheck
  - >> Det_ReportError
  [Called By]
  - >> main

  Adc_GetGroupStatus (Thumb, 156 bytes, Stack size 16 bytes, adc.o(.mcal_text))
  [Stack]

  - Max Depth = 200
  - Call Chain = Adc_GetGroupStatus ⇒ Adc_UpdataStatusInReadApi ⇒ Adc_Lld_StartConversion ⇒ CddDma_SetLogicChannelTransfer ⇒ Dma_Lld_SetChannelTransfer
  [Calls]
  - >> Adc_Lld_GroupIndexCheck
  - >> Det_ReportError
  - >> Adc_UpdataStatusInReadApi
  [Called By]
  - >> main
  - >> ADC0_Group2CallBack

  Adc_GetStreamLastPointer (Thumb, 384 bytes, Stack size 32 bytes, adc.o(.mcal_text))
  [Stack]

  - Max Depth = 216
  - Call Chain = Adc_GetStreamLastPointer ⇒ Adc_HandleHwReloadAfterRead ⇒ Adc_Lld_StartConversion ⇒ CddDma_SetLogicChannelTransfer ⇒ Dma_Lld_SetChannelTransfer
  [Calls]
  - >> SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_01
  - >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_01
  - >> Adc_Lld_GroupIndexCheck
  - >> Det_ReportError
  - >> Adc_HandleHwReloadAfterRead
  - >> Adc_UpdataStatusInReadApi
  [Called By]
  - >> main

  Adc_Init (Thumb, 272 bytes, Stack size 40 bytes, adc.o(.mcal_text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Adc_Init
  [Calls]
  - >> Adc_Lld_InitTempSensor
  - >> Adc_Lld_DisableIntcandHwTrigger
  - >> Adc_Lld_HwClockInit
  - >> Adc_Lld_HwUnitEnable
  - >> Adc_Lld_StopConversion
  - >> Det_ReportError
  [Called By]
  - >> main

  Adc_ReadGroup (Thumb, 400 bytes, Stack size 32 bytes, adc.o(.mcal_text))
  [Stack]

  - Max Depth = 216
  - Call Chain = Adc_ReadGroup ⇒ Adc_HandleHwReloadAfterRead ⇒ Adc_Lld_StartConversion ⇒ CddDma_SetLogicChannelTransfer ⇒ Dma_Lld_SetChannelTransfer
  [Calls]
  - >> SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_02
  - >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_02
  - >> Adc_Lld_GroupIndexCheck
  - >> Det_ReportRuntimeError
  - >> Det_ReportError
  - >> Adc_HandleHwReloadAfterRead
  - >> Adc_UpdataStatusInReadApi
  [Called By]
  - >> main
  - >> ADC0_Group2CallBack

  Adc_SetupResultBuffer (Thumb, 184 bytes, Stack size 16 bytes, adc.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Adc_SetupResultBuffer ⇒ Adc_Lld_GroupIndexCheck
  [Calls]
  - >> Adc_Lld_GroupIndexCheck
  - >> Det_ReportRuntimeError
  - >> Det_ReportError
  [Called By]
  - >> main

  Adc_StartGroupConversion (Thumb, 404 bytes, Stack size 24 bytes, adc.o(.mcal_text))
  [Stack]

  - Max Depth = 176
  - Call Chain = Adc_StartGroupConversion ⇒ Adc_Lld_StartConversion ⇒ CddDma_SetLogicChannelTransfer ⇒ Dma_Lld_SetChannelTransfer
  [Calls]
  - >> SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_03
  - >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_03
  - >> Adc_Lld_StartConversion
  - >> Adc_Lld_LoadGroupToHwUnit
  - >> Adc_Lld_GroupIndexCheck
  - >> Det_ReportRuntimeError
  - >> Det_ReportError
  [Called By]
  - >> main

  Adc_StopGroupConversion (Thumb, 664 bytes, Stack size 40 bytes, adc.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_04
  - >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_04
  - >> Adc_Lld_StopConversion
  - >> Adc_Lld_StartConversion
  - >> Adc_Lld_LoadGroupToHwUnit
  - >> Adc_Lld_ClearSeqConvEndIntFlag
  - >> Adc_Lld_GroupIndexCheck
  - >> Det_ReportError

  ADC0_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, adc_irq.o(.mcal_text))
  [Stack]

  - Max Depth = 192
  - Call Chain = ADC0_IRQHandler ⇒ Adc_Lld_IrqProcess ⇒ Adc_Lld_StartConversion ⇒ CddDma_SetLogicChannelTransfer ⇒ Dma_Lld_SetChannelTransfer
  [Calls]
  - >> Adc_Lld_IrqProcess
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  ADC1_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, adc_irq.o(.mcal_text))
  [Stack]

  - Max Depth = 192
  - Call Chain = ADC1_IRQHandler ⇒ Adc_Lld_IrqProcess ⇒ Adc_Lld_StartConversion ⇒ CddDma_SetLogicChannelTransfer ⇒ Dma_Lld_SetChannelTransfer
  [Calls]
  - >> Adc_Lld_IrqProcess
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  Adc_Lld_GetRunningGroupIndex (Thumb, 138 bytes, Stack size 8 bytes, adc_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Adc_Lld_GetRunningGroupIndex
  [Called By]
  - >> Adc_HandleHwReloadAfterRead
  - >> Adc_UpdataStatusInReadApi

  Adc_Lld_GroupIndexCheck (Thumb, 92 bytes, Stack size 8 bytes, adc_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Adc_Lld_GroupIndexCheck
  [Called By]
  - >> Adc_StopGroupConversion
  - >> Adc_DisableGroupNotification
  - >> Adc_HandleHwReloadAfterRead
  - >> Adc_UpdataStatusInReadApi
  - >> Adc_GetStreamLastPointer
  - >> Adc_StartGroupConversion
  - >> Adc_EnableGroupNotification
  - >> Adc_SetupResultBuffer
  - >> Adc_ReadGroup
  - >> Adc_GetGroupStatus

  Adc_Lld_InitTempSensor (Thumb, 22 bytes, Stack size 0 bytes, adc_lld.o(.mcal_text))
  [Called By]

  - >> Adc_Init

  Adc_Lld_HwUnitEnable (Thumb, 46 bytes, Stack size 0 bytes, adc_lld.o(.mcal_text))
  [Called By]

  - >> Adc_Init

  Adc_Lld_HwClockInit (Thumb, 38 bytes, Stack size 0 bytes, adc_lld.o(.mcal_text))
  [Called By]

  - >> Adc_Init

  Adc_Lld_StopConversion (Thumb, 46 bytes, Stack size 0 bytes, adc_lld.o(.mcal_text))
  [Called By]

  - >> Adc_StopGroupConversion
  - >> Adc_HandleHwReloadAfterRead
  - >> Adc_UpdataStatusInReadApi
  - >> Adc_Init

  Adc_Lld_StartConversion (Thumb, 390 bytes, Stack size 40 bytes, adc_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 152
  - Call Chain = Adc_Lld_StartConversion ⇒ CddDma_SetLogicChannelTransfer ⇒ Dma_Lld_SetChannelTransfer
  [Calls]
  - >> CddDma_StartChannel
  - >> CddDma_InstallCallback
  - >> CddDma_SetLogicChannelTransfer
  [Called By]
  - >> Adc_Lld_DmaTransEndNotification
  - >> Adc_Lld_IrqProcess
  - >> Adc_StopGroupConversion
  - >> Adc_HandleHwReloadAfterRead
  - >> Adc_UpdataStatusInReadApi
  - >> Adc_StartGroupConversion

  Adc_Lld_DisableIntcandHwTrigger (Thumb, 26 bytes, Stack size 0 bytes, adc_lld.o(.mcal_text))
  [Called By]

  - >> Adc_Init

  Adc_Lld_DeinitHwUnit (Thumb, 150 bytes, Stack size 0 bytes, adc_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Adc_DeInit

  Adc_Lld_ReadSeqConvEndIntFlag (Thumb, 20 bytes, Stack size 0 bytes, adc_lld.o(.mcal_text))
  [Called By]

  - >> Adc_UpdataStatusInReadApi

  Adc_Lld_ClearSeqConvEndIntFlag (Thumb, 18 bytes, Stack size 0 bytes, adc_lld.o(.mcal_text))
  [Called By]

  - >> Adc_StopGroupConversion
  - >> Adc_HandleHwReloadAfterRead
  - >> Adc_UpdataStatusInReadApi

  Adc_Lld_ReadConversionResults (Thumb, 234 bytes, Stack size 28 bytes, adc_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 28
  - Call Chain = Adc_Lld_ReadConversionResults
  [Called By]
  - >> Adc_Lld_IrqProcess
  - >> Adc_UpdataStatusInReadApi

  Adc_Lld_LoadGroupToHwUnit (Thumb, 250 bytes, Stack size 20 bytes, adc_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 20
  - Call Chain = Adc_Lld_LoadGroupToHwUnit
  [Called By]
  - >> Adc_Lld_DmaTransEndNotification
  - >> Adc_Lld_IrqProcess
  - >> Adc_StopGroupConversion
  - >> Adc_HandleHwReloadAfterRead
  - >> Adc_UpdataStatusInReadApi
  - >> Adc_StartGroupConversion

  Adc_Lld_GroupStatusUpdata (Thumb, 110 bytes, Stack size 0 bytes, adc_lld.o(.mcal_text))
  [Called By]

  - >> Adc_UpdataStatusInReadApi

  Adc_Lld_QueueDataUpdata (Thumb, 150 bytes, Stack size 16 bytes, adc_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Adc_Lld_QueueDataUpdata
  [Calls]
  - >> SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_05
  - >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_05
  [Called By]
  - >> Adc_UpdataStatusInReadApi

  Adc_Lld_IrqProcess (Thumb, 606 bytes, Stack size 40 bytes, adc_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 192
  - Call Chain = Adc_Lld_IrqProcess ⇒ Adc_Lld_StartConversion ⇒ CddDma_SetLogicChannelTransfer ⇒ Dma_Lld_SetChannelTransfer
  [Calls]
  - >> SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_05
  - >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_05
  - >> Adc_Lld_StartConversion
  - >> Adc_Lld_LoadGroupToHwUnit
  - >> Adc_Lld_ReadConversionResults
  [Called By]
  - >> ADC1_IRQHandler
  - >> ADC0_IRQHandler

  Adc_Lld_DmaTransEndNotification (Thumb, 874 bytes, Stack size 56 bytes, adc_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 208
  - Call Chain = Adc_Lld_DmaTransEndNotification ⇒ Adc_Lld_StartConversion ⇒ CddDma_SetLogicChannelTransfer ⇒ Dma_Lld_SetChannelTransfer
  [Calls]
  - >> CddDma_StopChannel
  - >> SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_05
  - >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_05
  - >> Adc_Lld_StartConversion
  - >> Adc_Lld_LoadGroupToHwUnit
  [Address Reference Count : 1]
  - adc_lld.o(.mcal_text)

  SchM_Adc_ReadMsr (Thumb, 6 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text), UNUSED)

  SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_00 (Thumb, 42 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text), UNUSED)

  SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_00 (Thumb, 40 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text), UNUSED)

  SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_01 (Thumb, 42 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text))
  [Called By]

  - >> Adc_GetStreamLastPointer

  SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_01 (Thumb, 40 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text))
  [Called By]

  - >> Adc_GetStreamLastPointer

  SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_02 (Thumb, 42 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text))
  [Called By]

  - >> Adc_ReadGroup

  SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_02 (Thumb, 40 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text))
  [Called By]

  - >> Adc_ReadGroup

  SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_03 (Thumb, 42 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text))
  [Called By]

  - >> Adc_StartGroupConversion

  SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_03 (Thumb, 40 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text))
  [Called By]

  - >> Adc_StartGroupConversion

  SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_04 (Thumb, 42 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text), UNUSED)
  [Called By]

  - >> Adc_StopGroupConversion

  SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_04 (Thumb, 40 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text), UNUSED)
  [Called By]

  - >> Adc_StopGroupConversion

  SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_05 (Thumb, 42 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text))
  [Called By]

  - >> Adc_Lld_DmaTransEndNotification
  - >> Adc_Lld_IrqProcess
  - >> Adc_Lld_QueueDataUpdata

  SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_05 (Thumb, 40 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text))
  [Called By]

  - >> Adc_Lld_DmaTransEndNotification
  - >> Adc_Lld_IrqProcess
  - >> Adc_Lld_QueueDataUpdata

  SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_06 (Thumb, 42 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text))
  [Called By]

  - >> Adc_HandleHwReloadAfterRead

  SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_06 (Thumb, 40 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text))
  [Called By]

  - >> Adc_HandleHwReloadAfterRead

  Dio_Lld_WriteSetOutGPIOPort (Thumb, 14 bytes, Stack size 0 bytes, dio_lld.o(.mcal_text), UNUSED)

  Dio_Lld_WriteClrOutGPIOPort (Thumb, 14 bytes, Stack size 0 bytes, dio_lld.o(.mcal_text), UNUSED)

  Dio_Lld_WriteGPIOPin (Thumb, 40 bytes, Stack size 0 bytes, dio_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Dio_WriteChannel

  Dio_Lld_ReadGPIOPin (Thumb, 20 bytes, Stack size 0 bytes, dio_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Dio_ReadChannel

  Dio_Lld_WriteGPIOPort (Thumb, 14 bytes, Stack size 0 bytes, dio_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Dio_WritePort

  Dio_Lld_ReadGPIOPort (Thumb, 14 bytes, Stack size 0 bytes, dio_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Dio_ReadPort

  Dio_Lld_ToggleGPIOPin (Thumb, 44 bytes, Stack size 8 bytes, dio_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Dio_Lld_ToggleGPIOPin
  [Called By]
  - >> Dio_FlipChannel

  Dio_FlipChannel (Thumb, 10 bytes, Stack size 0 bytes, dio.o(.mcal_text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Dio_FlipChannel ⇒ Dio_Lld_ToggleGPIOPin
  [Calls]
  - >> Dio_Lld_ToggleGPIOPin
  [Called By]
  - >> main

  Dio_ReadChannel (Thumb, 10 bytes, Stack size 0 bytes, dio.o(.mcal_text), UNUSED)
  [Calls]

  - >> Dio_Lld_ReadGPIOPin

  Dio_ReadPort (Thumb, 4 bytes, Stack size 0 bytes, dio.o(.mcal_text), UNUSED)
  [Calls]

  - >> Dio_Lld_ReadGPIOPort

  Dio_WriteChannel (Thumb, 12 bytes, Stack size 0 bytes, dio.o(.mcal_text), UNUSED)
  [Calls]

  - >> Dio_Lld_WriteGPIOPin

  Dio_WritePort (Thumb, 4 bytes, Stack size 0 bytes, dio.o(.mcal_text), UNUSED)
  [Calls]

  - >> Dio_Lld_WriteGPIOPort

  CddDma_Init (Thumb, 14 bytes, Stack size 0 bytes, cdddma.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = CddDma_Init ⇒ Dma_Lld_Init
  [Calls]
  - >> Dma_Lld_Init
  [Called By]
  - >> main

  CddDma_DeInit (Thumb, 28 bytes, Stack size 8 bytes, cdddma.o(.mcal_text), UNUSED)
  [Calls]

  - >> Dma_Lld_Deinit

  CddDma_SetLogicChannelTransfer (Thumb, 74 bytes, Stack size 88 bytes, cdddma.o(.mcal_text))
  [Stack]

  - Max Depth = 112
  - Call Chain = CddDma_SetLogicChannelTransfer ⇒ Dma_Lld_SetChannelTransfer
  [Calls]
  - >> Dma_Lld_SetChannelTransfer
  [Called By]
  - >> Adc_Lld_StartConversion

  CddDma_StartChannel (Thumb, 6 bytes, Stack size 0 bytes, cdddma.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CddDma_StartChannel ⇒ Dma_Lld_SetDmaRequestCmd
  [Calls]
  - >> Dma_Lld_SetDmaRequestCmd
  [Called By]
  - >> Adc_Lld_StartConversion

  CddDma_StopChannel (Thumb, 6 bytes, Stack size 0 bytes, cdddma.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CddDma_StopChannel ⇒ Dma_Lld_SetDmaRequestCmd
  [Calls]
  - >> Dma_Lld_SetDmaRequestCmd
  [Called By]
  - >> Adc_Lld_DmaTransEndNotification

  CddDma_SoftTrigger (Thumb, 4 bytes, Stack size 0 bytes, cdddma.o(.mcal_text), UNUSED)
  [Calls]

  - >> Dma_Lld_TriggerChannelStart

  CddDma_ChannelRamReloadConfig (Thumb, 224 bytes, Stack size 104 bytes, cdddma.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_00
  - >> Dma_Lld_PushConfigToScts
  - >> SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_00

  CddDma_InstallCallback (Thumb, 4 bytes, Stack size 0 bytes, cdddma.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = CddDma_InstallCallback ⇒ Dma_Lld_InstallCallback
  [Calls]
  - >> Dma_Lld_InstallCallback
  [Called By]
  - >> Adc_Lld_StartConversion

  CddDma_InstallErrorCallback (Thumb, 4 bytes, Stack size 0 bytes, cdddma.o(.mcal_text), UNUSED)
  [Calls]

  - >> Dma_Lld_InstallErrorCallback

  CddDma_GetChannelStatus (Thumb, 4 bytes, Stack size 0 bytes, cdddma.o(.mcal_text), UNUSED)
  [Calls]

  - >> Dma_Lld_GetChannelStatus

  CddDma_ClearChannelDoneStatus (Thumb, 4 bytes, Stack size 0 bytes, cdddma.o(.mcal_text), UNUSED)
  [Calls]

  - >> Dma_Lld_ClearChannelDoneStatus

  CddDma_GetChannelRemainingTriggerCount (Thumb, 4 bytes, Stack size 0 bytes, cdddma.o(.mcal_text), UNUSED)
  [Calls]

  - >> Dma_Lld_GetRemainingTriggerCount

  Dma_Lld_TransferCancel (Thumb, 18 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text), UNUSED)

  Dma_Lld_Init (Thumb, 364 bytes, Stack size 32 bytes, cdddma_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 32
  - Call Chain = Dma_Lld_Init
  [Calls]
  - >> SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_02
  - >> SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_10
  - >> SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_10
  - >> SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_02
  [Called By]
  - >> CddDma_Init

  Dma_Lld_Deinit (Thumb, 56 bytes, Stack size 8 bytes, cdddma_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_03
  - >> SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_03
  [Called By]
  - >> CddDma_DeInit

  Dma_Lld_SetDmaRequestCmd (Thumb, 76 bytes, Stack size 16 bytes, cdddma_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Dma_Lld_SetDmaRequestCmd
  [Calls]
  - >> SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_10
  - >> SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_10
  [Called By]
  - >> CddDma_StopChannel
  - >> CddDma_StartChannel

  Dma_Lld_TriggerChannelStart (Thumb, 20 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> CddDma_SoftTrigger

  Dma_Lld_SetChannelTransfer (Thumb, 642 bytes, Stack size 24 bytes, cdddma_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 24
  - Call Chain = Dma_Lld_SetChannelTransfer
  [Calls]
  - >> SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_04
  - >> SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_01
  - >> SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_01
  - >> SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_04
  [Called By]
  - >> CddDma_SetLogicChannelTransfer

  Dma_Lld_GetChannelStatus (Thumb, 74 bytes, Stack size 16 bytes, cdddma_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_05
  - >> SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_05
  [Called By]
  - >> CddDma_GetChannelStatus

  Dma_Lld_ClearChannelDoneStatus (Thumb, 18 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> CddDma_ClearChannelDoneStatus

  Dma_Lld_GetRemainingTriggerCount (Thumb, 36 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> CddDma_GetChannelRemainingTriggerCount

  Dma_Lld_PushConfigToScts (Thumb, 148 bytes, Stack size 16 bytes, cdddma_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_06
  - >> SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_06
  [Called By]
  - >> CddDma_ChannelRamReloadConfig

  Dma_Lld_InstallCallback (Thumb, 40 bytes, Stack size 16 bytes, cdddma_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Dma_Lld_InstallCallback
  [Calls]
  - >> SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_07
  - >> SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_07
  [Called By]
  - >> CddDma_InstallCallback

  Dma_Lld_InstallErrorCallback (Thumb, 40 bytes, Stack size 16 bytes, cdddma_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_08
  - >> SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_08
  [Called By]
  - >> CddDma_InstallErrorCallback

  DMA_Error_IRQHandler (Thumb, 106 bytes, Stack size 16 bytes, cdddma_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = DMA_Error_IRQHandler
  [Calls]
  - >> SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_09
  - >> SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_09
  - >> SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_10
  - >> SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_10
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA0_IRQHandler (Thumb, 36 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA1_IRQHandler (Thumb, 36 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA2_IRQHandler (Thumb, 36 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA3_IRQHandler (Thumb, 36 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA4_IRQHandler (Thumb, 36 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA5_IRQHandler (Thumb, 38 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA6_IRQHandler (Thumb, 40 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA7_IRQHandler (Thumb, 40 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA8_IRQHandler (Thumb, 42 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA9_IRQHandler (Thumb, 42 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA10_IRQHandler (Thumb, 42 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA11_IRQHandler (Thumb, 42 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA12_IRQHandler (Thumb, 42 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA13_IRQHandler (Thumb, 42 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA14_IRQHandler (Thumb, 42 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA15_IRQHandler (Thumb, 42 bytes, Stack size 0 bytes, cdddma_lld.o(.mcal_text))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SchM_CddDma_ReadMsr (Thumb, 6 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text), UNUSED)

  SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_00 (Thumb, 42 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text), UNUSED)
  [Called By]

  - >> CddDma_ChannelRamReloadConfig

  SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_00 (Thumb, 40 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text), UNUSED)
  [Called By]

  - >> CddDma_ChannelRamReloadConfig

  SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_01 (Thumb, 42 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text))
  [Called By]

  - >> Dma_Lld_SetChannelTransfer

  SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_01 (Thumb, 40 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text))
  [Called By]

  - >> Dma_Lld_SetChannelTransfer

  SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_02 (Thumb, 42 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text))
  [Called By]

  - >> Dma_Lld_Init

  SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_02 (Thumb, 40 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text))
  [Called By]

  - >> Dma_Lld_Init

  SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_03 (Thumb, 42 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text), UNUSED)
  [Called By]

  - >> Dma_Lld_Deinit

  SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_03 (Thumb, 40 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text), UNUSED)
  [Called By]

  - >> Dma_Lld_Deinit

  SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_04 (Thumb, 42 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text))
  [Called By]

  - >> Dma_Lld_SetChannelTransfer

  SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_04 (Thumb, 40 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text))
  [Called By]

  - >> Dma_Lld_SetChannelTransfer

  SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_05 (Thumb, 42 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text), UNUSED)
  [Called By]

  - >> Dma_Lld_GetChannelStatus

  SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_05 (Thumb, 40 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text), UNUSED)
  [Called By]

  - >> Dma_Lld_GetChannelStatus

  SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_06 (Thumb, 42 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text), UNUSED)
  [Called By]

  - >> Dma_Lld_PushConfigToScts

  SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_06 (Thumb, 40 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text), UNUSED)
  [Called By]

  - >> Dma_Lld_PushConfigToScts

  SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_07 (Thumb, 42 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text))
  [Called By]

  - >> Dma_Lld_InstallCallback

  SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_07 (Thumb, 40 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text))
  [Called By]

  - >> Dma_Lld_InstallCallback

  SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_08 (Thumb, 42 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text), UNUSED)
  [Called By]

  - >> Dma_Lld_InstallErrorCallback

  SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_08 (Thumb, 40 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text), UNUSED)
  [Called By]

  - >> Dma_Lld_InstallErrorCallback

  SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_09 (Thumb, 42 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text))
  [Called By]

  - >> DMA_Error_IRQHandler

  SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_09 (Thumb, 40 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text))
  [Called By]

  - >> DMA_Error_IRQHandler

  SchM_Enter_CddDma_CDDDMA_EXCLUSIVE_AREA_10 (Thumb, 42 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text))
  [Called By]

  - >> DMA_Error_IRQHandler
  - >> Dma_Lld_SetDmaRequestCmd
  - >> Dma_Lld_Init

  SchM_Exit_CddDma_CDDDMA_EXCLUSIVE_AREA_10 (Thumb, 40 bytes, Stack size 0 bytes, schm_cdddma.o(.mcal_text))
  [Called By]

  - >> DMA_Error_IRQHandler
  - >> Dma_Lld_SetDmaRequestCmd
  - >> Dma_Lld_Init

  Port_Init (Thumb, 44 bytes, Stack size 8 bytes, port.o(.mcal_text))
  [Stack]

  - Max Depth = 76
  - Call Chain = Port_Init ⇒ Port_Lld_Init
  [Calls]
  - >> Port_Lld_Init
  - >> Det_ReportError
  [Called By]
  - >> main

  Port_RefreshPortDirection (Thumb, 38 bytes, Stack size 0 bytes, port.o(.mcal_text), UNUSED)
  [Calls]

  - >> Port_Lld_RefreshPortDirection
  - >> Det_ReportError

  Port_SetPinDirection (Thumb, 114 bytes, Stack size 16 bytes, port.o(.mcal_text), UNUSED)
  [Calls]

  - >> Port_Lld_SetPinDirection
  - >> Port_Lld_IsPinDireChangeable
  - >> Det_ReportError

  Port_SetPinMode (Thumb, 134 bytes, Stack size 16 bytes, port.o(.mcal_text), UNUSED)
  [Calls]

  - >> Port_Lld_SetPinMode
  - >> Port_Lld_IsPinModeChangeable
  - >> Det_ReportError

  Port_Lld_Init (Thumb, 476 bytes, Stack size 68 bytes, port_lld.o(.mcal_text))
  [Stack]

  - Max Depth = 68
  - Call Chain = Port_Lld_Init
  [Called By]
  - >> Port_Init

  Port_Lld_RefreshPortDirection (Thumb, 164 bytes, Stack size 40 bytes, port_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Enter_Port_PORT_EXCLUSIVE_AREA_02
  - >> SchM_Exit_Port_PORT_EXCLUSIVE_AREA_02
  [Called By]
  - >> Port_RefreshPortDirection

  Port_Lld_IsPinDireChangeable (Thumb, 48 bytes, Stack size 0 bytes, port_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Port_SetPinDirection

  Port_Lld_IsPinModeChangeable (Thumb, 48 bytes, Stack size 0 bytes, port_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Port_SetPinMode

  Port_Lld_SetPinDirection (Thumb, 86 bytes, Stack size 24 bytes, port_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_Port_PORT_EXCLUSIVE_AREA_00
  - >> SchM_Enter_Port_PORT_EXCLUSIVE_AREA_00
  [Called By]
  - >> Port_SetPinDirection

  Port_Lld_SetPinMode (Thumb, 42 bytes, Stack size 16 bytes, port_lld.o(.mcal_text), UNUSED)
  [Calls]

  - >> SchM_Exit_Port_PORT_EXCLUSIVE_AREA_01
  - >> SchM_Enter_Port_PORT_EXCLUSIVE_AREA_01
  [Called By]
  - >> Port_SetPinMode

  SchM_Port_ReadMsr (Thumb, 6 bytes, Stack size 0 bytes, schm_port.o(.mcal_text), UNUSED)

  SchM_Enter_Port_PORT_EXCLUSIVE_AREA_00 (Thumb, 42 bytes, Stack size 0 bytes, schm_port.o(.mcal_text), UNUSED)
  [Called By]

  - >> Port_Lld_SetPinDirection

  SchM_Exit_Port_PORT_EXCLUSIVE_AREA_00 (Thumb, 40 bytes, Stack size 0 bytes, schm_port.o(.mcal_text), UNUSED)
  [Called By]

  - >> Port_Lld_SetPinDirection

  SchM_Enter_Port_PORT_EXCLUSIVE_AREA_01 (Thumb, 42 bytes, Stack size 0 bytes, schm_port.o(.mcal_text), UNUSED)
  [Called By]

  - >> Port_Lld_SetPinMode

  SchM_Exit_Port_PORT_EXCLUSIVE_AREA_01 (Thumb, 40 bytes, Stack size 0 bytes, schm_port.o(.mcal_text), UNUSED)
  [Called By]

  - >> Port_Lld_SetPinMode

  SchM_Enter_Port_PORT_EXCLUSIVE_AREA_02 (Thumb, 42 bytes, Stack size 0 bytes, schm_port.o(.mcal_text), UNUSED)
  [Called By]

  - >> Port_Lld_RefreshPortDirection

  SchM_Exit_Port_PORT_EXCLUSIVE_AREA_02 (Thumb, 40 bytes, Stack size 0 bytes, schm_port.o(.mcal_text), UNUSED)
  [Called By]

  - >> Port_Lld_RefreshPortDirection

  IntCtrl_Lld_Init (Thumb, 236 bytes, Stack size 16 bytes, intctrl_lld.o(.mcal_text), UNUSED)

  IntCtrl_Lld_ClearPending (Thumb, 48 bytes, Stack size 0 bytes, intctrl_lld.o(.mcal_text), UNUSED)

  IntCtrl_Lld_SetPriority (Thumb, 44 bytes, Stack size 0 bytes, intctrl_lld.o(.mcal_text))
  [Called By]

  - >> Platform_SetIrqPriority
  - >> Platform_Mld_Init

  IntCtrl_Lld_EnableIrq (Thumb, 48 bytes, Stack size 0 bytes, intctrl_lld.o(.mcal_text))
  [Called By]

  - >> Platform_SetIrq
  - >> Platform_Mld_Init

  IntCtrl_Lld_DisableIrq (Thumb, 56 bytes, Stack size 0 bytes, intctrl_lld.o(.mcal_text))
  [Called By]

  - >> Platform_SetIrq
  - >> Platform_Mld_Init

  IntCtrl_Lld_InstallHandler (Thumb, 78 bytes, Stack size 8 bytes, intctrl_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Platform_InstallIrqHandler

  IntCtrl_Lld_GetPriority (Thumb, 36 bytes, Stack size 0 bytes, intctrl_lld.o(.mcal_text), UNUSED)
  [Called By]

  - >> Platform_GetIrqPriority

  Sys_GetCoreID (Thumb, 4 bytes, Stack size 0 bytes, osif.o(.mcal_text))
  [Called By]

  - >> VectorTableCopy

  Platform_Mld_Init (Thumb, 84 bytes, Stack size 16 bytes, platform_mld.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Platform_Mld_Init
  [Calls]
  - >> IntCtrl_Lld_DisableIrq
  - >> IntCtrl_Lld_EnableIrq
  - >> IntCtrl_Lld_SetPriority
  [Called By]
  - >> Platform_Init

  Platform_Init (Thumb, 32 bytes, Stack size 0 bytes, platform.o(.mcal_text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Platform_Init ⇒ Platform_Mld_Init
  [Calls]
  - >> Platform_Mld_Init
  - >> Det_ReportError
  [Called By]
  - >> main

  Platform_SetIrq (Thumb, 42 bytes, Stack size 8 bytes, platform.o(.mcal_text), UNUSED)
  [Calls]

  - >> IntCtrl_Lld_DisableIrq
  - >> IntCtrl_Lld_EnableIrq
  - >> Det_ReportError

  Platform_SetIrqPriority (Thumb, 34 bytes, Stack size 8 bytes, platform.o(.mcal_text), UNUSED)
  [Calls]

  - >> IntCtrl_Lld_SetPriority
  - >> Det_ReportError

  Platform_GetIrqPriority (Thumb, 46 bytes, Stack size 8 bytes, platform.o(.mcal_text), UNUSED)
  [Calls]

  - >> IntCtrl_Lld_GetPriority
  - >> Det_ReportError

  Platform_InstallIrqHandler (Thumb, 54 bytes, Stack size 8 bytes, platform.o(.mcal_text), UNUSED)
  [Calls]

  - >> IntCtrl_Lld_InstallHandler
  - >> Det_ReportError

  ### Local Symbols

  Adc_UpdataStatusInReadApi (Thumb, 238 bytes, Stack size 32 bytes, adc.o(.mcal_text))
  [Stack]

  - Max Depth = 184
  - Call Chain = Adc_UpdataStatusInReadApi ⇒ Adc_Lld_StartConversion ⇒ CddDma_SetLogicChannelTransfer ⇒ Dma_Lld_SetChannelTransfer
  [Calls]
  - >> Adc_Lld_StopConversion
  - >> Adc_Lld_StartConversion
  - >> Adc_Lld_LoadGroupToHwUnit
  - >> Adc_Lld_QueueDataUpdata
  - >> Adc_Lld_ClearSeqConvEndIntFlag
  - >> Adc_Lld_GroupStatusUpdata
  - >> Adc_Lld_ReadConversionResults
  - >> Adc_Lld_ReadSeqConvEndIntFlag
  - >> Adc_Lld_GetRunningGroupIndex
  - >> Adc_Lld_GroupIndexCheck
  [Called By]
  - >> Adc_GetStreamLastPointer
  - >> Adc_ReadGroup
  - >> Adc_GetGroupStatus

  Adc_HandleHwReloadAfterRead (Thumb, 556 bytes, Stack size 32 bytes, adc.o(.mcal_text))
  [Stack]

  - Max Depth = 184
  - Call Chain = Adc_HandleHwReloadAfterRead ⇒ Adc_Lld_StartConversion ⇒ CddDma_SetLogicChannelTransfer ⇒ Dma_Lld_SetChannelTransfer
  [Calls]
  - >> SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_06
  - >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_06
  - >> Adc_Lld_StopConversion
  - >> Adc_Lld_StartConversion
  - >> Adc_Lld_LoadGroupToHwUnit
  - >> Adc_Lld_ClearSeqConvEndIntFlag
  - >> Adc_Lld_GetRunningGroupIndex
  - >> Adc_Lld_GroupIndexCheck
  [Called By]
  - >> Adc_GetStreamLastPointer
  - >> Adc_ReadGroup

  ### Undefined Global Symbols