# Static Call Graph for image .\Objects\MCAL_MC03_DeepSleep_AdcCompare_Wakeup.axf

#<CALLGRAPH># ARM Linker, 6220000: Last Updated: Tue Jul 14 15:17:38 2026

### Maximum Stack Usage = 232 bytes + Unknown(Functions without stacksize, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

Reset_Handler ⇒ main ⇒ Board_Init ⇒ CddUart_Init ⇒ CddUart_Mld_Init ⇒ UART_Lld_Init ⇒ UART_Lld_SetBaudRate

### Functions with no stack information

- RamInit0
- Reset_Handler

### Function Pointers

- ACMP0_IRQHandler from vector_table_copy.o(.text.ACMP0_IRQHandler) referenced from vector.o(.isr_vector)
- ADC0_IRQHandler from adc_irq.o(.mcal_text) referenced from vector.o(.isr_vector)
- Adc_ConvCompleteCallback from main.o(.text.Adc_ConvCompleteCallback) referenced from adc_pbcfg.o(.mcal_const_cfg)
- BusFault_Handler from vector_table_copy.o(.text.BusFault_Handler) referenced from vector.o(.isr_vector)
- CAN0_Error_IRQHandler from vector_table_copy.o(.text.CAN0_Error_IRQHandler) referenced from vector.o(.isr_vector)
- CAN0_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
- CAN0_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
- CAN0_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
- CAN0_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
- CAN0_ORed_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_IRQHandler) referenced from vector.o(.isr_vector)
- CAN0_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN0_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
- CAN1_Error_IRQHandler from vector_table_copy.o(.text.CAN1_Error_IRQHandler) referenced from vector.o(.isr_vector)
- CAN1_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
- CAN1_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
- CAN1_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
- CAN1_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
- CAN1_ORed_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_IRQHandler) referenced from vector.o(.isr_vector)
- CAN1_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN1_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
- DMA0_IRQHandler from vector_table_copy.o(.text.DMA0_IRQHandler) referenced from vector.o(.isr_vector)
- DMA1_IRQHandler from vector_table_copy.o(.text.DMA1_IRQHandler) referenced from vector.o(.isr_vector)
- DMA2_IRQHandler from vector_table_copy.o(.text.DMA2_IRQHandler) referenced from vector.o(.isr_vector)
- DMA3_IRQHandler from vector_table_copy.o(.text.DMA3_IRQHandler) referenced from vector.o(.isr_vector)
- DMA_Error_IRQHandler from vector_table_copy.o(.text.DMA_Error_IRQHandler) referenced from vector.o(.isr_vector)
- DebugMon_Handler from vector_table_copy.o(.text.DebugMon_Handler) referenced from vector.o(.isr_vector)
- DefaultISR from vector_table_copy.o(.text.DefaultISR) referenced 85 times from vector.o(.isr_vector)
- EFM_Ecc_IRQHandler from vector_table_copy.o(.text.EFM_Ecc_IRQHandler) referenced from vector.o(.isr_vector)
- EFM_Error_IRQHandler from vector_table_copy.o(.text.EFM_Error_IRQHandler) referenced from vector.o(.isr_vector)
- EFM_IRQHandler from vector_table_copy.o(.text.EFM_IRQHandler) referenced from vector.o(.isr_vector)
- EMU_DB_IRQHandler from vector_table_copy.o(.text.EMU_DB_IRQHandler) referenced from vector.o(.isr_vector)
- EMU_SB_IRQHandler from vector_table_copy.o(.text.EMU_SB_IRQHandler) referenced from vector.o(.isr_vector)
- GPIOA_IRQHandler from vector_table_copy.o(.text.GPIOA_IRQHandler) referenced from vector.o(.isr_vector)
- GPIOB_IRQHandler from vector_table_copy.o(.text.GPIOB_IRQHandler) referenced from vector.o(.isr_vector)
- GPIOC_IRQHandler from vector_table_copy.o(.text.GPIOC_IRQHandler) referenced from vector.o(.isr_vector)
- GPIOD_IRQHandler from vector_table_copy.o(.text.GPIOD_IRQHandler) referenced from vector.o(.isr_vector)
- GPIOE_IRQHandler from vector_table_copy.o(.text.GPIOE_IRQHandler) referenced from vector.o(.isr_vector)
- HCU_IRQHandler from vector_table_copy.o(.text.HCU_IRQHandler) referenced from vector.o(.isr_vector)
- HardFault_Handler from vector_table_copy.o(.text.HardFault_Handler) referenced from vector.o(.isr_vector)
- I2C0_Master_IRQHandler from vector_table_copy.o(.text.I2C0_Master_IRQHandler) referenced from vector.o(.isr_vector)
- I2C0_Slave_IRQHandler from vector_table_copy.o(.text.I2C0_Slave_IRQHandler) referenced from vector.o(.isr_vector)
- I2C1_Master_IRQHandler from vector_table_copy.o(.text.I2C1_Master_IRQHandler) referenced from vector.o(.isr_vector)
- MPWM0_Ch0_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch0_IRQHandler) referenced from vector.o(.isr_vector)
- MPWM0_Ch0_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch0_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
- MPWM0_Ch1_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
- MPWM0_Ch1_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch1_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
- MPWM0_Ch2_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch2_IRQHandler) referenced from vector.o(.isr_vector)
- MPWM0_Ch2_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch2_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
- MPWM0_Ch3_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
- MPWM0_Ch3_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch3_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
- MPWM0_Ch4_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch4_IRQHandler) referenced from vector.o(.isr_vector)
- MPWM0_Ch4_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch4_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
- MPWM0_Ch5_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
- MPWM0_Ch5_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch5_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
- MPWM0_Ch6_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch6_IRQHandler) referenced from vector.o(.isr_vector)
- MPWM0_Ch6_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch6_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
- MPWM0_Ch7_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
- MPWM0_Ch7_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch7_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
- MemManage_Handler from vector_table_copy.o(.text.MemManage_Handler) referenced from vector.o(.isr_vector)
- NMI_Handler from vector_table_copy.o(.text.NMI_Handler) referenced from vector.o(.isr_vector)
- PCU_IRQHandler from vector_table_copy.o(.text.PCU_IRQHandler) referenced from vector.o(.isr_vector)
- PendSV_Handler from vector_table_copy.o(.text.PendSV_Handler) referenced from vector.o(.isr_vector)
- RamInit1 from raminit1.o(.text.RamInit1) referenced from startup.o(.text)
- RamInit2 from raminit2.o(.text.RamInit2) referenced from startup.o(.text)
- Reset_Handler from startup.o(.text) referenced from vector.o(.isr_vector)
- SCU_IRQHandler from vector_table_copy.o(.text.SCU_IRQHandler) referenced from vector.o(.isr_vector)
- SPI0_IRQHandler from vector_table_copy.o(.text.SPI0_IRQHandler) referenced from vector.o(.isr_vector)
- SPI1_IRQHandler from vector_table_copy.o(.text.SPI1_IRQHandler) referenced from vector.o(.isr_vector)
- SPI2_IRQHandler from vector_table_copy.o(.text.SPI2_IRQHandler) referenced from vector.o(.isr_vector)
- SVC_Handler from vector_table_copy.o(.text.SVC_Handler) referenced from vector.o(.isr_vector)
- SysTick_Handler from vector_table_copy.o(.text.SysTick_Handler) referenced from vector.o(.isr_vector)
- SystemInit from system.o(.text.SystemInit) referenced from startup.o(.text)
- TRNG_IRQHandler from vector_table_copy.o(.text.TRNG_IRQHandler) referenced from vector.o(.isr_vector)
- UART0_IRQHandler from vector_table_copy.o(.text.UART0_IRQHandler) referenced from vector.o(.isr_vector)
- UART1_IRQHandler from cdduart_lld_uart_irq.o(.mcal_text) referenced from vector.o(.isr_vector)
- UART2_IRQHandler from vector_table_copy.o(.text.UART2_IRQHandler) referenced from vector.o(.isr_vector)
- UsageFault_Handler from vector_table_copy.o(.text.UsageFault_Handler) referenced from vector.o(.isr_vector)
- VectorTableCopy from vector_table_copy.o(.text.VectorTableCopy) referenced from startup.o(.text)
- Wdg_Mld_Isr from vector_table_copy.o(.text.Wdg_Mld_Isr) referenced from vector.o(.isr_vector)
- eTMR0_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
- eTMR0_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
- eTMR0_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
- eTMR0_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
- eTMR0_Fault_IRQHandler from vector_table_copy.o(.text.eTMR0_Fault_IRQHandler) referenced from vector.o(.isr_vector)
- eTMR0_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR0_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
- eTMR1_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
- eTMR1_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
- eTMR1_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
- eTMR1_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
- eTMR1_Fault_IRQHandler from vector_table_copy.o(.text.eTMR1_Fault_IRQHandler) referenced from vector.o(.isr_vector)
- eTMR1_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR1_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
- lpTMR0_IRQHandler from vector_table_copy.o(.text.lpTMR0_IRQHandler) referenced from vector.o(.isr_vector)
- pTMR_Ch0_IRQHandler from vector_table_copy.o(.text.pTMR_Ch0_IRQHandler) referenced from vector.o(.isr_vector)
- pTMR_Ch1_IRQHandler from vector_table_copy.o(.text.pTMR_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
- pTMR_Ch2_IRQHandler from vector_table_copy.o(.text.pTMR_Ch2_IRQHandler) referenced from vector.o(.isr_vector)
- pTMR_Ch3_IRQHandler from vector_table_copy.o(.text.pTMR_Ch3_IRQHandler) referenced from vector.o(.isr_vector)

### Global Symbols

RamInit0 (Thumb, 0 bytes, Stack size unknown bytes, raminit0.o(.text))
[Called By]

- >> Reset_Handler

Reset_Handler (Thumb, 0 bytes, Stack size unknown bytes, startup.o(.text))
[Stack]

- Max Depth = 232 + Unknown Stack Size
- Call Chain = Reset_Handler ⇒ main ⇒ Board_Init ⇒ CddUart_Init ⇒ CddUart_Mld_Init ⇒ UART_Lld_Init ⇒ UART_Lld_SetBaudRate

[Calls]

- >> RamInit0
- >> main

[Address Reference Count : 1]

- vector.o(.isr_vector)

strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
[Called By]

- >> Uart1_PrintString

ACMP0_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.ACMP0_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = ACMP0_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

Adc_ConvCompleteCallback (Thumb, 24 bytes, Stack size 0 bytes, main.o(.text.Adc_ConvCompleteCallback))
[Address Reference Count : 1]

- adc_pbcfg.o(.mcal_const_cfg)

BusFault_Handler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.BusFault_Handler))
[Stack]

- Max Depth = 8
- Call Chain = BusFault_Handler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

CAN0_Error_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.CAN0_Error_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = CAN0_Error_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

CAN0_ORed_0_15_MB_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.CAN0_ORed_0_15_MB_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = CAN0_ORed_0_15_MB_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

CAN0_ORed_16_31_MB_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.CAN0_ORed_16_31_MB_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = CAN0_ORed_16_31_MB_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

CAN0_ORed_32_47_MB_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.CAN0_ORed_32_47_MB_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = CAN0_ORed_32_47_MB_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

CAN0_ORed_48_63_MB_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.CAN0_ORed_48_63_MB_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = CAN0_ORed_48_63_MB_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

CAN0_ORed_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.CAN0_ORed_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = CAN0_ORed_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

CAN0_Wake_Up_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.CAN0_Wake_Up_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = CAN0_Wake_Up_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

CAN1_Error_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.CAN1_Error_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = CAN1_Error_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

CAN1_ORed_0_15_MB_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.CAN1_ORed_0_15_MB_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = CAN1_ORed_0_15_MB_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

CAN1_ORed_16_31_MB_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.CAN1_ORed_16_31_MB_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = CAN1_ORed_16_31_MB_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

CAN1_ORed_32_47_MB_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.CAN1_ORed_32_47_MB_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = CAN1_ORed_32_47_MB_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

CAN1_ORed_48_63_MB_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.CAN1_ORed_48_63_MB_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = CAN1_ORed_48_63_MB_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

CAN1_ORed_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.CAN1_ORed_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = CAN1_ORed_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

CAN1_Wake_Up_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.CAN1_Wake_Up_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = CAN1_Wake_Up_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

DMA0_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.DMA0_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = DMA0_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

DMA1_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.DMA1_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = DMA1_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

DMA2_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.DMA2_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = DMA2_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

DMA3_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.DMA3_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = DMA3_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

DMA_Error_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.DMA_Error_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = DMA_Error_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

DebugMon_Handler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.DebugMon_Handler))
[Stack]

- Max Depth = 8
- Call Chain = DebugMon_Handler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

DefaultISR (Thumb, 4 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DefaultISR))
[Called By]

- >> pTMR_Ch3_IRQHandler
- >> pTMR_Ch2_IRQHandler
- >> pTMR_Ch1_IRQHandler
- >> pTMR_Ch0_IRQHandler
- >> lpTMR0_IRQHandler
- >> eTMR1_Ovf_IRQHandler
- >> eTMR1_Fault_IRQHandler
- >> eTMR1_Ch6_Ch7_IRQHandler
- >> eTMR1_Ch4_Ch5_IRQHandler
- >> eTMR1_Ch2_Ch3_IRQHandler
- >> eTMR1_Ch0_Ch1_IRQHandler
- >> eTMR0_Ovf_IRQHandler
- >> eTMR0_Fault_IRQHandler
- >> eTMR0_Ch6_Ch7_IRQHandler
- >> eTMR0_Ch4_Ch5_IRQHandler
- >> eTMR0_Ch2_Ch3_IRQHandler
- >> eTMR0_Ch0_Ch1_IRQHandler
- >> Wdg_Mld_Isr
- >> UsageFault_Handler
- >> UART2_IRQHandler
- >> UART0_IRQHandler
- >> TRNG_IRQHandler
- >> SysTick_Handler
- >> SVC_Handler
- >> SPI2_IRQHandler
- >> SPI1_IRQHandler
- >> SPI0_IRQHandler
- >> SCU_IRQHandler
- >> PendSV_Handler
- >> PCU_IRQHandler
- >> NMI_Handler
- >> MemManage_Handler
- >> MPWM0_Ch7_Ovf_IRQHandler
- >> MPWM0_Ch7_IRQHandler
- >> MPWM0_Ch6_Ovf_IRQHandler
- >> MPWM0_Ch6_IRQHandler
- >> MPWM0_Ch5_Ovf_IRQHandler
- >> MPWM0_Ch5_IRQHandler
- >> MPWM0_Ch4_Ovf_IRQHandler
- >> MPWM0_Ch4_IRQHandler
- >> MPWM0_Ch3_Ovf_IRQHandler
- >> MPWM0_Ch3_IRQHandler
- >> MPWM0_Ch2_Ovf_IRQHandler
- >> MPWM0_Ch2_IRQHandler
- >> MPWM0_Ch1_Ovf_IRQHandler
- >> MPWM0_Ch1_IRQHandler
- >> MPWM0_Ch0_Ovf_IRQHandler
- >> MPWM0_Ch0_IRQHandler
- >> I2C1_Master_IRQHandler
- >> I2C0_Slave_IRQHandler
- >> I2C0_Master_IRQHandler
- >> HardFault_Handler
- >> HCU_IRQHandler
- >> GPIOE_IRQHandler
- >> GPIOD_IRQHandler
- >> GPIOC_IRQHandler
- >> GPIOB_IRQHandler
- >> GPIOA_IRQHandler
- >> EMU_SB_IRQHandler
- >> EMU_DB_IRQHandler
- >> EFM_IRQHandler
- >> EFM_Error_IRQHandler
- >> EFM_Ecc_IRQHandler
- >> DebugMon_Handler
- >> DMA_Error_IRQHandler
- >> DMA3_IRQHandler
- >> DMA2_IRQHandler
- >> DMA1_IRQHandler
- >> DMA0_IRQHandler
- >> CAN1_Wake_Up_IRQHandler
- >> CAN1_ORed_IRQHandler
- >> CAN1_ORed_48_63_MB_IRQHandler
- >> CAN1_ORed_32_47_MB_IRQHandler
- >> CAN1_ORed_16_31_MB_IRQHandler
- >> CAN1_ORed_0_15_MB_IRQHandler
- >> CAN1_Error_IRQHandler
- >> CAN0_Wake_Up_IRQHandler
- >> CAN0_ORed_IRQHandler
- >> CAN0_ORed_48_63_MB_IRQHandler
- >> CAN0_ORed_32_47_MB_IRQHandler
- >> CAN0_ORed_16_31_MB_IRQHandler
- >> CAN0_ORed_0_15_MB_IRQHandler
- >> CAN0_Error_IRQHandler
- >> BusFault_Handler
- >> ACMP0_IRQHandler

[Address Reference Count : 1]

- vector.o(.isr_vector)

Delay (Thumb, 28 bytes, Stack size 8 bytes, main.o(.text.Delay))
[Stack]

- Max Depth = 8
- Call Chain = Delay

[Called By]

- >> main

Det_ReportError (Thumb, 94 bytes, Stack size 8 bytes, det.o(.text.Det_ReportError))
[Stack]

- Max Depth = 8
- Call Chain = Det_ReportError

[Called By]

- >> CddUart_GetVersionInfo
- >> CddUart_GetStatus
- >> CddUart_AsyncSend
- >> CddUart_AsyncReceive
- >> CddUart_SyncReceive
- >> CddUart_SetCallBack
- >> CddUart_SetBuffer
- >> CddUart_Abort
- >> CddUart_GetBaudrate
- >> CddUart_SetBaudrate
- >> CddUart_Deinit
- >> CddUart_StartAsyncSend
- >> CddUart_StartAsyncReceive
- >> CddUart_StartSyncReceive
- >> CddUart_StartSyncSend
- >> Mcu_GetResetRawValue
- >> Mcu_InitRamSection
- >> Mcu_GetResetReason
- >> Mcu_GetPllStatus
- >> Adc_StopGroupConversion
- >> Adc_GetStreamLastPointer
- >> Adc_DisableGroupNotification
- >> Adc_DeInit
- >> Adc_InitAndGroupValidErrCheck
- >> Adc_Init
- >> CddUart_Init
- >> Mcu_SetMode
- >> Adc_StartGroupConversion
- >> Adc_EnableGroupNotification
- >> Adc_SetupResultBuffer
- >> Mcu_InitClock
- >> Mcu_Init
- >> CddUart_SyncSend

Det_ReportRuntimeError (Thumb, 94 bytes, Stack size 8 bytes, det.o(.text.Det_ReportRuntimeError))
[Stack]

- Max Depth = 8
- Call Chain = Det_ReportRuntimeError

[Called By]

- >> Adc_ReadGroup
- >> Adc_DeInit
- >> Adc_StartGroupConversion
- >> Adc_SetupResultBuffer

EFM_Ecc_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.EFM_Ecc_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = EFM_Ecc_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

EFM_Error_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.EFM_Error_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = EFM_Error_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

EFM_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.EFM_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = EFM_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

EMU_DB_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.EMU_DB_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = EMU_DB_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

EMU_SB_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.EMU_SB_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = EMU_SB_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

GPIOA_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.GPIOA_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = GPIOA_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

GPIOB_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.GPIOB_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = GPIOB_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

GPIOC_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.GPIOC_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = GPIOC_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

GPIOD_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.GPIOD_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = GPIOD_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

GPIOE_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.GPIOE_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = GPIOE_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

HCU_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.HCU_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = HCU_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

HardFault_Handler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.HardFault_Handler))
[Stack]

- Max Depth = 8
- Call Chain = HardFault_Handler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

I2C0_Master_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.I2C0_Master_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = I2C0_Master_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

I2C0_Slave_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.I2C0_Slave_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = I2C0_Slave_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

I2C1_Master_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.I2C1_Master_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = I2C1_Master_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

MPWM0_Ch0_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.MPWM0_Ch0_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = MPWM0_Ch0_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

MPWM0_Ch0_Ovf_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.MPWM0_Ch0_Ovf_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = MPWM0_Ch0_Ovf_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

MPWM0_Ch1_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.MPWM0_Ch1_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = MPWM0_Ch1_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

MPWM0_Ch1_Ovf_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.MPWM0_Ch1_Ovf_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = MPWM0_Ch1_Ovf_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

MPWM0_Ch2_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.MPWM0_Ch2_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = MPWM0_Ch2_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

MPWM0_Ch2_Ovf_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.MPWM0_Ch2_Ovf_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = MPWM0_Ch2_Ovf_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

MPWM0_Ch3_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.MPWM0_Ch3_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = MPWM0_Ch3_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

MPWM0_Ch3_Ovf_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.MPWM0_Ch3_Ovf_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = MPWM0_Ch3_Ovf_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

MPWM0_Ch4_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.MPWM0_Ch4_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = MPWM0_Ch4_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

MPWM0_Ch4_Ovf_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.MPWM0_Ch4_Ovf_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = MPWM0_Ch4_Ovf_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

MPWM0_Ch5_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.MPWM0_Ch5_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = MPWM0_Ch5_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

MPWM0_Ch5_Ovf_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.MPWM0_Ch5_Ovf_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = MPWM0_Ch5_Ovf_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

MPWM0_Ch6_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.MPWM0_Ch6_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = MPWM0_Ch6_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

MPWM0_Ch6_Ovf_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.MPWM0_Ch6_Ovf_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = MPWM0_Ch6_Ovf_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

MPWM0_Ch7_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.MPWM0_Ch7_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = MPWM0_Ch7_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

MPWM0_Ch7_Ovf_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.MPWM0_Ch7_Ovf_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = MPWM0_Ch7_Ovf_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

MemManage_Handler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.MemManage_Handler))
[Stack]

- Max Depth = 8
- Call Chain = MemManage_Handler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

NMI_Handler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.NMI_Handler))
[Stack]

- Max Depth = 8
- Call Chain = NMI_Handler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

PCU_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.PCU_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = PCU_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

PendSV_Handler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.PendSV_Handler))
[Stack]

- Max Depth = 8
- Call Chain = PendSV_Handler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

RamInit1 (Thumb, 504 bytes, Stack size 48 bytes, raminit1.o(.text.RamInit1))
[Stack]

- Max Depth = 52
- Call Chain = RamInit1 ⇒ IsPOR

[Calls]

- >> IsPOR

[Address Reference Count : 1]

- startup.o(.text)

RamInit2 (Thumb, 2 bytes, Stack size 0 bytes, raminit2.o(.text.RamInit2))
[Address Reference Count : 1]

- startup.o(.text)

SCU_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.SCU_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = SCU_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

SPI0_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.SPI0_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = SPI0_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

SPI1_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.SPI1_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = SPI1_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

SPI2_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.SPI2_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = SPI2_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

SVC_Handler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.SVC_Handler))
[Stack]

- Max Depth = 8
- Call Chain = SVC_Handler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

SysTick_Handler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.SysTick_Handler))
[Stack]

- Max Depth = 8
- Call Chain = SysTick_Handler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

SystemInit (Thumb, 66 bytes, Stack size 8 bytes, system.o(.text.SystemInit))
[Stack]

- Max Depth = 72
- Call Chain = SystemInit ⇒ Mpu_Lld_M33_Init ⇒ ARM_MPU_SetRegion ⇒ ARM_MPU_SetRegionEx

[Calls]

- >> Mpu_Lld_M33_Init

[Address Reference Count : 1]

- startup.o(.text)

TRNG_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.TRNG_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = TRNG_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

UART0_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.UART0_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = UART0_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

UART2_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.UART2_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = UART2_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

Uart1_PrintString (Thumb, 46 bytes, Stack size 16 bytes, main.o(.text.Uart1_PrintString))
[Stack]

- Max Depth = 56
- Call Chain = Uart1_PrintString ⇒ CddUart_SyncSend ⇒ Det_ReportError

[Calls]

- >> strlen
- >> CddUart_SyncSend

[Called By]

- >> main

UsageFault_Handler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.UsageFault_Handler))
[Stack]

- Max Depth = 8
- Call Chain = UsageFault_Handler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

VectorTableCopy (Thumb, 116 bytes, Stack size 32 bytes, vector_table_copy.o(.text.VectorTableCopy))
[Stack]

- Max Depth = 32
- Call Chain = VectorTableCopy

[Calls]

- >> Sys_GetCoreID

[Address Reference Count : 1]

- startup.o(.text)

Wdg_Mld_Isr (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.Wdg_Mld_Isr))
[Stack]

- Max Depth = 8
- Call Chain = Wdg_Mld_Isr

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

eTMR0_Ch0_Ch1_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.eTMR0_Ch0_Ch1_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = eTMR0_Ch0_Ch1_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

eTMR0_Ch2_Ch3_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.eTMR0_Ch2_Ch3_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = eTMR0_Ch2_Ch3_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

eTMR0_Ch4_Ch5_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.eTMR0_Ch4_Ch5_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = eTMR0_Ch4_Ch5_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

eTMR0_Ch6_Ch7_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.eTMR0_Ch6_Ch7_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = eTMR0_Ch6_Ch7_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

eTMR0_Fault_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.eTMR0_Fault_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = eTMR0_Fault_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

eTMR0_Ovf_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.eTMR0_Ovf_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = eTMR0_Ovf_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

eTMR1_Ch0_Ch1_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.eTMR1_Ch0_Ch1_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = eTMR1_Ch0_Ch1_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

eTMR1_Ch2_Ch3_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.eTMR1_Ch2_Ch3_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = eTMR1_Ch2_Ch3_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

eTMR1_Ch4_Ch5_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.eTMR1_Ch4_Ch5_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = eTMR1_Ch4_Ch5_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

eTMR1_Ch6_Ch7_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.eTMR1_Ch6_Ch7_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = eTMR1_Ch6_Ch7_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

eTMR1_Fault_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.eTMR1_Fault_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = eTMR1_Fault_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

eTMR1_Ovf_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.eTMR1_Ovf_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = eTMR1_Ovf_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

lpTMR0_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.lpTMR0_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = lpTMR0_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

main (Thumb, 626 bytes, Stack size 48 bytes, main.o(.text.main))
[Stack]

- Max Depth = 232
- Call Chain = main ⇒ Board_Init ⇒ CddUart_Init ⇒ CddUart_Mld_Init ⇒ UART_Lld_Init ⇒ UART_Lld_SetBaudRate

[Calls]

- >> Mcu_SetMode
- >> Adc_StartGroupConversion
- >> Adc_EnableGroupNotification
- >> Adc_SetupResultBuffer
- >> Mcu_InitClock
- >> Mcu_Init
- >> Delay
- >> Uart1_PrintString
- >> Board_Init

[Called By]

- >> Reset_Handler

pTMR_Ch0_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.pTMR_Ch0_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = pTMR_Ch0_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

pTMR_Ch1_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.pTMR_Ch1_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = pTMR_Ch1_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

pTMR_Ch2_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.pTMR_Ch2_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = pTMR_Ch2_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

pTMR_Ch3_IRQHandler (Thumb, 8 bytes, Stack size 8 bytes, vector_table_copy.o(.text.pTMR_Ch3_IRQHandler))
[Stack]

- Max Depth = 8
- Call Chain = pTMR_Ch3_IRQHandler

[Calls]

- >> DefaultISR

[Address Reference Count : 1]

- vector.o(.isr_vector)

Adc_DeInit (Thumb, 452 bytes, Stack size 16 bytes, adc.o(.mcal_text), UNUSED)
[Calls]

- >> Adc_Lld_DeinitHwUnit
- >> Det_ReportRuntimeError
- >> Det_ReportError

Adc_DisableGroupNotification (Thumb, 206 bytes, Stack size 24 bytes, adc.o(.mcal_text), UNUSED)
[Calls]

- >> Adc_Lld_GroupIndexCheck
- >> Det_ReportError
- >> Adc_ValidGroupCheck

Adc_EnableGroupNotification (Thumb, 204 bytes, Stack size 24 bytes, adc.o(.mcal_text))
[Stack]

- Max Depth = 32
- Call Chain = Adc_EnableGroupNotification ⇒ Adc_Lld_GroupIndexCheck

[Calls]

- >> Adc_Lld_GroupIndexCheck
- >> Det_ReportError
- >> Adc_ValidGroupCheck

[Called By]

- >> main

Adc_GetGroupStatus (Thumb, 136 bytes, Stack size 16 bytes, adc.o(.mcal_text), UNUSED)
[Calls]

- >> Adc_Lld_GroupIndexCheck
- >> Adc_UpdataStatusInReadApi
- >> Adc_InitAndGroupValidErrCheck

Adc_GetStreamLastPointer (Thumb, 282 bytes, Stack size 32 bytes, adc.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_01
- >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_01
- >> Adc_Lld_GroupIndexCheck
- >> Det_ReportError
- >> Adc_HandleHwReloadAfterRead
- >> Adc_SwStateAndRdRstInGetStream
- >> Adc_UpdataStatusInReadApi
- >> Adc_InitAndGroupValidErrCheck

Adc_Init (Thumb, 520 bytes, Stack size 24 bytes, adc.o(.mcal_text))
[Stack]

- Max Depth = 68
- Call Chain = Adc_Init ⇒ Adc_Lld_HwUnitEnable ⇒ Adc_Lld_Enable ⇒ Adc_Lld_GetADEN

[Calls]

- >> Adc_Lld_HwUnitEnable
- >> Adc_Lld_InitTempSensor
- >> Adc_Lld_DisableIntcandHwTrigger
- >> Adc_Lld_HwClockInit
- >> Adc_Lld_StopConversion
- >> Det_ReportError

[Called By]

- >> Board_Init

Adc_ReadGroup (Thumb, 272 bytes, Stack size 24 bytes, adc.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_02
- >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_02
- >> Adc_Lld_GroupIndexCheck
- >> Det_ReportRuntimeError
- >> Adc_SwStateAndRdRstInReadApi
- >> Adc_HandleHwReloadAfterRead
- >> Adc_UpdataStatusInReadApi
- >> Adc_InitAndGroupValidErrCheck

Adc_SetupResultBuffer (Thumb, 250 bytes, Stack size 24 bytes, adc.o(.mcal_text))
[Stack]

- Max Depth = 32
- Call Chain = Adc_SetupResultBuffer ⇒ Adc_Lld_GroupIndexCheck

[Calls]

- >> Adc_Lld_GroupIndexCheck
- >> Det_ReportRuntimeError
- >> Det_ReportError
- >> Adc_ValidGroupCheck

[Called By]

- >> main

Adc_StartGroupConversion (Thumb, 562 bytes, Stack size 16 bytes, adc.o(.mcal_text))
[Stack]

- Max Depth = 76
- Call Chain = Adc_StartGroupConversion ⇒ Adc_Lld_LoadGroupToHwUnit ⇒ Adc_Lld_StopConversion ⇒ Adc_Lld_GetStopStatus

[Calls]

- >> SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_03
- >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_03
- >> Adc_Lld_StartConversion
- >> Adc_Lld_LoadGroupToHwUnit
- >> Adc_Lld_GroupIndexCheck
- >> Det_ReportRuntimeError
- >> Det_ReportError
- >> Adc_InitAndGroupValidErrCheck

[Called By]

- >> main

Adc_StopGroupConversion (Thumb, 690 bytes, Stack size 24 bytes, adc.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_04
- >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_04
- >> Adc_Lld_StopConversion
- >> Adc_Lld_StartConversion
- >> Adc_Lld_GroupIndexCheck
- >> Det_ReportError
- >> Adc_LimitQueueIndex
- >> Adc_GroupsInQueueUpdate
- >> Adc_CheckGroupQueueIndex
- >> Adc_InitAndGroupValidErrCheck

ADC0_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, adc_irq.o(.mcal_text))
[Stack]

- Max Depth = 108
- Call Chain = ADC0_IRQHandler ⇒ Adc_Lld_IrqProcess ⇒ Adc_Lld_RestartAdcHardWare ⇒ Adc_Lld_LoadGroupToHwUnit ⇒ Adc_Lld_StopConversion ⇒ Adc_Lld_GetStopStatus

[Calls]

- >> Adc_Lld_IrqProcess

[Address Reference Count : 1]

- vector.o(.isr_vector)

Adc_Lld_GetRunningGroupIndex (Thumb, 72 bytes, Stack size 16 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 24
- Call Chain = Adc_Lld_GetRunningGroupIndex ⇒ Adc_Lld_GroupIndexCheck

[Calls]

- >> Adc_Lld_GroupIndexCheck

[Called By]

- >> Adc_Lld_IrqProcess
- >> Adc_HandleHwRunAgainInBusy
- >> Adc_UpdataStatusInReadApi

Adc_Lld_GroupIndexCheck (Thumb, 146 bytes, Stack size 8 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 8
- Call Chain = Adc_Lld_GroupIndexCheck

[Called By]

- >> Adc_Lld_RestartAdcHardWare
- >> Adc_StopGroupConversion
- >> Adc_ReadGroup
- >> Adc_GetStreamLastPointer
- >> Adc_Lld_GetRunningGroupIndex
- >> Adc_GetGroupStatus
- >> Adc_DisableGroupNotification
- >> Adc_GroupsInQueueUpdate
- >> Adc_HwHandleInIdle
- >> Adc_HandleHwReloadAfterRead
- >> Adc_UpdataStatusInReadApi
- >> Adc_StartGroupConversion
- >> Adc_EnableGroupNotification
- >> Adc_SetupResultBuffer

Adc_Lld_InitTempSensor (Thumb, 30 bytes, Stack size 16 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 28
- Call Chain = Adc_Lld_InitTempSensor ⇒ Adc_Lld_SetTSEN

[Calls]

- >> Adc_Lld_SetTSEN

[Called By]

- >> Adc_Init

Adc_Lld_HwUnitEnable (Thumb, 28 bytes, Stack size 16 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 44
- Call Chain = Adc_Lld_HwUnitEnable ⇒ Adc_Lld_Enable ⇒ Adc_Lld_GetADEN

[Calls]

- >> Adc_Lld_Enable

[Called By]

- >> Adc_Init

Adc_Lld_HwClockInit (Thumb, 48 bytes, Stack size 16 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 28
- Call Chain = Adc_Lld_HwClockInit ⇒ Adc_Lld_SetStartUpTime

[Calls]

- >> Adc_Lld_SetStartUpTime
- >> Adc_Lld_SetPrescaler

[Called By]

- >> Adc_Init

Adc_Lld_StopConversion (Thumb, 108 bytes, Stack size 24 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 28
- Call Chain = Adc_Lld_StopConversion ⇒ Adc_Lld_GetStopStatus

[Calls]

- >> Adc_Lld_GetStopStatus
- >> Adc_Lld_SetStopConversion

[Called By]

- >> Adc_Lld_IrqProcess
- >> Adc_StopGroupConversion
- >> Adc_Lld_LoadGroupToHwUnit
- >> Adc_Lld_DeinitHwUnit
- >> Adc_GroupsInQueueUpdate
- >> Adc_HwHandleInIdle
- >> Adc_HandleHwReloadAfterRead
- >> Adc_UpdataStatusInReadApi
- >> Adc_Init

Adc_Lld_StartConversion (Thumb, 68 bytes, Stack size 16 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 52
- Call Chain = Adc_Lld_StartConversion ⇒ Adc_Lld_ClearFIFOInvalidData ⇒ Adc_Lld_GetFIFOEmptyFlag

[Calls]

- >> Adc_Lld_SetStartConversion
- >> Adc_Lld_ClearFIFOInvalidData
- >> Adc_Lld_GetStartConversion

[Called By]

- >> Adc_Lld_RestartAdcHardWare
- >> Adc_StopGroupConversion
- >> Adc_GroupsInQueueUpdate
- >> Adc_HandleHwReloadAfterRead
- >> Adc_UpdataStatusInReadApi
- >> Adc_StartGroupConversion

Adc_Lld_DisableIntcandHwTrigger (Thumb, 50 bytes, Stack size 16 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 28
- Call Chain = Adc_Lld_DisableIntcandHwTrigger ⇒ Adc_Lld_SetTriggerMode

[Calls]

- >> Adc_Lld_SetTriggerMode
- >> Adc_Lld_DisableAllInt

[Called By]

- >> Adc_Init

Adc_Lld_DeinitHwUnit (Thumb, 64 bytes, Stack size 16 bytes, adc_lld.o(.mcal_text), UNUSED)
[Calls]

- >> Adc_Lld_ResetRegister
- >> Adc_Lld_Disable
- >> Adc_Lld_ClearFIFOInvalidData
- >> Adc_Lld_StopConversion

[Called By]

- >> Adc_DeInit

Adc_Lld_ReadSeqConvEndIntFlag (Thumb, 46 bytes, Stack size 16 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 28
- Call Chain = Adc_Lld_ReadSeqConvEndIntFlag ⇒ Adc_Lld_GetEOSEQIntFlag

[Calls]

- >> Adc_Lld_GetEOSEQIntFlag

[Called By]

- >> Adc_Lld_IrqProcess
- >> Adc_UpdataStatusInReadApi

Adc_Lld_ClearSeqConvEndIntFlag (Thumb, 32 bytes, Stack size 16 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 20
- Call Chain = Adc_Lld_ClearSeqConvEndIntFlag ⇒ Adc_Lld_ClearEOSEQIntFlag

[Calls]

- >> Adc_Lld_ClearEOSEQIntFlag

[Called By]

- >> Adc_Lld_IrqProcess
- >> Adc_GroupsInQueueUpdate
- >> Adc_HwHandleInIdle
- >> Adc_UpdateStatusReadGroupNoInt
- >> Adc_UpdataStatusInReadApi

Adc_Lld_ReadConversionResults (Thumb, 214 bytes, Stack size 24 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 36
- Call Chain = Adc_Lld_ReadConversionResults ⇒ Adc_Lld_LimitCheck

[Calls]

- >> Adc_Lld_LimitCheck
- >> Adc_Lld_ReadFIFO

[Called By]

- >> Adc_Lld_IrqProcess
- >> Adc_UpdateStatusReadGroupNoInt

Adc_Lld_LoadGroupToHwUnit (Thumb, 564 bytes, Stack size 32 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 60
- Call Chain = Adc_Lld_LoadGroupToHwUnit ⇒ Adc_Lld_StopConversion ⇒ Adc_Lld_GetStopStatus

[Calls]

- >> Adc_Lld_SetRegiterINTE
- >> Adc_Lld_ClearRegsiterSTS
- >> ADC_Lld_SetSequeceChannel
- >> Adc_Lld_SetRegisterCFG0
- >> Adc_Lld_SetSampleTime
- >> Adc_Lld_StopConversion

[Called By]

- >> Adc_Lld_RestartAdcHardWare
- >> Adc_GroupsInQueueUpdate
- >> Adc_HwHandleInIdle
- >> Adc_HandleHwRunAgainInBusy
- >> Adc_HandleHwReloadAfterRead
- >> Adc_UpdataStatusInReadApi
- >> Adc_StartGroupConversion

Adc_Lld_GroupStatusUpdata (Thumb, 244 bytes, Stack size 8 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 8
- Call Chain = Adc_Lld_GroupStatusUpdata

[Called By]

- >> Adc_Lld_IrqProcess
- >> Adc_UpdateStatusReadGroupNoInt

Adc_Lld_QueueDataUpdata (Thumb, 290 bytes, Stack size 16 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 28
- Call Chain = Adc_Lld_QueueDataUpdata ⇒ SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_05 ⇒ SchM_Adc_ReadMsr

[Calls]

- >> SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_05
- >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_05

[Called By]

- >> Adc_Lld_IrqProcess
- >> Adc_UpdataStatusInReadApi

Adc_Lld_IrqProcess (Thumb, 584 bytes, Stack size 24 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 100
- Call Chain = Adc_Lld_IrqProcess ⇒ Adc_Lld_RestartAdcHardWare ⇒ Adc_Lld_LoadGroupToHwUnit ⇒ Adc_Lld_StopConversion ⇒ Adc_Lld_GetStopStatus

[Calls]

- >> Adc_Lld_ClearAllIntcFlag
- >> Adc_Lld_RestartAdcHardWare
- >> Adc_Lld_GroupStatusUpdata
- >> Adc_Lld_ReadConversionResults
- >> Adc_Lld_ClearSeqConvEndIntFlag
- >> Adc_Lld_StopConversion
- >> Adc_Lld_QueueDataUpdata
- >> Adc_Lld_ReadSeqConvEndIntFlag
- >> Adc_Lld_GetRunningGroupIndex

[Called By]

- >> ADC0_IRQHandler

SchM_Adc_ReadMsr (Thumb, 14 bytes, Stack size 4 bytes, schm_adc.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = SchM_Adc_ReadMsr

[Called By]

- >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_00
- >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_05
- >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_04
- >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_03
- >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_02
- >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_06
- >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_01

SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_00 (Thumb, 62 bytes, Stack size 8 bytes, schm_adc.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Adc_ReadMsr

SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_00 (Thumb, 50 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text), UNUSED)

SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_01 (Thumb, 62 bytes, Stack size 8 bytes, schm_adc.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Adc_ReadMsr

[Called By]

- >> Adc_GetStreamLastPointer

SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_01 (Thumb, 50 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text), UNUSED)
[Called By]

- >> Adc_GetStreamLastPointer

SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_02 (Thumb, 62 bytes, Stack size 8 bytes, schm_adc.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Adc_ReadMsr

[Called By]

- >> Adc_ReadGroup

SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_02 (Thumb, 50 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text), UNUSED)
[Called By]

- >> Adc_ReadGroup

SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_03 (Thumb, 62 bytes, Stack size 8 bytes, schm_adc.o(.mcal_text))
[Stack]

- Max Depth = 12
- Call Chain = SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_03 ⇒ SchM_Adc_ReadMsr

[Calls]

- >> SchM_Adc_ReadMsr

[Called By]

- >> Adc_StartGroupConversion

SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_03 (Thumb, 50 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text))
[Called By]

- >> Adc_StartGroupConversion

SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_04 (Thumb, 62 bytes, Stack size 8 bytes, schm_adc.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Adc_ReadMsr

[Called By]

- >> Adc_StopGroupConversion
- >> Adc_GroupsInQueueUpdate

SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_04 (Thumb, 50 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text), UNUSED)
[Called By]

- >> Adc_StopGroupConversion
- >> Adc_GroupsInQueueUpdate

SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_05 (Thumb, 62 bytes, Stack size 8 bytes, schm_adc.o(.mcal_text))
[Stack]

- Max Depth = 12
- Call Chain = SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_05 ⇒ SchM_Adc_ReadMsr

[Calls]

- >> SchM_Adc_ReadMsr

[Called By]

- >> Adc_Lld_QueueDataUpdata

SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_05 (Thumb, 50 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text))
[Called By]

- >> Adc_Lld_QueueDataUpdata

SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_06 (Thumb, 62 bytes, Stack size 8 bytes, schm_adc.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Adc_ReadMsr

[Called By]

- >> Adc_HandleHwReloadAfterRead

SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_06 (Thumb, 50 bytes, Stack size 0 bytes, schm_adc.o(.mcal_text), UNUSED)
[Called By]

- >> Adc_HandleHwReloadAfterRead

Port_Init (Thumb, 28 bytes, Stack size 16 bytes, port.o(.mcal_text))
[Stack]

- Max Depth = 68
- Call Chain = Port_Init ⇒ Port_Lld_Init ⇒ Port_Lld_InitMode ⇒ Port_Lld_InitGPIOMode

[Calls]

- >> Port_Lld_Init

[Called By]

- >> Board_Init

Port_RefreshPortDirection (Thumb, 18 bytes, Stack size 8 bytes, port.o(.mcal_text), UNUSED)
[Calls]

- >> Port_Lld_RefreshPortDirection

Port_SetPinDirection (Thumb, 48 bytes, Stack size 16 bytes, port.o(.mcal_text), UNUSED)
[Calls]

- >> Port_Lld_SetPinDirection

Port_SetPinMode (Thumb, 48 bytes, Stack size 16 bytes, port.o(.mcal_text), UNUSED)
[Calls]

- >> Port_Lld_SetPinMode

Port_Lld_Init (Thumb, 192 bytes, Stack size 24 bytes, port_lld.o(.mcal_text))
[Stack]

- Max Depth = 52
- Call Chain = Port_Lld_Init ⇒ Port_Lld_InitMode ⇒ Port_Lld_InitGPIOMode

[Calls]

- >> Port_Lld_InitMode
- >> Port_Lld_InitPull

[Called By]

- >> Port_Init

Port_Lld_RefreshPortDirection (Thumb, 280 bytes, Stack size 24 bytes, port_lld.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_Port_PORT_EXCLUSIVE_AREA_02
- >> SchM_Enter_Port_PORT_EXCLUSIVE_AREA_02

[Called By]

- >> Port_RefreshPortDirection

Port_Lld_IsPinDireChangeable (Thumb, 146 bytes, Stack size 20 bytes, port_lld.o(.mcal_text), UNUSED)

Port_Lld_IsPinModeChangeable (Thumb, 146 bytes, Stack size 20 bytes, port_lld.o(.mcal_text), UNUSED)

Port_Lld_SetPinDirection (Thumb, 182 bytes, Stack size 16 bytes, port_lld.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_Port_PORT_EXCLUSIVE_AREA_00
- >> SchM_Enter_Port_PORT_EXCLUSIVE_AREA_00

[Called By]

- >> Port_SetPinDirection

Port_Lld_SetPinMode (Thumb, 76 bytes, Stack size 16 bytes, port_lld.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_Port_PORT_EXCLUSIVE_AREA_01
- >> SchM_Enter_Port_PORT_EXCLUSIVE_AREA_01

[Called By]

- >> Port_SetPinMode

SchM_Port_ReadMsr (Thumb, 14 bytes, Stack size 4 bytes, schm_port.o(.mcal_text), UNUSED)
[Called By]

- >> SchM_Enter_Port_PORT_EXCLUSIVE_AREA_01
- >> SchM_Enter_Port_PORT_EXCLUSIVE_AREA_00
- >> SchM_Enter_Port_PORT_EXCLUSIVE_AREA_02

SchM_Enter_Port_PORT_EXCLUSIVE_AREA_00 (Thumb, 62 bytes, Stack size 8 bytes, schm_port.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Port_ReadMsr

[Called By]

- >> Port_Lld_SetPinDirection

SchM_Exit_Port_PORT_EXCLUSIVE_AREA_00 (Thumb, 50 bytes, Stack size 0 bytes, schm_port.o(.mcal_text), UNUSED)
[Called By]

- >> Port_Lld_SetPinDirection

SchM_Enter_Port_PORT_EXCLUSIVE_AREA_01 (Thumb, 62 bytes, Stack size 8 bytes, schm_port.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Port_ReadMsr

[Called By]

- >> Port_Lld_SetPinMode

SchM_Exit_Port_PORT_EXCLUSIVE_AREA_01 (Thumb, 50 bytes, Stack size 0 bytes, schm_port.o(.mcal_text), UNUSED)
[Called By]

- >> Port_Lld_SetPinMode

SchM_Enter_Port_PORT_EXCLUSIVE_AREA_02 (Thumb, 62 bytes, Stack size 8 bytes, schm_port.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Port_ReadMsr

[Called By]

- >> Port_Lld_RefreshPortDirection

SchM_Exit_Port_PORT_EXCLUSIVE_AREA_02 (Thumb, 50 bytes, Stack size 0 bytes, schm_port.o(.mcal_text), UNUSED)
[Called By]

- >> Port_Lld_RefreshPortDirection

IntCtrl_Lld_Init (Thumb, 138 bytes, Stack size 16 bytes, intctrl_lld.o(.mcal_text), UNUSED)
[Calls]

- >> IntCtrl_Lld_DisableIrq
- >> IntCtrl_Lld_EnableIrq
- >> IntCtrl_Lld_SetPriority
- >> IntCtrl_Lld_ClearPending

IntCtrl_Lld_ClearPending (Thumb, 20 bytes, Stack size 16 bytes, intctrl_lld.o(.mcal_text), UNUSED)
[Calls]

- >> IntCtrl_Lld_ClrPendingPrivileged

[Called By]

- >> IntCtrl_Lld_Init

IntCtrl_Lld_SetPriority (Thumb, 28 bytes, Stack size 16 bytes, intctrl_lld.o(.mcal_text))
[Stack]

- Max Depth = 40
- Call Chain = IntCtrl_Lld_SetPriority ⇒ IntCtrl_Lld_SetPriPrivileged ⇒ __NVIC_SetPriority

[Calls]

- >> IntCtrl_Lld_SetPriPrivileged

[Called By]

- >> Platform_Mld_SetIrqPriority
- >> Platform_Mld_InitIntCtrl
- >> IntCtrl_Lld_Init

IntCtrl_Lld_EnableIrq (Thumb, 20 bytes, Stack size 16 bytes, intctrl_lld.o(.mcal_text))
[Stack]

- Max Depth = 36
- Call Chain = IntCtrl_Lld_EnableIrq ⇒ IntCtrl_Lld_EnableIrqPrivileged ⇒ __NVIC_EnableIRQ

[Calls]

- >> IntCtrl_Lld_EnableIrqPrivileged

[Called By]

- >> Platform_Mld_SetIrq
- >> Platform_Mld_InitIntCtrl
- >> IntCtrl_Lld_Init

IntCtrl_Lld_DisableIrq (Thumb, 20 bytes, Stack size 16 bytes, intctrl_lld.o(.mcal_text))
[Stack]

- Max Depth = 36
- Call Chain = IntCtrl_Lld_DisableIrq ⇒ IntCtrl_Lld_DisableIrqPrivileged ⇒ __NVIC_DisableIRQ

[Calls]

- >> IntCtrl_Lld_DisableIrqPrivileged

[Called By]

- >> Platform_Mld_SetIrq
- >> Platform_Mld_InitIntCtrl
- >> IntCtrl_Lld_Init

IntCtrl_Lld_InstallHandler (Thumb, 28 bytes, Stack size 24 bytes, intctrl_lld.o(.mcal_text), UNUSED)
[Calls]

- >> IntCtrl_Lld_InstIsrPrivileged

[Called By]

- >> Platform_Mld_InstallIrqHandler

IntCtrl_Lld_GetPriority (Thumb, 20 bytes, Stack size 16 bytes, intctrl_lld.o(.mcal_text), UNUSED)
[Calls]

- >> IntCtrl_Lld_GetPriPrivileged

[Called By]

- >> Platform_Mld_GetIrqPriority

Sys_GetCoreID (Thumb, 4 bytes, Stack size 0 bytes, osif.o(.mcal_text))
[Called By]

- >> VectorTableCopy

Platform_Mld_Init (Thumb, 62 bytes, Stack size 16 bytes, platform_mld.o(.mcal_text))
[Stack]

- Max Depth = 72
- Call Chain = Platform_Mld_Init ⇒ Platform_Mld_InitIntCtrl ⇒ IntCtrl_Lld_SetPriority ⇒ IntCtrl_Lld_SetPriPrivileged ⇒ __NVIC_SetPriority

[Calls]

- >> Platform_Mld_InitIntCtrl

[Called By]

- >> Platform_Init

Platform_Init (Thumb, 38 bytes, Stack size 16 bytes, platform.o(.mcal_text))
[Stack]

- Max Depth = 88
- Call Chain = Platform_Init ⇒ Platform_Mld_Init ⇒ Platform_Mld_InitIntCtrl ⇒ IntCtrl_Lld_SetPriority ⇒ IntCtrl_Lld_SetPriPrivileged ⇒ __NVIC_SetPriority

[Calls]

- >> Platform_Mld_Init

[Called By]

- >> Board_Init

Platform_SetIrq (Thumb, 38 bytes, Stack size 16 bytes, platform.o(.mcal_text), UNUSED)
[Calls]

- >> Platform_Mld_SetIrq

Platform_SetIrqPriority (Thumb, 38 bytes, Stack size 16 bytes, platform.o(.mcal_text), UNUSED)
[Calls]

- >> Platform_Mld_SetIrqPriority

Platform_GetIrqPriority (Thumb, 36 bytes, Stack size 24 bytes, platform.o(.mcal_text), UNUSED)
[Calls]

- >> Platform_Mld_GetIrqPriority

Platform_InstallIrqHandler (Thumb, 38 bytes, Stack size 24 bytes, platform.o(.mcal_text), UNUSED)
[Calls]

- >> Platform_Mld_InstallIrqHandler

Mpu_Lld_M33_Init (Thumb, 248 bytes, Stack size 24 bytes, mpu_lld_m33.o(.mcal_text))
[Stack]

- Max Depth = 64
- Call Chain = Mpu_Lld_M33_Init ⇒ ARM_MPU_SetRegion ⇒ ARM_MPU_SetRegionEx

[Calls]

- >> ARM_MPU_Enable
- >> ARM_MPU_SetRegion
- >> ARM_MPU_SetMemAttr
- >> ARM_MPU_ClrRegion
- >> ARM_MPU_Disable

[Called By]

- >> SystemInit

Mcu_GetPllStatus (Thumb, 46 bytes, Stack size 16 bytes, mcu.o(.mcal_text), UNUSED)
[Calls]

- >> Det_ReportError

Mcu_GetResetReason (Thumb, 56 bytes, Stack size 16 bytes, mcu.o(.mcal_text), UNUSED)
[Calls]

- >> Mcu_Lld_GetResetValue
- >> Det_ReportError

Mcu_Init (Thumb, 134 bytes, Stack size 24 bytes, mcu.o(.mcal_text))
[Stack]

- Max Depth = 32
- Call Chain = Mcu_Init ⇒ Mcu_Lld_SetPcu

[Calls]

- >> Mcu_Lld_SetPcu
- >> Mcu_Lld_SetRcu
- >> Det_ReportError

[Called By]

- >> main

Mcu_InitClock (Thumb, 160 bytes, Stack size 16 bytes, mcu.o(.mcal_text))
[Stack]

- Max Depth = 84
- Call Chain = Mcu_InitClock ⇒ Mcu_Lld_InitClock ⇒ Mcu_Lld_SetClockSource ⇒ Mcu_Lld_SwitchSystemClock ⇒ Mcu_Lld_SetSystemClockSource

[Calls]

- >> Mcu_Lld_InitClock
- >> Det_ReportError

[Called By]

- >> main

Mcu_InitRamSection (Thumb, 148 bytes, Stack size 32 bytes, mcu.o(.mcal_text), UNUSED)
[Calls]

- >> Mcu_Lld_SetRamSection
- >> Det_ReportError

Mcu_SetMode (Thumb, 106 bytes, Stack size 16 bytes, mcu.o(.mcal_text))
[Stack]

- Max Depth = 40
- Call Chain = Mcu_SetMode ⇒ Mcu_Lld_SetMode

[Calls]

- >> SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00
- >> Mcu_Lld_SetMode
- >> SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00
- >> Det_ReportError

[Called By]

- >> main

Mcu_GetResetRawValue (Thumb, 52 bytes, Stack size 16 bytes, mcu.o(.mcal_text), UNUSED)
[Calls]

- >> Mcu_Lld_GetResetRawValue
- >> Det_ReportError

Mcu_180_GetCoreClockFrequency (Thumb, 80 bytes, Stack size 16 bytes, mcu.o(.mcal_text), UNUSED)
[Calls]

- >> Mcu_Lld_GetCoreClockFrequency

Mcu_Lld_SystemReset (Thumb, 52 bytes, Stack size 4 bytes, mcu_lld.o(.mcal_text), UNUSED)

Mcu_Lld_SetRcu (Thumb, 60 bytes, Stack size 4 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = Mcu_Lld_SetRcu

[Called By]

- >> Mcu_Init

Mcu_Lld_SetRamSection (Thumb, 64 bytes, Stack size 12 bytes, mcu_lld.o(.mcal_text), UNUSED)
[Called By]

- >> Mcu_InitRamSection

Mcu_Lld_SetMode (Thumb, 236 bytes, Stack size 24 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 24
- Call Chain = Mcu_Lld_SetMode

[Calls]

- >> Mcu_Lld_DisableAllCmu

[Called By]

- >> Mcu_SetMode

Mcu_Lld_SetClockSource (Thumb, 80 bytes, Stack size 16 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 52
- Call Chain = Mcu_Lld_SetClockSource ⇒ Mcu_Lld_SwitchSystemClock ⇒ Mcu_Lld_SetSystemClockSource

[Calls]

- >> Mcu_Lld_SetClockOut
- >> Mcu_Lld_ClkOutDisable
- >> Mcu_Lld_SetCmu
- >> Mcu_Lld_SwitchSystemClock

[Called By]

- >> Mcu_Lld_InitClock

Mcu_Lld_SetPeripheralClock (Thumb, 158 bytes, Stack size 20 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 20
- Call Chain = Mcu_Lld_SetPeripheralClock

[Called By]

- >> Mcu_Lld_InitClock

Mcu_Lld_InitClock (Thumb, 174 bytes, Stack size 16 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 68
- Call Chain = Mcu_Lld_InitClock ⇒ Mcu_Lld_SetClockSource ⇒ Mcu_Lld_SwitchSystemClock ⇒ Mcu_Lld_SetSystemClockSource

[Calls]

- >> Mcu_Lld_SetPeripheralClock
- >> Mcu_Lld_SetClockSource
- >> Mcu_Lld_InitClockDivider
- >> Mcu_Lld_EfmPrescaler
- >> Mcu_Lld_InitFxosc
- >> Mcu_Lld_InitFirc
- >> Mcu_Lld_InitSirc
- >> Mcu_Lld_SwitchSystemClock
- >> Mcu_Lld_DisableAllCmu

[Called By]

- >> Mcu_InitClock

Mcu_Lld_GetResetRawValue (Thumb, 32 bytes, Stack size 4 bytes, mcu_lld.o(.mcal_text), UNUSED)
[Called By]

- >> Mcu_GetResetRawValue
- >> Mcu_Lld_GetResetValue

Mcu_Lld_GetResetValue (Thumb, 220 bytes, Stack size 24 bytes, mcu_lld.o(.mcal_text), UNUSED)
[Calls]

- >> Mcu_Lld_GetResetRawValue

[Called By]

- >> Mcu_GetResetReason

Mcu_Lld_GetCoreClockFrequency (Thumb, 116 bytes, Stack size 32 bytes, mcu_lld.o(.mcal_text), UNUSED)
[Calls]

- >> Mcu_Lld_GetCoreDiv
- >> Mcu_Lld_GetCoreClockSource

[Called By]

- >> Mcu_180_GetCoreClockFrequency

Mcu_Lld_SetPcu (Thumb, 286 bytes, Stack size 8 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 8
- Call Chain = Mcu_Lld_SetPcu

[Called By]

- >> Mcu_Init

SchM_Mcu_ReadMsr (Thumb, 14 bytes, Stack size 4 bytes, schm_mcu.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = SchM_Mcu_ReadMsr

[Called By]

- >> SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00

SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00 (Thumb, 62 bytes, Stack size 8 bytes, schm_mcu.o(.mcal_text))
[Stack]

- Max Depth = 12
- Call Chain = SchM_Enter_Mcu_MCU_EXCLUSIVE_AREA_00 ⇒ SchM_Mcu_ReadMsr

[Calls]

- >> SchM_Mcu_ReadMsr

[Called By]

- >> Mcu_SetMode

SchM_Exit_Mcu_MCU_EXCLUSIVE_AREA_00 (Thumb, 50 bytes, Stack size 0 bytes, schm_mcu.o(.mcal_text))
[Called By]

- >> Mcu_SetMode

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_00 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

[Called By]

- >> UART_Lld_ClearErrorFlags

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_00 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Called By]

- >> UART_Lld_ClearErrorFlags

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_01 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

[Called By]

- >> UART_SetTransmitterCmd

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_01 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Called By]

- >> UART_SetTransmitterCmd

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_02 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

[Called By]

- >> UART_SetReceiverCmd

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_02 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Called By]

- >> UART_SetReceiverCmd

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_03 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

[Called By]

- >> UART_SetBaudRateDivisor

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_03 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Called By]

- >> UART_SetBaudRateDivisor

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_04 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

[Called By]

- >> UART_SetOversamplingRatio

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_04 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Called By]

- >> UART_SetOversamplingRatio

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_05 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

[Called By]

- >> UART_EnableBothEdgeSamplingCmd

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_05 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Called By]

- >> UART_EnableBothEdgeSamplingCmd

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_06 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

[Called By]

- >> UART_SetBitCountPerChar

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_06 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Called By]

- >> UART_SetBitCountPerChar

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_07 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

[Called By]

- >> UART_SetIntMode

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_07 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Called By]

- >> UART_SetIntMode

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_08 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

[Called By]

- >> UART_GetIntMode

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_08 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Called By]

- >> UART_GetIntMode

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_09 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

[Called By]

- >> UART_GetStatusFlag

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_09 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Called By]

- >> UART_GetStatusFlag

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_10 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_10 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_11 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_11 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_12 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_12 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_13 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_13 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_14 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_14 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_15 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_15 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_16 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_16 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_17 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_17 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_18 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_18 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_19 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_19 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_20 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_20 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_21 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

[Called By]

- >> CddUart_StartSyncSend

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_21 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_StartSyncSend

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_22 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

[Called By]

- >> CddUart_StartSyncReceive

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_22 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_StartSyncReceive

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_23 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

[Called By]

- >> CddUart_StartAsyncReceive

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_23 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_StartAsyncReceive

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_24 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

[Called By]

- >> CddUart_StartAsyncSend

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_24 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_StartAsyncSend

SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_25 (Thumb, 62 bytes, Stack size 8 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_CddUart_ReadMsr

SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_25 (Thumb, 50 bytes, Stack size 0 bytes, schm_cdduart.o(.mcal_text), UNUSED)

CddUart_Init (Thumb, 280 bytes, Stack size 16 bytes, cdduart.o(.mcal_text))
[Stack]

- Max Depth = 176
- Call Chain = CddUart_Init ⇒ CddUart_Mld_Init ⇒ UART_Lld_Init ⇒ UART_Lld_SetBaudRate

[Calls]

- >> CddUart_Mld_Init
- >> Det_ReportError

[Called By]

- >> Board_Init

CddUart_Deinit (Thumb, 366 bytes, Stack size 24 bytes, cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> CddUart_Mld_Deinit
- >> CddUart_Mld_GetTransmitStatus
- >> CddUart_Mld_GetReceiveStatus
- >> Det_ReportError

CddUart_SetBaudrate (Thumb, 240 bytes, Stack size 24 bytes, cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> CddUart_Mld_SetBaudrate
- >> CddUart_Mld_GetTransmitStatus
- >> CddUart_Mld_GetReceiveStatus
- >> Det_ReportError

CddUart_GetBaudrate (Thumb, 126 bytes, Stack size 24 bytes, cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> CddUart_Mld_GetBaudrate
- >> Det_ReportError

CddUart_Abort (Thumb, 126 bytes, Stack size 16 bytes, cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> CddUart_Mld_AbortReceivingData
- >> CddUart_Mld_AbortSendingData
- >> Det_ReportError

CddUart_SetBuffer (Thumb, 154 bytes, Stack size 32 bytes, cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> Det_ReportError

CddUart_SetCallBack (Thumb, 114 bytes, Stack size 24 bytes, cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> Det_ReportError

CddUart_SyncSend (Thumb, 166 bytes, Stack size 32 bytes, cdduart.o(.mcal_text))
[Stack]

- Max Depth = 40
- Call Chain = CddUart_SyncSend ⇒ Det_ReportError

[Calls]

- >> Det_ReportError

[Called By]

- >> Uart1_PrintString

CddUart_SyncReceive (Thumb, 166 bytes, Stack size 32 bytes, cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> Det_ReportError

CddUart_AsyncReceive (Thumb, 154 bytes, Stack size 24 bytes, cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> Det_ReportError

CddUart_AsyncSend (Thumb, 154 bytes, Stack size 24 bytes, cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> Det_ReportError

CddUart_GetStatus (Thumb, 154 bytes, Stack size 24 bytes, cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> CddUart_Mld_GetTransmitStatus
- >> CddUart_Mld_GetReceiveStatus
- >> Det_ReportError

CddUart_GetVersionInfo (Thumb, 62 bytes, Stack size 16 bytes, cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> Det_ReportError

CddUart_Mld_Init (Thumb, 160 bytes, Stack size 24 bytes, cdduart_mld.o(.mcal_text))
[Stack]

- Max Depth = 160
- Call Chain = CddUart_Mld_Init ⇒ UART_Lld_Init ⇒ UART_Lld_SetBaudRate

[Calls]

- >> UART_Lld_Init

[Called By]

- >> CddUart_Init

CddUart_Mld_Deinit (Thumb, 110 bytes, Stack size 16 bytes, cdduart_mld.o(.mcal_text), UNUSED)
[Calls]

- >> UART_Lld_Deinit

[Called By]

- >> CddUart_Deinit

CddUart_Mld_SetBaudrate (Thumb, 90 bytes, Stack size 24 bytes, cdduart_mld.o(.mcal_text), UNUSED)
[Calls]

- >> UART_Lld_SetBaudRate

[Called By]

- >> CddUart_SetBaudrate

CddUart_Mld_GetBaudrate (Thumb, 64 bytes, Stack size 24 bytes, cdduart_mld.o(.mcal_text), UNUSED)
[Calls]

- >> UART_Lld_GetBaudRate

[Called By]

- >> CddUart_GetBaudrate

CddUart_Mld_AbortSendingData (Thumb, 82 bytes, Stack size 16 bytes, cdduart_mld.o(.mcal_text), UNUSED)
[Calls]

- >> UART_Lld_AbortSendingData

[Called By]

- >> CddUart_Abort

CddUart_Mld_AbortReceivingData (Thumb, 82 bytes, Stack size 16 bytes, cdduart_mld.o(.mcal_text), UNUSED)
[Calls]

- >> UART_Lld_AbortReceivingData

[Called By]

- >> CddUart_Abort

CddUart_Mld_SetTxBuffer (Thumb, 68 bytes, Stack size 24 bytes, cdduart_mld.o(.mcal_text), UNUSED)
[Calls]

- >> UART_Lld_SetTxBuffer

[Called By]

- >> CddUart_StartSetBuffer

CddUart_Mld_SetCallBack (Thumb, 64 bytes, Stack size 24 bytes, cdduart_mld.o(.mcal_text), UNUSED)
[Calls]

- >> UART_Lld_SetCallback

[Called By]

- >> CddUart_StartSetCallBackFun

CddUart_Mld_SetRxBuffer (Thumb, 68 bytes, Stack size 24 bytes, cdduart_mld.o(.mcal_text), UNUSED)
[Calls]

- >> UART_Lld_SetRxBuffer

[Called By]

- >> CddUart_StartSetBuffer

CddUart_Mld_SyncSend (Thumb, 130 bytes, Stack size 32 bytes, cdduart_mld.o(.mcal_text), UNUSED)
[Calls]

- >> UART_Lld_SendDataBlocking

[Called By]

- >> CddUart_StartSyncSend

CddUart_Mld_SyncReceive (Thumb, 130 bytes, Stack size 32 bytes, cdduart_mld.o(.mcal_text), UNUSED)
[Calls]

- >> UART_Lld_ReceiveDataBlocking

[Called By]

- >> CddUart_StartSyncReceive

CddUart_Mld_AsyncReceive (Thumb, 90 bytes, Stack size 24 bytes, cdduart_mld.o(.mcal_text), UNUSED)
[Calls]

- >> UART_Lld_ReceiveData

[Called By]

- >> CddUart_StartAsyncReceive

CddUart_Mld_AsyncSend (Thumb, 90 bytes, Stack size 24 bytes, cdduart_mld.o(.mcal_text), UNUSED)
[Calls]

- >> UART_Lld_SendData

[Called By]

- >> CddUart_StartAsyncSend

CddUart_Mld_SetTransmitStatus (Thumb, 68 bytes, Stack size 16 bytes, cdduart_mld.o(.mcal_text), UNUSED)
[Calls]

- >> UART_Lld_SetTransmitStatus

[Called By]

- >> CddUart_StartAsyncSend
- >> CddUart_StartSyncSend

CddUart_Mld_GetTransmitStatus (Thumb, 78 bytes, Stack size 24 bytes, cdduart_mld.o(.mcal_text), UNUSED)
[Calls]

- >> UART_Lld_GetTransmitStatus

[Called By]

- >> CddUart_GetStatus
- >> CddUart_SetBaudrate
- >> CddUart_Deinit
- >> CddUart_StartAsyncSend
- >> CddUart_StartSyncSend

CddUart_Mld_SetReceiveStatus (Thumb, 68 bytes, Stack size 16 bytes, cdduart_mld.o(.mcal_text), UNUSED)
[Calls]

- >> UART_Lld_SetReceiveStatus

[Called By]

- >> CddUart_StartAsyncReceive
- >> CddUart_StartSyncReceive

CddUart_Mld_GetReceiveStatus (Thumb, 78 bytes, Stack size 24 bytes, cdduart_mld.o(.mcal_text), UNUSED)
[Calls]

- >> UART_Lld_GetReceiveStatus

[Called By]

- >> CddUart_GetStatus
- >> CddUart_SetBaudrate
- >> CddUart_Deinit
- >> CddUart_StartAsyncReceive
- >> CddUart_StartSyncReceive

UART_Lld_Init (Thumb, 554 bytes, Stack size 72 bytes, cdduart_lld_uart.o(.mcal_text))
[Stack]

- Max Depth = 136
- Call Chain = UART_Lld_Init ⇒ UART_Lld_SetBaudRate

[Calls]

- >> UART_Lld_SetBaudRate

[Called By]

- >> CddUart_Mld_Init

UART_Lld_SetBaudRate (Thumb, 438 bytes, Stack size 64 bytes, cdduart_lld_uart.o(.mcal_text))
[Stack]

- Max Depth = 64
- Call Chain = UART_Lld_SetBaudRate

[Called By]

- >> UART_Lld_Init
- >> CddUart_Mld_SetBaudrate

UART_Lld_Deinit (Thumb, 190 bytes, Stack size 48 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_Mld_Deinit

UART_Lld_SetCallback (Thumb, 82 bytes, Stack size 16 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_Mld_SetCallBack

UART_Lld_SendDataBlocking (Thumb, 232 bytes, Stack size 40 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_Mld_SyncSend

UART_Lld_SendData (Thumb, 102 bytes, Stack size 32 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_Mld_AsyncSend

UART_Lld_SetTransmitStatus (Thumb, 42 bytes, Stack size 12 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_Mld_SetTransmitStatus

UART_Lld_GetTransmitStatus (Thumb, 118 bytes, Stack size 16 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_Mld_GetTransmitStatus

UART_Lld_AbortSendingData (Thumb, 100 bytes, Stack size 24 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_Mld_AbortSendingData

UART_Lld_ReceiveDataBlocking (Thumb, 232 bytes, Stack size 40 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_Mld_SyncReceive

UART_Lld_ReceiveData (Thumb, 102 bytes, Stack size 32 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_Mld_AsyncReceive

UART_Lld_SetReceiveStatus (Thumb, 42 bytes, Stack size 12 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_Mld_SetReceiveStatus

UART_Lld_GetReceiveStatus (Thumb, 118 bytes, Stack size 16 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_Mld_GetReceiveStatus

UART_Lld_AbortReceivingData (Thumb, 100 bytes, Stack size 24 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_Mld_AbortReceivingData

UART_Lld_GetBaudRate (Thumb, 122 bytes, Stack size 32 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_Mld_GetBaudrate

UART_Lld_SetTxBuffer (Thumb, 84 bytes, Stack size 20 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_Mld_SetTxBuffer

UART_Lld_SetRxBuffer (Thumb, 84 bytes, Stack size 20 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Called By]

- >> CddUart_Mld_SetRxBuffer

UART_Lld_IRQHandler (Thumb, 190 bytes, Stack size 16 bytes, cdduart_lld_uart.o(.mcal_text))
[Stack]

- Max Depth = 40
- Call Chain = UART_Lld_IRQHandler ⇒ UART_Lld_TxEmptyIrqHandler

[Calls]

- >> UART_Lld_IdleLineIrqHandler
- >> UART_Lld_TxCompleteIrqHandler
- >> UART_Lld_TxEmptyIrqHandler
- >> UART_Lld_RxIrqHandler
- >> UART_Lld_ErrIrqHandler

[Called By]

- >> UART1_IRQHandler

UART_Lld_ErrIrqHandler (Thumb, 386 bytes, Stack size 24 bytes, cdduart_lld_uart.o(.mcal_text))
[Stack]

- Max Depth = 24
- Call Chain = UART_Lld_ErrIrqHandler

[Called By]

- >> UART_Lld_IRQHandler

UART_Lld_RxIrqHandler (Thumb, 126 bytes, Stack size 16 bytes, cdduart_lld_uart.o(.mcal_text))
[Stack]

- Max Depth = 16
- Call Chain = UART_Lld_RxIrqHandler

[Called By]

- >> UART_Lld_IRQHandler

UART_Lld_TxEmptyIrqHandler (Thumb, 162 bytes, Stack size 24 bytes, cdduart_lld_uart.o(.mcal_text))
[Stack]

- Max Depth = 24
- Call Chain = UART_Lld_TxEmptyIrqHandler

[Called By]

- >> UART_Lld_IRQHandler

UART_Lld_TxCompleteIrqHandler (Thumb, 90 bytes, Stack size 16 bytes, cdduart_lld_uart.o(.mcal_text))
[Stack]

- Max Depth = 16
- Call Chain = UART_Lld_TxCompleteIrqHandler

[Called By]

- >> UART_Lld_IRQHandler

UART_Lld_IdleLineIrqHandler (Thumb, 110 bytes, Stack size 16 bytes, cdduart_lld_uart.o(.mcal_text))
[Stack]

- Max Depth = 16
- Call Chain = UART_Lld_IdleLineIrqHandler

[Called By]

- >> UART_Lld_IRQHandler

UART1_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, cdduart_lld_uart_irq.o(.mcal_text))
[Stack]

- Max Depth = 48
- Call Chain = UART1_IRQHandler ⇒ UART_Lld_IRQHandler ⇒ UART_Lld_TxEmptyIrqHandler

[Calls]

- >> UART_Lld_IRQHandler

[Address Reference Count : 1]

- vector.o(.isr_vector)

### Local Symbols

Board_Init (Thumb, 46 bytes, Stack size 8 bytes, main.o(.text.Board_Init))
[Stack]

- Max Depth = 184
- Call Chain = Board_Init ⇒ CddUart_Init ⇒ CddUart_Mld_Init ⇒ UART_Lld_Init ⇒ UART_Lld_SetBaudRate

[Calls]

- >> Adc_Init
- >> CddUart_Init
- >> Platform_Init
- >> Port_Init

[Called By]

- >> main

IsPOR (Thumb, 40 bytes, Stack size 4 bytes, raminit1.o(.text.IsPOR))
[Stack]

- Max Depth = 4
- Call Chain = IsPOR

[Called By]

- >> RamInit1

Adc_ValidGroupCheck (Thumb, 132 bytes, Stack size 4 bytes, adc.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = Adc_ValidGroupCheck

[Called By]

- >> Adc_DisableGroupNotification
- >> Adc_InitAndGroupValidErrCheck
- >> Adc_EnableGroupNotification
- >> Adc_SetupResultBuffer

Adc_InitAndGroupValidErrCheck (Thumb, 110 bytes, Stack size 16 bytes, adc.o(.mcal_text))
[Stack]

- Max Depth = 24
- Call Chain = Adc_InitAndGroupValidErrCheck ⇒ Det_ReportError

[Calls]

- >> Det_ReportError
- >> Adc_ValidGroupCheck

[Called By]

- >> Adc_StopGroupConversion
- >> Adc_ReadGroup
- >> Adc_GetStreamLastPointer
- >> Adc_GetGroupStatus
- >> Adc_StartGroupConversion

Adc_UpdataStatusInReadApi (Thumb, 244 bytes, Stack size 16 bytes, adc.o(.mcal_text), UNUSED)
[Calls]

- >> Adc_Lld_ClearSeqConvEndIntFlag
- >> Adc_Lld_StopConversion
- >> Adc_Lld_StartConversion
- >> Adc_Lld_LoadGroupToHwUnit
- >> Adc_Lld_QueueDataUpdata
- >> Adc_Lld_ReadSeqConvEndIntFlag
- >> Adc_Lld_GetRunningGroupIndex
- >> Adc_Lld_GroupIndexCheck
- >> Adc_UpdateStatusReadGroupNoInt

[Called By]

- >> Adc_ReadGroup
- >> Adc_GetStreamLastPointer
- >> Adc_GetGroupStatus

Adc_UpdateStatusReadGroupNoInt (Thumb, 250 bytes, Stack size 24 bytes, adc.o(.mcal_text), UNUSED)
[Calls]

- >> Adc_Lld_GroupStatusUpdata
- >> Adc_Lld_ReadConversionResults
- >> Adc_Lld_ClearSeqConvEndIntFlag

[Called By]

- >> Adc_UpdataStatusInReadApi

Adc_SwStateAndRdRstInGetStream (Thumb, 256 bytes, Stack size 24 bytes, adc.o(.mcal_text), UNUSED)
[Calls]

- >> Adc_UpdataStatusAfterReadData

[Called By]

- >> Adc_GetStreamLastPointer

Adc_HandleHwReloadAfterRead (Thumb, 312 bytes, Stack size 16 bytes, adc.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_06
- >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_06
- >> Adc_Lld_StopConversion
- >> Adc_Lld_StartConversion
- >> Adc_Lld_LoadGroupToHwUnit
- >> Adc_Lld_GroupIndexCheck
- >> Adc_HwHandleInIdle
- >> Adc_HandleHwRunAgainInBusy

[Called By]

- >> Adc_ReadGroup
- >> Adc_GetStreamLastPointer

Adc_UpdataStatusAfterReadData (Thumb, 280 bytes, Stack size 8 bytes, adc.o(.mcal_text), UNUSED)
[Called By]

- >> Adc_SwStateAndRdRstInReadApi
- >> Adc_SwStateAndRdRstInGetStream

Adc_HandleHwRunAgainInBusy (Thumb, 312 bytes, Stack size 16 bytes, adc.o(.mcal_text), UNUSED)
[Calls]

- >> Adc_Lld_LoadGroupToHwUnit
- >> Adc_Lld_GetRunningGroupIndex
- >> Adc_CheckGroupQueueIndex

[Called By]

- >> Adc_HandleHwReloadAfterRead

Adc_HwHandleInIdle (Thumb, 344 bytes, Stack size 16 bytes, adc.o(.mcal_text), UNUSED)
[Calls]

- >> Adc_Lld_ClearSeqConvEndIntFlag
- >> Adc_Lld_StopConversion
- >> Adc_Lld_LoadGroupToHwUnit
- >> Adc_Lld_GroupIndexCheck
- >> Adc_LimitQueueIndex
- >> Adc_CheckGroupQueueIndex

[Called By]

- >> Adc_HandleHwReloadAfterRead

Adc_SwStateAndRdRstInReadApi (Thumb, 252 bytes, Stack size 24 bytes, adc.o(.mcal_text), UNUSED)
[Calls]

- >> Adc_UpdataStatusAfterReadData

[Called By]

- >> Adc_ReadGroup

Adc_CheckGroupQueueIndex (Thumb, 194 bytes, Stack size 8 bytes, adc.o(.mcal_text), UNUSED)
[Called By]

- >> Adc_StopGroupConversion
- >> Adc_HwHandleInIdle
- >> Adc_HandleHwRunAgainInBusy

Adc_GroupsInQueueUpdate (Thumb, 330 bytes, Stack size 24 bytes, adc.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_Adc_ADC_EXCLUSIVE_AREA_04
- >> SchM_Enter_Adc_ADC_EXCLUSIVE_AREA_04
- >> Adc_Lld_ClearSeqConvEndIntFlag
- >> Adc_Lld_StopConversion
- >> Adc_Lld_StartConversion
- >> Adc_Lld_LoadGroupToHwUnit
- >> Adc_Lld_GroupIndexCheck
- >> Adc_LimitQueueIndex

[Called By]

- >> Adc_StopGroupConversion

Adc_LimitQueueIndex (Thumb, 52 bytes, Stack size 4 bytes, adc.o(.mcal_text), UNUSED)
[Called By]

- >> Adc_StopGroupConversion
- >> Adc_GroupsInQueueUpdate
- >> Adc_HwHandleInIdle

Adc_Lld_SetTSEN (Thumb, 54 bytes, Stack size 12 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 12
- Call Chain = Adc_Lld_SetTSEN

[Called By]

- >> Adc_Lld_InitTempSensor

Adc_Lld_Enable (Thumb, 98 bytes, Stack size 24 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 28
- Call Chain = Adc_Lld_Enable ⇒ Adc_Lld_GetADEN

[Calls]

- >> Adc_Lld_GetADEN
- >> Adc_Lld_SetADEN

[Called By]

- >> Adc_Lld_HwUnitEnable

Adc_Lld_SetADEN (Thumb, 18 bytes, Stack size 4 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = Adc_Lld_SetADEN

[Called By]

- >> Adc_Lld_Enable

Adc_Lld_GetADEN (Thumb, 16 bytes, Stack size 4 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = Adc_Lld_GetADEN

[Called By]

- >> Adc_Lld_Enable

Adc_Lld_SetPrescaler (Thumb, 48 bytes, Stack size 12 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 12
- Call Chain = Adc_Lld_SetPrescaler

[Called By]

- >> Adc_Lld_HwClockInit

Adc_Lld_SetStartUpTime (Thumb, 42 bytes, Stack size 12 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 12
- Call Chain = Adc_Lld_SetStartUpTime

[Called By]

- >> Adc_Lld_HwClockInit

Adc_Lld_SetStopConversion (Thumb, 18 bytes, Stack size 4 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = Adc_Lld_SetStopConversion

[Called By]

- >> Adc_Lld_StopConversion

Adc_Lld_GetStopStatus (Thumb, 16 bytes, Stack size 4 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = Adc_Lld_GetStopStatus

[Called By]

- >> Adc_Lld_StopConversion

Adc_Lld_GetStartConversion (Thumb, 16 bytes, Stack size 4 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = Adc_Lld_GetStartConversion

[Called By]

- >> Adc_Lld_StartConversion

Adc_Lld_ClearFIFOInvalidData (Thumb, 104 bytes, Stack size 24 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 36
- Call Chain = Adc_Lld_ClearFIFOInvalidData ⇒ Adc_Lld_GetFIFOEmptyFlag

[Calls]

- >> Adc_Lld_ReadFIFO
- >> Adc_Lld_GetFIFOEmptyFlag

[Called By]

- >> Adc_Lld_StartConversion
- >> Adc_Lld_DeinitHwUnit

Adc_Lld_SetStartConversion (Thumb, 18 bytes, Stack size 4 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = Adc_Lld_SetStartConversion

[Called By]

- >> Adc_Lld_StartConversion

Adc_Lld_GetFIFOEmptyFlag (Thumb, 46 bytes, Stack size 12 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 12
- Call Chain = Adc_Lld_GetFIFOEmptyFlag

[Called By]

- >> Adc_Lld_ClearFIFOInvalidData

Adc_Lld_ReadFIFO (Thumb, 14 bytes, Stack size 4 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = Adc_Lld_ReadFIFO

[Called By]

- >> Adc_Lld_ClearFIFOInvalidData
- >> Adc_Lld_ReadConversionResults

Adc_Lld_DisableAllInt (Thumb, 14 bytes, Stack size 4 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = Adc_Lld_DisableAllInt

[Called By]

- >> Adc_Lld_DisableIntcandHwTrigger

Adc_Lld_SetTriggerMode (Thumb, 48 bytes, Stack size 12 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 12
- Call Chain = Adc_Lld_SetTriggerMode

[Called By]

- >> Adc_Lld_DisableIntcandHwTrigger

Adc_Lld_Disable (Thumb, 100 bytes, Stack size 24 bytes, adc_lld.o(.mcal_text), UNUSED)
[Calls]

- >> Adc_Lld_GetADDISStatus
- >> Adc_Lld_SetADDIS

[Called By]

- >> Adc_Lld_DeinitHwUnit

Adc_Lld_ResetRegister (Thumb, 108 bytes, Stack size 8 bytes, adc_lld.o(.mcal_text), UNUSED)
[Called By]

- >> Adc_Lld_DeinitHwUnit

Adc_Lld_SetADDIS (Thumb, 18 bytes, Stack size 4 bytes, adc_lld.o(.mcal_text), UNUSED)
[Called By]

- >> Adc_Lld_Disable

Adc_Lld_GetADDISStatus (Thumb, 16 bytes, Stack size 4 bytes, adc_lld.o(.mcal_text), UNUSED)
[Called By]

- >> Adc_Lld_Disable

Adc_Lld_GetEOSEQIntFlag (Thumb, 46 bytes, Stack size 12 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 12
- Call Chain = Adc_Lld_GetEOSEQIntFlag

[Called By]

- >> Adc_Lld_ReadSeqConvEndIntFlag

Adc_Lld_ClearEOSEQIntFlag (Thumb, 14 bytes, Stack size 4 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = Adc_Lld_ClearEOSEQIntFlag

[Called By]

- >> Adc_Lld_ClearSeqConvEndIntFlag

Adc_Lld_LimitCheck (Thumb, 498 bytes, Stack size 12 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 12
- Call Chain = Adc_Lld_LimitCheck

[Called By]

- >> Adc_Lld_ReadConversionResults

Adc_Lld_SetSampleTime (Thumb, 42 bytes, Stack size 12 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 12
- Call Chain = Adc_Lld_SetSampleTime

[Called By]

- >> Adc_Lld_LoadGroupToHwUnit

Adc_Lld_SetRegisterCFG0 (Thumb, 16 bytes, Stack size 8 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 8
- Call Chain = Adc_Lld_SetRegisterCFG0

[Called By]

- >> Adc_Lld_LoadGroupToHwUnit

ADC_Lld_SetSequeceChannel (Thumb, 44 bytes, Stack size 8 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 8
- Call Chain = ADC_Lld_SetSequeceChannel

[Called By]

- >> Adc_Lld_LoadGroupToHwUnit

Adc_Lld_ClearRegsiterSTS (Thumb, 16 bytes, Stack size 4 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = Adc_Lld_ClearRegsiterSTS

[Called By]

- >> Adc_Lld_ClearAllIntcFlag
- >> Adc_Lld_LoadGroupToHwUnit

Adc_Lld_SetRegiterINTE (Thumb, 16 bytes, Stack size 8 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 8
- Call Chain = Adc_Lld_SetRegiterINTE

[Called By]

- >> Adc_Lld_LoadGroupToHwUnit

Adc_Lld_RestartAdcHardWare (Thumb, 80 bytes, Stack size 16 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 76
- Call Chain = Adc_Lld_RestartAdcHardWare ⇒ Adc_Lld_LoadGroupToHwUnit ⇒ Adc_Lld_StopConversion ⇒ Adc_Lld_GetStopStatus

[Calls]

- >> Adc_Lld_StartConversion
- >> Adc_Lld_LoadGroupToHwUnit
- >> Adc_Lld_GroupIndexCheck

[Called By]

- >> Adc_Lld_IrqProcess

Adc_Lld_ClearAllIntcFlag (Thumb, 32 bytes, Stack size 16 bytes, adc_lld.o(.mcal_text))
[Stack]

- Max Depth = 20
- Call Chain = Adc_Lld_ClearAllIntcFlag ⇒ Adc_Lld_ClearRegsiterSTS

[Calls]

- >> Adc_Lld_ClearRegsiterSTS

[Called By]

- >> Adc_Lld_IrqProcess

Port_Lld_InitPull (Thumb, 108 bytes, Stack size 12 bytes, port_lld.o(.mcal_text))
[Stack]

- Max Depth = 12
- Call Chain = Port_Lld_InitPull

[Called By]

- >> Port_Lld_Init

Port_Lld_InitMode (Thumb, 234 bytes, Stack size 16 bytes, port_lld.o(.mcal_text))
[Stack]

- Max Depth = 28
- Call Chain = Port_Lld_InitMode ⇒ Port_Lld_InitGPIOMode

[Calls]

- >> Port_Lld_InitGPIOMode

[Called By]

- >> Port_Lld_Init

Port_Lld_InitGPIOMode (Thumb, 472 bytes, Stack size 12 bytes, port_lld.o(.mcal_text))
[Stack]

- Max Depth = 12
- Call Chain = Port_Lld_InitGPIOMode

[Called By]

- >> Port_Lld_InitMode

IntCtrl_Lld_ClrPendingPrivileged (Thumb, 20 bytes, Stack size 16 bytes, intctrl_lld.o(.mcal_text), UNUSED)
[Calls]

- >> __NVIC_ClearPendingIRQ

[Called By]

- >> IntCtrl_Lld_ClearPending

IntCtrl_Lld_SetPriPrivileged (Thumb, 28 bytes, Stack size 16 bytes, intctrl_lld.o(.mcal_text))
[Stack]

- Max Depth = 24
- Call Chain = IntCtrl_Lld_SetPriPrivileged ⇒ __NVIC_SetPriority

[Calls]

- >> __NVIC_SetPriority

[Called By]

- >> IntCtrl_Lld_SetPriority

IntCtrl_Lld_EnableIrqPrivileged (Thumb, 20 bytes, Stack size 16 bytes, intctrl_lld.o(.mcal_text))
[Stack]

- Max Depth = 20
- Call Chain = IntCtrl_Lld_EnableIrqPrivileged ⇒ __NVIC_EnableIRQ

[Calls]

- >> __NVIC_EnableIRQ

[Called By]

- >> IntCtrl_Lld_EnableIrq

IntCtrl_Lld_DisableIrqPrivileged (Thumb, 20 bytes, Stack size 16 bytes, intctrl_lld.o(.mcal_text))
[Stack]

- Max Depth = 20
- Call Chain = IntCtrl_Lld_DisableIrqPrivileged ⇒ __NVIC_DisableIRQ

[Calls]

- >> __NVIC_DisableIRQ

[Called By]

- >> IntCtrl_Lld_DisableIrq

IntCtrl_Lld_InstIsrPrivileged (Thumb, 72 bytes, Stack size 16 bytes, intctrl_lld.o(.mcal_text), UNUSED)
[Called By]

- >> IntCtrl_Lld_InstallHandler

__NVIC_EnableIRQ (Thumb, 48 bytes, Stack size 4 bytes, intctrl_lld.o(.text.__NVIC_EnableIRQ))
[Stack]

- Max Depth = 4
- Call Chain = __NVIC_EnableIRQ

[Called By]

- >> IntCtrl_Lld_EnableIrqPrivileged

__NVIC_DisableIRQ (Thumb, 56 bytes, Stack size 4 bytes, intctrl_lld.o(.text.__NVIC_DisableIRQ))
[Stack]

- Max Depth = 4
- Call Chain = __NVIC_DisableIRQ

[Called By]

- >> IntCtrl_Lld_DisableIrqPrivileged

__NVIC_SetPriority (Thumb, 66 bytes, Stack size 8 bytes, intctrl_lld.o(.text.__NVIC_SetPriority))
[Stack]

- Max Depth = 8
- Call Chain = __NVIC_SetPriority

[Called By]

- >> IntCtrl_Lld_SetPriPrivileged

IntCtrl_Lld_GetPriPrivileged (Thumb, 34 bytes, Stack size 16 bytes, intctrl_lld.o(.mcal_text), UNUSED)
[Calls]

- >> __NVIC_GetPriority

[Called By]

- >> IntCtrl_Lld_GetPriority

__NVIC_GetPriority (Thumb, 66 bytes, Stack size 8 bytes, intctrl_lld.o(.text.__NVIC_GetPriority), UNUSED)
[Called By]

- >> IntCtrl_Lld_GetPriPrivileged

__NVIC_ClearPendingIRQ (Thumb, 48 bytes, Stack size 4 bytes, intctrl_lld.o(.text.__NVIC_ClearPendingIRQ), UNUSED)
[Called By]

- >> IntCtrl_Lld_ClrPendingPrivileged

Platform_Mld_InitIntCtrl (Thumb, 110 bytes, Stack size 16 bytes, platform_mld.o(.mcal_text))
[Stack]

- Max Depth = 56
- Call Chain = Platform_Mld_InitIntCtrl ⇒ IntCtrl_Lld_SetPriority ⇒ IntCtrl_Lld_SetPriPrivileged ⇒ __NVIC_SetPriority

[Calls]

- >> IntCtrl_Lld_DisableIrq
- >> IntCtrl_Lld_EnableIrq
- >> IntCtrl_Lld_SetPriority

[Called By]

- >> Platform_Mld_Init

Platform_Mld_SetIrq (Thumb, 46 bytes, Stack size 16 bytes, platform.o(.mcal_text), UNUSED)
[Calls]

- >> IntCtrl_Lld_DisableIrq
- >> IntCtrl_Lld_EnableIrq

[Called By]

- >> Platform_SetIrq

Platform_Mld_SetIrqPriority (Thumb, 28 bytes, Stack size 16 bytes, platform.o(.mcal_text), UNUSED)
[Calls]

- >> IntCtrl_Lld_SetPriority

[Called By]

- >> Platform_SetIrqPriority

Platform_Mld_GetIrqPriority (Thumb, 20 bytes, Stack size 16 bytes, platform.o(.mcal_text), UNUSED)
[Calls]

- >> IntCtrl_Lld_GetPriority

[Called By]

- >> Platform_GetIrqPriority

Platform_Mld_InstallIrqHandler (Thumb, 28 bytes, Stack size 24 bytes, platform.o(.mcal_text), UNUSED)
[Calls]

- >> IntCtrl_Lld_InstallHandler

[Called By]

- >> Platform_InstallIrqHandler

ARM_MPU_Disable (Thumb, 46 bytes, Stack size 0 bytes, mpu_lld_m33.o(.text.ARM_MPU_Disable))
[Called By]

- >> Mpu_Lld_M33_Init

ARM_MPU_ClrRegion (Thumb, 24 bytes, Stack size 16 bytes, mpu_lld_m33.o(.text.ARM_MPU_ClrRegion))
[Stack]

- Max Depth = 24
- Call Chain = ARM_MPU_ClrRegion ⇒ ARM_MPU_ClrRegionEx

[Calls]

- >> ARM_MPU_ClrRegionEx

[Called By]

- >> Mpu_Lld_M33_Init

ARM_MPU_SetMemAttr (Thumb, 36 bytes, Stack size 16 bytes, mpu_lld_m33.o(.text.ARM_MPU_SetMemAttr))
[Stack]

- Max Depth = 32
- Call Chain = ARM_MPU_SetMemAttr ⇒ ARM_MPU_SetMemAttrEx

[Calls]

- >> ARM_MPU_SetMemAttrEx

[Called By]

- >> Mpu_Lld_M33_Init

ARM_MPU_SetRegion (Thumb, 32 bytes, Stack size 24 bytes, mpu_lld_m33.o(.text.ARM_MPU_SetRegion))
[Stack]

- Max Depth = 40
- Call Chain = ARM_MPU_SetRegion ⇒ ARM_MPU_SetRegionEx

[Calls]

- >> ARM_MPU_SetRegionEx

[Called By]

- >> Mpu_Lld_M33_Init

ARM_MPU_Enable (Thumb, 52 bytes, Stack size 4 bytes, mpu_lld_m33.o(.text.ARM_MPU_Enable))
[Stack]

- Max Depth = 4
- Call Chain = ARM_MPU_Enable

[Called By]

- >> Mpu_Lld_M33_Init

ARM_MPU_ClrRegionEx (Thumb, 22 bytes, Stack size 8 bytes, mpu_lld_m33.o(.text.ARM_MPU_ClrRegionEx))
[Stack]

- Max Depth = 8
- Call Chain = ARM_MPU_ClrRegionEx

[Called By]

- >> ARM_MPU_ClrRegion

ARM_MPU_SetMemAttrEx (Thumb, 100 bytes, Stack size 16 bytes, mpu_lld_m33.o(.text.ARM_MPU_SetMemAttrEx))
[Stack]

- Max Depth = 16
- Call Chain = ARM_MPU_SetMemAttrEx

[Called By]

- >> ARM_MPU_SetMemAttr

ARM_MPU_SetRegionEx (Thumb, 32 bytes, Stack size 16 bytes, mpu_lld_m33.o(.text.ARM_MPU_SetRegionEx))
[Stack]

- Max Depth = 16
- Call Chain = ARM_MPU_SetRegionEx

[Called By]

- >> ARM_MPU_SetRegion

Mcu_Lld_DisableAllCmu (Thumb, 18 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
[Called By]

- >> Mcu_Lld_SetMode
- >> Mcu_Lld_InitClock

Mcu_Lld_SwitchSystemClock (Thumb, 120 bytes, Stack size 32 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 36
- Call Chain = Mcu_Lld_SwitchSystemClock ⇒ Mcu_Lld_SetSystemClockSource

[Calls]

- >> Mcu_Lld_GetSystemClockStatus
- >> Mcu_Lld_SetSystemClockSource

[Called By]

- >> Mcu_Lld_SetClockSource
- >> Mcu_Lld_InitClock

Mcu_Lld_SetCmu (Thumb, 196 bytes, Stack size 20 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 20
- Call Chain = Mcu_Lld_SetCmu

[Called By]

- >> Mcu_Lld_SetClockSource

Mcu_Lld_ClkOutDisable (Thumb, 18 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
[Called By]

- >> Mcu_Lld_SetClockSource

Mcu_Lld_SetClockOut (Thumb, 50 bytes, Stack size 4 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = Mcu_Lld_SetClockOut

[Called By]

- >> Mcu_Lld_SetClockSource

Mcu_Lld_SetSystemClockSource (Thumb, 30 bytes, Stack size 4 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = Mcu_Lld_SetSystemClockSource

[Called By]

- >> Mcu_Lld_SwitchSystemClock

Mcu_Lld_GetSystemClockStatus (Thumb, 16 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
[Called By]

- >> Mcu_Lld_SwitchSystemClock

Mcu_Lld_InitSirc (Thumb, 90 bytes, Stack size 12 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 12
- Call Chain = Mcu_Lld_InitSirc

[Called By]

- >> Mcu_Lld_InitClock

Mcu_Lld_InitFirc (Thumb, 148 bytes, Stack size 32 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 40
- Call Chain = Mcu_Lld_InitFirc ⇒ Mcu_Lld_FircEnable

[Calls]

- >> Mcu_Lld_FircDisable
- >> Mcu_Lld_GetClockStatus
- >> Mcu_Lld_FircEnable

[Called By]

- >> Mcu_Lld_InitClock

Mcu_Lld_InitFxosc (Thumb, 238 bytes, Stack size 32 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 52
- Call Chain = Mcu_Lld_InitFxosc ⇒ Mcu_Lld_SetFxoscClock

[Calls]

- >> Mcu_Lld_FxoscDisable
- >> Mcu_Lld_SetFxoscGain
- >> Mcu_Lld_SetFxoscClock
- >> Mcu_Lld_GetClockStatus

[Called By]

- >> Mcu_Lld_InitClock

Mcu_Lld_EfmPrescaler (Thumb, 50 bytes, Stack size 8 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 8
- Call Chain = Mcu_Lld_EfmPrescaler

[Called By]

- >> Mcu_Lld_InitClock

Mcu_Lld_InitClockDivider (Thumb, 144 bytes, Stack size 32 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 44
- Call Chain = Mcu_Lld_InitClockDivider ⇒ Mcu_Lld_SetClockDivider

[Calls]

- >> Mcu_Lld_GetDividerStatus
- >> Mcu_Lld_SetClockDivider

[Called By]

- >> Mcu_Lld_InitClock

Mcu_Lld_FircEnable (Thumb, 72 bytes, Stack size 8 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 8
- Call Chain = Mcu_Lld_FircEnable

[Called By]

- >> Mcu_Lld_InitFirc

Mcu_Lld_GetClockStatus (Thumb, 22 bytes, Stack size 4 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = Mcu_Lld_GetClockStatus

[Called By]

- >> Mcu_Lld_InitFxosc
- >> Mcu_Lld_InitFirc

Mcu_Lld_FircDisable (Thumb, 18 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
[Called By]

- >> Mcu_Lld_InitFirc

Mcu_Lld_SetFxoscClock (Thumb, 120 bytes, Stack size 20 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 20
- Call Chain = Mcu_Lld_SetFxoscClock

[Called By]

- >> Mcu_Lld_InitFxosc

Mcu_Lld_SetFxoscGain (Thumb, 30 bytes, Stack size 4 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 4
- Call Chain = Mcu_Lld_SetFxoscGain

[Called By]

- >> Mcu_Lld_InitFxosc

Mcu_Lld_FxoscDisable (Thumb, 18 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
[Called By]

- >> Mcu_Lld_InitFxosc

Mcu_Lld_SetClockDivider (Thumb, 62 bytes, Stack size 12 bytes, mcu_lld.o(.mcal_text))
[Stack]

- Max Depth = 12
- Call Chain = Mcu_Lld_SetClockDivider

[Called By]

- >> Mcu_Lld_InitClockDivider

Mcu_Lld_GetDividerStatus (Thumb, 12 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text))
[Called By]

- >> Mcu_Lld_InitClockDivider

Mcu_Lld_GetCoreClockSource (Thumb, 26 bytes, Stack size 4 bytes, mcu_lld.o(.mcal_text), UNUSED)
[Called By]

- >> Mcu_Lld_GetCoreClockFrequency

Mcu_Lld_GetCoreDiv (Thumb, 22 bytes, Stack size 0 bytes, mcu_lld.o(.mcal_text), UNUSED)
[Called By]

- >> Mcu_Lld_GetCoreClockFrequency

SchM_CddUart_ReadMsr (Thumb, 14 bytes, Stack size 4 bytes, schm_cdduart.o(.mcal_text), UNUSED)
[Called By]

- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_25
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_24
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_23
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_22
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_21
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_20
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_19
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_18
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_17
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_16
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_15
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_14
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_13
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_12
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_11
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_10
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_09
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_08
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_07
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_06
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_05
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_04
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_03
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_02
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_01
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_00

CddUart_StartSetBuffer (Thumb, 64 bytes, Stack size 24 bytes, cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> CddUart_Mld_SetRxBuffer
- >> CddUart_Mld_SetTxBuffer

CddUart_StartSetCallBackFun (Thumb, 28 bytes, Stack size 16 bytes, cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> CddUart_Mld_SetCallBack

CddUart_StartSyncSend (Thumb, 130 bytes, Stack size 24 bytes, cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> CddUart_Mld_SyncSend
- >> CddUart_Mld_SetTransmitStatus
- >> CddUart_Mld_GetTransmitStatus
- >> SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_21
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_21
- >> Det_ReportError

CddUart_StartSyncReceive (Thumb, 130 bytes, Stack size 24 bytes, cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> CddUart_Mld_SyncReceive
- >> CddUart_Mld_SetReceiveStatus
- >> CddUart_Mld_GetReceiveStatus
- >> SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_22
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_22
- >> Det_ReportError

CddUart_StartAsyncReceive (Thumb, 108 bytes, Stack size 24 bytes, cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> CddUart_Mld_AsyncReceive
- >> CddUart_Mld_SetReceiveStatus
- >> CddUart_Mld_GetReceiveStatus
- >> SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_23
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_23
- >> Det_ReportError

CddUart_StartAsyncSend (Thumb, 108 bytes, Stack size 24 bytes, cdduart.o(.mcal_text), UNUSED)
[Calls]

- >> CddUart_Mld_AsyncSend
- >> CddUart_Mld_SetTransmitStatus
- >> CddUart_Mld_GetTransmitStatus
- >> SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_24
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_24
- >> Det_ReportError

UART_SetBitCountPerChar (Thumb, 72 bytes, Stack size 24 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_06
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_06

UART_SetIntMode (Thumb, 64 bytes, Stack size 16 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_07
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_07

UART_EnableBothEdgeSamplingCmd (Thumb, 28 bytes, Stack size 16 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_05
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_05

UART_SetOversamplingRatio (Thumb, 54 bytes, Stack size 24 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_04
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_04

UART_SetBaudRateDivisor (Thumb, 54 bytes, Stack size 24 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_03
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_03

UART_SetTransmitterCmd (Thumb, 126 bytes, Stack size 32 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_01
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_01

UART_GetStatusFlag (Thumb, 54 bytes, Stack size 16 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_09
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_09

UART_SetReceiverCmd (Thumb, 126 bytes, Stack size 32 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_02
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_02

UART_GetIntMode (Thumb, 54 bytes, Stack size 16 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_08
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_08

UART_Lld_ClearErrorFlags (Thumb, 42 bytes, Stack size 24 bytes, cdduart_lld_uart.o(.mcal_text), UNUSED)
[Calls]

- >> SchM_Exit_CddUart_CDDUART_EXCLUSIVE_AREA_00
- >> SchM_Enter_CddUart_CDDUART_EXCLUSIVE_AREA_00

### Undefined Global Symbols