#

##

##

##

##

##

##

    µVision Build Log
    Tool Versions:
    IDE-Version: ¦ÌVision V5.29.0.0
    Copyright (C) 2019 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: 1 3309701887@qq.com, 1, LIC=TA39H-WIZ2T-79FG1-C4XP7-QQ668-DP0FL

    Tool Versions:
    Toolchain:       MDK-ARM Professional  Version: 5.29.0.0
    Toolchain Path:  D:\keil\ARM\ARM\ARMCLANG\Bin
    C Compiler:      ArmClang.exe V6.13.1
    Assembler:       Armasm.exe V6.13.1
    Linker/Locator:  ArmLink.exe V6.13.1
    Library Manager: ArmAr.exe V6.13.1
    Hex Converter:   FromElf.exe V6.13.1
    CPU DLL:         SARMCM3.DLL V5.29.0.0
    Dialog DLL:      DCM.DLL V1.17.3.0
    Target DLL:      Segger\JL2CM3.dll V2.99.36.0
    Dialog DLL:      TCM.DLL V1.36.5.0

    Project:
    C:\Users\33097\Desktop\shangyu\Power_Pin_Wakeup_From_deepsleep_Demo\KEIL\Power_Pin_Wakeup_From_Powerdown_Mode_Demo.uvprojx
    Project File Date:  04/09/2025

    Output:
    *** Using Compiler 'V6.13.1', folder: 'D:\keil\ARM\ARM\ARMCLANG\Bin'
    Rebuild target 'Power_Pin_Wakeup_From_Powerdown_Mode_Demo'
    compiling pin_mux.c...
    compiling clock_config.c...
    ../app/main.c(101): warning: incompatible pointer types passing 'volatile uint8_t (*)[1024]' to parameter of type 'uint8_t *' (aka 'unsigned char *') [-Wincompatible-pointer-types]
        LINFlexD_UART_DRV_ReceiveData(2, &buff, sizeof(buff));
                                         ^~~~~
    ../platform/drivers/inc\linflexd_uart_driver.h(381): note: passing argument to parameter 'rxBuff' here
                                           uint8_t *rxBuff,
                                                    ^
    ../app/main.c(111): warning: incompatible pointer types passing 'volatile uint8_t (*)[1024]' to parameter of type 'const uint8_t *' (aka 'const unsigned char *') [-Wincompatible-pointer-types]
                                                            LINFlexD_UART_DRV_SendDataBlocking(2,&buff,8,0xFF);
                                                                                                 ^~~~~
    ../platform/drivers/inc\linflexd_uart_driver.h(280): note: passing argument to parameter 'txBuff' here
                                                const uint8_t *txBuff,
                                                               ^
    2 warnings generated.
    compiling main.c...
    assembling RamInit0.S...
    compiling RamInit2.c...
    compiling interrupt_config.c...
    compiling dma_config.c...
    compiling linflexd_uart_config.c...
    compiling RamInit1.c...
    assembling vector.S...
    assembling startup.S...
    compiling vector_table_copy.c...
    compiling power_config.c...
    compiling utility_print_config.c...
    compiling pins_port_hw_access.c...
    compiling secure_boot_YTM32B1HA0.c...
    compiling pins_driver.c...
    compiling clock_YTM32B1Hx.c...
    compiling interrupt_manager.c...
    compiling system_YTM32B1HA0.c...
    compiling dma_irq.c...
    compiling dma_hw_access.c...
    compiling linflexd_uart_irq.c...
    compiling power_manager.c...
    compiling dma_driver.c...
    compiling linflexd_uart_driver.c...
    compiling power_manager_YTM32B1Hx.c...
    compiling printf.c...
    compiling osif_baremetal.c...
    linking...
    .\Objects\Power_Pin_Wakeup_From_Powerdown_Mode_Demo.axf: Warning: L6319W: Ignoring --keep command. Cannot find section *(.sb_config_group).
    Program Size: Code=12036 RO-data=840 RW-data=52 ZI-data=67920
    Finished: 0 information, 1 warning and 0 error messages.
    FromELF: creating hex file...
    After Build - User command #1: fromelf --bin --bincombined --output=Objects\Power_Pin_Wakeup_From_Powerdown_Mode_Demo.bin .\Objects\Power_Pin_Wakeup_From_Powerdown_Mode_Demo.axf
    After Build - User command #2: fromelf --m32 --m32combined --output=Objects\Power_Pin_Wakeup_From_Powerdown_Mode_Demo.srec .\Objects\Power_Pin_Wakeup_From_Powerdown_Mode_Demo.axf
    ".\Objects\Power_Pin_Wakeup_From_Powerdown_Mode_Demo.axf" - 0 Error(s), 3 Warning(s).

    Software Packages used:

    Package Vendor: YTMicro
                    https://doc.ytmicro.com/keil/YTMicro.YTM32B1HA0_DFP.1.2.0.pack
                    YTMicro.YTM32B1HA0_DFP.1.2.0
                    Device Family Pack for YTM32B1HA0

    Collection of Component include folders:
      .\RTE\_Power_Pin_Wakeup_From_Powerdown_Mode_Demo
      D:\keil\ARM\packs\YTMicro\YTM32B1HA0_DFP\1.2.0\Device\Include

    Collection of Component Files used:
    Build Time Elapsed:  00:00:04