# Static Call Graph for image .\Objects\Rtc_Wakeup_Demo.axf

#<CALLGRAPH># ARM Linker, 6130100: Last Updated: Tue Apr 8 14:47:26 2025

### Maximum Stack Usage = 608 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

Reset_Handler ⇒ main ⇒ printf_ ⇒ _vsnprintf ⇒ _ftoa ⇒ _etoa ⇒ _ftoa (Cycle)

### Functions with no stack information

- RamInit0
- Reset_Handler

### Mutually Recursive functions

- _etoa ⇒ _ftoa
- DefaultISR ⇒ DefaultISR

  ### Function Pointers

  - ACMP0_IRQHandler from vector_table_copy.o(.text.ACMP0_IRQHandler) referenced from vector.o(.isr_vector)
  - ACMP1_IRQHandler from vector_table_copy.o(.text.ACMP1_IRQHandler) referenced from vector.o(.isr_vector)
  - ADC0_IRQHandler from vector_table_copy.o(.text.ADC0_IRQHandler) referenced from vector.o(.isr_vector)
  - ADC1_IRQHandler from vector_table_copy.o(.text.ADC1_IRQHandler) referenced from vector.o(.isr_vector)
  - BusFault_Handler from vector_table_copy.o(.text.BusFault_Handler) referenced from vector.o(.isr_vector)
  - CAN0_Error_IRQHandler from vector_table_copy.o(.text.CAN0_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_112_127_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_112_127_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_64_79_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_64_79_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_80_95_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_80_95_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_96_111_MB_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_96_111_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_BusOff_Warning_IRQHandler from vector_table_copy.o(.text.CAN0_ORed_BusOff_Warning_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN0_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_Error_IRQHandler from vector_table_copy.o(.text.CAN1_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_112_127_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_112_127_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_64_79_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_64_79_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_80_95_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_80_95_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_96_111_MB_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_96_111_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_BusOff_Warning_IRQHandler from vector_table_copy.o(.text.CAN1_ORed_BusOff_Warning_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN1_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_Error_IRQHandler from vector_table_copy.o(.text.CAN2_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_ORed_BusOff_Warning_IRQHandler from vector_table_copy.o(.text.CAN2_ORed_BusOff_Warning_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN2_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN2_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_Error_IRQHandler from vector_table_copy.o(.text.CAN3_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_ORed_BusOff_Warning_IRQHandler from vector_table_copy.o(.text.CAN3_ORed_BusOff_Warning_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN3_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN3_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_Error_IRQHandler from vector_table_copy.o(.text.CAN4_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_32_47_MB_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_48_63_MB_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_ORed_BusOff_Warning_IRQHandler from vector_table_copy.o(.text.CAN4_ORed_BusOff_Warning_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN4_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN4_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_Error_IRQHandler from vector_table_copy.o(.text.CAN5_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN5_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN5_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_ORed_BusOff_Warning_IRQHandler from vector_table_copy.o(.text.CAN5_ORed_BusOff_Warning_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN5_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN5_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN6_Error_IRQHandler from vector_table_copy.o(.text.CAN6_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN6_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN6_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN6_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN6_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN6_ORed_BusOff_Warning_IRQHandler from vector_table_copy.o(.text.CAN6_ORed_BusOff_Warning_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN6_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN6_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN7_Error_IRQHandler from vector_table_copy.o(.text.CAN7_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN7_ORed_0_15_MB_IRQHandler from vector_table_copy.o(.text.CAN7_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN7_ORed_16_31_MB_IRQHandler from vector_table_copy.o(.text.CAN7_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN7_ORed_BusOff_Warning_IRQHandler from vector_table_copy.o(.text.CAN7_ORed_BusOff_Warning_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN7_Wake_Up_IRQHandler from vector_table_copy.o(.text.CAN7_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CMU_IRQHandler from vector_table_copy.o(.text.CMU_IRQHandler) referenced from vector.o(.isr_vector)
  - CORE_CTI_IRQHandler from vector_table_copy.o(.text.CORE_CTI_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA0_IRQHandler from dma_irq.o(.text.DMA0_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA10_IRQHandler from dma_irq.o(.text.DMA10_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA11_IRQHandler from dma_irq.o(.text.DMA11_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA12_IRQHandler from dma_irq.o(.text.DMA12_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA13_IRQHandler from dma_irq.o(.text.DMA13_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA14_IRQHandler from dma_irq.o(.text.DMA14_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA15_IRQHandler from dma_irq.o(.text.DMA15_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA16_IRQHandler from dma_irq.o(.text.DMA16_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA17_IRQHandler from dma_irq.o(.text.DMA17_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA18_IRQHandler from dma_irq.o(.text.DMA18_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA19_IRQHandler from dma_irq.o(.text.DMA19_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA1_IRQHandler from dma_irq.o(.text.DMA1_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA20_IRQHandler from dma_irq.o(.text.DMA20_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA21_IRQHandler from dma_irq.o(.text.DMA21_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA22_IRQHandler from dma_irq.o(.text.DMA22_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA23_IRQHandler from dma_irq.o(.text.DMA23_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA24_IRQHandler from dma_irq.o(.text.DMA24_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA25_IRQHandler from dma_irq.o(.text.DMA25_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA26_IRQHandler from dma_irq.o(.text.DMA26_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA27_IRQHandler from dma_irq.o(.text.DMA27_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA28_IRQHandler from dma_irq.o(.text.DMA28_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA29_IRQHandler from dma_irq.o(.text.DMA29_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA2_IRQHandler from dma_irq.o(.text.DMA2_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA30_IRQHandler from dma_irq.o(.text.DMA30_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA31_IRQHandler from dma_irq.o(.text.DMA31_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA3_IRQHandler from dma_irq.o(.text.DMA3_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA4_IRQHandler from dma_irq.o(.text.DMA4_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA5_IRQHandler from dma_irq.o(.text.DMA5_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA6_IRQHandler from dma_irq.o(.text.DMA6_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA7_IRQHandler from dma_irq.o(.text.DMA7_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA8_IRQHandler from dma_irq.o(.text.DMA8_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA9_IRQHandler from dma_irq.o(.text.DMA9_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA_Error_IRQHandler from dma_irq.o(.text.DMA_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - DebugMon_Handler from vector_table_copy.o(.text.DebugMon_Handler) referenced from vector.o(.isr_vector)
  - DefaultISR from vector_table_copy.o(.text.DefaultISR) referenced 26 times from vector.o(.isr_vector)
  - DefaultISR from vector_table_copy.o(.text.DefaultISR) referenced 2 times from linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_Deinit)
  - EFM_Ecc_IRQHandler from vector_table_copy.o(.text.EFM_Ecc_IRQHandler) referenced from vector.o(.isr_vector)
  - EFM_Error_IRQHandler from vector_table_copy.o(.text.EFM_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - EFM_IRQHandler from vector_table_copy.o(.text.EFM_IRQHandler) referenced from vector.o(.isr_vector)
  - EMU0_IRQHandler from vector_table_copy.o(.text.EMU0_IRQHandler) referenced from vector.o(.isr_vector)
  - ENET_ECC_IRQHandler from vector_table_copy.o(.text.ENET_ECC_IRQHandler) referenced from vector.o(.isr_vector)
  - ENET_IRQHandler from vector_table_copy.o(.text.ENET_IRQHandler) referenced from vector.o(.isr_vector)
  - ENET_RX_IRQHandler from vector_table_copy.o(.text.ENET_RX_IRQHandler) referenced from vector.o(.isr_vector)
  - ENET_TX_IRQHandler from vector_table_copy.o(.text.ENET_TX_IRQHandler) referenced from vector.o(.isr_vector)
  - FMU_Alarm_IRQHandler from vector_table_copy.o(.text.FMU_Alarm_IRQHandler) referenced from vector.o(.isr_vector)
  - FMU_MISC_IRQHandler from vector_table_copy.o(.text.FMU_MISC_IRQHandler) referenced from vector.o(.isr_vector)
  - FPU_IRQHandler from vector_table_copy.o(.text.FPU_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOA_IRQHandler from vector_table_copy.o(.text.GPIOA_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOB_IRQHandler from vector_table_copy.o(.text.GPIOB_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOC_IRQHandler from vector_table_copy.o(.text.GPIOC_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOD_IRQHandler from vector_table_copy.o(.text.GPIOD_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOE_IRQHandler from vector_table_copy.o(.text.GPIOE_IRQHandler) referenced from vector.o(.isr_vector)
  - HCU_IRQHandler from vector_table_copy.o(.text.HCU_IRQHandler) referenced from vector.o(.isr_vector)
  - HardFault_Handler from vector_table_copy.o(.text.HardFault_Handler) referenced from vector.o(.isr_vector)
  - I2C0_Master_Slave_IRQHandler from vector_table_copy.o(.text.I2C0_Master_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C1_Master_Slave_IRQHandler from vector_table_copy.o(.text.I2C1_Master_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C2_Master_Slave_IRQHandler from vector_table_copy.o(.text.I2C2_Master_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C3_Master_Slave_IRQHandler from vector_table_copy.o(.text.I2C3_Master_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C4_Master_Slave_IRQHandler from vector_table_copy.o(.text.I2C4_Master_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - INTM_IRQHandler from vector_table_copy.o(.text.INTM_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD0_IRQHandler from vector_table_copy.o(.text.LINFlexD0_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD0_UART_IRQHandler from linflexd_uart_irq.o(.text.LINFlexD0_UART_IRQHandler) referenced from linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)
  - LINFlexD1_IRQHandler from vector_table_copy.o(.text.LINFlexD1_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD1_UART_IRQHandler from linflexd_uart_irq.o(.text.LINFlexD1_UART_IRQHandler) referenced from linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)
  - LINFlexD2_IRQHandler from vector_table_copy.o(.text.LINFlexD2_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD2_UART_IRQHandler from linflexd_uart_irq.o(.text.LINFlexD2_UART_IRQHandler) referenced from linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)
  - LINFlexD3_IRQHandler from vector_table_copy.o(.text.LINFlexD3_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD3_UART_IRQHandler from linflexd_uart_irq.o(.text.LINFlexD3_UART_IRQHandler) referenced from linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)
  - LINFlexD4_IRQHandler from vector_table_copy.o(.text.LINFlexD4_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD4_UART_IRQHandler from linflexd_uart_irq.o(.text.LINFlexD4_UART_IRQHandler) referenced from linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)
  - LINFlexD5_IRQHandler from vector_table_copy.o(.text.LINFlexD5_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD5_UART_IRQHandler from linflexd_uart_irq.o(.text.LINFlexD5_UART_IRQHandler) referenced from linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)
  - LINFlexD6_IRQHandler from vector_table_copy.o(.text.LINFlexD6_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD7_IRQHandler from vector_table_copy.o(.text.LINFlexD7_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD8_IRQHandler from vector_table_copy.o(.text.LINFlexD8_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD9_IRQHandler from vector_table_copy.o(.text.LINFlexD9_IRQHandler) referenced from vector.o(.isr_vector)
  - LINFlexD_UART_DRV_CompleteReceiveUsingDma from linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_CompleteReceiveUsingDma) referenced 2 times from linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_StartReceiveUsingDma)
  - LINFlexD_UART_DRV_CompleteSendUsingDma from linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_CompleteSendUsingDma) referenced 2 times from linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_StartSendUsingDma)
  - MPWM0_Ch0_Ch7_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch0_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch8_Ch15_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch8_Ch15_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM1_Ch0_Ch7_IRQHandler from vector_table_copy.o(.text.MPWM1_Ch0_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM1_Ch8_Ch15_IRQHandler from vector_table_copy.o(.text.MPWM1_Ch8_Ch15_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM2_Ch0_Ch7_IRQHandler from vector_table_copy.o(.text.MPWM2_Ch0_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM2_Ch8_Ch15_IRQHandler from vector_table_copy.o(.text.MPWM2_Ch8_Ch15_IRQHandler) referenced from vector.o(.isr_vector)
  - MemManage_Handler from vector_table_copy.o(.text.MemManage_Handler) referenced from vector.o(.isr_vector)
  - NMI_Handler from vector_table_copy.o(.text.NMI_Handler) referenced from vector.o(.isr_vector)
  - PCU_IRQHandler from vector_table_copy.o(.text.PCU_IRQHandler) referenced from vector.o(.isr_vector)
  - PTU0_IRQHandler from vector_table_copy.o(.text.PTU0_IRQHandler) referenced from vector.o(.isr_vector)
  - PTU1_IRQHandler from vector_table_copy.o(.text.PTU1_IRQHandler) referenced from vector.o(.isr_vector)
  - PendSV_Handler from vector_table_copy.o(.text.PendSV_Handler) referenced from vector.o(.isr_vector)
  - QSPI_IRQHandler from vector_table_copy.o(.text.QSPI_IRQHandler) referenced from vector.o(.isr_vector)
  - RTC_IRQHandler from rtc_irq.o(.text.RTC_IRQHandler) referenced from vector.o(.isr_vector)
  - RTC_Seconds_IRQHandler from rtc_irq.o(.text.RTC_Seconds_IRQHandler) referenced from vector.o(.isr_vector)
  - RamInit1 from raminit1.o(.text.RamInit1) referenced from startup.o(.text)
  - RamInit2 from raminit2.o(.text.RamInit2) referenced from startup.o(.text)
  - Reset_Handler from startup.o(.text) referenced from vector.o(.isr_vector)
  - SAI0_IRQHandler from vector_table_copy.o(.text.SAI0_IRQHandler) referenced from vector.o(.isr_vector)
  - SAI1_IRQHandler from vector_table_copy.o(.text.SAI1_IRQHandler) referenced from vector.o(.isr_vector)
  - SENT0_IRQHandler from vector_table_copy.o(.text.SENT0_IRQHandler) referenced from vector.o(.isr_vector)
  - SENT1_IRQHandler from vector_table_copy.o(.text.SENT1_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI0_IRQHandler from vector_table_copy.o(.text.SPI0_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI1_IRQHandler from vector_table_copy.o(.text.SPI1_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI2_IRQHandler from vector_table_copy.o(.text.SPI2_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI3_IRQHandler from vector_table_copy.o(.text.SPI3_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI4_IRQHandler from vector_table_copy.o(.text.SPI4_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI5_IRQHandler from vector_table_copy.o(.text.SPI5_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI6_IRQHandler from vector_table_copy.o(.text.SPI6_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI7_IRQHandler from vector_table_copy.o(.text.SPI7_IRQHandler) referenced from vector.o(.isr_vector)
  - SVC_Handler from vector_table_copy.o(.text.SVC_Handler) referenced from vector.o(.isr_vector)
  - SysTick_Handler from osif_baremetal.o(.text.SysTick_Handler) referenced from vector.o(.isr_vector)
  - SystemInit from system_ytm32b1ha0.o(.text.SystemInit) referenced from startup.o(.text)
  - TMR0_IRQHandler from vector_table_copy.o(.text.TMR0_IRQHandler) referenced from vector.o(.isr_vector)
  - TMR1_IRQHandler from vector_table_copy.o(.text.TMR1_IRQHandler) referenced from vector.o(.isr_vector)
  - TRNG_IRQHandler from vector_table_copy.o(.text.TRNG_IRQHandler) referenced from vector.o(.isr_vector)
  - UsageFault_Handler from vector_table_copy.o(.text.UsageFault_Handler) referenced from vector.o(.isr_vector)
  - VectorTableCopy from vector_table_copy.o(.text.VectorTableCopy) referenced from startup.o(.text)
  - WDG0_IRQHandler from vector_table_copy.o(.text.WDG0_IRQHandler) referenced from vector.o(.isr_vector)
  - WKU_IRQHandler from vector_table_copy.o(.text.WKU_IRQHandler) referenced from vector.o(.isr_vector)
  - _out_char from printf.o(.text._out_char) referenced 2 times from printf.o(.text.printf_)
  - _out_null from printf.o(.text._out_null) referenced 2 times from printf.o(.text._vsnprintf)
  - alarm_callback from main.o(.text.alarm_callback) referenced from rtc_config.o(.data.rtc_config0Alarm)
  - eTMR0_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Fault_IRQHandler from vector_table_copy.o(.text.eTMR0_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR0_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Fault_IRQHandler from vector_table_copy.o(.text.eTMR1_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR1_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR2_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR2_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR2_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR2_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Fault_IRQHandler from vector_table_copy.o(.text.eTMR2_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR2_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR2_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR3_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR3_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR3_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR3_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Fault_IRQHandler from vector_table_copy.o(.text.eTMR3_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR3_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR3_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR4_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR4_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR4_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR4_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Fault_IRQHandler from vector_table_copy.o(.text.eTMR4_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR4_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR4_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR5_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR5_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR5_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR5_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Fault_IRQHandler from vector_table_copy.o(.text.eTMR5_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR5_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR5_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - lpTMR0_IRQHandler from vector_table_copy.o(.text.lpTMR0_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR0_Ch0_IRQHandler from vector_table_copy.o(.text.pTMR0_Ch0_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR0_Ch1_IRQHandler from vector_table_copy.o(.text.pTMR0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR0_Ch2_IRQHandler from vector_table_copy.o(.text.pTMR0_Ch2_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR0_Ch3_IRQHandler from vector_table_copy.o(.text.pTMR0_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR1_Ch0_IRQHandler from vector_table_copy.o(.text.pTMR1_Ch0_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR1_Ch1_IRQHandler from vector_table_copy.o(.text.pTMR1_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR1_Ch2_IRQHandler from vector_table_copy.o(.text.pTMR1_Ch2_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR1_Ch3_IRQHandler from vector_table_copy.o(.text.pTMR1_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR2_Ch0_IRQHandler from vector_table_copy.o(.text.pTMR2_Ch0_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR2_Ch1_IRQHandler from vector_table_copy.o(.text.pTMR2_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR2_Ch2_IRQHandler from vector_table_copy.o(.text.pTMR2_Ch2_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR2_Ch3_IRQHandler from vector_table_copy.o(.text.pTMR2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - second_callback from main.o(.text.second_callback) referenced from rtc_config.o(.data.rtc_config0Seconds)

  ### Global Symbols

  RamInit0 (Thumb, 0 bytes, Stack size unknown bytes, raminit0.o(.text))
  [Called By]

  - >> Reset_Handler

  Reset_Handler (Thumb, 0 bytes, Stack size unknown bytes, startup.o(.text))
  [Stack]

  - Max Depth = 608 + Unknown Stack Size
  - Call Chain = Reset_Handler ⇒ main ⇒ printf_ ⇒ _vsnprintf ⇒ _ftoa ⇒ _etoa ⇒ _ftoa (Cycle)
  [Calls]
  - >> RamInit0
  - >> main
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_uldivmod
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _ntoa_long_long

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> VectorTableCopy

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr
  - >> _ntoa_format
  - >> _ftoa

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> _ftoa

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text))
  [Calls]

  - >> __aeabi_memset
  [Called By]
  - >> LINFlexD_UART_DRV_Init
  - >> DMA_DRV_ClearStructure

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> RamInit1

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_dadd (Thumb, 322 bytes, Stack size 48 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_lasr
  - >> __aeabi_llsl
  - >> _double_round
  - >> _double_epilogue
  [Called By]
  - >> __aeabi_drsub
  - >> __aeabi_dsub
  - >> _etoa

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dsub ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> _ftoa
  - >> _etoa

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> _ftoa
  - >> _etoa

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> _double_round
  [Called By]
  - >> _etoa

  __aeabi_dcmple (Thumb, 54 bytes, Stack size 12 bytes, dcmple.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = __aeabi_dcmple
  [Called By]
  - >> _ftoa

  __aeabi_dcmplt (Thumb, 54 bytes, Stack size 12 bytes, dcmplt.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = __aeabi_dcmplt
  [Called By]
  - >> _ftoa
  - >> _etoa

  __aeabi_dcmpge (Thumb, 54 bytes, Stack size 12 bytes, dcmpge.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = __aeabi_dcmpge
  [Called By]
  - >> _ftoa
  - >> _etoa

  __aeabi_dcmpgt (Thumb, 54 bytes, Stack size 12 bytes, dcmpgt.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = __aeabi_dcmpgt
  [Called By]
  - >> _ftoa
  - >> _etoa

  __aeabi_i2d (Thumb, 34 bytes, Stack size 16 bytes, dflti.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_i2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> _ftoa
  - >> _etoa

  __aeabi_ui2d (Thumb, 26 bytes, Stack size 16 bytes, dfltui.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_ui2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> _ftoa

  __aeabi_d2iz (Thumb, 62 bytes, Stack size 16 bytes, dfixi.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_d2iz
  [Calls]
  - >> __aeabi_llsr
  [Called By]
  - >> _ftoa
  - >> _etoa

  __aeabi_d2uiz (Thumb, 50 bytes, Stack size 8 bytes, dfixui.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_d2uiz
  [Calls]
  - >> __aeabi_llsr
  [Called By]
  - >> _ftoa

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> _double_epilogue
  - >> __aeabi_uldivmod
  - >> __aeabi_dadd

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> _double_epilogue
  - >> __aeabi_uldivmod
  - >> __aeabi_d2uiz
  - >> __aeabi_d2iz

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text))
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  __I$use$fp (Thumb, 0 bytes, Stack size 8 bytes, iusefp.o(.text), UNUSED)

  _double_round (Thumb, 30 bytes, Stack size 8 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _double_round
  [Called By]
  - >> _double_epilogue
  - >> __aeabi_ddiv
  - >> __aeabi_dadd

  _double_epilogue (Thumb, 156 bytes, Stack size 32 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  - >> _double_round
  [Called By]
  - >> __aeabi_ui2d
  - >> __aeabi_i2d
  - >> __aeabi_dmul
  - >> __aeabi_dadd

  ACMP0_IRQHandler (Thumb, 0 bytes, Stack size 8 bytes, vector_table_copy.o(.text.ACMP0_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = ACMP0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  ACMP1_IRQHandler (Thumb, 0 bytes, Stack size 8 bytes, vector_table_copy.o(.text.ACMP1_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = ACMP1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  ADC0_IRQHandler (Thumb, 0 bytes, Stack size 8 bytes, vector_table_copy.o(.text.ADC0_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  ADC1_IRQHandler (Thumb, 0 bytes, Stack size 8 bytes, vector_table_copy.o(.text.ADC1_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  BusFault_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.BusFault_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_112_127_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_112_127_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_32_47_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_32_47_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_48_63_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_48_63_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_64_79_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_64_79_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_80_95_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_80_95_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_96_111_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_96_111_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_ORed_BusOff_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_ORed_BusOff_Warning_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN0_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_112_127_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_112_127_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_32_47_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_32_47_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_48_63_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_48_63_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_64_79_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_64_79_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_80_95_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_80_95_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_96_111_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_96_111_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_ORed_BusOff_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_ORed_BusOff_Warning_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN1_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN1_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN2_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN2_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN2_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN2_ORed_32_47_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_32_47_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN2_ORed_48_63_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_48_63_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN2_ORed_BusOff_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_ORed_BusOff_Warning_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN2_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN2_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN3_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN3_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN3_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN3_ORed_32_47_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_32_47_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN3_ORed_48_63_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_48_63_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN3_ORed_BusOff_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_ORed_BusOff_Warning_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN3_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN3_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN4_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN4_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN4_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN4_ORed_32_47_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_32_47_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN4_ORed_48_63_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_48_63_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN4_ORed_BusOff_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_ORed_BusOff_Warning_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN4_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN4_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN5_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN5_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN5_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN5_ORed_BusOff_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_ORed_BusOff_Warning_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN5_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN5_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN6_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN6_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN6_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN6_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN6_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN6_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN6_ORed_BusOff_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN6_ORed_BusOff_Warning_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN6_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN6_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN7_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN7_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN7_ORed_0_15_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN7_ORed_0_15_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN7_ORed_16_31_MB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN7_ORed_16_31_MB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN7_ORed_BusOff_Warning_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN7_ORed_BusOff_Warning_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN7_Wake_Up_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CAN7_Wake_Up_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CLOCK_DRV_GetFreq (Thumb, 362 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.CLOCK_DRV_GetFreq))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> CLOCK_DRV_GetPllFreq
  - >> SCU_GetSysClkSrc
  - >> SCU_GetSysClkDiv
  - >> SCU_GetSlowBusClkDiv
  - >> SCU_GetFastBusClkDiv
  - >> CLOCK_GetIpcCtrlReg
  [Called By]
  - >> CLOCK_SYS_GetFreq

  CLOCK_DRV_GetPllFreq (Thumb, 68 bytes, Stack size 16 bytes, clock_ytm32b1hx.o(.text.CLOCK_DRV_GetPllFreq))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_DRV_GetPllFreq
  [Calls]
  - >> SCU_GetPllRefClkDiv
  - >> SCU_GetPllRefClk
  - >> SCU_GetPllLock
  - >> SCU_GetPllFeedBackDiv
  [Called By]
  - >> CLOCK_DRV_GetFreq
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_DRV_Init (Thumb, 26 bytes, Stack size 8 bytes, clock_ytm32b1hx.o(.text.CLOCK_DRV_Init))
  [Stack]

  - Max Depth = 64
  - Call Chain = CLOCK_DRV_Init ⇒ CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_WaitFXOSCValid
  [Calls]
  - >> CLOCK_SYS_SetScuConfiguration
  - >> CLOCK_SYS_SetIpcConfiguration
  [Called By]
  - >> CLOCK_SYS_SetConfiguration

  CLOCK_SYS_GetFreq (Thumb, 4 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_GetFreq))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> CLOCK_DRV_GetFreq
  [Called By]
  - >> LINFlexD_UART_DRV_Init
  - >> LINFlexD_UART_DRV_Deinit
  - >> CLOCK_SYS_SetScuConfiguration
  - >> LINFlexD_UART_DRV_SetBaudRate
  - >> osif_UpdateTickConfig

  CLOCK_SYS_Init (Thumb, 56 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_Init))
  [Called By]

  - >> Board_Init

  CLOCK_SYS_SetConfiguration (Thumb, 4 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_SetConfiguration))
  [Stack]

  - Max Depth = 64
  - Call Chain = CLOCK_SYS_SetConfiguration ⇒ CLOCK_DRV_Init ⇒ CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_WaitFXOSCValid
  [Calls]
  - >> CLOCK_DRV_Init
  [Called By]
  - >> CLOCK_SYS_UpdateConfiguration

  CLOCK_SYS_UpdateConfiguration (Thumb, 288 bytes, Stack size 40 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_UpdateConfiguration))
  [Stack]

  - Max Depth = 104
  - Call Chain = CLOCK_SYS_UpdateConfiguration ⇒ CLOCK_SYS_SetConfiguration ⇒ CLOCK_DRV_Init ⇒ CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_WaitFXOSCValid
  [Calls]
  - >> INT_SYS_EnableIRQGlobal
  - >> INT_SYS_DisableIRQGlobal
  - >> CLOCK_SYS_SetConfiguration
  [Called By]
  - >> Board_Init

  CLOCK_SYS_WaitFXOSCValid (Thumb, 94 bytes, Stack size 32 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_WaitFXOSCValid))
  [Stack]

  - Max Depth = 32
  - Call Chain = CLOCK_SYS_WaitFXOSCValid
  [Calls]
  - >> SCU_SetFxoscGain
  - >> SCU_GetFXOSCValid
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration
  - >> POWER_SYS_SwitchToLowPowerMode

  CMU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CMU_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CORE_CTI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.CORE_CTI_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DMA0_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA0_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA0_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA10_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA10_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA10_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA11_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA11_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA11_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA12_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA12_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA12_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA13_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA13_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA13_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA14_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA14_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA14_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA15_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA15_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA15_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA16_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA16_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA16_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA17_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA17_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA17_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA18_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA18_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA18_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA19_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA19_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA19_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA1_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA1_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA1_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA20_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA20_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA20_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA21_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA21_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA21_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA22_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA22_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA22_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA23_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA23_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA23_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA24_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA24_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA24_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA25_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA25_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA25_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA26_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA26_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA26_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA27_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA27_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA27_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA28_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA28_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA28_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA29_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA29_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA29_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA2_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA2_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA2_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA30_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA30_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA30_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA31_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA31_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA31_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA3_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA3_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA3_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA4_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA4_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA4_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA5_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA5_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA5_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA6_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA6_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA6_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA7_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA7_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA7_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA8_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA8_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA8_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA9_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA9_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA9_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMAMUX_Init (Thumb, 16 bytes, Stack size 0 bytes, dma_hw_access.o(.text.DMAMUX_Init))
  [Called By]

  - >> DMA_DRV_Init

  DMA_CTSClearReg (Thumb, 56 bytes, Stack size 0 bytes, dma_hw_access.o(.text.DMA_CTSClearReg))
  [Called By]

  - >> DMA_Init
  - >> DMA_DRV_ConfigSingleBlockTransfer
  - >> DMA_DRV_ChannelInit

  DMA_CTSSetAttribute (Thumb, 36 bytes, Stack size 8 bytes, dma_hw_access.o(.text.DMA_CTSSetAttribute))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_CTSSetAttribute
  [Called By]
  - >> DMA_DRV_ConfigSingleBlockTransfer

  DMA_CTSSetNbytes (Thumb, 48 bytes, Stack size 0 bytes, dma_hw_access.o(.text.DMA_CTSSetNbytes))
  [Called By]

  - >> DMA_DRV_ConfigSingleBlockTransfer

  DMA_CTSSetTriggerCount (Thumb, 70 bytes, Stack size 0 bytes, dma_hw_access.o(.text.DMA_CTSSetTriggerCount))
  [Called By]

  - >> DMA_DRV_SetTriggerLoopIterationCount
  - >> DMA_DRV_ConfigSingleBlockTransfer
  - >> DMA_DRV_ConfigMultiBlockTransfer

  DMA_DRV_ChannelInit (Thumb, 98 bytes, Stack size 24 bytes, dma_driver.o(.text.DMA_DRV_ChannelInit))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA_DRV_ChannelInit ⇒ DMA_DRV_SetChannelRequestAndTrigger
  [Calls]
  - >> DMA_SetErrorIntCmd
  - >> DMA_DRV_SetChannelRequestAndTrigger
  - >> DMA_DRV_InstallCallback
  - >> DMA_CTSClearReg
  - >> DMA_DRV_ClearStructure
  [Called By]
  - >> DMA_DRV_Init

  DMA_DRV_ConfigMultiBlockTransfer (Thumb, 62 bytes, Stack size 32 bytes, dma_driver.o(.text.DMA_DRV_ConfigMultiBlockTransfer))
  [Stack]

  - Max Depth = 88
  - Call Chain = DMA_DRV_ConfigMultiBlockTransfer ⇒ DMA_DRV_ConfigSingleBlockTransfer ⇒ DMA_CTSSetAttribute
  [Calls]
  - >> DMA_DRV_ConfigSingleBlockTransfer
  - >> DMA_CTSSetTriggerCount
  - >> DMA_CTSSetDisableDmaRequestAfterCTSDoneCmd
  [Called By]
  - >> LINFlexD_UART_DRV_StartSendUsingDma
  - >> LINFlexD_UART_DRV_StartReceiveUsingDma

  DMA_DRV_ConfigSingleBlockTransfer (Thumb, 264 bytes, Stack size 48 bytes, dma_driver.o(.text.DMA_DRV_ConfigSingleBlockTransfer))
  [Stack]

  - Max Depth = 56
  - Call Chain = DMA_DRV_ConfigSingleBlockTransfer ⇒ DMA_CTSSetAttribute
  [Calls]
  - >> DMA_SetDmaRequestCmd
  - >> DMA_CTSSetTriggerCount
  - >> DMA_CTSSetNbytes
  - >> DMA_CTSSetAttribute
  - >> DMA_CTSClearReg
  - >> DMA_SetTransferLoopMappingCmd
  - >> DMA_CTSSetSrcOffset
  - >> DMA_CTSSetSrcAddr
  - >> DMA_CTSSetMajorCompleteIntCmd
  - >> DMA_CTSSetEngineStall
  - >> DMA_CTSSetDestOffset
  - >> DMA_CTSSetDestAddr
  [Called By]
  - >> DMA_DRV_ConfigMultiBlockTransfer

  DMA_DRV_Deinit (Thumb, 80 bytes, Stack size 16 bytes, dma_driver.o(.text.DMA_DRV_Deinit))
  [Stack]

  - Max Depth = 48
  - Call Chain = DMA_DRV_Deinit ⇒ DMA_DRV_ReleaseChannel ⇒ DMA_DRV_ClearStructure
  [Calls]
  - >> DMA_DRV_ReleaseChannel
  - >> INT_SYS_DisableIRQ
  [Called By]
  - >> main

  DMA_DRV_ErrorIRQHandler (Thumb, 76 bytes, Stack size 16 bytes, dma_driver.o(.text.DMA_DRV_ErrorIRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA_DRV_ErrorIRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_SetDmaRequestCmd
  - >> DMA_DRV_ClearIntStatus
  - >> DMA_ClearErrorIntStatusFlag
  [Called By]
  - >> DMA_Error_IRQHandler

  DMA_DRV_GetDmaRegBaseAddr (Thumb, 8 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_DRV_GetDmaRegBaseAddr))
  [Called By]

  - >> DMA_Error_IRQHandler

  DMA_DRV_IRQHandler (Thumb, 42 bytes, Stack size 8 bytes, dma_driver.o(.text.DMA_DRV_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_ClearIntStatus
  [Called By]
  - >> DMA9_IRQHandler
  - >> DMA8_IRQHandler
  - >> DMA7_IRQHandler
  - >> DMA6_IRQHandler
  - >> DMA5_IRQHandler
  - >> DMA4_IRQHandler
  - >> DMA3_IRQHandler
  - >> DMA31_IRQHandler
  - >> DMA30_IRQHandler
  - >> DMA2_IRQHandler
  - >> DMA29_IRQHandler
  - >> DMA28_IRQHandler
  - >> DMA27_IRQHandler
  - >> DMA26_IRQHandler
  - >> DMA25_IRQHandler
  - >> DMA24_IRQHandler
  - >> DMA23_IRQHandler
  - >> DMA22_IRQHandler
  - >> DMA21_IRQHandler
  - >> DMA20_IRQHandler
  - >> DMA1_IRQHandler
  - >> DMA19_IRQHandler
  - >> DMA18_IRQHandler
  - >> DMA17_IRQHandler
  - >> DMA16_IRQHandler
  - >> DMA15_IRQHandler
  - >> DMA14_IRQHandler
  - >> DMA13_IRQHandler
  - >> DMA12_IRQHandler
  - >> DMA11_IRQHandler
  - >> DMA10_IRQHandler
  - >> DMA0_IRQHandler

  DMA_DRV_Init (Thumb, 136 bytes, Stack size 32 bytes, dma_driver.o(.text.DMA_DRV_Init))
  [Stack]

  - Max Depth = 64
  - Call Chain = DMA_DRV_Init ⇒ DMA_DRV_ChannelInit ⇒ DMA_DRV_SetChannelRequestAndTrigger
  [Calls]
  - >> INT_SYS_EnableIRQ
  - >> DMA_Init
  - >> DMA_DRV_ChannelInit
  - >> DMAMUX_Init
  - >> DMA_SetHaltOnErrorCmd
  - >> DMA_DRV_ClearStructure
  [Called By]
  - >> main

  DMA_DRV_InstallCallback (Thumb, 28 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_DRV_InstallCallback))
  [Called By]

  - >> DMA_DRV_ChannelInit
  - >> LINFlexD_UART_DRV_StartSendUsingDma
  - >> LINFlexD_UART_DRV_StartReceiveUsingDma

  DMA_DRV_ReleaseChannel (Thumb, 58 bytes, Stack size 24 bytes, dma_driver.o(.text.DMA_DRV_ReleaseChannel))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA_DRV_ReleaseChannel ⇒ DMA_DRV_ClearStructure
  [Calls]
  - >> DMA_SetDmaRequestCmd
  - >> DMA_DRV_ClearStructure
  [Called By]
  - >> main
  - >> DMA_DRV_Deinit

  DMA_DRV_SetChannelRequestAndTrigger (Thumb, 20 bytes, Stack size 8 bytes, dma_driver.o(.text.DMA_DRV_SetChannelRequestAndTrigger))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_DRV_SetChannelRequestAndTrigger
  [Calls]
  - >> DMAMUX_SetChannelSource
  [Called By]
  - >> DMA_DRV_ChannelInit

  DMA_DRV_SetDestAddr (Thumb, 20 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_DRV_SetDestAddr))
  [Calls]

  - >> DMA_CTSSetDestAddr
  [Called By]
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingDma

  DMA_DRV_SetSrcAddr (Thumb, 20 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_DRV_SetSrcAddr))
  [Calls]

  - >> DMA_CTSSetSrcAddr
  [Called By]
  - >> LINFlexD_UART_DRV_CompleteSendUsingDma

  DMA_DRV_SetTriggerLoopIterationCount (Thumb, 20 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_DRV_SetTriggerLoopIterationCount))
  [Calls]

  - >> DMA_CTSSetTriggerCount
  [Called By]
  - >> LINFlexD_UART_DRV_CompleteSendUsingDma
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingDma

  DMA_DRV_StartChannel (Thumb, 22 bytes, Stack size 8 bytes, dma_driver.o(.text.DMA_DRV_StartChannel))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_DRV_StartChannel
  [Calls]
  - >> DMA_SetDmaRequestCmd
  [Called By]
  - >> main
  - >> LINFlexD_UART_DRV_StartSendUsingDma
  - >> LINFlexD_UART_DRV_StartReceiveUsingDma
  - >> LINFlexD_UART_DRV_CompleteSendUsingDma
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingDma

  DMA_DRV_StopChannel (Thumb, 22 bytes, Stack size 8 bytes, dma_driver.o(.text.DMA_DRV_StopChannel))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_DRV_StopChannel
  [Calls]
  - >> DMA_SetDmaRequestCmd
  [Called By]
  - >> main
  - >> LINFlexD_UART_DRV_CompleteSendUsingDma
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingDma

  DMA_Error_IRQHandler (Thumb, 44 bytes, Stack size 16 bytes, dma_irq.o(.text.DMA_Error_IRQHandler))
  [Stack]

  - Max Depth = 48
  - Call Chain = DMA_Error_IRQHandler ⇒ DMA_DRV_ErrorIRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_GetErrorIntStatusFlag
  - >> DMA_DRV_GetDmaRegBaseAddr
  - >> DMA_DRV_ErrorIRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA_Init (Thumb, 38 bytes, Stack size 16 bytes, dma_hw_access.o(.text.DMA_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = DMA_Init
  [Calls]
  - >> DMA_CTSClearReg
  [Called By]
  - >> DMA_DRV_Init

  DMA_SetDmaRequestCmd (Thumb, 22 bytes, Stack size 0 bytes, dma_hw_access.o(.text.DMA_SetDmaRequestCmd))
  [Called By]

  - >> DMA_DRV_StopChannel
  - >> DMA_DRV_StartChannel
  - >> DMA_DRV_ReleaseChannel
  - >> DMA_DRV_ErrorIRQHandler
  - >> DMA_DRV_ConfigSingleBlockTransfer

  DMA_SetErrorIntCmd (Thumb, 22 bytes, Stack size 0 bytes, dma_hw_access.o(.text.DMA_SetErrorIntCmd))
  [Called By]

  - >> DMA_DRV_ChannelInit

  DebugMon_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DebugMon_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DefaultISR (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DefaultISR))
  [Calls]

  - >> DefaultISR
  [Called By]
  - >> DefaultISR
  [Address Reference Count : 2]
  - vector.o(.isr_vector)
  - linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_Deinit)

  EFM_Ecc_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_Ecc_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  EFM_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  EFM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  EMU0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EMU0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  ENET_ECC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ENET_ECC_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  ENET_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ENET_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  ENET_RX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ENET_RX_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  ENET_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.ENET_TX_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  FMU_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.FMU_Alarm_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  FMU_MISC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.FMU_MISC_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.FPU_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOA_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOC_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOD_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOE_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  HCU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.HCU_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  HardFault_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.HardFault_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  I2C0_Master_Slave_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C0_Master_Slave_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  I2C1_Master_Slave_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C1_Master_Slave_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  I2C2_Master_Slave_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C2_Master_Slave_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  I2C3_Master_Slave_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C3_Master_Slave_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  I2C4_Master_Slave_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C4_Master_Slave_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  INTM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.INTM_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  INT_SYS_ClearPending (Thumb, 4 bytes, Stack size 0 bytes, interrupt_manager.o(.text.INT_SYS_ClearPending))
  [Calls]

  - >> __NVIC_ClearPendingIRQ
  [Called By]
  - >> RTC_DRV_Init
  - >> RTC_DRV_Deinit

  INT_SYS_DisableIRQ (Thumb, 4 bytes, Stack size 0 bytes, interrupt_manager.o(.text.INT_SYS_DisableIRQ))
  [Calls]

  - >> __NVIC_DisableIRQ
  [Called By]
  - >> RTC_DRV_Init
  - >> RTC_DRV_Deinit
  - >> LINFlexD_UART_DRV_Deinit
  - >> DMA_DRV_Deinit
  - >> RTC_DRV_ConfigureSecondsInt
  - >> RTC_DRV_ConfigureOverflowInt
  - >> RTC_DRV_ConfigureAlarmInt

  INT_SYS_DisableIRQGlobal (Thumb, 18 bytes, Stack size 0 bytes, interrupt_manager.o(.text.INT_SYS_DisableIRQGlobal))
  [Called By]

  - >> CLOCK_SYS_UpdateConfiguration
  - >> osif_DisableIrqGlobal

  INT_SYS_EnableIRQ (Thumb, 4 bytes, Stack size 0 bytes, interrupt_manager.o(.text.INT_SYS_EnableIRQ))
  [Calls]

  - >> __NVIC_EnableIRQ
  [Called By]
  - >> LINFlexD_UART_DRV_Init
  - >> DMA_DRV_Init
  - >> RTC_DRV_ConfigureSecondsInt
  - >> RTC_DRV_ConfigureOverflowInt
  - >> RTC_DRV_ConfigureAlarmInt

  INT_SYS_EnableIRQGlobal (Thumb, 28 bytes, Stack size 0 bytes, interrupt_manager.o(.text.INT_SYS_EnableIRQGlobal))
  [Called By]

  - >> CLOCK_SYS_UpdateConfiguration
  - >> osif_EnableIrqGlobal

  INT_SYS_InstallHandler (Thumb, 128 bytes, Stack size 16 bytes, interrupt_manager.o(.text.INT_SYS_InstallHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = INT_SYS_InstallHandler
  [Called By]
  - >> LINFlexD_UART_DRV_Init
  - >> LINFlexD_UART_DRV_Deinit

  LINFlexD0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD0_UART_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, linflexd_uart_irq.o(.text.LINFlexD0_UART_IRQHandler))
  [Stack]

  - Max Depth = 56
  - Call Chain = LINFlexD0_UART_IRQHandler ⇒ LINFlexD_UART_DRV_IRQHandler ⇒ LINFlexD_UART_DRV_TxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost
  [Calls]
  - >> LINFlexD_UART_DRV_IRQHandler
  [Address Reference Count : 1]
  - linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)

  LINFlexD1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD1_UART_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, linflexd_uart_irq.o(.text.LINFlexD1_UART_IRQHandler))
  [Stack]

  - Max Depth = 56
  - Call Chain = LINFlexD1_UART_IRQHandler ⇒ LINFlexD_UART_DRV_IRQHandler ⇒ LINFlexD_UART_DRV_TxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost
  [Calls]
  - >> LINFlexD_UART_DRV_IRQHandler
  [Address Reference Count : 1]
  - linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)

  LINFlexD2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD2_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD2_UART_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, linflexd_uart_irq.o(.text.LINFlexD2_UART_IRQHandler))
  [Stack]

  - Max Depth = 56
  - Call Chain = LINFlexD2_UART_IRQHandler ⇒ LINFlexD_UART_DRV_IRQHandler ⇒ LINFlexD_UART_DRV_TxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost
  [Calls]
  - >> LINFlexD_UART_DRV_IRQHandler
  [Address Reference Count : 1]
  - linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)

  LINFlexD3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD3_UART_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, linflexd_uart_irq.o(.text.LINFlexD3_UART_IRQHandler))
  [Stack]

  - Max Depth = 56
  - Call Chain = LINFlexD3_UART_IRQHandler ⇒ LINFlexD_UART_DRV_IRQHandler ⇒ LINFlexD_UART_DRV_TxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost
  [Calls]
  - >> LINFlexD_UART_DRV_IRQHandler
  [Address Reference Count : 1]
  - linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)

  LINFlexD4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD4_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD4_UART_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, linflexd_uart_irq.o(.text.LINFlexD4_UART_IRQHandler))
  [Stack]

  - Max Depth = 56
  - Call Chain = LINFlexD4_UART_IRQHandler ⇒ LINFlexD_UART_DRV_IRQHandler ⇒ LINFlexD_UART_DRV_TxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost
  [Calls]
  - >> LINFlexD_UART_DRV_IRQHandler
  [Address Reference Count : 1]
  - linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)

  LINFlexD5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD5_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD5_UART_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, linflexd_uart_irq.o(.text.LINFlexD5_UART_IRQHandler))
  [Stack]

  - Max Depth = 56
  - Call Chain = LINFlexD5_UART_IRQHandler ⇒ LINFlexD_UART_DRV_IRQHandler ⇒ LINFlexD_UART_DRV_TxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost
  [Calls]
  - >> LINFlexD_UART_DRV_IRQHandler
  [Address Reference Count : 1]
  - linflexd_uart_irq.o(.rodata.g_uartLINFlexDIsr)

  LINFlexD6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD6_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD7_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD8_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.LINFlexD9_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  LINFlexD_UART_DRV_AbortReceivingData (Thumb, 50 bytes, Stack size 8 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_AbortReceivingData))
  [Stack]

  - Max Depth = 32
  - Call Chain = LINFlexD_UART_DRV_AbortReceivingData ⇒ LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts ⇒ OSIF_SemaPost
  [Calls]
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingDma
  [Called By]
  - >> main

  LINFlexD_UART_DRV_AbortSendingData (Thumb, 50 bytes, Stack size 8 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_AbortSendingData))
  [Stack]

  - Max Depth = 32
  - Call Chain = LINFlexD_UART_DRV_AbortSendingData ⇒ LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost
  [Calls]
  - >> LINFlexD_UART_DRV_CompleteSendUsingInterrupts
  - >> LINFlexD_UART_DRV_CompleteSendUsingDma
  [Called By]
  - >> main

  LINFlexD_UART_DRV_Deinit (Thumb, 156 bytes, Stack size 32 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_Deinit))
  [Stack]

  - Max Depth = 48
  - Call Chain = LINFlexD_UART_DRV_Deinit ⇒ INT_SYS_InstallHandler
  [Calls]
  - >> INT_SYS_InstallHandler
  - >> INT_SYS_DisableIRQ
  - >> CLOCK_SYS_GetFreq
  - >> OSIF_SemaDestroy
  - >> LINFlexD_SetInterruptMode
  [Called By]
  - >> main

  LINFlexD_UART_DRV_ErrIRQHandler (Thumb, 124 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_ErrIRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = LINFlexD_UART_DRV_ErrIRQHandler ⇒ LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts ⇒ OSIF_SemaPost
  [Calls]
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingDma
  - >> LINFlexD_GetStatusFlag
  - >> LINFlexD_ClearStatusFlag
  [Called By]
  - >> LINFlexD_UART_DRV_IRQHandler

  LINFlexD_UART_DRV_IRQHandler (Thumb, 100 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_IRQHandler))
  [Stack]

  - Max Depth = 56
  - Call Chain = LINFlexD_UART_DRV_IRQHandler ⇒ LINFlexD_UART_DRV_TxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost
  [Calls]
  - >> LINFlexD_UART_DRV_TxIRQHandler
  - >> LINFlexD_UART_DRV_RxTOHandler
  - >> LINFlexD_UART_DRV_RxIRQHandler
  - >> LINFlexD_UART_DRV_ErrIRQHandler
  - >> LINFlexD_IsInterruptEnabled
  - >> LINFlexD_GetStatusFlag
  [Called By]
  - >> LINFlexD5_UART_IRQHandler
  - >> LINFlexD4_UART_IRQHandler
  - >> LINFlexD3_UART_IRQHandler
  - >> LINFlexD2_UART_IRQHandler
  - >> LINFlexD1_UART_IRQHandler
  - >> LINFlexD0_UART_IRQHandler

  LINFlexD_UART_DRV_Init (Thumb, 324 bytes, Stack size 32 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = LINFlexD_UART_DRV_Init ⇒ LINFlexD_UART_DRV_SetBaudRate ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> INT_SYS_InstallHandler
  - >> INT_SYS_EnableIRQ
  - >> CLOCK_SYS_GetFreq
  - >> OSIF_SemaCreate
  - >> LINFlexD_UART_DRV_SetBaudRate
  - >> LINFlexD_SetUartWordLength
  - >> LINFlexD_SetTxStopBitsCount
  - >> LINFlexD_SetTxMode
  - >> LINFlexD_SetTxDataFieldLength
  - >> LINFlexD_SetRxStopBitsCount
  - >> LINFlexD_SetRxMode
  - >> LINFlexD_SetRxDataFieldLength
  - >> LINFlexD_SetParityType
  - >> LINFlexD_SetParityControl
  - >> LINFlexD_SetMode
  - >> LINFlexD_SetInterruptMode
  - >> LINFlexD_GetLinState
  - >> LINFlexD_EnterNormalMode
  - >> LINFlexD_EnterInitMode
  - >> __aeabi_memclr
  [Called By]
  - >> main
  - >> UTILITY_PRINT_Init

  LINFlexD_UART_DRV_ReceiveDataBlocking (Thumb, 134 bytes, Stack size 32 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_ReceiveDataBlocking))
  [Stack]

  - Max Depth = 160
  - Call Chain = LINFlexD_UART_DRV_ReceiveDataBlocking ⇒ LINFlexD_UART_DRV_StartReceiveUsingDma ⇒ DMA_DRV_ConfigMultiBlockTransfer ⇒ DMA_DRV_ConfigSingleBlockTransfer ⇒ DMA_CTSSetAttribute
  [Calls]
  - >> OSIF_SemaWait
  - >> LINFlexD_UART_DRV_StartReceiveUsingInterrupts
  - >> LINFlexD_UART_DRV_StartReceiveUsingDma
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingDma
  [Called By]
  - >> main

  LINFlexD_UART_DRV_RxIRQHandler (Thumb, 124 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_RxIRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = LINFlexD_UART_DRV_RxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts ⇒ OSIF_SemaPost
  [Calls]
  - >> LINFlexD_UART_DRV_GetData
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts
  - >> LINFlexD_ClearStatusFlag
  [Called By]
  - >> LINFlexD_UART_DRV_IRQHandler

  LINFlexD_UART_DRV_RxTOHandler (Thumb, 120 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_RxTOHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = LINFlexD_UART_DRV_RxTOHandler ⇒ LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts ⇒ OSIF_SemaPost
  [Calls]
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts
  - >> LINFlexD_SetInterruptMode
  - >> LINFlexD_SetIdleTimeoutValue
  - >> LINFlexD_GetStatusFlag
  - >> LINFlexD_ClearStatusFlag
  [Called By]
  - >> LINFlexD_UART_DRV_IRQHandler

  LINFlexD_UART_DRV_SendDataBlocking (Thumb, 134 bytes, Stack size 32 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_SendDataBlocking))
  [Stack]

  - Max Depth = 160
  - Call Chain = LINFlexD_UART_DRV_SendDataBlocking ⇒ LINFlexD_UART_DRV_StartSendUsingDma ⇒ DMA_DRV_ConfigMultiBlockTransfer ⇒ DMA_DRV_ConfigSingleBlockTransfer ⇒ DMA_CTSSetAttribute
  [Calls]
  - >> OSIF_SemaWait
  - >> LINFlexD_UART_DRV_StartSendUsingInterrupts
  - >> LINFlexD_UART_DRV_StartSendUsingDma
  - >> LINFlexD_UART_DRV_CompleteSendUsingInterrupts
  - >> LINFlexD_UART_DRV_CompleteSendUsingDma
  [Called By]
  - >> main

  LINFlexD_UART_DRV_SendDataPolling (Thumb, 156 bytes, Stack size 24 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_SendDataPolling))
  [Stack]

  - Max Depth = 40
  - Call Chain = LINFlexD_UART_DRV_SendDataPolling ⇒ LINFlexD_UART_DRV_PutData
  [Calls]
  - >> LINFlexD_UART_DRV_PutData
  - >> LINFlexD_SetTransmitterState
  - >> LINFlexD_GetStatusFlag
  - >> LINFlexD_ClearStatusFlag
  [Called By]
  - >> printf_char

  LINFlexD_UART_DRV_SetBaudRate (Thumb, 210 bytes, Stack size 24 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_SetBaudRate))
  [Stack]

  - Max Depth = 40
  - Call Chain = LINFlexD_UART_DRV_SetBaudRate ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> CLOCK_SYS_GetFreq
  - >> LINFlexD_SetIntegerBaudRate
  - >> LINFlexD_SetFractionalBaudRate
  - >> LINFlexD_GetLinState
  - >> LINFlexD_EnterNormalMode
  - >> LINFlexD_EnterInitMode
  [Called By]
  - >> LINFlexD_UART_DRV_Init

  LINFlexD_UART_DRV_TxIRQHandler (Thumb, 96 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_TxIRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = LINFlexD_UART_DRV_TxIRQHandler ⇒ LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost
  [Calls]
  - >> LINFlexD_UART_DRV_PutData
  - >> LINFlexD_UART_DRV_CompleteSendUsingInterrupts
  - >> LINFlexD_ClearStatusFlag
  [Called By]
  - >> LINFlexD_UART_DRV_IRQHandler

  MPWM0_Ch0_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch0_Ch7_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM0_Ch8_Ch15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch8_Ch15_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM1_Ch0_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM1_Ch0_Ch7_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM1_Ch8_Ch15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM1_Ch8_Ch15_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM2_Ch0_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM2_Ch0_Ch7_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM2_Ch8_Ch15_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM2_Ch8_Ch15_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MemManage_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MemManage_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  NMI_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.NMI_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  OSIF_SemaCreate (Thumb, 20 bytes, Stack size 0 bytes, osif_baremetal.o(.text.OSIF_SemaCreate))
  [Calls]

  - >> osif_EnableIrqGlobal
  - >> osif_DisableIrqGlobal
  [Called By]
  - >> LINFlexD_UART_DRV_Init

  OSIF_SemaDestroy (Thumb, 4 bytes, Stack size 0 bytes, osif_baremetal.o(.text.OSIF_SemaDestroy))
  [Called By]

  - >> LINFlexD_UART_DRV_Deinit

  OSIF_SemaPost (Thumb, 34 bytes, Stack size 8 bytes, osif_baremetal.o(.text.OSIF_SemaPost))
  [Stack]

  - Max Depth = 8
  - Call Chain = OSIF_SemaPost
  [Calls]
  - >> osif_EnableIrqGlobal
  - >> osif_DisableIrqGlobal
  [Called By]
  - >> LINFlexD_UART_DRV_CompleteSendUsingInterrupts
  - >> LINFlexD_UART_DRV_CompleteSendUsingDma
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingDma

  OSIF_SemaWait (Thumb, 106 bytes, Stack size 24 bytes, osif_baremetal.o(.text.OSIF_SemaWait))
  [Stack]

  - Max Depth = 64
  - Call Chain = OSIF_SemaWait ⇒ osif_UpdateTickConfig ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> osif_UpdateTickConfig
  - >> osif_GetCurrentTickCount
  - >> osif_EnableIrqGlobal
  - >> osif_DisableIrqGlobal
  [Called By]
  - >> LINFlexD_UART_DRV_SendDataBlocking
  - >> LINFlexD_UART_DRV_ReceiveDataBlocking

  OSIF_TimeDelay (Thumb, 40 bytes, Stack size 16 bytes, osif_baremetal.o(.text.OSIF_TimeDelay))
  [Stack]

  - Max Depth = 56
  - Call Chain = OSIF_TimeDelay ⇒ osif_UpdateTickConfig ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> osif_UpdateTickConfig
  - >> osif_GetCurrentTickCount
  [Called By]
  - >> main

  PCU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.PCU_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  PINS_DRV_Init (Thumb, 26 bytes, Stack size 16 bytes, pins_driver.o(.text.PINS_DRV_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = PINS_DRV_Init ⇒ PINS_Init ⇒ PINS_GPIO_WritePin
  [Calls]
  - >> PINS_Init
  [Called By]
  - >> Board_Init

  PINS_Init (Thumb, 252 bytes, Stack size 16 bytes, pins_port_hw_access.o(.text.PINS_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = PINS_Init ⇒ PINS_GPIO_WritePin
  [Calls]
  - >> PINS_GPIO_WritePin
  - >> PINS_ConfigDigitalFilter
  [Called By]
  - >> PINS_DRV_Init

  POWER_SYS_DoInit (Thumb, 4 bytes, Stack size 0 bytes, power_manager_ytm32b1hx.o(.text.POWER_SYS_DoInit))
  [Called By]

  - >> POWER_SYS_Init

  POWER_SYS_DoSetMode (Thumb, 10 bytes, Stack size 8 bytes, power_manager_ytm32b1hx.o(.text.POWER_SYS_DoSetMode))
  [Stack]

  - Max Depth = 64
  - Call Chain = POWER_SYS_DoSetMode ⇒ POWER_SYS_SwitchToLowPowerMode ⇒ CLOCK_SYS_WaitFXOSCValid
  [Calls]
  - >> POWER_SYS_SwitchToLowPowerMode
  [Called By]
  - >> POWER_SYS_SetMode

  POWER_SYS_Init (Thumb, 46 bytes, Stack size 0 bytes, power_manager.o(.text.POWER_SYS_Init))
  [Calls]

  - >> POWER_SYS_DoInit
  [Called By]
  - >> main

  POWER_SYS_SetMode (Thumb, 126 bytes, Stack size 32 bytes, power_manager.o(.text.POWER_SYS_SetMode))
  [Stack]

  - Max Depth = 96
  - Call Chain = POWER_SYS_SetMode ⇒ POWER_SYS_DoSetMode ⇒ POWER_SYS_SwitchToLowPowerMode ⇒ CLOCK_SYS_WaitFXOSCValid
  [Calls]
  - >> POWER_SYS_DoSetMode
  - >> POWER_SYS_CallbacksManagement
  [Called By]
  - >> main

  PTU0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.PTU0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  PTU1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.PTU1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  PendSV_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.PendSV_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  QSPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.QSPI_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  RTC_ConfigureClockOut (Thumb, 58 bytes, Stack size 0 bytes, rtc_hw_access.o(.text.RTC_ConfigureClockOut))
  [Called By]

  - >> RTC_DRV_Init

  RTC_DRV_ConfigureAlarmInt (Thumb, 96 bytes, Stack size 24 bytes, rtc_driver.o(.text.RTC_DRV_ConfigureAlarmInt))
  [Stack]

  - Max Depth = 56
  - Call Chain = RTC_DRV_ConfigureAlarmInt ⇒ RTC_DRV_ConvertTimeDateToSeconds
  [Calls]
  - >> INT_SYS_EnableIRQ
  - >> INT_SYS_DisableIRQ
  - >> RTC_DRV_IsTimeDateCorrectFormat
  - >> RTC_DRV_ConvertTimeDateToSeconds
  - >> RTC_SetTimeAlarmRegister
  - >> RTC_SetTimeAlarmIntEnable
  - >> RTC_GetTimeSecondsRegister
  [Called By]
  - >> RTC_DRV_Init

  RTC_DRV_ConfigureOverflowInt (Thumb, 48 bytes, Stack size 16 bytes, rtc_driver.o(.text.RTC_DRV_ConfigureOverflowInt))
  [Stack]

  - Max Depth = 16
  - Call Chain = RTC_DRV_ConfigureOverflowInt
  [Calls]
  - >> INT_SYS_EnableIRQ
  - >> INT_SYS_DisableIRQ
  - >> RTC_SetTimeOverflowIntEnable
  [Called By]
  - >> RTC_DRV_Init

  RTC_DRV_ConfigureSecondsInt (Thumb, 58 bytes, Stack size 16 bytes, rtc_driver.o(.text.RTC_DRV_ConfigureSecondsInt))
  [Stack]

  - Max Depth = 16
  - Call Chain = RTC_DRV_ConfigureSecondsInt
  [Calls]
  - >> INT_SYS_EnableIRQ
  - >> INT_SYS_DisableIRQ
  - >> RTC_SetTimeSecondsIntEnable
  - >> RTC_SetTimeSecondsIntConf
  [Called By]
  - >> RTC_DRV_Init

  RTC_DRV_ConvertSecondsToTimeDate (Thumb, 202 bytes, Stack size 24 bytes, rtc_driver.o(.text.RTC_DRV_ConvertSecondsToTimeDate))
  [Stack]

  - Max Depth = 24
  - Call Chain = RTC_DRV_ConvertSecondsToTimeDate
  [Calls]
  - >> RTC_DRV_IsYearLeap
  [Called By]
  - >> RTC_DRV_GetCurrentTimeDate

  RTC_DRV_ConvertTimeDateToSeconds (Thumb, 186 bytes, Stack size 32 bytes, rtc_driver.o(.text.RTC_DRV_ConvertTimeDateToSeconds))
  [Stack]

  - Max Depth = 32
  - Call Chain = RTC_DRV_ConvertTimeDateToSeconds
  [Calls]
  - >> RTC_DRV_IsYearLeap
  [Called By]
  - >> RTC_DRV_SetTimeDate
  - >> RTC_DRV_ConfigureAlarmInt

  RTC_DRV_Deinit (Thumb, 48 bytes, Stack size 8 bytes, rtc_driver.o(.text.RTC_DRV_Deinit))
  [Stack]

  - Max Depth = 8
  - Call Chain = RTC_DRV_Deinit
  [Calls]
  - >> INT_SYS_DisableIRQ
  - >> INT_SYS_ClearPending
  - >> RTC_SoftwareReset
  - >> RTC_GetTimeCounterEnable
  [Called By]
  - >> main

  RTC_DRV_GetCurrentTimeDate (Thumb, 64 bytes, Stack size 24 bytes, rtc_driver.o(.text.RTC_DRV_GetCurrentTimeDate))
  [Stack]

  - Max Depth = 48
  - Call Chain = RTC_DRV_GetCurrentTimeDate ⇒ RTC_DRV_ConvertSecondsToTimeDate
  [Calls]
  - >> RTC_DRV_ConvertSecondsToTimeDate
  - >> RTC_GetTimeSecondsRegister
  [Called By]
  - >> second_callback
  - >> main

  RTC_DRV_IRQHandler (Thumb, 124 bytes, Stack size 24 bytes, rtc_driver.o(.text.RTC_DRV_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = RTC_DRV_IRQHandler
  [Calls]
  - >> RTC_SetTimeAlarmRegister
  - >> RTC_GetTimeSecondsRegister
  - >> RTC_GetTimeAlarmFlag
  [Called By]
  - >> RTC_IRQHandler

  RTC_DRV_Init (Thumb, 186 bytes, Stack size 32 bytes, rtc_driver.o(.text.RTC_DRV_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = RTC_DRV_Init ⇒ RTC_DRV_ConfigureAlarmInt ⇒ RTC_DRV_ConvertTimeDateToSeconds
  [Calls]
  - >> INT_SYS_DisableIRQ
  - >> INT_SYS_ClearPending
  - >> RTC_DRV_ConfigureSecondsInt
  - >> RTC_DRV_ConfigureOverflowInt
  - >> RTC_DRV_ConfigureAlarmInt
  - >> RTC_ConfigureClockOut
  - >> RTC_SoftwareReset
  - >> RTC_SetTimeCompensation
  - >> RTC_SetDebugMode
  - >> RTC_SetClockSource
  - >> RTC_GetTimeCounterEnable
  - >> RTC_EnableRegisterUnlock
  - >> RTC_ClearIntEnable
  [Called By]
  - >> main

  RTC_DRV_IsTimeDateCorrectFormat (Thumb, 98 bytes, Stack size 16 bytes, rtc_driver.o(.text.RTC_DRV_IsTimeDateCorrectFormat))
  [Stack]

  - Max Depth = 16
  - Call Chain = RTC_DRV_IsTimeDateCorrectFormat
  [Calls]
  - >> RTC_DRV_IsYearLeap
  [Called By]
  - >> RTC_DRV_SetTimeDate
  - >> RTC_DRV_ConfigureAlarmInt

  RTC_DRV_IsYearLeap (Thumb, 60 bytes, Stack size 0 bytes, rtc_driver.o(.text.RTC_DRV_IsYearLeap))
  [Called By]

  - >> RTC_DRV_IsTimeDateCorrectFormat
  - >> RTC_DRV_ConvertTimeDateToSeconds
  - >> RTC_DRV_ConvertSecondsToTimeDate

  RTC_DRV_SecondsIRQHandler (Thumb, 40 bytes, Stack size 8 bytes, rtc_driver.o(.text.RTC_DRV_SecondsIRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = RTC_DRV_SecondsIRQHandler
  [Calls]
  - >> RTC_ClearTimeSecondsIntFlag
  [Called By]
  - >> RTC_Seconds_IRQHandler

  RTC_DRV_SetTimeDate (Thumb, 48 bytes, Stack size 16 bytes, rtc_driver.o(.text.RTC_DRV_SetTimeDate))
  [Stack]

  - Max Depth = 48
  - Call Chain = RTC_DRV_SetTimeDate ⇒ RTC_DRV_ConvertTimeDateToSeconds
  [Calls]
  - >> RTC_SetTimeSecondsRegister
  - >> RTC_DRV_IsTimeDateCorrectFormat
  - >> RTC_DRV_ConvertTimeDateToSeconds
  [Called By]
  - >> main

  RTC_DRV_StartCounter (Thumb, 10 bytes, Stack size 0 bytes, rtc_driver.o(.text.RTC_DRV_StartCounter))
  [Stack]

  - Max Depth = 8
  - Call Chain = RTC_DRV_StartCounter ⇒ RTC_Enable
  [Calls]
  - >> RTC_Enable
  [Called By]
  - >> main

  RTC_Enable (Thumb, 26 bytes, Stack size 8 bytes, rtc_hw_access.o(.text.RTC_Enable))
  [Stack]

  - Max Depth = 8
  - Call Chain = RTC_Enable
  [Calls]
  - >> RTC_SetTimeCounterEnable
  - >> RTC_GetTimeCounterEnable
  [Called By]
  - >> RTC_DRV_StartCounter

  RTC_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, rtc_irq.o(.text.RTC_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = RTC_IRQHandler ⇒ RTC_DRV_IRQHandler
  [Calls]
  - >> RTC_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  RTC_Seconds_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, rtc_irq.o(.text.RTC_Seconds_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = RTC_Seconds_IRQHandler ⇒ RTC_DRV_SecondsIRQHandler
  [Calls]
  - >> RTC_DRV_SecondsIRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  RTC_SetTimeSecondsRegister (Thumb, 22 bytes, Stack size 16 bytes, rtc_hw_access.o(.text.RTC_SetTimeSecondsRegister))
  [Stack]

  - Max Depth = 16
  - Call Chain = RTC_SetTimeSecondsRegister
  [Calls]
  - >> RTC_GetTimeCounterEnable
  [Called By]
  - >> RTC_DRV_SetTimeDate

  RamInit1 (Thumb, 268 bytes, Stack size 32 bytes, raminit1.o(.text.RamInit1))
  [Stack]

  - Max Depth = 32
  - Call Chain = RamInit1
  [Calls]
  - >> IsPOR
  - >> __aeabi_memclr4
  [Address Reference Count : 1]
  - startup.o(.text)

  RamInit2 (Thumb, 2 bytes, Stack size 0 bytes, raminit2.o(.text.RamInit2))
  [Address Reference Count : 1]

  - startup.o(.text)

  SAI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SAI0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SAI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SAI1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SENT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SENT0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SENT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SENT1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI2_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI4_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI5_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI6_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI7_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SVC_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SVC_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SysTick_Handler (Thumb, 4 bytes, Stack size 0 bytes, osif_baremetal.o(.text.SysTick_Handler))
  [Calls]

  - >> osif_Tick
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SystemInit (Thumb, 60 bytes, Stack size 0 bytes, system_ytm32b1ha0.o(.text.SystemInit))
  [Address Reference Count : 1]

  - startup.o(.text)

  TMR0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.TMR0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  TMR1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.TMR1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  TRNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.TRNG_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  UTILITY_PRINT_Init (Thumb, 22 bytes, Stack size 0 bytes, utility_print_config.o(.text.UTILITY_PRINT_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = UTILITY_PRINT_Init ⇒ LINFlexD_UART_DRV_Init ⇒ LINFlexD_UART_DRV_SetBaudRate ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> LINFlexD_UART_DRV_Init
  [Called By]
  - >> Board_Init

  UsageFault_Handler (Thumb, 0 bytes, Stack size 8 bytes, vector_table_copy.o(.text.UsageFault_Handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = UsageFault_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  VectorTableCopy (Thumb, 74 bytes, Stack size 8 bytes, vector_table_copy.o(.text.VectorTableCopy))
  [Stack]

  - Max Depth = 8
  - Call Chain = VectorTableCopy
  [Calls]
  - >> __aeabi_memcpy4
  [Address Reference Count : 1]
  - startup.o(.text)

  WDG0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.WDG0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  WKU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.WKU_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  alarm_callback (Thumb, 32 bytes, Stack size 0 bytes, main.o(.text.alarm_callback))
  [Stack]

  - Max Depth = 576
  - Call Chain = alarm_callback ⇒ printf_ ⇒ _vsnprintf ⇒ _ftoa ⇒ _etoa ⇒ _ftoa (Cycle)
  [Calls]
  - >> printf_
  [Address Reference Count : 1]
  - rtc_config.o(.data.rtc_config0Alarm)

  eTMR0_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR0_Ch0_Ch1_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR0_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR0_Ch2_Ch3_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR0_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR0_Ch4_Ch5_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR0_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR0_Ch6_Ch7_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR0_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Fault_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR0_Fault_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR0_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR0_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR0_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR0_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR1_Ch0_Ch1_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR1_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR1_Ch2_Ch3_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR1_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR1_Ch4_Ch5_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR1_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR1_Ch6_Ch7_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR1_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Fault_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR1_Fault_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR1_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR1_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR1_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR1_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR2_Ch0_Ch1_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR2_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR2_Ch2_Ch3_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR2_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR2_Ch4_Ch5_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR2_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR2_Ch6_Ch7_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR2_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Fault_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR2_Fault_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR2_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR2_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR2_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR2_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR3_Ch0_Ch1_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR3_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR3_Ch2_Ch3_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR3_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR3_Ch4_Ch5_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR3_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR3_Ch6_Ch7_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR3_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Fault_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR3_Fault_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR3_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR3_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR3_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR3_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR4_Ch0_Ch1_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR4_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR4_Ch2_Ch3_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR4_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR4_Ch4_Ch5_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR4_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR4_Ch6_Ch7_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR4_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Fault_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR4_Fault_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR4_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR4_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR4_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR4_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR5_Ch0_Ch1_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR5_Ch0_Ch1_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR5_Ch2_Ch3_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR5_Ch2_Ch3_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR5_Ch4_Ch5_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR5_Ch4_Ch5_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR5_Ch6_Ch7_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR5_Ch6_Ch7_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Fault_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR5_Fault_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR5_Fault_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  eTMR5_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.eTMR5_Ovf_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = eTMR5_Ovf_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  lpTMR0_IRQHandler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.lpTMR0_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = lpTMR0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  main (Thumb, 676 bytes, Stack size 32 bytes, main.o(.text.main))
  [Stack]

  - Max Depth = 608
  - Call Chain = main ⇒ printf_ ⇒ _vsnprintf ⇒ _ftoa ⇒ _etoa ⇒ _ftoa (Cycle)
  [Calls]
  - >> printf_
  - >> RTC_DRV_StartCounter
  - >> RTC_DRV_SetTimeDate
  - >> RTC_DRV_Init
  - >> RTC_DRV_GetCurrentTimeDate
  - >> RTC_DRV_Deinit
  - >> POWER_SYS_SetMode
  - >> POWER_SYS_Init
  - >> OSIF_TimeDelay
  - >> LINFlexD_UART_DRV_SendDataBlocking
  - >> LINFlexD_UART_DRV_ReceiveDataBlocking
  - >> LINFlexD_UART_DRV_Init
  - >> LINFlexD_UART_DRV_Deinit
  - >> LINFlexD_UART_DRV_AbortSendingData
  - >> LINFlexD_UART_DRV_AbortReceivingData
  - >> DMA_DRV_StopChannel
  - >> DMA_DRV_StartChannel
  - >> DMA_DRV_ReleaseChannel
  - >> DMA_DRV_Init
  - >> DMA_DRV_Deinit
  - >> Board_Init
  [Called By]
  - >> Reset_Handler

  pTMR0_Ch0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR0_Ch0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR0_Ch1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR0_Ch2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR0_Ch2_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR0_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR0_Ch3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR1_Ch0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR1_Ch0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR1_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR1_Ch1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR1_Ch2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR1_Ch2_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR1_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR1_Ch3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR2_Ch0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR2_Ch0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR2_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR2_Ch1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR2_Ch2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR2_Ch2_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR2_Ch3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  printf_ (Thumb, 58 bytes, Stack size 0 bytes, printf.o(.text.printf_))
  [Stack]

  - Max Depth = 576
  - Call Chain = printf_ ⇒ _vsnprintf ⇒ _ftoa ⇒ _etoa ⇒ _ftoa (Cycle)
  [Calls]
  - >> _vsnprintf
  [Called By]
  - >> main
  - >> alarm_callback

  printf_char (Thumb, 24 bytes, Stack size 16 bytes, utility_print_config.o(.text.printf_char))
  [Stack]

  - Max Depth = 56
  - Call Chain = printf_char ⇒ LINFlexD_UART_DRV_SendDataPolling ⇒ LINFlexD_UART_DRV_PutData
  [Calls]
  - >> LINFlexD_UART_DRV_SendDataPolling
  [Called By]
  - >> _out_char

  second_callback (Thumb, 16 bytes, Stack size 24 bytes, main.o(.text.second_callback))
  [Stack]

  - Max Depth = 72
  - Call Chain = second_callback ⇒ RTC_DRV_GetCurrentTimeDate ⇒ RTC_DRV_ConvertSecondsToTimeDate
  [Calls]
  - >> RTC_DRV_GetCurrentTimeDate
  [Address Reference Count : 1]
  - rtc_config.o(.data.rtc_config0Seconds)

  ### Local Symbols

  Board_Init (Thumb, 56 bytes, Stack size 8 bytes, main.o(.text.Board_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = Board_Init ⇒ CLOCK_SYS_UpdateConfiguration ⇒ CLOCK_SYS_SetConfiguration ⇒ CLOCK_DRV_Init ⇒ CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_WaitFXOSCValid
  [Calls]
  - >> UTILITY_PRINT_Init
  - >> PINS_DRV_Init
  - >> CLOCK_SYS_UpdateConfiguration
  - >> CLOCK_SYS_Init
  [Called By]
  - >> main

  IsPOR (Thumb, 16 bytes, Stack size 0 bytes, raminit1.o(.text.IsPOR))
  [Called By]

  - >> RamInit1

  CLOCK_GetIpcCtrlReg (Thumb, 26 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.CLOCK_GetIpcCtrlReg))
  [Called By]

  - >> CLOCK_DRV_GetFreq
  - >> CLOCK_SYS_SetIpcConfiguration

  CLOCK_SCU_WaitDividerStable (Thumb, 32 bytes, Stack size 8 bytes, clock_ytm32b1hx.o(.text.CLOCK_SCU_WaitDividerStable))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLOCK_SCU_WaitDividerStable
  [Calls]
  - >> SCU_GetDividerStable
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SCU_WaitPllLock (Thumb, 32 bytes, Stack size 8 bytes, clock_ytm32b1hx.o(.text.CLOCK_SCU_WaitPllLock))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLOCK_SCU_WaitPllLock
  [Calls]
  - >> SCU_GetPllLock
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_ConfigureClkOut (Thumb, 24 bytes, Stack size 8 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_ConfigureClkOut))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLOCK_SYS_ConfigureClkOut
  [Calls]
  - >> SCU_SetClkOutSrc
  - >> SCU_SetClkOutDiv
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_ConfigureSystemClock (Thumb, 38 bytes, Stack size 16 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_ConfigureSystemClock))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_SYS_ConfigureSystemClock
  [Calls]
  - >> SCU_SetSysClkSrc
  - >> SCU_GetSysClkSrc
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_DisableClkOut (Thumb, 6 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_DisableClkOut))
  [Calls]

  - >> SCU_SetClkOutSrc
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_DisableCmu (Thumb, 18 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_DisableCmu))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_SetCmuChannelConfiguration (Thumb, 56 bytes, Stack size 16 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_SetCmuChannelConfiguration))
  [Stack]

  - Max Depth = 24
  - Call Chain = CLOCK_SYS_SetCmuChannelConfiguration ⇒ SCU_SetCmuChResetEnable
  [Calls]
  - >> SCU_SetCmuChResetEnable
  - >> SCU_SetCmuChRefClock
  - >> SCU_SetCmuChEnable
  - >> SCU_SetCmuChCompLow
  - >> SCU_SetCmuChCompHigh
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_SetDefaultCmuChannelConfiguration (Thumb, 88 bytes, Stack size 16 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_SetDefaultCmuChannelConfiguration))
  [Stack]

  - Max Depth = 24
  - Call Chain = CLOCK_SYS_SetDefaultCmuChannelConfiguration ⇒ SCU_SetCmuChResetEnable
  [Calls]
  - >> SCU_SetCmuChResetEnable
  - >> SCU_SetCmuChRefClock
  - >> SCU_SetCmuChEnable
  - >> SCU_SetCmuChCompLow
  - >> SCU_SetCmuChCompHigh
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_SetIpcConfiguration (Thumb, 64 bytes, Stack size 16 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_SetIpcConfiguration))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_SYS_SetIpcConfiguration
  [Calls]
  - >> IPC_SetPeripheralClockControl
  - >> IPC_SetClockMode
  - >> CLOCK_GetIpcCtrlReg
  [Called By]
  - >> CLOCK_DRV_Init

  CLOCK_SYS_SetScuConfiguration (Thumb, 550 bytes, Stack size 24 bytes, clock_ytm32b1hx.o(.text.CLOCK_SYS_SetScuConfiguration))
  [Stack]

  - Max Depth = 56
  - Call Chain = CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_WaitFXOSCValid
  [Calls]
  - >> CLOCK_SYS_WaitFXOSCValid
  - >> CLOCK_SYS_GetFreq
  - >> CLOCK_DRV_GetPllFreq
  - >> SCU_SxoscStandbyEnable
  - >> SCU_SxoscPowerDownEnable
  - >> SCU_SxoscDeepSleepEnable
  - >> SCU_SircStandbyEnable
  - >> SCU_SircPowerDownEnable
  - >> SCU_SircDeepSleepEnable
  - >> SCU_SetSysClkDiv
  - >> SCU_SetSxoscGain
  - >> SCU_SetSxoscBypassMode
  - >> SCU_SetSlowBusClkDiv
  - >> SCU_SetPllRefClkDiv
  - >> SCU_SetPllRefClk
  - >> SCU_SetPllFeedBackDiv
  - >> SCU_SetFxoscGain
  - >> SCU_SetFxoscComp
  - >> SCU_SetFxoscBypassMode
  - >> SCU_SetFastBusClkDiv
  - >> SCU_GetSxoscEnableFlag
  - >> SCU_FircDeepSleepEnable
  - >> SCU_EnableSxosc
  - >> SCU_EnablePll
  - >> SCU_EnableFxosc
  - >> SCU_EnableFirc
  - >> CLOCK_SYS_SetDefaultCmuChannelConfiguration
  - >> CLOCK_SYS_SetCmuChannelConfiguration
  - >> CLOCK_SYS_DisableCmu
  - >> CLOCK_SYS_DisableClkOut
  - >> CLOCK_SYS_ConfigureSystemClock
  - >> CLOCK_SYS_ConfigureClkOut
  - >> CLOCK_SCU_WaitPllLock
  - >> CLOCK_SCU_WaitDividerStable
  [Called By]
  - >> CLOCK_DRV_Init

  IPC_SetClockMode (Thumb, 10 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.IPC_SetClockMode))
  [Called By]

  - >> CLOCK_SYS_SetIpcConfiguration

  IPC_SetPeripheralClockControl (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.IPC_SetPeripheralClockControl))
  [Called By]

  - >> CLOCK_SYS_SetIpcConfiguration

  SCU_EnableFirc (Thumb, 18 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_EnableFirc))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_EnableFxosc (Thumb, 18 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_EnableFxosc))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_EnablePll (Thumb, 18 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_EnablePll))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_EnableSxosc (Thumb, 18 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_EnableSxosc))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_FircDeepSleepEnable (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_FircDeepSleepEnable))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_GetDividerStable (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetDividerStable))
  [Called By]

  - >> CLOCK_SCU_WaitDividerStable

  SCU_GetFXOSCValid (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetFXOSCValid))
  [Called By]

  - >> CLOCK_SYS_WaitFXOSCValid

  SCU_GetFastBusClkDiv (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetFastBusClkDiv))
  [Called By]

  - >> CLOCK_DRV_GetFreq

  SCU_GetPllFeedBackDiv (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetPllFeedBackDiv))
  [Called By]

  - >> CLOCK_DRV_GetPllFreq

  SCU_GetPllLock (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetPllLock))
  [Called By]

  - >> CLOCK_DRV_GetPllFreq
  - >> CLOCK_SCU_WaitPllLock

  SCU_GetPllRefClk (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetPllRefClk))
  [Called By]

  - >> CLOCK_DRV_GetPllFreq

  SCU_GetPllRefClkDiv (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetPllRefClkDiv))
  [Called By]

  - >> CLOCK_DRV_GetPllFreq

  SCU_GetSlowBusClkDiv (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetSlowBusClkDiv))
  [Called By]

  - >> CLOCK_DRV_GetFreq

  SCU_GetSxoscEnableFlag (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetSxoscEnableFlag))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_GetSysClkDiv (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetSysClkDiv))
  [Called By]

  - >> CLOCK_DRV_GetFreq

  SCU_GetSysClkSrc (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_GetSysClkSrc))
  [Called By]

  - >> CLOCK_DRV_GetFreq
  - >> CLOCK_SYS_ConfigureSystemClock

  SCU_SetClkOutDiv (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetClkOutDiv))
  [Called By]

  - >> CLOCK_SYS_ConfigureClkOut

  SCU_SetClkOutSrc (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetClkOutSrc))
  [Called By]

  - >> CLOCK_SYS_DisableClkOut
  - >> CLOCK_SYS_ConfigureClkOut

  SCU_SetCmuChCompHigh (Thumb, 12 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetCmuChCompHigh))
  [Called By]

  - >> CLOCK_SYS_SetDefaultCmuChannelConfiguration
  - >> CLOCK_SYS_SetCmuChannelConfiguration

  SCU_SetCmuChCompLow (Thumb, 12 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetCmuChCompLow))
  [Called By]

  - >> CLOCK_SYS_SetDefaultCmuChannelConfiguration
  - >> CLOCK_SYS_SetCmuChannelConfiguration

  SCU_SetCmuChEnable (Thumb, 38 bytes, Stack size 8 bytes, clock_ytm32b1hx.o(.text.SCU_SetCmuChEnable))
  [Stack]

  - Max Depth = 8
  - Call Chain = SCU_SetCmuChEnable
  [Called By]
  - >> CLOCK_SYS_SetDefaultCmuChannelConfiguration
  - >> CLOCK_SYS_SetCmuChannelConfiguration

  SCU_SetCmuChRefClock (Thumb, 40 bytes, Stack size 8 bytes, clock_ytm32b1hx.o(.text.SCU_SetCmuChRefClock))
  [Stack]

  - Max Depth = 8
  - Call Chain = SCU_SetCmuChRefClock
  [Called By]
  - >> CLOCK_SYS_SetDefaultCmuChannelConfiguration
  - >> CLOCK_SYS_SetCmuChannelConfiguration

  SCU_SetCmuChResetEnable (Thumb, 40 bytes, Stack size 8 bytes, clock_ytm32b1hx.o(.text.SCU_SetCmuChResetEnable))
  [Stack]

  - Max Depth = 8
  - Call Chain = SCU_SetCmuChResetEnable
  [Called By]
  - >> CLOCK_SYS_SetDefaultCmuChannelConfiguration
  - >> CLOCK_SYS_SetCmuChannelConfiguration

  SCU_SetFastBusClkDiv (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetFastBusClkDiv))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetFxoscBypassMode (Thumb, 24 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetFxoscBypassMode))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetFxoscComp (Thumb, 24 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetFxoscComp))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetFxoscGain (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetFxoscGain))
  [Called By]

  - >> CLOCK_SYS_WaitFXOSCValid
  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetPllFeedBackDiv (Thumb, 26 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetPllFeedBackDiv))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetPllRefClk (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetPllRefClk))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetPllRefClkDiv (Thumb, 26 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetPllRefClkDiv))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetSlowBusClkDiv (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetSlowBusClkDiv))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetSxoscBypassMode (Thumb, 24 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetSxoscBypassMode))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetSxoscGain (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetSxoscGain))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetSysClkDiv (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetSysClkDiv))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetSysClkSrc (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SetSysClkSrc))
  [Called By]

  - >> CLOCK_SYS_ConfigureSystemClock

  SCU_SircDeepSleepEnable (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SircDeepSleepEnable))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SircPowerDownEnable (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SircPowerDownEnable))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SircStandbyEnable (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SircStandbyEnable))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SxoscDeepSleepEnable (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SxoscDeepSleepEnable))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SxoscPowerDownEnable (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SxoscPowerDownEnable))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SxoscStandbyEnable (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1hx.o(.text.SCU_SxoscStandbyEnable))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  PINS_ConfigDigitalFilter (Thumb, 32 bytes, Stack size 0 bytes, pins_port_hw_access.o(.text.PINS_ConfigDigitalFilter))
  [Called By]

  - >> PINS_Init

  PINS_GPIO_WritePin (Thumb, 28 bytes, Stack size 8 bytes, pins_port_hw_access.o(.text.PINS_GPIO_WritePin))
  [Stack]

  - Max Depth = 8
  - Call Chain = PINS_GPIO_WritePin
  [Called By]
  - >> PINS_Init

  __NVIC_ClearPendingIRQ (Thumb, 32 bytes, Stack size 0 bytes, interrupt_manager.o(.text.__NVIC_ClearPendingIRQ))
  [Called By]

  - >> INT_SYS_ClearPending

  __NVIC_DisableIRQ (Thumb, 40 bytes, Stack size 0 bytes, interrupt_manager.o(.text.__NVIC_DisableIRQ))
  [Called By]

  - >> INT_SYS_DisableIRQ

  __NVIC_EnableIRQ (Thumb, 32 bytes, Stack size 0 bytes, interrupt_manager.o(.text.__NVIC_EnableIRQ))
  [Called By]

  - >> INT_SYS_EnableIRQ

  DMAMUX_SetChannelSource (Thumb, 8 bytes, Stack size 0 bytes, dma_driver.o(.text.DMAMUX_SetChannelSource))
  [Called By]

  - >> DMA_DRV_SetChannelRequestAndTrigger

  DMA_CTSSetDestAddr (Thumb, 10 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_CTSSetDestAddr))
  [Called By]

  - >> DMA_DRV_SetDestAddr
  - >> DMA_DRV_ConfigSingleBlockTransfer

  DMA_CTSSetDestOffset (Thumb, 10 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_CTSSetDestOffset))
  [Called By]

  - >> DMA_DRV_ConfigSingleBlockTransfer

  DMA_CTSSetDisableDmaRequestAfterCTSDoneCmd (Thumb, 22 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_CTSSetDisableDmaRequestAfterCTSDoneCmd))
  [Called By]

  - >> DMA_DRV_ConfigMultiBlockTransfer

  DMA_CTSSetEngineStall (Thumb, 22 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_CTSSetEngineStall))
  [Called By]

  - >> DMA_DRV_ConfigSingleBlockTransfer

  DMA_CTSSetMajorCompleteIntCmd (Thumb, 22 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_CTSSetMajorCompleteIntCmd))
  [Called By]

  - >> DMA_DRV_ConfigSingleBlockTransfer

  DMA_CTSSetSrcAddr (Thumb, 10 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_CTSSetSrcAddr))
  [Called By]

  - >> DMA_DRV_SetSrcAddr
  - >> DMA_DRV_ConfigSingleBlockTransfer

  DMA_CTSSetSrcOffset (Thumb, 10 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_CTSSetSrcOffset))
  [Called By]

  - >> DMA_DRV_ConfigSingleBlockTransfer

  DMA_ClearDoneStatusFlag (Thumb, 10 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_ClearDoneStatusFlag))
  [Called By]

  - >> DMA_DRV_ClearIntStatus

  DMA_ClearErrorIntStatusFlag (Thumb, 10 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_ClearErrorIntStatusFlag))
  [Called By]

  - >> DMA_DRV_ErrorIRQHandler

  DMA_ClearIntStatusFlag (Thumb, 12 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_ClearIntStatusFlag))
  [Called By]

  - >> DMA_DRV_ClearIntStatus

  DMA_DRV_ClearIntStatus (Thumb, 32 bytes, Stack size 16 bytes, dma_driver.o(.text.DMA_DRV_ClearIntStatus))
  [Stack]

  - Max Depth = 16
  - Call Chain = DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_ClearIntStatusFlag
  - >> DMA_ClearDoneStatusFlag
  [Called By]
  - >> DMA_DRV_IRQHandler
  - >> DMA_DRV_ErrorIRQHandler

  DMA_DRV_ClearStructure (Thumb, 18 bytes, Stack size 8 bytes, dma_driver.o(.text.DMA_DRV_ClearStructure))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_DRV_ClearStructure
  [Calls]
  - >> __aeabi_memclr
  [Called By]
  - >> DMA_DRV_ReleaseChannel
  - >> DMA_DRV_Init
  - >> DMA_DRV_ChannelInit

  DMA_SetHaltOnErrorCmd (Thumb, 14 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_SetHaltOnErrorCmd))
  [Called By]

  - >> DMA_DRV_Init

  DMA_SetTransferLoopMappingCmd (Thumb, 10 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_SetTransferLoopMappingCmd))
  [Called By]

  - >> DMA_DRV_ConfigSingleBlockTransfer

  DMA_GetErrorIntStatusFlag (Thumb, 4 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA_GetErrorIntStatusFlag))
  [Called By]

  - >> DMA_Error_IRQHandler

  LINFlexD_ClearStatusFlag (Thumb, 4 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_ClearStatusFlag))
  [Called By]

  - >> LINFlexD_UART_DRV_SendDataPolling
  - >> LINFlexD_UART_DRV_TxIRQHandler
  - >> LINFlexD_UART_DRV_RxTOHandler
  - >> LINFlexD_UART_DRV_RxIRQHandler
  - >> LINFlexD_UART_DRV_ErrIRQHandler
  - >> LINFlexD_UART_DRV_StartSendUsingInterrupts

  LINFlexD_EnterInitMode (Thumb, 12 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_EnterInitMode))
  [Called By]

  - >> LINFlexD_UART_DRV_Init
  - >> LINFlexD_UART_DRV_SetBaudRate

  LINFlexD_EnterNormalMode (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_EnterNormalMode))
  [Called By]

  - >> LINFlexD_UART_DRV_Init
  - >> LINFlexD_UART_DRV_SetBaudRate

  LINFlexD_GetLinState (Thumb, 8 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_GetLinState))
  [Called By]

  - >> LINFlexD_UART_DRV_Init
  - >> LINFlexD_UART_DRV_SetBaudRate

  LINFlexD_GetRxDataBuffer1Byte (Thumb, 6 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_GetRxDataBuffer1Byte))
  [Called By]

  - >> LINFlexD_UART_DRV_GetData

  LINFlexD_GetRxDataBuffer2Bytes (Thumb, 4 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_GetRxDataBuffer2Bytes))
  [Called By]

  - >> LINFlexD_UART_DRV_GetData

  LINFlexD_GetStatusFlag (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_GetStatusFlag))
  [Called By]

  - >> LINFlexD_UART_DRV_SendDataPolling
  - >> LINFlexD_UART_DRV_RxTOHandler
  - >> LINFlexD_UART_DRV_IRQHandler
  - >> LINFlexD_UART_DRV_ErrIRQHandler

  LINFlexD_IsInterruptEnabled (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_IsInterruptEnabled))
  [Called By]

  - >> LINFlexD_UART_DRV_IRQHandler

  LINFlexD_SetFractionalBaudRate (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetFractionalBaudRate))
  [Called By]

  - >> LINFlexD_UART_DRV_SetBaudRate

  LINFlexD_SetIdleTimeoutValue (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetIdleTimeoutValue))
  [Called By]

  - >> LINFlexD_UART_DRV_RxTOHandler

  LINFlexD_SetIntegerBaudRate (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetIntegerBaudRate))
  [Called By]

  - >> LINFlexD_UART_DRV_SetBaudRate

  LINFlexD_SetInterruptMode (Thumb, 20 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetInterruptMode))
  [Called By]

  - >> LINFlexD_UART_DRV_Init
  - >> LINFlexD_UART_DRV_Deinit
  - >> LINFlexD_UART_DRV_RxTOHandler
  - >> LINFlexD_UART_DRV_StartSendUsingInterrupts
  - >> LINFlexD_UART_DRV_StartReceiveUsingInterrupts
  - >> LINFlexD_UART_DRV_CompleteSendUsingInterrupts
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts

  LINFlexD_SetMode (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetMode))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetParityControl (Thumb, 14 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetParityControl))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetParityType (Thumb, 26 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetParityType))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetReceiverState (Thumb, 14 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetReceiverState))
  [Called By]

  - >> LINFlexD_UART_DRV_StartReceiveUsingInterrupts
  - >> LINFlexD_UART_DRV_StartReceiveUsingDma
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts
  - >> LINFlexD_UART_DRV_CompleteReceiveUsingDma

  LINFlexD_SetRxDataFieldLength (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetRxDataFieldLength))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetRxMode (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetRxMode))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetRxStopBitsCount (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetRxStopBitsCount))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetTransmitterState (Thumb, 14 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetTransmitterState))
  [Called By]

  - >> LINFlexD_UART_DRV_SendDataPolling
  - >> LINFlexD_UART_DRV_StartSendUsingInterrupts
  - >> LINFlexD_UART_DRV_StartSendUsingDma
  - >> LINFlexD_UART_DRV_CompleteSendUsingInterrupts
  - >> LINFlexD_UART_DRV_CompleteSendUsingDma

  LINFlexD_SetTxDataBuffer1Byte (Thumb, 6 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetTxDataBuffer1Byte))
  [Called By]

  - >> LINFlexD_UART_DRV_PutData

  LINFlexD_SetTxDataBuffer2Bytes (Thumb, 4 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetTxDataBuffer2Bytes))
  [Called By]

  - >> LINFlexD_UART_DRV_PutData

  LINFlexD_SetTxDataFieldLength (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetTxDataFieldLength))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetTxMode (Thumb, 10 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetTxMode))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetTxStopBitsCount (Thumb, 14 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetTxStopBitsCount))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_SetUartWordLength (Thumb, 26 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_SetUartWordLength))
  [Called By]

  - >> LINFlexD_UART_DRV_Init

  LINFlexD_UART_DRV_CompleteReceiveUsingDma (Thumb, 150 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_CompleteReceiveUsingDma))
  [Stack]

  - Max Depth = 24
  - Call Chain = LINFlexD_UART_DRV_CompleteReceiveUsingDma ⇒ DMA_DRV_StopChannel
  [Calls]
  - >> DMA_DRV_StopChannel
  - >> DMA_DRV_StartChannel
  - >> DMA_DRV_SetTriggerLoopIterationCount
  - >> DMA_DRV_SetDestAddr
  - >> OSIF_SemaPost
  - >> LINFlexD_SetReceiverState
  [Called By]
  - >> LINFlexD_UART_DRV_ReceiveDataBlocking
  - >> LINFlexD_UART_DRV_AbortReceivingData
  - >> LINFlexD_UART_DRV_ErrIRQHandler
  [Address Reference Count : 1]
  - linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_StartReceiveUsingDma)

  LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts (Thumb, 74 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts))
  [Stack]

  - Max Depth = 24
  - Call Chain = LINFlexD_UART_DRV_CompleteReceiveUsingInterrupts ⇒ OSIF_SemaPost
  [Calls]
  - >> OSIF_SemaPost
  - >> LINFlexD_SetReceiverState
  - >> LINFlexD_SetInterruptMode
  [Called By]
  - >> LINFlexD_UART_DRV_ReceiveDataBlocking
  - >> LINFlexD_UART_DRV_AbortReceivingData
  - >> LINFlexD_UART_DRV_RxTOHandler
  - >> LINFlexD_UART_DRV_RxIRQHandler
  - >> LINFlexD_UART_DRV_ErrIRQHandler

  LINFlexD_UART_DRV_CompleteSendUsingDma (Thumb, 134 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_CompleteSendUsingDma))
  [Stack]

  - Max Depth = 24
  - Call Chain = LINFlexD_UART_DRV_CompleteSendUsingDma ⇒ DMA_DRV_StopChannel
  [Calls]
  - >> DMA_DRV_StopChannel
  - >> DMA_DRV_StartChannel
  - >> DMA_DRV_SetTriggerLoopIterationCount
  - >> DMA_DRV_SetSrcAddr
  - >> OSIF_SemaPost
  - >> LINFlexD_SetTransmitterState
  [Called By]
  - >> LINFlexD_UART_DRV_SendDataBlocking
  - >> LINFlexD_UART_DRV_AbortSendingData
  [Address Reference Count : 1]
  - linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_StartSendUsingDma)

  LINFlexD_UART_DRV_CompleteSendUsingInterrupts (Thumb, 74 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_CompleteSendUsingInterrupts))
  [Stack]

  - Max Depth = 24
  - Call Chain = LINFlexD_UART_DRV_CompleteSendUsingInterrupts ⇒ OSIF_SemaPost
  [Calls]
  - >> OSIF_SemaPost
  - >> LINFlexD_SetTransmitterState
  - >> LINFlexD_SetInterruptMode
  [Called By]
  - >> LINFlexD_UART_DRV_SendDataBlocking
  - >> LINFlexD_UART_DRV_AbortSendingData
  - >> LINFlexD_UART_DRV_TxIRQHandler

  LINFlexD_UART_DRV_FlushRxFifo (Thumb, 18 bytes, Stack size 0 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_FlushRxFifo))
  [Called By]

  - >> LINFlexD_UART_DRV_StartReceiveUsingDma

  LINFlexD_UART_DRV_GetData (Thumb, 108 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_GetData))
  [Stack]

  - Max Depth = 16
  - Call Chain = LINFlexD_UART_DRV_GetData
  [Calls]
  - >> LINFlexD_GetRxDataBuffer2Bytes
  - >> LINFlexD_GetRxDataBuffer1Byte
  [Called By]
  - >> LINFlexD_UART_DRV_RxIRQHandler

  LINFlexD_UART_DRV_PutData (Thumb, 112 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_PutData))
  [Stack]

  - Max Depth = 16
  - Call Chain = LINFlexD_UART_DRV_PutData
  [Calls]
  - >> LINFlexD_SetTxDataBuffer2Bytes
  - >> LINFlexD_SetTxDataBuffer1Byte
  [Called By]
  - >> LINFlexD_UART_DRV_SendDataPolling
  - >> LINFlexD_UART_DRV_TxIRQHandler
  - >> LINFlexD_UART_DRV_StartSendUsingInterrupts

  LINFlexD_UART_DRV_StartReceiveUsingDma (Thumb, 160 bytes, Stack size 40 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_StartReceiveUsingDma))
  [Stack]

  - Max Depth = 128
  - Call Chain = LINFlexD_UART_DRV_StartReceiveUsingDma ⇒ DMA_DRV_ConfigMultiBlockTransfer ⇒ DMA_DRV_ConfigSingleBlockTransfer ⇒ DMA_CTSSetAttribute
  [Calls]
  - >> DMA_DRV_StartChannel
  - >> DMA_DRV_InstallCallback
  - >> DMA_DRV_ConfigMultiBlockTransfer
  - >> LINFlexD_UART_DRV_FlushRxFifo
  - >> LINFlexD_SetReceiverState
  [Called By]
  - >> LINFlexD_UART_DRV_ReceiveDataBlocking

  LINFlexD_UART_DRV_StartReceiveUsingInterrupts (Thumb, 72 bytes, Stack size 8 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_StartReceiveUsingInterrupts))
  [Stack]

  - Max Depth = 8
  - Call Chain = LINFlexD_UART_DRV_StartReceiveUsingInterrupts
  [Calls]
  - >> LINFlexD_SetReceiverState
  - >> LINFlexD_SetInterruptMode
  [Called By]
  - >> LINFlexD_UART_DRV_ReceiveDataBlocking

  LINFlexD_UART_DRV_StartSendUsingDma (Thumb, 154 bytes, Stack size 40 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_StartSendUsingDma))
  [Stack]

  - Max Depth = 128
  - Call Chain = LINFlexD_UART_DRV_StartSendUsingDma ⇒ DMA_DRV_ConfigMultiBlockTransfer ⇒ DMA_DRV_ConfigSingleBlockTransfer ⇒ DMA_CTSSetAttribute
  [Calls]
  - >> DMA_DRV_StartChannel
  - >> DMA_DRV_InstallCallback
  - >> DMA_DRV_ConfigMultiBlockTransfer
  - >> LINFlexD_SetTransmitterState
  [Called By]
  - >> LINFlexD_UART_DRV_SendDataBlocking

  LINFlexD_UART_DRV_StartSendUsingInterrupts (Thumb, 86 bytes, Stack size 16 bytes, linflexd_uart_driver.o(.text.LINFlexD_UART_DRV_StartSendUsingInterrupts))
  [Stack]

  - Max Depth = 32
  - Call Chain = LINFlexD_UART_DRV_StartSendUsingInterrupts ⇒ LINFlexD_UART_DRV_PutData
  [Calls]
  - >> LINFlexD_UART_DRV_PutData
  - >> LINFlexD_SetTransmitterState
  - >> LINFlexD_SetInterruptMode
  - >> LINFlexD_ClearStatusFlag
  [Called By]
  - >> LINFlexD_UART_DRV_SendDataBlocking

  RTC_ClearIntEnable (Thumb, 10 bytes, Stack size 0 bytes, rtc_driver.o(.text.RTC_ClearIntEnable))
  [Called By]

  - >> RTC_DRV_Init

  RTC_ClearTimeSecondsIntFlag (Thumb, 10 bytes, Stack size 0 bytes, rtc_driver.o(.text.RTC_ClearTimeSecondsIntFlag))
  [Called By]

  - >> RTC_DRV_SecondsIRQHandler

  RTC_EnableRegisterUnlock (Thumb, 10 bytes, Stack size 0 bytes, rtc_driver.o(.text.RTC_EnableRegisterUnlock))
  [Called By]

  - >> RTC_DRV_Init

  RTC_GetTimeAlarmFlag (Thumb, 8 bytes, Stack size 0 bytes, rtc_driver.o(.text.RTC_GetTimeAlarmFlag))
  [Called By]

  - >> RTC_DRV_IRQHandler

  RTC_GetTimeCounterEnable (Thumb, 8 bytes, Stack size 0 bytes, rtc_driver.o(.text.RTC_GetTimeCounterEnable))
  [Called By]

  - >> RTC_DRV_Init
  - >> RTC_DRV_Deinit

  RTC_GetTimeSecondsRegister (Thumb, 4 bytes, Stack size 0 bytes, rtc_driver.o(.text.RTC_GetTimeSecondsRegister))
  [Called By]

  - >> RTC_DRV_GetCurrentTimeDate
  - >> RTC_DRV_IRQHandler
  - >> RTC_DRV_ConfigureAlarmInt

  RTC_SetClockSource (Thumb, 10 bytes, Stack size 0 bytes, rtc_driver.o(.text.RTC_SetClockSource))
  [Called By]

  - >> RTC_DRV_Init

  RTC_SetDebugMode (Thumb, 18 bytes, Stack size 0 bytes, rtc_driver.o(.text.RTC_SetDebugMode))
  [Called By]

  - >> RTC_DRV_Init

  RTC_SetTimeAlarmIntEnable (Thumb, 14 bytes, Stack size 0 bytes, rtc_driver.o(.text.RTC_SetTimeAlarmIntEnable))
  [Called By]

  - >> RTC_DRV_ConfigureAlarmInt

  RTC_SetTimeAlarmRegister (Thumb, 8 bytes, Stack size 0 bytes, rtc_driver.o(.text.RTC_SetTimeAlarmRegister))
  [Called By]

  - >> RTC_DRV_IRQHandler
  - >> RTC_DRV_ConfigureAlarmInt

  RTC_SetTimeCompensation (Thumb, 22 bytes, Stack size 0 bytes, rtc_driver.o(.text.RTC_SetTimeCompensation))
  [Called By]

  - >> RTC_DRV_Init

  RTC_SetTimeOverflowIntEnable (Thumb, 12 bytes, Stack size 0 bytes, rtc_driver.o(.text.RTC_SetTimeOverflowIntEnable))
  [Called By]

  - >> RTC_DRV_ConfigureOverflowInt

  RTC_SetTimeSecondsIntConf (Thumb, 10 bytes, Stack size 0 bytes, rtc_driver.o(.text.RTC_SetTimeSecondsIntConf))
  [Called By]

  - >> RTC_DRV_ConfigureSecondsInt

  RTC_SetTimeSecondsIntEnable (Thumb, 14 bytes, Stack size 0 bytes, rtc_driver.o(.text.RTC_SetTimeSecondsIntEnable))
  [Called By]

  - >> RTC_DRV_ConfigureSecondsInt

  RTC_SoftwareReset (Thumb, 18 bytes, Stack size 0 bytes, rtc_driver.o(.text.RTC_SoftwareReset))
  [Called By]

  - >> RTC_DRV_Init
  - >> RTC_DRV_Deinit

  RTC_GetTimeCounterEnable (Thumb, 8 bytes, Stack size 0 bytes, rtc_hw_access.o(.text.RTC_GetTimeCounterEnable))
  [Called By]

  - >> RTC_SetTimeSecondsRegister
  - >> RTC_Enable

  RTC_SetTimeCounterEnable (Thumb, 12 bytes, Stack size 0 bytes, rtc_hw_access.o(.text.RTC_SetTimeCounterEnable))
  [Called By]

  - >> RTC_Enable

  POWER_SYS_CallbacksManagement (Thumb, 130 bytes, Stack size 40 bytes, power_manager.o(.text.POWER_SYS_CallbacksManagement))
  [Stack]

  - Max Depth = 40
  - Call Chain = POWER_SYS_CallbacksManagement
  [Called By]
  - >> POWER_SYS_SetMode

  POWER_SYS_SwitchToLowPowerMode (Thumb, 214 bytes, Stack size 24 bytes, power_manager_ytm32b1hx.o(.text.POWER_SYS_SwitchToLowPowerMode))
  [Stack]

  - Max Depth = 56
  - Call Chain = POWER_SYS_SwitchToLowPowerMode ⇒ CLOCK_SYS_WaitFXOSCValid
  [Calls]
  - >> CLOCK_SYS_WaitFXOSCValid
  [Called By]
  - >> POWER_SYS_DoSetMode

  osif_DisableIrqGlobal (Thumb, 4 bytes, Stack size 0 bytes, osif_baremetal.o(.text.osif_DisableIrqGlobal))
  [Calls]

  - >> INT_SYS_DisableIRQGlobal
  [Called By]
  - >> OSIF_SemaWait
  - >> OSIF_SemaPost
  - >> OSIF_SemaCreate

  osif_EnableIrqGlobal (Thumb, 4 bytes, Stack size 0 bytes, osif_baremetal.o(.text.osif_EnableIrqGlobal))
  [Calls]

  - >> INT_SYS_EnableIRQGlobal
  [Called By]
  - >> OSIF_SemaWait
  - >> OSIF_SemaPost
  - >> OSIF_SemaCreate

  osif_GetCurrentTickCount (Thumb, 12 bytes, Stack size 0 bytes, osif_baremetal.o(.text.osif_GetCurrentTickCount))
  [Called By]

  - >> OSIF_TimeDelay
  - >> OSIF_SemaWait

  osif_Tick (Thumb, 16 bytes, Stack size 0 bytes, osif_baremetal.o(.text.osif_Tick))
  [Called By]

  - >> SysTick_Handler

  osif_UpdateTickConfig (Thumb, 70 bytes, Stack size 24 bytes, osif_baremetal.o(.text.osif_UpdateTickConfig))
  [Stack]

  - Max Depth = 40
  - Call Chain = osif_UpdateTickConfig ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq ⇒ CLOCK_DRV_GetPllFreq
  [Calls]
  - >> CLOCK_SYS_GetFreq
  [Called By]
  - >> OSIF_TimeDelay
  - >> OSIF_SemaWait

  _atoi (Thumb, 62 bytes, Stack size 16 bytes, printf.o(.text._atoi))
  [Stack]

  - Max Depth = 16
  - Call Chain = _atoi
  [Calls]
  - >> _is_digit
  [Called By]
  - >> _vsnprintf

  _etoa (Thumb, 1112 bytes, Stack size 136 bytes, printf.o(.text._etoa))
  [Stack]

  - Max Depth = 336 + In Cycle
  - Call Chain = _etoa ⇒ _ftoa (Cycle)
  [Calls]
  - >> __aeabi_i2d
  - >> __aeabi_dsub
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dcmplt
  - >> __aeabi_dcmpgt
  - >> __aeabi_dcmpge
  - >> __aeabi_dadd
  - >> __aeabi_d2iz
  - >> _ntoa_long
  - >> _ftoa
  [Called By]
  - >> _vsnprintf
  - >> _ftoa

  _ftoa (Thumb, 1060 bytes, Stack size 144 bytes, printf.o(.text._ftoa))
  [Stack]

  - Max Depth = 480
  - Call Chain = _ftoa ⇒ _etoa ⇒ _ftoa (Cycle)
  [Calls]
  - >> __aeabi_memset4
  - >> __aeabi_memset
  - >> __aeabi_ui2d
  - >> __aeabi_i2d
  - >> __aeabi_dsub
  - >> __aeabi_dmul
  - >> __aeabi_dcmplt
  - >> __aeabi_dcmple
  - >> __aeabi_dcmpgt
  - >> __aeabi_dcmpge
  - >> __aeabi_d2uiz
  - >> __aeabi_d2iz
  - >> _out_rev
  - >> _etoa
  [Called By]
  - >> _vsnprintf
  - >> _etoa

  _is_digit (Thumb, 14 bytes, Stack size 0 bytes, printf.o(.text._is_digit))
  [Called By]

  - >> _vsnprintf
  - >> _atoi

  _ntoa_format (Thumb, 324 bytes, Stack size 56 bytes, printf.o(.text._ntoa_format))
  [Stack]

  - Max Depth = 104
  - Call Chain = _ntoa_format ⇒ _out_rev
  [Calls]
  - >> __aeabi_memset
  - >> _out_rev
  [Called By]
  - >> _ntoa_long_long
  - >> _ntoa_long

  _ntoa_long (Thumb, 150 bytes, Stack size 96 bytes, printf.o(.text._ntoa_long))
  [Stack]

  - Max Depth = 200
  - Call Chain = _ntoa_long ⇒ _ntoa_format ⇒ _out_rev
  [Calls]
  - >> _ntoa_format
  [Called By]
  - >> _vsnprintf
  - >> _etoa

  _ntoa_long_long (Thumb, 190 bytes, Stack size 120 bytes, printf.o(.text._ntoa_long_long))
  [Stack]

  - Max Depth = 224
  - Call Chain = _ntoa_long_long ⇒ _ntoa_format ⇒ _out_rev
  [Calls]
  - >> __aeabi_uldivmod
  - >> _ntoa_format
  [Called By]
  - >> _vsnprintf

  _out_char (Thumb, 10 bytes, Stack size 0 bytes, printf.o(.text._out_char))
  [Stack]

  - Max Depth = 56
  - Call Chain = _out_char ⇒ printf_char ⇒ LINFlexD_UART_DRV_SendDataPolling ⇒ LINFlexD_UART_DRV_PutData
  [Calls]
  - >> printf_char
  [Address Reference Count : 1]
  - printf.o(.text.printf_)

  _out_null (Thumb, 2 bytes, Stack size 0 bytes, printf.o(.text._out_null))
  [Address Reference Count : 1]

  - printf.o(.text._vsnprintf)

  _out_rev (Thumb, 170 bytes, Stack size 48 bytes, printf.o(.text._out_rev))
  [Stack]

  - Max Depth = 48
  - Call Chain = _out_rev
  [Called By]
  - >> _ntoa_format
  - >> _ftoa

  _strnlen_s (Thumb, 32 bytes, Stack size 0 bytes, printf.o(.text._strnlen_s))
  [Called By]

  - >> _vsnprintf

  _vsnprintf (Thumb, 1438 bytes, Stack size 96 bytes, printf.o(.text._vsnprintf))
  [Stack]

  - Max Depth = 576
  - Call Chain = _vsnprintf ⇒ _ftoa ⇒ _etoa ⇒ _ftoa (Cycle)
  [Calls]
  - >> _strnlen_s
  - >> _ntoa_long_long
  - >> _ntoa_long
  - >> _is_digit
  - >> _ftoa
  - >> _etoa
  - >> _atoi
  [Called By]
  - >> printf_

  ### Undefined Global Symbols