#

##

##

##

##

##

##

    µVision Build Log
    Tool Versions:
    IDE-Version: ¦ÌVision V5.36.0.0
    Copyright (C) 2021 ARM Ltd and ARM Germany GmbH. All rights reserved.
    License Information: 1 1, 1, LIC=VGXG8-3GI04-KPEZY-IXWG6-3NT0W-NCA2P

    Tool Versions:
    Toolchain:       MDK-ARM Plus  Version: 5.36.0.0
    Toolchain Path:  D:\soft_tool\Keil_v5\Keil_MDK\ARM\ARMCLANG\Bin
    C Compiler:      ArmClang.exe V6.16
    Assembler:       Armasm.exe V6.16
    Linker/Locator:  ArmLink.exe V6.16
    Library Manager: ArmAr.exe V6.16
    Hex Converter:   FromElf.exe V6.16
    CPU DLL:
    Dialog DLL:
    Target DLL:      Segger\JL2CM3.dll V2.99.40.0
    Dialog DLL:      TCM.DLL V1.53.0.0

    Project:
    D:\YunTu_Data\Demo\MC\Flexcan_Canfd_Demo\KEIL\Flexcan_Canfd_Demo.uvprojx
    Project File Date:  04/10/2025

    Output:
    *** Using Compiler 'V6.16', folder: 'D:\soft_tool\Keil_v5\Keil_MDK\ARM\ARMCLANG\Bin'
    Build target 'Flexcan_Canfd_Demo'
    compiling main.c...
    linking...
    Program Size: Code=17700 RO-data=596 RW-data=48 ZI-data=2772
    FromELF: creating hex file...
    After Build - User command #1: fromelf --bin --bincombined --output=Objects\Flexcan_Canfd_Demo.bin .\Objects\Flexcan_Canfd_Demo.axf
    After Build - User command #2: fromelf --m32 --m32combined --output=Objects\Flexcan_Canfd_Demo.srec .\Objects\Flexcan_Canfd_Demo.axf
    ".\Objects\Flexcan_Canfd_Demo.axf" - 0 Error(s), 0 Warning(s).

    Software Packages used:

    Package Vendor: YTMicro
                    https://doc.ytmicro.com/keil/YTMicro.YTM32B1MC0_DFP.1.2.0.pack
                    YTMicro.YTM32B1MC0_DFP.1.2.0
                    Device Family Pack for YTM32B1MC0

    Collection of Component include folders:
      D:\soft_tool\Keil_v5\Keil_MDK\ARM\PACK\YTMicro\YTM32B1MC0_DFP\1.2.0\Device\Include

    Collection of Component Files used:
    Build Time Elapsed:  00:00:02