# Static Call Graph for image .\Objects\Flexcan_Canfd_Demo.axf

#<CALLGRAPH># ARM Linker, 6160001: Last Updated: Thu Apr 10 11:12:16 2025

### Maximum Stack Usage = 528 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

Reset_Handler ⇒ main ⇒ printf_ ⇒ _vsnprintf ⇒ _ftoa ⇒ _etoa ⇒ _ftoa (Cycle)

### Functions with no stack information

- RamInit0
- Reset_Handler

### Mutually Recursive functions

- _etoa ⇒ _ftoa
- DefaultISR ⇒ DefaultISR

  ### Function Pointers

  - ACMP0_IRQHandler from vector_table_copy.o(.text.ACMP0_IRQHandler) referenced from vector.o(.isr_vector)
  - ADC0_IRQHandler from vector_table_copy.o(.text.ADC0_IRQHandler) referenced from vector.o(.isr_vector)
  - BusFault_Handler from vector_table_copy.o(.text.BusFault_Handler) referenced from vector.o(.isr_vector)
  - CAN0_Error_IRQHandler from flexcan_irq.o(.text.CAN0_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_0_15_MB_IRQHandler from flexcan_irq.o(.text.CAN0_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_16_31_MB_IRQHandler from flexcan_irq.o(.text.CAN0_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_32_47_MB_IRQHandler from flexcan_irq.o(.text.CAN0_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_48_63_MB_IRQHandler from flexcan_irq.o(.text.CAN0_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_ORed_IRQHandler from flexcan_irq.o(.text.CAN0_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN0_Wake_Up_IRQHandler from flexcan_irq.o(.text.CAN0_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_Error_IRQHandler from flexcan_irq.o(.text.CAN1_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_0_15_MB_IRQHandler from flexcan_irq.o(.text.CAN1_ORed_0_15_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_16_31_MB_IRQHandler from flexcan_irq.o(.text.CAN1_ORed_16_31_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_32_47_MB_IRQHandler from flexcan_irq.o(.text.CAN1_ORed_32_47_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_48_63_MB_IRQHandler from flexcan_irq.o(.text.CAN1_ORed_48_63_MB_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_ORed_IRQHandler from flexcan_irq.o(.text.CAN1_ORed_IRQHandler) referenced from vector.o(.isr_vector)
  - CAN1_Wake_Up_IRQHandler from flexcan_irq.o(.text.CAN1_Wake_Up_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA0_IRQHandler from dma_irq.o(.text.DMA0_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA1_IRQHandler from dma_irq.o(.text.DMA1_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA2_IRQHandler from dma_irq.o(.text.DMA2_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA3_IRQHandler from dma_irq.o(.text.DMA3_IRQHandler) referenced from vector.o(.isr_vector)
  - DMA_Error_IRQHandler from dma_irq.o(.text.DMA_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - DebugMon_Handler from vector_table_copy.o(.text.DebugMon_Handler) referenced from vector.o(.isr_vector)
  - DefaultISR from vector_table_copy.o(.text.DefaultISR) referenced 85 times from vector.o(.isr_vector)
  - EFM_Ecc_IRQHandler from vector_table_copy.o(.text.EFM_Ecc_IRQHandler) referenced from vector.o(.isr_vector)
  - EFM_Error_IRQHandler from vector_table_copy.o(.text.EFM_Error_IRQHandler) referenced from vector.o(.isr_vector)
  - EFM_IRQHandler from vector_table_copy.o(.text.EFM_IRQHandler) referenced from vector.o(.isr_vector)
  - EMU0_DB_IRQHandler from vector_table_copy.o(.text.EMU0_DB_IRQHandler) referenced from vector.o(.isr_vector)
  - EMU0_SB_IRQHandler from vector_table_copy.o(.text.EMU0_SB_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOA_IRQHandler from vector_table_copy.o(.text.GPIOA_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOB_IRQHandler from vector_table_copy.o(.text.GPIOB_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOC_IRQHandler from vector_table_copy.o(.text.GPIOC_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOD_IRQHandler from vector_table_copy.o(.text.GPIOD_IRQHandler) referenced from vector.o(.isr_vector)
  - GPIOE_IRQHandler from vector_table_copy.o(.text.GPIOE_IRQHandler) referenced from vector.o(.isr_vector)
  - HCU_IRQHandler from vector_table_copy.o(.text.HCU_IRQHandler) referenced from vector.o(.isr_vector)
  - HardFault_Handler from vector_table_copy.o(.text.HardFault_Handler) referenced from vector.o(.isr_vector)
  - I2C0_Master_IRQHandler from vector_table_copy.o(.text.I2C0_Master_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C0_Slave_IRQHandler from vector_table_copy.o(.text.I2C0_Slave_IRQHandler) referenced from vector.o(.isr_vector)
  - I2C1_Master_IRQHandler from vector_table_copy.o(.text.I2C1_Master_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch0_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch0_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch0_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch0_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch1_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch1_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch1_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch2_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch2_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch2_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch2_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch3_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch3_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch3_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch4_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch4_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch4_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch4_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch5_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch5_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch5_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch6_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch6_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch6_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch6_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch7_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - MPWM0_Ch7_Ovf_IRQHandler from vector_table_copy.o(.text.MPWM0_Ch7_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - MemManage_Handler from vector_table_copy.o(.text.MemManage_Handler) referenced from vector.o(.isr_vector)
  - NMI_Handler from vector_table_copy.o(.text.NMI_Handler) referenced from vector.o(.isr_vector)
  - PCU_IRQHandler from vector_table_copy.o(.text.PCU_IRQHandler) referenced from vector.o(.isr_vector)
  - PendSV_Handler from vector_table_copy.o(.text.PendSV_Handler) referenced from vector.o(.isr_vector)
  - RamInit1 from raminit1.o(.text.RamInit1) referenced from startup.o(.text)
  - RamInit2 from raminit2.o(.text.RamInit2) referenced from startup.o(.text)
  - Reset_Handler from startup.o(.text) referenced from vector.o(.isr_vector)
  - SCU_IRQHandler from vector_table_copy.o(.text.SCU_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI0_IRQHandler from vector_table_copy.o(.text.SPI0_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI1_IRQHandler from vector_table_copy.o(.text.SPI1_IRQHandler) referenced from vector.o(.isr_vector)
  - SPI2_IRQHandler from vector_table_copy.o(.text.SPI2_IRQHandler) referenced from vector.o(.isr_vector)
  - SVC_Handler from vector_table_copy.o(.text.SVC_Handler) referenced from vector.o(.isr_vector)
  - SysTick_Handler from osif_baremetal.o(.text.SysTick_Handler) referenced from vector.o(.isr_vector)
  - SystemInit from system_ytm32b1mc0.o(.text.SystemInit) referenced from startup.o(.text)
  - TRNG_IRQHandler from vector_table_copy.o(.text.TRNG_IRQHandler) referenced from vector.o(.isr_vector)
  - UART0_IRQHandler from vector_table_copy.o(.text.UART0_IRQHandler) referenced from vector.o(.isr_vector)
  - UART0_IrqHandler from uart_irq.o(.text.UART0_IrqHandler) referenced from uart_irq.o(.data.g_uartIsr)
  - UART1_IRQHandler from vector_table_copy.o(.text.UART1_IRQHandler) referenced from vector.o(.isr_vector)
  - UART1_IrqHandler from uart_irq.o(.text.UART1_IrqHandler) referenced from uart_irq.o(.data.g_uartIsr)
  - UART2_IRQHandler from vector_table_copy.o(.text.UART2_IRQHandler) referenced from vector.o(.isr_vector)
  - UART2_IrqHandler from uart_irq.o(.text.UART2_IrqHandler) referenced from uart_irq.o(.data.g_uartIsr)
  - UsageFault_Handler from vector_table_copy.o(.text.UsageFault_Handler) referenced from vector.o(.isr_vector)
  - VectorTableCopy from vector_table_copy.o(.text.VectorTableCopy) referenced from startup.o(.text)
  - WDG0_IRQHandler from vector_table_copy.o(.text.WDG0_IRQHandler) referenced from vector.o(.isr_vector)
  - _out_char from printf.o(.text._out_char) referenced 2 times from printf.o(.text.printf_)
  - _out_null from printf.o(.text._out_null) referenced 2 times from printf.o(.text._vsnprintf)
  - eTMR0_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR0_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Fault_IRQHandler from vector_table_copy.o(.text.eTMR0_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR0_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR0_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch0_Ch1_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch2_Ch3_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch2_Ch3_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch4_Ch5_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch4_Ch5_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ch6_Ch7_IRQHandler from vector_table_copy.o(.text.eTMR1_Ch6_Ch7_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Fault_IRQHandler from vector_table_copy.o(.text.eTMR1_Fault_IRQHandler) referenced from vector.o(.isr_vector)
  - eTMR1_Ovf_IRQHandler from vector_table_copy.o(.text.eTMR1_Ovf_IRQHandler) referenced from vector.o(.isr_vector)
  - lpTMR0_IRQHandler from vector_table_copy.o(.text.lpTMR0_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR0_Ch0_IRQHandler from vector_table_copy.o(.text.pTMR0_Ch0_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR0_Ch1_IRQHandler from vector_table_copy.o(.text.pTMR0_Ch1_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR0_Ch2_IRQHandler from vector_table_copy.o(.text.pTMR0_Ch2_IRQHandler) referenced from vector.o(.isr_vector)
  - pTMR0_Ch3_IRQHandler from vector_table_copy.o(.text.pTMR0_Ch3_IRQHandler) referenced from vector.o(.isr_vector)

  ### Global Symbols

  RamInit0 (Thumb, 0 bytes, Stack size unknown bytes, raminit0.o(.text))
  [Called By]

  - >> Reset_Handler

  Reset_Handler (Thumb, 0 bytes, Stack size unknown bytes, startup.o(.text))
  [Stack]

  - Max Depth = 528 + Unknown Stack Size
  - Call Chain = Reset_Handler ⇒ main ⇒ printf_ ⇒ _vsnprintf ⇒ _ftoa ⇒ _etoa ⇒ _ftoa (Cycle)
  [Calls]
  - >> RamInit0
  - >> main
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_uldivmod
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _ntoa_long_long

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> VectorTableCopy

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr
  - >> _ntoa_format
  - >> _ftoa

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> _ftoa

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text))
  [Calls]

  - >> __aeabi_memset
  [Called By]
  - >> UART_DRV_Init

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> RamInit1

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_dadd (Thumb, 322 bytes, Stack size 48 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_lasr
  - >> __aeabi_llsl
  - >> _double_round
  - >> _double_epilogue
  [Called By]
  - >> __aeabi_drsub
  - >> __aeabi_dsub
  - >> _etoa

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dsub ⇒ __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_dadd
  [Called By]
  - >> _ftoa
  - >> _etoa

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> _ftoa
  - >> _etoa

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> _double_round
  [Called By]
  - >> _etoa

  __aeabi_dcmple (Thumb, 54 bytes, Stack size 12 bytes, dcmple.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = __aeabi_dcmple
  [Called By]
  - >> _ftoa

  __aeabi_dcmplt (Thumb, 54 bytes, Stack size 12 bytes, dcmplt.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = __aeabi_dcmplt
  [Called By]
  - >> _ftoa
  - >> _etoa

  __aeabi_dcmpge (Thumb, 54 bytes, Stack size 12 bytes, dcmpge.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = __aeabi_dcmpge
  [Called By]
  - >> _ftoa
  - >> _etoa

  __aeabi_dcmpgt (Thumb, 54 bytes, Stack size 12 bytes, dcmpgt.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = __aeabi_dcmpgt
  [Called By]
  - >> _ftoa
  - >> _etoa

  __aeabi_i2d (Thumb, 34 bytes, Stack size 16 bytes, dflti.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_i2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> _ftoa
  - >> _etoa

  __aeabi_ui2d (Thumb, 26 bytes, Stack size 16 bytes, dfltui.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_ui2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> _ftoa

  __aeabi_d2iz (Thumb, 62 bytes, Stack size 16 bytes, dfixi.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = __aeabi_d2iz
  [Calls]
  - >> __aeabi_llsr
  [Called By]
  - >> _ftoa
  - >> _etoa

  __aeabi_d2uiz (Thumb, 50 bytes, Stack size 8 bytes, dfixui.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_d2uiz
  [Calls]
  - >> __aeabi_llsr
  [Called By]
  - >> _ftoa

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> _double_epilogue
  - >> __aeabi_uldivmod
  - >> __aeabi_dadd

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> _double_epilogue
  - >> __aeabi_uldivmod
  - >> __aeabi_d2uiz
  - >> __aeabi_d2iz

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text))
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  __I$use$fp (Thumb, 0 bytes, Stack size 8 bytes, iusefp.o(.text), UNUSED)

  _double_round (Thumb, 30 bytes, Stack size 8 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _double_round
  [Called By]
  - >> _double_epilogue
  - >> __aeabi_ddiv
  - >> __aeabi_dadd

  _double_epilogue (Thumb, 156 bytes, Stack size 32 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  - >> _double_round
  [Called By]
  - >> __aeabi_ui2d
  - >> __aeabi_i2d
  - >> __aeabi_dmul
  - >> __aeabi_dadd

  ACMP0_IRQHandler (Thumb, 0 bytes, Stack size 8 bytes, vector_table_copy.o(.text.ACMP0_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = ACMP0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  ADC0_IRQHandler (Thumb, 0 bytes, Stack size 8 bytes, vector_table_copy.o(.text.ADC0_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = ADC0_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  BusFault_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.BusFault_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  CAN0_Error_IRQHandler (Thumb, 10 bytes, Stack size 0 bytes, flexcan_irq.o(.text.CAN0_Error_IRQHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = CAN0_Error_IRQHandler ⇒ FLEXCAN_Error_IRQHandler
  [Calls]
  - >> FLEXCAN_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_0_15_MB_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, flexcan_irq.o(.text.CAN0_ORed_0_15_MB_IRQHandler))
  [Stack]

  - Max Depth = 184
  - Call Chain = CAN0_ORed_0_15_MB_IRQHandler ⇒ FLEXCAN_IRQHandler ⇒ FLEXCAN_IRQHandlerRxMB ⇒ FLEXCAN_GetMsgBuff ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_16_31_MB_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, flexcan_irq.o(.text.CAN0_ORed_16_31_MB_IRQHandler))
  [Stack]

  - Max Depth = 184
  - Call Chain = CAN0_ORed_16_31_MB_IRQHandler ⇒ FLEXCAN_IRQHandler ⇒ FLEXCAN_IRQHandlerRxMB ⇒ FLEXCAN_GetMsgBuff ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_32_47_MB_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, flexcan_irq.o(.text.CAN0_ORed_32_47_MB_IRQHandler))
  [Stack]

  - Max Depth = 184
  - Call Chain = CAN0_ORed_32_47_MB_IRQHandler ⇒ FLEXCAN_IRQHandler ⇒ FLEXCAN_IRQHandlerRxMB ⇒ FLEXCAN_GetMsgBuff ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_48_63_MB_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, flexcan_irq.o(.text.CAN0_ORed_48_63_MB_IRQHandler))
  [Stack]

  - Max Depth = 184
  - Call Chain = CAN0_ORed_48_63_MB_IRQHandler ⇒ FLEXCAN_IRQHandler ⇒ FLEXCAN_IRQHandlerRxMB ⇒ FLEXCAN_GetMsgBuff ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_ORed_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, flexcan_irq.o(.text.CAN0_ORed_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN0_ORed_IRQHandler
  [Calls]
  - >> FLEXCAN_BusOff_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN0_Wake_Up_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, flexcan_irq.o(.text.CAN0_Wake_Up_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = CAN0_Wake_Up_IRQHandler ⇒ FLEXCAN_WakeUpHandler
  [Calls]
  - >> FLEXCAN_WakeUpHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_Error_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, flexcan_irq.o(.text.CAN1_Error_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = CAN1_Error_IRQHandler ⇒ FLEXCAN_Error_IRQHandler
  [Calls]
  - >> FLEXCAN_Error_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_0_15_MB_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, flexcan_irq.o(.text.CAN1_ORed_0_15_MB_IRQHandler))
  [Stack]

  - Max Depth = 184
  - Call Chain = CAN1_ORed_0_15_MB_IRQHandler ⇒ FLEXCAN_IRQHandler ⇒ FLEXCAN_IRQHandlerRxMB ⇒ FLEXCAN_GetMsgBuff ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_16_31_MB_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, flexcan_irq.o(.text.CAN1_ORed_16_31_MB_IRQHandler))
  [Stack]

  - Max Depth = 184
  - Call Chain = CAN1_ORed_16_31_MB_IRQHandler ⇒ FLEXCAN_IRQHandler ⇒ FLEXCAN_IRQHandlerRxMB ⇒ FLEXCAN_GetMsgBuff ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_32_47_MB_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, flexcan_irq.o(.text.CAN1_ORed_32_47_MB_IRQHandler))
  [Stack]

  - Max Depth = 184
  - Call Chain = CAN1_ORed_32_47_MB_IRQHandler ⇒ FLEXCAN_IRQHandler ⇒ FLEXCAN_IRQHandlerRxMB ⇒ FLEXCAN_GetMsgBuff ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_48_63_MB_IRQHandler (Thumb, 14 bytes, Stack size 8 bytes, flexcan_irq.o(.text.CAN1_ORed_48_63_MB_IRQHandler))
  [Stack]

  - Max Depth = 184
  - Call Chain = CAN1_ORed_48_63_MB_IRQHandler ⇒ FLEXCAN_IRQHandler ⇒ FLEXCAN_IRQHandlerRxMB ⇒ FLEXCAN_GetMsgBuff ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_ORed_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, flexcan_irq.o(.text.CAN1_ORed_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN1_ORed_IRQHandler
  [Calls]
  - >> FLEXCAN_BusOff_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CAN1_Wake_Up_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, flexcan_irq.o(.text.CAN1_Wake_Up_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = CAN1_Wake_Up_IRQHandler ⇒ FLEXCAN_WakeUpHandler
  [Calls]
  - >> FLEXCAN_WakeUpHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  CLOCK_DRV_GetFreq (Thumb, 276 bytes, Stack size 16 bytes, clock_ytm32b1mx.o(.text.CLOCK_DRV_GetFreq))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_DRV_GetFreq
  [Calls]
  - >> SCU_GetSysClkSrc
  - >> SCU_GetSysClkDiv
  - >> SCU_GetSlowBusClkDiv
  - >> SCU_GetFastBusClkDiv
  - >> CLOCK_GetIpcCtrlReg
  [Called By]
  - >> CLOCK_SYS_GetFreq

  CLOCK_DRV_Init (Thumb, 24 bytes, Stack size 8 bytes, clock_ytm32b1mx.o(.text.CLOCK_DRV_Init))
  [Stack]

  - Max Depth = 64
  - Call Chain = CLOCK_DRV_Init ⇒ CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_WaitFXOSCValid
  [Calls]
  - >> CLOCK_SYS_SetScuConfiguration
  - >> CLOCK_SYS_SetIpcConfiguration
  [Called By]
  - >> CLOCK_SYS_SetConfiguration

  CLOCK_SYS_GetFreq (Thumb, 8 bytes, Stack size 8 bytes, clock_ytm32b1mx.o(.text.CLOCK_SYS_GetFreq))
  [Stack]

  - Max Depth = 24
  - Call Chain = CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq
  [Calls]
  - >> CLOCK_DRV_GetFreq
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration
  - >> UART_DRV_Init
  - >> UART_DRV_SetBaudRate

  CLOCK_SYS_Init (Thumb, 56 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.CLOCK_SYS_Init))
  [Called By]

  - >> Board_Init

  CLOCK_SYS_SetConfiguration (Thumb, 8 bytes, Stack size 8 bytes, clock_ytm32b1mx.o(.text.CLOCK_SYS_SetConfiguration))
  [Stack]

  - Max Depth = 72
  - Call Chain = CLOCK_SYS_SetConfiguration ⇒ CLOCK_DRV_Init ⇒ CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_WaitFXOSCValid
  [Calls]
  - >> CLOCK_DRV_Init
  [Called By]
  - >> CLOCK_SYS_UpdateConfiguration

  CLOCK_SYS_UpdateConfiguration (Thumb, 348 bytes, Stack size 40 bytes, clock_ytm32b1mx.o(.text.CLOCK_SYS_UpdateConfiguration))
  [Stack]

  - Max Depth = 112
  - Call Chain = CLOCK_SYS_UpdateConfiguration ⇒ CLOCK_SYS_SetConfiguration ⇒ CLOCK_DRV_Init ⇒ CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_WaitFXOSCValid
  [Calls]
  - >> CLOCK_SYS_SetConfiguration
  - >> INT_SYS_EnableIRQGlobal
  - >> INT_SYS_DisableIRQGlobal
  [Called By]
  - >> Board_Init

  CLOCK_SYS_WaitFXOSCValid (Thumb, 90 bytes, Stack size 32 bytes, clock_ytm32b1mx.o(.text.CLOCK_SYS_WaitFXOSCValid))
  [Stack]

  - Max Depth = 32
  - Call Chain = CLOCK_SYS_WaitFXOSCValid
  [Calls]
  - >> SCU_SetFxoscGain
  - >> SCU_GetFXOSCValid
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  DMA0_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA0_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA0_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA1_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA1_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA1_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA2_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA2_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA2_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA3_IRQHandler (Thumb, 10 bytes, Stack size 8 bytes, dma_irq.o(.text.DMA3_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA3_IRQHandler ⇒ DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_IRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA_DRV_ErrorIRQHandler (Thumb, 76 bytes, Stack size 16 bytes, dma_driver.o(.text.DMA_DRV_ErrorIRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = DMA_DRV_ErrorIRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_SetDmaRequestCmd
  - >> DMA_DRV_ClearIntStatus
  - >> DMA_ClearErrorIntStatusFlag
  [Called By]
  - >> DMA_Error_IRQHandler

  DMA_DRV_GetDmaRegBaseAddr (Thumb, 10 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_DRV_GetDmaRegBaseAddr))
  [Called By]

  - >> DMA_Error_IRQHandler

  DMA_DRV_IRQHandler (Thumb, 38 bytes, Stack size 8 bytes, dma_driver.o(.text.DMA_DRV_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = DMA_DRV_IRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_DRV_ClearIntStatus
  [Called By]
  - >> DMA3_IRQHandler
  - >> DMA2_IRQHandler
  - >> DMA1_IRQHandler
  - >> DMA0_IRQHandler

  DMA_DRV_StopChannel (Thumb, 24 bytes, Stack size 8 bytes, dma_driver.o(.text.DMA_DRV_StopChannel))
  [Stack]

  - Max Depth = 8
  - Call Chain = DMA_DRV_StopChannel
  [Calls]
  - >> DMA_SetDmaRequestCmd
  [Called By]
  - >> FLEXCAN_CompleteRxMessageFifoData
  - >> UART_DRV_StopTxDma
  - >> UART_DRV_StopRxDma

  DMA_Error_IRQHandler (Thumb, 40 bytes, Stack size 16 bytes, dma_irq.o(.text.DMA_Error_IRQHandler))
  [Stack]

  - Max Depth = 48
  - Call Chain = DMA_Error_IRQHandler ⇒ DMA_DRV_ErrorIRQHandler ⇒ DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_GetErrorIntStatusFlag
  - >> DMA_DRV_GetDmaRegBaseAddr
  - >> DMA_DRV_ErrorIRQHandler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  DMA_SetDmaRequestCmd (Thumb, 22 bytes, Stack size 0 bytes, dma_hw_access.o(.text.DMA_SetDmaRequestCmd))
  [Called By]

  - >> DMA_DRV_StopChannel
  - >> DMA_DRV_ErrorIRQHandler

  DebugMon_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DebugMon_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  DefaultISR (Thumb, 2 bytes, Stack size 0 bytes, vector_table_copy.o(.text.DefaultISR))
  [Calls]

  - >> DefaultISR
  [Called By]
  - >> DefaultISR
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  EFM_Ecc_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_Ecc_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  EFM_Error_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_Error_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  EFM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EFM_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  EMU0_DB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EMU0_DB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  EMU0_SB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.EMU0_SB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  FLEXCAN_BusOff_IRQHandler (Thumb, 46 bytes, Stack size 0 bytes, flexcan_driver.o(.text.FLEXCAN_BusOff_IRQHandler))
  [Calls]

  - >> FLEXCAN_ClearBusOffIntStatusFlag
  [Called By]
  - >> CAN1_ORed_IRQHandler
  - >> CAN0_ORed_IRQHandler

  FLEXCAN_ClearBusOffIntStatusFlag (Thumb, 16 bytes, Stack size 0 bytes, flexcan_hw_access.o(.text.FLEXCAN_ClearBusOffIntStatusFlag))
  [Called By]

  - >> FLEXCAN_BusOff_IRQHandler

  FLEXCAN_ClearErrIntStatusFlag (Thumb, 22 bytes, Stack size 0 bytes, flexcan_hw_access.o(.text.FLEXCAN_ClearErrIntStatusFlag))
  [Called By]

  - >> FLEXCAN_Error_IRQHandler

  FLEXCAN_DRV_ConfigRxMb (Thumb, 144 bytes, Stack size 40 bytes, flexcan_driver.o(.text.FLEXCAN_DRV_ConfigRxMb))
  [Stack]

  - Max Depth = 96
  - Call Chain = FLEXCAN_DRV_ConfigRxMb ⇒ FLEXCAN_SetRxMsgBuff ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_SetRxMsgBuff
  - >> FLEXCAN_IsOutOfRangeMbIdx
  - >> FLEXCAN_ClearMsgBuffIntStatusFlag
  [Called By]
  - >> main

  FLEXCAN_DRV_ConfigTxMb (Thumb, 88 bytes, Stack size 48 bytes, flexcan_driver.o(.text.FLEXCAN_DRV_ConfigTxMb))
  [Stack]

  - Max Depth = 104
  - Call Chain = FLEXCAN_DRV_ConfigTxMb ⇒ FLEXCAN_SetTxMsgBuff ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_SetTxMsgBuff
  - >> FLEXCAN_IsOutOfRangeMbIdx
  [Called By]
  - >> main

  FLEXCAN_DRV_GetTransferStatus (Thumb, 34 bytes, Stack size 0 bytes, flexcan_driver.o(.text.FLEXCAN_DRV_GetTransferStatus))
  [Called By]

  - >> main

  FLEXCAN_DRV_Init (Thumb, 446 bytes, Stack size 56 bytes, flexcan_driver.o(.text.FLEXCAN_DRV_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = FLEXCAN_DRV_Init ⇒ FLEXCAN_SetMaxMsgBuffNum ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> OSIF_SemaDestroy
  - >> OSIF_SemaCreate
  - >> FLEXCAN_SetPayloadSize
  - >> FLEXCAN_SetOperationMode
  - >> FLEXCAN_SetMaxMsgBuffNum
  - >> FLEXCAN_Init
  - >> FLEXCAN_ExitFreezeMode
  - >> FLEXCAN_EnterFreezeMode
  - >> FLEXCAN_EnableRxFifo
  - >> FLEXCAN_Enable
  - >> FLEXCAN_Disable
  - >> FLEXCAN_SetTimeSegments
  - >> FLEXCAN_SetStuffBitCount
  - >> FLEXCAN_SetSelfReception
  - >> FLEXCAN_SetRxFifoDMA
  - >> FLEXCAN_SetFDTimeSegments
  - >> FLEXCAN_SetFDEnabled
  - >> FLEXCAN_SetExtendedTimeSegments
  - >> FLEXCAN_SelectClock
  - >> FLEXCAN_IsRxFifoEnabled
  - >> FLEXCAN_IsFDEnabled
  - >> FLEXCAN_IsEnabled
  - >> FLEXCAN_InstanceHasFD
  - >> FLEXCAN_EnableIRQs
  [Called By]
  - >> main

  FLEXCAN_DRV_Receive (Thumb, 48 bytes, Stack size 16 bytes, flexcan_driver.o(.text.FLEXCAN_DRV_Receive))
  [Stack]

  - Max Depth = 64
  - Call Chain = FLEXCAN_DRV_Receive ⇒ FLEXCAN_StartRxMessageBufferData ⇒ FLEXCAN_SetMsgBuffIntCmd
  [Calls]
  - >> FLEXCAN_IsOutOfRangeMbIdx
  - >> FLEXCAN_StartRxMessageBufferData
  [Called By]
  - >> main

  FLEXCAN_Disable (Thumb, 24 bytes, Stack size 0 bytes, flexcan_hw_access.o(.text.FLEXCAN_Disable))
  [Called By]

  - >> FLEXCAN_DRV_Init

  FLEXCAN_Enable (Thumb, 40 bytes, Stack size 0 bytes, flexcan_hw_access.o(.text.FLEXCAN_Enable))
  [Called By]

  - >> FLEXCAN_DRV_Init

  FLEXCAN_EnableRxFifo (Thumb, 68 bytes, Stack size 16 bytes, flexcan_hw_access.o(.text.FLEXCAN_EnableRxFifo))
  [Stack]

  - Max Depth = 24
  - Call Chain = FLEXCAN_EnableRxFifo ⇒ FLEXCAN_GetMaxMbNum
  [Calls]
  - >> FLEXCAN_GetMaxMbNum
  - >> FLEXCAN_IsFDEnabled
  [Called By]
  - >> FLEXCAN_DRV_Init

  FLEXCAN_EnterFreezeMode (Thumb, 174 bytes, Stack size 24 bytes, flexcan_hw_access.o(.text.FLEXCAN_EnterFreezeMode))
  [Stack]

  - Max Depth = 32
  - Call Chain = FLEXCAN_EnterFreezeMode ⇒ FLEXCAN_GetMaxMbNum
  [Calls]
  - >> FLEXCAN_GetMaxMbNum
  - >> FLEXCAN_IsFDEnabled
  - >> FLEXCAN_GetFreezeMode
  [Called By]
  - >> FLEXCAN_SetOperationMode
  - >> FLEXCAN_DRV_Init

  FLEXCAN_Error_IRQHandler (Thumb, 194 bytes, Stack size 16 bytes, flexcan_driver.o(.text.FLEXCAN_Error_IRQHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = FLEXCAN_Error_IRQHandler
  [Calls]
  - >> FLEXCAN_ClearErrIntStatusFlag
  [Called By]
  - >> CAN1_Error_IRQHandler
  - >> CAN0_Error_IRQHandler

  FLEXCAN_ExitFreezeMode (Thumb, 24 bytes, Stack size 0 bytes, flexcan_hw_access.o(.text.FLEXCAN_ExitFreezeMode))
  [Called By]

  - >> FLEXCAN_DRV_Init

  FLEXCAN_GetMaxMbNum (Thumb, 40 bytes, Stack size 8 bytes, flexcan_hw_access.o(.text.FLEXCAN_GetMaxMbNum))
  [Stack]

  - Max Depth = 8
  - Call Chain = FLEXCAN_GetMaxMbNum
  [Called By]
  - >> FLEXCAN_SetMaxMsgBuffNum
  - >> FLEXCAN_Init
  - >> FLEXCAN_EnterFreezeMode
  - >> FLEXCAN_EnableRxFifo
  - >> FLEXCAN_StartRxMessageBufferData
  - >> FLEXCAN_ClearRAM

  FLEXCAN_GetMsgBuff (Thumb, 134 bytes, Stack size 24 bytes, flexcan_hw_access.o(.text.FLEXCAN_GetMsgBuff))
  [Stack]

  - Max Depth = 48
  - Call Chain = FLEXCAN_GetMsgBuff ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_GetMsgBuffRegion
  - >> FLEXCAN_GetPayloadSize
  - >> FLEXCAN_ComputePayloadSize
  [Called By]
  - >> FLEXCAN_IRQHandler
  - >> FLEXCAN_IRQHandlerRxMB

  FLEXCAN_GetMsgBuffRegion (Thumb, 50 bytes, Stack size 16 bytes, flexcan_hw_access.o(.text.FLEXCAN_GetMsgBuffRegion))
  [Stack]

  - Max Depth = 24
  - Call Chain = FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_GetPayloadSize
  [Called By]
  - >> FLEXCAN_SetTxMsgBuff
  - >> FLEXCAN_SetRxMsgBuff
  - >> FLEXCAN_SetMaxMsgBuffNum
  - >> FLEXCAN_LockRxMsgBuff
  - >> FLEXCAN_GetMsgBuff
  - >> FLEXCAN_IRQHandlerRxMB

  FLEXCAN_GetPayloadSize (Thumb, 30 bytes, Stack size 8 bytes, flexcan_hw_access.o(.text.FLEXCAN_GetPayloadSize))
  [Stack]

  - Max Depth = 8
  - Call Chain = FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_IsFDEnabled
  [Called By]
  - >> FLEXCAN_SetMaxMsgBuffNum
  - >> FLEXCAN_GetMsgBuffRegion
  - >> FLEXCAN_GetMsgBuff

  FLEXCAN_IRQHandler (Thumb, 270 bytes, Stack size 104 bytes, flexcan_driver.o(.text.FLEXCAN_IRQHandler))
  [Stack]

  - Max Depth = 176
  - Call Chain = FLEXCAN_IRQHandler ⇒ FLEXCAN_IRQHandlerRxMB ⇒ FLEXCAN_GetMsgBuff ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_LockRxMsgBuff
  - >> FLEXCAN_GetMsgBuff
  - >> FLEXCAN_UnlockRxMsgBuff
  - >> FLEXCAN_IsRxFifoEnabled
  - >> FLEXCAN_IRQHandlerRxMB
  - >> FLEXCAN_IRQHandlerRxFIFO
  - >> FLEXCAN_GetMsgBuffIntStatusFlag
  - >> FLEXCAN_CompleteTransfer
  - >> FLEXCAN_ClearMsgBuffIntStatusFlag
  [Called By]
  - >> CAN1_ORed_48_63_MB_IRQHandler
  - >> CAN1_ORed_32_47_MB_IRQHandler
  - >> CAN1_ORed_16_31_MB_IRQHandler
  - >> CAN1_ORed_0_15_MB_IRQHandler
  - >> CAN0_ORed_48_63_MB_IRQHandler
  - >> CAN0_ORed_32_47_MB_IRQHandler
  - >> CAN0_ORed_16_31_MB_IRQHandler
  - >> CAN0_ORed_0_15_MB_IRQHandler

  FLEXCAN_Init (Thumb, 72 bytes, Stack size 16 bytes, flexcan_hw_access.o(.text.FLEXCAN_Init))
  [Stack]

  - Max Depth = 32
  - Call Chain = FLEXCAN_Init ⇒ FLEXCAN_ClearRAM ⇒ FLEXCAN_GetMaxMbNum
  [Calls]
  - >> FLEXCAN_GetMaxMbNum
  - >> FLEXCAN_ClearRAM
  [Called By]
  - >> FLEXCAN_DRV_Init

  FLEXCAN_IsOutOfRangeMbIdx (Thumb, 46 bytes, Stack size 16 bytes, flexcan_hw_access.o(.text.FLEXCAN_IsOutOfRangeMbIdx))
  [Stack]

  - Max Depth = 16
  - Call Chain = FLEXCAN_IsOutOfRangeMbIdx
  [Calls]
  - >> RxFifoOcuppiedLastMsgBuff
  - >> FLEXCAN_IsRxFifoEnabled
  [Called By]
  - >> FLEXCAN_DRV_Receive
  - >> FLEXCAN_DRV_ConfigTxMb
  - >> FLEXCAN_DRV_ConfigRxMb

  FLEXCAN_LockRxMsgBuff (Thumb, 10 bytes, Stack size 8 bytes, flexcan_hw_access.o(.text.FLEXCAN_LockRxMsgBuff))
  [Stack]

  - Max Depth = 32
  - Call Chain = FLEXCAN_LockRxMsgBuff ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_GetMsgBuffRegion
  [Called By]
  - >> FLEXCAN_IRQHandler
  - >> FLEXCAN_IRQHandlerRxMB

  FLEXCAN_ReadRxFifo (Thumb, 70 bytes, Stack size 16 bytes, flexcan_hw_access.o(.text.FLEXCAN_ReadRxFifo))
  [Stack]

  - Max Depth = 16
  - Call Chain = FLEXCAN_ReadRxFifo
  [Calls]
  - >> FLEXCAN_ComputePayloadSize
  [Called By]
  - >> FLEXCAN_IRQHandlerRxFIFO

  FLEXCAN_SetMaxMsgBuffNum (Thumb, 146 bytes, Stack size 32 bytes, flexcan_hw_access.o(.text.FLEXCAN_SetMaxMsgBuffNum))
  [Stack]

  - Max Depth = 56
  - Call Chain = FLEXCAN_SetMaxMsgBuffNum ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_GetMsgBuffRegion
  - >> FLEXCAN_GetMaxMbNum
  - >> FLEXCAN_GetPayloadSize
  - >> FLEXCAN_IsRxFifoEnabled
  [Called By]
  - >> FLEXCAN_DRV_Init

  FLEXCAN_SetMsgBuffIntCmd (Thumb, 74 bytes, Stack size 16 bytes, flexcan_hw_access.o(.text.FLEXCAN_SetMsgBuffIntCmd))
  [Stack]

  - Max Depth = 16
  - Call Chain = FLEXCAN_SetMsgBuffIntCmd
  [Calls]
  - >> INT_SYS_EnableIRQGlobal
  - >> INT_SYS_DisableIRQGlobal
  [Called By]
  - >> FLEXCAN_StartRxMessageBufferData
  - >> FLEXCAN_CompleteTransfer
  - >> FLEXCAN_CompleteRxMessageFifoData

  FLEXCAN_SetOperationMode (Thumb, 92 bytes, Stack size 8 bytes, flexcan_hw_access.o(.text.FLEXCAN_SetOperationMode))
  [Stack]

  - Max Depth = 40
  - Call Chain = FLEXCAN_SetOperationMode ⇒ FLEXCAN_EnterFreezeMode ⇒ FLEXCAN_GetMaxMbNum
  [Calls]
  - >> FLEXCAN_EnterFreezeMode
  - >> FLEXCAN_SetSelfReception
  [Called By]
  - >> FLEXCAN_DRV_Init

  FLEXCAN_SetPayloadSize (Thumb, 52 bytes, Stack size 16 bytes, flexcan_hw_access.o(.text.FLEXCAN_SetPayloadSize))
  [Stack]

  - Max Depth = 16
  - Call Chain = FLEXCAN_SetPayloadSize
  [Calls]
  - >> FLEXCAN_IsFDEnabled
  [Called By]
  - >> FLEXCAN_DRV_Init

  FLEXCAN_SetRxMsgBuff (Thumb, 180 bytes, Stack size 32 bytes, flexcan_hw_access.o(.text.FLEXCAN_SetRxMsgBuff))
  [Stack]

  - Max Depth = 56
  - Call Chain = FLEXCAN_SetRxMsgBuff ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_GetMsgBuffRegion
  - >> RxFifoOcuppiedLastMsgBuff
  [Called By]
  - >> FLEXCAN_DRV_ConfigRxMb

  FLEXCAN_SetTxMsgBuff (Thumb, 354 bytes, Stack size 32 bytes, flexcan_hw_access.o(.text.FLEXCAN_SetTxMsgBuff))
  [Stack]

  - Max Depth = 56
  - Call Chain = FLEXCAN_SetTxMsgBuff ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_GetMsgBuffRegion
  - >> RxFifoOcuppiedLastMsgBuff
  - >> FLEXCAN_IsFDEnabled
  - >> FLEXCAN_ComputePayloadSize
  - >> FLEXCAN_ComputeDLCValue
  [Called By]
  - >> FLEXCAN_DRV_ConfigTxMb

  FLEXCAN_WakeUpHandler (Thumb, 64 bytes, Stack size 16 bytes, flexcan_driver.o(.text.FLEXCAN_WakeUpHandler))
  [Stack]

  - Max Depth = 16
  - Call Chain = FLEXCAN_WakeUpHandler
  [Calls]
  - >> FLEXCAN_GetWAKINT
  - >> FLEXCAN_ClearWAKINT
  [Called By]
  - >> CAN1_Wake_Up_IRQHandler
  - >> CAN0_Wake_Up_IRQHandler

  GPIOA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOA_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOB_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOB_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOC_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOD_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  GPIOE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.GPIOE_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  HCU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.HCU_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  HardFault_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.HardFault_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  I2C0_Master_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C0_Master_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  I2C0_Slave_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C0_Slave_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  I2C1_Master_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.I2C1_Master_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  INT_SYS_DisableIRQGlobal (Thumb, 18 bytes, Stack size 0 bytes, interrupt_manager.o(.text.INT_SYS_DisableIRQGlobal))
  [Called By]

  - >> FLEXCAN_SetMsgBuffIntCmd
  - >> CLOCK_SYS_UpdateConfiguration
  - >> osif_DisableIrqGlobal

  INT_SYS_EnableIRQ (Thumb, 8 bytes, Stack size 8 bytes, interrupt_manager.o(.text.INT_SYS_EnableIRQ))
  [Stack]

  - Max Depth = 8
  - Call Chain = INT_SYS_EnableIRQ
  [Calls]
  - >> __NVIC_EnableIRQ
  [Called By]
  - >> FLEXCAN_EnableIRQs
  - >> UART_DRV_Init

  INT_SYS_EnableIRQGlobal (Thumb, 28 bytes, Stack size 0 bytes, interrupt_manager.o(.text.INT_SYS_EnableIRQGlobal))
  [Called By]

  - >> FLEXCAN_SetMsgBuffIntCmd
  - >> CLOCK_SYS_UpdateConfiguration
  - >> osif_EnableIrqGlobal

  INT_SYS_InstallHandler (Thumb, 30 bytes, Stack size 0 bytes, interrupt_manager.o(.text.INT_SYS_InstallHandler))
  [Called By]

  - >> UART_DRV_Init

  MPWM0_Ch0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM0_Ch0_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch0_Ovf_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM0_Ch1_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch1_Ovf_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM0_Ch2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch2_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM0_Ch2_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch2_Ovf_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM0_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM0_Ch3_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch3_Ovf_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM0_Ch4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch4_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM0_Ch4_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch4_Ovf_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM0_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch5_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM0_Ch5_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch5_Ovf_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM0_Ch6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch6_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM0_Ch6_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch6_Ovf_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM0_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch7_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MPWM0_Ch7_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MPWM0_Ch7_Ovf_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  MemManage_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.MemManage_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  NMI_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.NMI_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  OSIF_SemaCreate (Thumb, 20 bytes, Stack size 0 bytes, osif_baremetal.o(.text.OSIF_SemaCreate))
  [Stack]

  - Max Depth = 8
  - Call Chain = OSIF_SemaCreate ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> osif_EnableIrqGlobal
  - >> osif_DisableIrqGlobal
  [Called By]
  - >> UART_DRV_Init
  - >> FLEXCAN_DRV_Init

  OSIF_SemaDestroy (Thumb, 4 bytes, Stack size 0 bytes, osif_baremetal.o(.text.OSIF_SemaDestroy))
  [Called By]

  - >> FLEXCAN_DRV_Init

  OSIF_SemaPost (Thumb, 34 bytes, Stack size 8 bytes, osif_baremetal.o(.text.OSIF_SemaPost))
  [Stack]

  - Max Depth = 16
  - Call Chain = OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> osif_EnableIrqGlobal
  - >> osif_DisableIrqGlobal
  [Called By]
  - >> FLEXCAN_CompleteTransfer
  - >> FLEXCAN_CompleteRxMessageFifoData
  - >> UART_DRV_StopTxDma
  - >> UART_DRV_StopRxDma
  - >> UART_DRV_CompleteSendDataUsingInt
  - >> UART_DRV_CompleteReceiveDataUsingInt

  PCU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.PCU_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  PINS_DRV_Init (Thumb, 26 bytes, Stack size 16 bytes, pins_driver.o(.text.PINS_DRV_Init))
  [Stack]

  - Max Depth = 32
  - Call Chain = PINS_DRV_Init ⇒ PINS_Init
  [Calls]
  - >> PINS_Init
  [Called By]
  - >> Board_Init

  PINS_Init (Thumb, 258 bytes, Stack size 16 bytes, pins_port_hw_access.o(.text.PINS_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = PINS_Init
  [Calls]
  - >> PINS_GPIO_WritePin
  - >> PINS_ConfigDigitalFilter
  [Called By]
  - >> PINS_DRV_Init

  PendSV_Handler (Thumb, 0 bytes, Stack size 32 bytes, vector_table_copy.o(.text.PendSV_Handler))
  [Stack]

  - Max Depth = 32
  - Call Chain = PendSV_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  RamInit1 (Thumb, 248 bytes, Stack size 32 bytes, raminit1.o(.text.RamInit1))
  [Stack]

  - Max Depth = 32
  - Call Chain = RamInit1
  [Calls]
  - >> IsPOR
  - >> __aeabi_memclr4
  [Address Reference Count : 1]
  - startup.o(.text)

  RamInit2 (Thumb, 2 bytes, Stack size 0 bytes, raminit2.o(.text.RamInit2))
  [Address Reference Count : 1]

  - startup.o(.text)

  SCU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SCU_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SPI2_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SVC_Handler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.SVC_Handler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  SysTick_Handler (Thumb, 8 bytes, Stack size 0 bytes, osif_baremetal.o(.text.SysTick_Handler))
  [Calls]

  - >> osif_Tick
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  SystemInit (Thumb, 60 bytes, Stack size 0 bytes, system_ytm32b1mc0.o(.text.SystemInit))
  [Address Reference Count : 1]

  - startup.o(.text)

  TRNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.TRNG_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.UART0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  UART0_IrqHandler (Thumb, 10 bytes, Stack size 0 bytes, uart_irq.o(.text.UART0_IrqHandler))
  [Stack]

  - Max Depth = 88
  - Call Chain = UART0_IrqHandler ⇒ UART_DRV_IRQHandler ⇒ UART_DRV_RxIrqHandler ⇒ UART_DRV_CompleteReceiveDataUsingInt ⇒ UART_DRV_SetErrorInterrupts ⇒ UART_SetErrorInterrupts
  [Calls]
  - >> UART_DRV_IRQHandler
  [Address Reference Count : 1]
  - uart_irq.o(.data.g_uartIsr)

  UART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.UART1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  UART1_IrqHandler (Thumb, 10 bytes, Stack size 0 bytes, uart_irq.o(.text.UART1_IrqHandler))
  [Stack]

  - Max Depth = 88
  - Call Chain = UART1_IrqHandler ⇒ UART_DRV_IRQHandler ⇒ UART_DRV_RxIrqHandler ⇒ UART_DRV_CompleteReceiveDataUsingInt ⇒ UART_DRV_SetErrorInterrupts ⇒ UART_SetErrorInterrupts
  [Calls]
  - >> UART_DRV_IRQHandler
  [Address Reference Count : 1]
  - uart_irq.o(.data.g_uartIsr)

  UART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.UART2_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  UART2_IrqHandler (Thumb, 10 bytes, Stack size 0 bytes, uart_irq.o(.text.UART2_IrqHandler))
  [Stack]

  - Max Depth = 88
  - Call Chain = UART2_IrqHandler ⇒ UART_DRV_IRQHandler ⇒ UART_DRV_RxIrqHandler ⇒ UART_DRV_CompleteReceiveDataUsingInt ⇒ UART_DRV_SetErrorInterrupts ⇒ UART_SetErrorInterrupts
  [Calls]
  - >> UART_DRV_IRQHandler
  [Address Reference Count : 1]
  - uart_irq.o(.data.g_uartIsr)

  UART_ClearStatusFlag (Thumb, 8 bytes, Stack size 0 bytes, uart_hw_access.o(.text.UART_ClearStatusFlag))
  [Called By]

  - >> UART_DRV_ErrIrqHandler

  UART_DRV_IRQHandler (Thumb, 112 bytes, Stack size 16 bytes, uart_driver.o(.text.UART_DRV_IRQHandler))
  [Stack]

  - Max Depth = 88
  - Call Chain = UART_DRV_IRQHandler ⇒ UART_DRV_RxIrqHandler ⇒ UART_DRV_CompleteReceiveDataUsingInt ⇒ UART_DRV_SetErrorInterrupts ⇒ UART_SetErrorInterrupts
  [Calls]
  - >> UART_GetStatusFlag
  - >> UART_GetIntMode
  - >> UART_DRV_TxEmptyIrqHandler
  - >> UART_DRV_TxCompleteIrqHandler
  - >> UART_DRV_RxIrqHandler
  - >> UART_DRV_ErrIrqHandler
  [Called By]
  - >> UART2_IrqHandler
  - >> UART1_IrqHandler
  - >> UART0_IrqHandler

  UART_DRV_Init (Thumb, 218 bytes, Stack size 24 bytes, uart_driver.o(.text.UART_DRV_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = UART_DRV_Init ⇒ UART_DRV_SetBaudRate ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq
  [Calls]
  - >> OSIF_SemaCreate
  - >> INT_SYS_InstallHandler
  - >> INT_SYS_EnableIRQ
  - >> CLOCK_SYS_GetFreq
  - >> __aeabi_memclr
  - >> UART_SetParityMode
  - >> UART_SetBitCountPerChar
  - >> UART_Init
  - >> UART_DRV_SetLineIdleDetect
  - >> UART_DRV_SetBaudRate
  - >> UART_SetStopBitCount
  [Called By]
  - >> UTILITY_PRINT_Init

  UART_DRV_SendDataPolling (Thumb, 122 bytes, Stack size 24 bytes, uart_driver.o(.text.UART_DRV_SendDataPolling))
  [Stack]

  - Max Depth = 32
  - Call Chain = UART_DRV_SendDataPolling ⇒ UART_DRV_PutData
  [Calls]
  - >> UART_GetStatusFlag
  - >> UART_SetTransmitterCmd
  - >> UART_DRV_PutData
  [Called By]
  - >> printf_char

  UART_DRV_SetBaudRate (Thumb, 222 bytes, Stack size 40 bytes, uart_driver.o(.text.UART_DRV_SetBaudRate))
  [Stack]

  - Max Depth = 64
  - Call Chain = UART_DRV_SetBaudRate ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq
  [Calls]
  - >> CLOCK_SYS_GetFreq
  - >> UART_SetOversamplingRatio
  - >> UART_SetBaudRateDivisor
  - >> UART_EnableBothEdgeSamplingCmd
  [Called By]
  - >> UART_DRV_Init

  UART_DRV_SetLineIdleDetect (Thumb, 36 bytes, Stack size 16 bytes, uart_driver.o(.text.UART_DRV_SetLineIdleDetect))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_DRV_SetLineIdleDetect
  [Calls]
  - >> UART_SetIntMode
  - >> UART_SetLineIdleSize
  [Called By]
  - >> UART_DRV_Init

  UART_GetIntMode (Thumb, 10 bytes, Stack size 0 bytes, uart_hw_access.o(.text.UART_GetIntMode))
  [Called By]

  - >> UART_DRV_IRQHandler
  - >> UART_DRV_ErrIrqHandler

  UART_GetStatusFlag (Thumb, 10 bytes, Stack size 0 bytes, uart_hw_access.o(.text.UART_GetStatusFlag))
  [Called By]

  - >> UART_DRV_SendDataPolling
  - >> UART_DRV_IRQHandler
  - >> UART_DRV_ErrIrqHandler

  UART_Getchar10 (Thumb, 10 bytes, Stack size 0 bytes, uart_hw_access.o(.text.UART_Getchar10))
  [Called By]

  - >> UART_DRV_GetData

  UART_Getchar7 (Thumb, 10 bytes, Stack size 0 bytes, uart_hw_access.o(.text.UART_Getchar7))
  [Called By]

  - >> UART_DRV_GetData

  UART_Getchar8 (Thumb, 6 bytes, Stack size 0 bytes, uart_hw_access.o(.text.UART_Getchar8))
  [Called By]

  - >> UART_DRV_GetData

  UART_Getchar9 (Thumb, 10 bytes, Stack size 0 bytes, uart_hw_access.o(.text.UART_Getchar9))
  [Called By]

  - >> UART_DRV_GetData

  UART_Init (Thumb, 30 bytes, Stack size 0 bytes, uart_hw_access.o(.text.UART_Init))
  [Called By]

  - >> UART_DRV_Init

  UART_Putchar10 (Thumb, 4 bytes, Stack size 0 bytes, uart_hw_access.o(.text.UART_Putchar10))
  [Called By]

  - >> UART_DRV_PutData

  UART_Putchar9 (Thumb, 4 bytes, Stack size 0 bytes, uart_hw_access.o(.text.UART_Putchar9))
  [Called By]

  - >> UART_DRV_PutData

  UART_SetBitCountPerChar (Thumb, 20 bytes, Stack size 0 bytes, uart_hw_access.o(.text.UART_SetBitCountPerChar))
  [Called By]

  - >> UART_DRV_Init

  UART_SetErrorInterrupts (Thumb, 46 bytes, Stack size 16 bytes, uart_hw_access.o(.text.UART_SetErrorInterrupts))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_SetErrorInterrupts
  [Calls]
  - >> UART_SetIntMode
  [Called By]
  - >> UART_DRV_SetErrorInterrupts

  UART_SetIntMode (Thumb, 16 bytes, Stack size 0 bytes, uart_hw_access.o(.text.UART_SetIntMode))
  [Called By]

  - >> UART_SetErrorInterrupts
  - >> UART_DRV_SetLineIdleDetect
  - >> UART_DRV_TxEmptyIrqHandler
  - >> UART_DRV_StopTxDma
  - >> UART_DRV_SetErrorInterrupts
  - >> UART_DRV_CompleteSendDataUsingInt
  - >> UART_DRV_CompleteReceiveDataUsingInt

  UART_SetParityMode (Thumb, 24 bytes, Stack size 0 bytes, uart_hw_access.o(.text.UART_SetParityMode))
  [Called By]

  - >> UART_DRV_Init

  UTILITY_PRINT_Init (Thumb, 26 bytes, Stack size 8 bytes, utility_print_config.o(.text.UTILITY_PRINT_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = UTILITY_PRINT_Init ⇒ UART_DRV_Init ⇒ UART_DRV_SetBaudRate ⇒ CLOCK_SYS_GetFreq ⇒ CLOCK_DRV_GetFreq
  [Calls]
  - >> UART_DRV_Init
  [Called By]
  - >> Board_Init

  UsageFault_Handler (Thumb, 0 bytes, Stack size 8 bytes, vector_table_copy.o(.text.UsageFault_Handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = UsageFault_Handler
  [Address Reference Count : 1]
  - vector.o(.isr_vector)

  VectorTableCopy (Thumb, 74 bytes, Stack size 8 bytes, vector_table_copy.o(.text.VectorTableCopy))
  [Stack]

  - Max Depth = 8
  - Call Chain = VectorTableCopy
  [Calls]
  - >> __aeabi_memcpy4
  [Address Reference Count : 1]
  - startup.o(.text)

  WDG0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.WDG0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR0_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ch0_Ch1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR0_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ch2_Ch3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR0_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ch4_Ch5_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR0_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ch6_Ch7_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR0_Fault_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Fault_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR0_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR0_Ovf_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR1_Ch0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ch0_Ch1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR1_Ch2_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ch2_Ch3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR1_Ch4_Ch5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ch4_Ch5_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR1_Ch6_Ch7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ch6_Ch7_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR1_Fault_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Fault_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  eTMR1_Ovf_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.eTMR1_Ovf_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  lpTMR0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.lpTMR0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  main (Thumb, 164 bytes, Stack size 0 bytes, main.o(.text.main))
  [Stack]

  - Max Depth = 528
  - Call Chain = main ⇒ printf_ ⇒ _vsnprintf ⇒ _ftoa ⇒ _etoa ⇒ _ftoa (Cycle)
  [Calls]
  - >> printf_
  - >> FLEXCAN_DRV_Receive
  - >> FLEXCAN_DRV_Init
  - >> FLEXCAN_DRV_GetTransferStatus
  - >> FLEXCAN_DRV_ConfigTxMb
  - >> FLEXCAN_DRV_ConfigRxMb
  - >> Board_Init
  [Called By]
  - >> Reset_Handler

  pTMR0_Ch0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR0_Ch0_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR0_Ch1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR0_Ch1_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR0_Ch2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR0_Ch2_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  pTMR0_Ch3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, vector_table_copy.o(.text.pTMR0_Ch3_IRQHandler))
  [Address Reference Count : 1]

  - vector.o(.isr_vector)

  printf_ (Thumb, 56 bytes, Stack size 0 bytes, printf.o(.text.printf_))
  [Stack]

  - Max Depth = 528
  - Call Chain = printf_ ⇒ _vsnprintf ⇒ _ftoa ⇒ _etoa ⇒ _ftoa (Cycle)
  [Calls]
  - >> _vsnprintf
  [Called By]
  - >> main

  printf_char (Thumb, 24 bytes, Stack size 16 bytes, utility_print_config.o(.text.printf_char))
  [Stack]

  - Max Depth = 48
  - Call Chain = printf_char ⇒ UART_DRV_SendDataPolling ⇒ UART_DRV_PutData
  [Calls]
  - >> UART_DRV_SendDataPolling
  [Called By]
  - >> _out_char

  ### Local Symbols

  Board_Init (Thumb, 54 bytes, Stack size 8 bytes, main.o(.text.Board_Init))
  [Stack]

  - Max Depth = 120
  - Call Chain = Board_Init ⇒ CLOCK_SYS_UpdateConfiguration ⇒ CLOCK_SYS_SetConfiguration ⇒ CLOCK_DRV_Init ⇒ CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_WaitFXOSCValid
  [Calls]
  - >> UTILITY_PRINT_Init
  - >> PINS_DRV_Init
  - >> CLOCK_SYS_UpdateConfiguration
  - >> CLOCK_SYS_Init
  [Called By]
  - >> main

  IsPOR (Thumb, 16 bytes, Stack size 0 bytes, raminit1.o(.text.IsPOR))
  [Called By]

  - >> RamInit1

  CLOCK_GetIpcCtrlReg (Thumb, 26 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.CLOCK_GetIpcCtrlReg))
  [Called By]

  - >> CLOCK_DRV_GetFreq
  - >> CLOCK_SYS_SetIpcConfiguration

  CLOCK_SCU_WaitDividerStable (Thumb, 36 bytes, Stack size 8 bytes, clock_ytm32b1mx.o(.text.CLOCK_SCU_WaitDividerStable))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLOCK_SCU_WaitDividerStable
  [Calls]
  - >> SCU_GetDividerStable
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_ConfigureClkOut (Thumb, 18 bytes, Stack size 8 bytes, clock_ytm32b1mx.o(.text.CLOCK_SYS_ConfigureClkOut))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLOCK_SYS_ConfigureClkOut
  [Calls]
  - >> SCU_SetClkOutSrc
  - >> SCU_SetClkOutDiv
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_ConfigureSystemClock (Thumb, 40 bytes, Stack size 16 bytes, clock_ytm32b1mx.o(.text.CLOCK_SYS_ConfigureSystemClock))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_SYS_ConfigureSystemClock
  [Calls]
  - >> SCU_SetSysClkSrc
  - >> SCU_GetSysClkSrc
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_DisableClkOut (Thumb, 10 bytes, Stack size 8 bytes, clock_ytm32b1mx.o(.text.CLOCK_SYS_DisableClkOut))
  [Stack]

  - Max Depth = 8
  - Call Chain = CLOCK_SYS_DisableClkOut
  [Calls]
  - >> SCU_SetClkOutSrc
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_DisableCmu (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.CLOCK_SYS_DisableCmu))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_SetCmuChannelConfiguration (Thumb, 50 bytes, Stack size 16 bytes, clock_ytm32b1mx.o(.text.CLOCK_SYS_SetCmuChannelConfiguration))
  [Stack]

  - Max Depth = 24
  - Call Chain = CLOCK_SYS_SetCmuChannelConfiguration ⇒ SCU_SetCmuChResetEnable
  [Calls]
  - >> SCU_SetCmuChResetEnable
  - >> SCU_SetCmuChEnable
  - >> SCU_SetCmuChCompLow
  - >> SCU_SetCmuChCompHigh
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_SetDefaultCmuChannelConfiguration (Thumb, 64 bytes, Stack size 16 bytes, clock_ytm32b1mx.o(.text.CLOCK_SYS_SetDefaultCmuChannelConfiguration))
  [Stack]

  - Max Depth = 24
  - Call Chain = CLOCK_SYS_SetDefaultCmuChannelConfiguration ⇒ SCU_SetCmuChResetEnable
  [Calls]
  - >> SCU_SetCmuChResetEnable
  - >> SCU_SetCmuChEnable
  - >> SCU_SetCmuChCompLow
  - >> SCU_SetCmuChCompHigh
  [Called By]
  - >> CLOCK_SYS_SetScuConfiguration

  CLOCK_SYS_SetIpcConfiguration (Thumb, 64 bytes, Stack size 16 bytes, clock_ytm32b1mx.o(.text.CLOCK_SYS_SetIpcConfiguration))
  [Stack]

  - Max Depth = 16
  - Call Chain = CLOCK_SYS_SetIpcConfiguration
  [Calls]
  - >> IPC_SetPeripheralClockControl
  - >> IPC_SetClockMode
  - >> CLOCK_GetIpcCtrlReg
  [Called By]
  - >> CLOCK_DRV_Init

  CLOCK_SYS_SetScuConfiguration (Thumb, 310 bytes, Stack size 24 bytes, clock_ytm32b1mx.o(.text.CLOCK_SYS_SetScuConfiguration))
  [Stack]

  - Max Depth = 56
  - Call Chain = CLOCK_SYS_SetScuConfiguration ⇒ CLOCK_SYS_WaitFXOSCValid
  [Calls]
  - >> CLOCK_SYS_WaitFXOSCValid
  - >> CLOCK_SYS_GetFreq
  - >> SCU_SircStandbyEnable
  - >> SCU_SircDeepSleepEnable
  - >> SCU_SetSysClkDiv
  - >> SCU_SetSlowBusClkDiv
  - >> SCU_SetFxoscGain
  - >> SCU_SetFxoscBypassMode
  - >> SCU_SetFastBusClkDiv
  - >> SCU_FircDeepSleepEnable
  - >> SCU_EnableFxosc
  - >> SCU_EnableFirc
  - >> CLOCK_SYS_SetDefaultCmuChannelConfiguration
  - >> CLOCK_SYS_SetCmuChannelConfiguration
  - >> CLOCK_SYS_DisableCmu
  - >> CLOCK_SYS_DisableClkOut
  - >> CLOCK_SYS_ConfigureSystemClock
  - >> CLOCK_SYS_ConfigureClkOut
  - >> CLOCK_SCU_WaitDividerStable
  [Called By]
  - >> CLOCK_DRV_Init

  IPC_SetClockMode (Thumb, 10 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.IPC_SetClockMode))
  [Called By]

  - >> CLOCK_SYS_SetIpcConfiguration

  IPC_SetPeripheralClockControl (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.IPC_SetPeripheralClockControl))
  [Called By]

  - >> CLOCK_SYS_SetIpcConfiguration

  SCU_EnableFirc (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_EnableFirc))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_EnableFxosc (Thumb, 20 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_EnableFxosc))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_FircDeepSleepEnable (Thumb, 22 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_FircDeepSleepEnable))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_GetDividerStable (Thumb, 22 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_GetDividerStable))
  [Called By]

  - >> CLOCK_SCU_WaitDividerStable

  SCU_GetFXOSCValid (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_GetFXOSCValid))
  [Called By]

  - >> CLOCK_SYS_WaitFXOSCValid

  SCU_GetFastBusClkDiv (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_GetFastBusClkDiv))
  [Called By]

  - >> CLOCK_DRV_GetFreq

  SCU_GetSlowBusClkDiv (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_GetSlowBusClkDiv))
  [Called By]

  - >> CLOCK_DRV_GetFreq

  SCU_GetSysClkDiv (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_GetSysClkDiv))
  [Called By]

  - >> CLOCK_DRV_GetFreq

  SCU_GetSysClkSrc (Thumb, 16 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_GetSysClkSrc))
  [Called By]

  - >> CLOCK_DRV_GetFreq
  - >> CLOCK_SYS_ConfigureSystemClock

  SCU_SetClkOutDiv (Thumb, 22 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_SetClkOutDiv))
  [Called By]

  - >> CLOCK_SYS_ConfigureClkOut

  SCU_SetClkOutSrc (Thumb, 18 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_SetClkOutSrc))
  [Called By]

  - >> CLOCK_SYS_DisableClkOut
  - >> CLOCK_SYS_ConfigureClkOut

  SCU_SetCmuChCompHigh (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_SetCmuChCompHigh))
  [Called By]

  - >> CLOCK_SYS_SetDefaultCmuChannelConfiguration
  - >> CLOCK_SYS_SetCmuChannelConfiguration

  SCU_SetCmuChCompLow (Thumb, 14 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_SetCmuChCompLow))
  [Called By]

  - >> CLOCK_SYS_SetDefaultCmuChannelConfiguration
  - >> CLOCK_SYS_SetCmuChannelConfiguration

  SCU_SetCmuChEnable (Thumb, 32 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_SetCmuChEnable))
  [Called By]

  - >> CLOCK_SYS_SetDefaultCmuChannelConfiguration
  - >> CLOCK_SYS_SetCmuChannelConfiguration

  SCU_SetCmuChResetEnable (Thumb, 42 bytes, Stack size 8 bytes, clock_ytm32b1mx.o(.text.SCU_SetCmuChResetEnable))
  [Stack]

  - Max Depth = 8
  - Call Chain = SCU_SetCmuChResetEnable
  [Called By]
  - >> CLOCK_SYS_SetDefaultCmuChannelConfiguration
  - >> CLOCK_SYS_SetCmuChannelConfiguration

  SCU_SetFastBusClkDiv (Thumb, 18 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_SetFastBusClkDiv))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetFxoscBypassMode (Thumb, 24 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_SetFxoscBypassMode))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetFxoscGain (Thumb, 18 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_SetFxoscGain))
  [Called By]

  - >> CLOCK_SYS_WaitFXOSCValid
  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetSlowBusClkDiv (Thumb, 18 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_SetSlowBusClkDiv))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetSysClkDiv (Thumb, 18 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_SetSysClkDiv))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SetSysClkSrc (Thumb, 18 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_SetSysClkSrc))
  [Called By]

  - >> CLOCK_SYS_ConfigureSystemClock

  SCU_SircDeepSleepEnable (Thumb, 22 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_SircDeepSleepEnable))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  SCU_SircStandbyEnable (Thumb, 22 bytes, Stack size 0 bytes, clock_ytm32b1mx.o(.text.SCU_SircStandbyEnable))
  [Called By]

  - >> CLOCK_SYS_SetScuConfiguration

  PINS_ConfigDigitalFilter (Thumb, 32 bytes, Stack size 0 bytes, pins_port_hw_access.o(.text.PINS_ConfigDigitalFilter))
  [Called By]

  - >> PINS_Init

  PINS_GPIO_WritePin (Thumb, 22 bytes, Stack size 0 bytes, pins_port_hw_access.o(.text.PINS_GPIO_WritePin))
  [Called By]

  - >> PINS_Init

  __NVIC_EnableIRQ (Thumb, 32 bytes, Stack size 0 bytes, interrupt_manager.o(.text.__NVIC_EnableIRQ))
  [Called By]

  - >> INT_SYS_EnableIRQ

  DMA_ClearDoneStatusFlag (Thumb, 10 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_ClearDoneStatusFlag))
  [Called By]

  - >> DMA_DRV_ClearIntStatus

  DMA_ClearErrorIntStatusFlag (Thumb, 10 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_ClearErrorIntStatusFlag))
  [Called By]

  - >> DMA_DRV_ErrorIRQHandler

  DMA_ClearIntStatusFlag (Thumb, 12 bytes, Stack size 0 bytes, dma_driver.o(.text.DMA_ClearIntStatusFlag))
  [Called By]

  - >> DMA_DRV_ClearIntStatus

  DMA_DRV_ClearIntStatus (Thumb, 32 bytes, Stack size 16 bytes, dma_driver.o(.text.DMA_DRV_ClearIntStatus))
  [Stack]

  - Max Depth = 16
  - Call Chain = DMA_DRV_ClearIntStatus
  [Calls]
  - >> DMA_ClearIntStatusFlag
  - >> DMA_ClearDoneStatusFlag
  [Called By]
  - >> DMA_DRV_IRQHandler
  - >> DMA_DRV_ErrorIRQHandler

  DMA_GetErrorIntStatusFlag (Thumb, 4 bytes, Stack size 0 bytes, dma_irq.o(.text.DMA_GetErrorIntStatusFlag))
  [Called By]

  - >> DMA_Error_IRQHandler

  FLEXCAN_ClearMsgBuffIntStatusFlag (Thumb, 28 bytes, Stack size 0 bytes, flexcan_driver.o(.text.FLEXCAN_ClearMsgBuffIntStatusFlag))
  [Called By]

  - >> FLEXCAN_IRQHandler
  - >> FLEXCAN_IRQHandlerRxMB
  - >> FLEXCAN_IRQHandlerRxFIFO
  - >> FLEXCAN_DRV_ConfigRxMb

  FLEXCAN_ClearWAKINT (Thumb, 10 bytes, Stack size 0 bytes, flexcan_driver.o(.text.FLEXCAN_ClearWAKINT))
  [Called By]

  - >> FLEXCAN_WakeUpHandler

  FLEXCAN_CompleteRxMessageFifoData (Thumb, 172 bytes, Stack size 16 bytes, flexcan_driver.o(.text.FLEXCAN_CompleteRxMessageFifoData))
  [Stack]

  - Max Depth = 32
  - Call Chain = FLEXCAN_CompleteRxMessageFifoData ⇒ FLEXCAN_SetMsgBuffIntCmd
  [Calls]
  - >> FLEXCAN_SetMsgBuffIntCmd
  - >> DMA_DRV_StopChannel
  - >> OSIF_SemaPost
  [Called By]
  - >> FLEXCAN_IRQHandlerRxFIFO

  FLEXCAN_CompleteTransfer (Thumb, 58 bytes, Stack size 16 bytes, flexcan_driver.o(.text.FLEXCAN_CompleteTransfer))
  [Stack]

  - Max Depth = 32
  - Call Chain = FLEXCAN_CompleteTransfer ⇒ FLEXCAN_SetMsgBuffIntCmd
  [Calls]
  - >> FLEXCAN_SetMsgBuffIntCmd
  - >> OSIF_SemaPost
  [Called By]
  - >> FLEXCAN_IRQHandler
  - >> FLEXCAN_IRQHandlerRxMB

  FLEXCAN_EnableIRQs (Thumb, 96 bytes, Stack size 16 bytes, flexcan_driver.o(.text.FLEXCAN_EnableIRQs))
  [Stack]

  - Max Depth = 24
  - Call Chain = FLEXCAN_EnableIRQs ⇒ INT_SYS_EnableIRQ
  [Calls]
  - >> INT_SYS_EnableIRQ
  [Called By]
  - >> FLEXCAN_DRV_Init

  FLEXCAN_GetMsgBuffIntStatusFlag (Thumb, 52 bytes, Stack size 0 bytes, flexcan_driver.o(.text.FLEXCAN_GetMsgBuffIntStatusFlag))
  [Called By]

  - >> FLEXCAN_IRQHandler

  FLEXCAN_GetWAKINT (Thumb, 8 bytes, Stack size 0 bytes, flexcan_driver.o(.text.FLEXCAN_GetWAKINT))
  [Called By]

  - >> FLEXCAN_WakeUpHandler

  FLEXCAN_IRQHandlerRxFIFO (Thumb, 146 bytes, Stack size 16 bytes, flexcan_driver.o(.text.FLEXCAN_IRQHandlerRxFIFO))
  [Stack]

  - Max Depth = 48
  - Call Chain = FLEXCAN_IRQHandlerRxFIFO ⇒ FLEXCAN_CompleteRxMessageFifoData ⇒ FLEXCAN_SetMsgBuffIntCmd
  [Calls]
  - >> FLEXCAN_ReadRxFifo
  - >> FLEXCAN_CompleteRxMessageFifoData
  - >> FLEXCAN_ClearMsgBuffIntStatusFlag
  [Called By]
  - >> FLEXCAN_IRQHandler

  FLEXCAN_IRQHandlerRxMB (Thumb, 156 bytes, Stack size 24 bytes, flexcan_driver.o(.text.FLEXCAN_IRQHandlerRxMB))
  [Stack]

  - Max Depth = 72
  - Call Chain = FLEXCAN_IRQHandlerRxMB ⇒ FLEXCAN_GetMsgBuff ⇒ FLEXCAN_GetMsgBuffRegion ⇒ FLEXCAN_GetPayloadSize
  [Calls]
  - >> FLEXCAN_LockRxMsgBuff
  - >> FLEXCAN_GetMsgBuffRegion
  - >> FLEXCAN_GetMsgBuff
  - >> FLEXCAN_UnlockRxMsgBuff
  - >> FLEXCAN_IsRxFifoEnabled
  - >> FLEXCAN_CompleteTransfer
  - >> FLEXCAN_ClearMsgBuffIntStatusFlag
  [Called By]
  - >> FLEXCAN_IRQHandler

  FLEXCAN_InstanceHasFD (Thumb, 12 bytes, Stack size 0 bytes, flexcan_driver.o(.text.FLEXCAN_InstanceHasFD))
  [Called By]

  - >> FLEXCAN_DRV_Init

  FLEXCAN_IsEnabled (Thumb, 8 bytes, Stack size 0 bytes, flexcan_driver.o(.text.FLEXCAN_IsEnabled))
  [Called By]

  - >> FLEXCAN_DRV_Init

  FLEXCAN_IsFDEnabled (Thumb, 8 bytes, Stack size 0 bytes, flexcan_driver.o(.text.FLEXCAN_IsFDEnabled))
  [Called By]

  - >> FLEXCAN_DRV_Init

  FLEXCAN_IsRxFifoEnabled (Thumb, 8 bytes, Stack size 0 bytes, flexcan_driver.o(.text.FLEXCAN_IsRxFifoEnabled))
  [Called By]

  - >> FLEXCAN_IRQHandler
  - >> FLEXCAN_StartRxMessageBufferData
  - >> FLEXCAN_IRQHandlerRxMB
  - >> FLEXCAN_DRV_Init

  FLEXCAN_SelectClock (Thumb, 10 bytes, Stack size 0 bytes, flexcan_driver.o(.text.FLEXCAN_SelectClock))
  [Called By]

  - >> FLEXCAN_DRV_Init

  FLEXCAN_SetExtendedTimeSegments (Thumb, 70 bytes, Stack size 16 bytes, flexcan_driver.o(.text.FLEXCAN_SetExtendedTimeSegments))
  [Stack]

  - Max Depth = 16
  - Call Chain = FLEXCAN_SetExtendedTimeSegments
  [Called By]
  - >> FLEXCAN_DRV_Init

  FLEXCAN_SetFDEnabled (Thumb, 38 bytes, Stack size 0 bytes, flexcan_driver.o(.text.FLEXCAN_SetFDEnabled))
  [Called By]

  - >> FLEXCAN_DRV_Init

  FLEXCAN_SetFDTimeSegments (Thumb, 84 bytes, Stack size 16 bytes, flexcan_driver.o(.text.FLEXCAN_SetFDTimeSegments))
  [Stack]

  - Max Depth = 16
  - Call Chain = FLEXCAN_SetFDTimeSegments
  [Called By]
  - >> FLEXCAN_DRV_Init

  FLEXCAN_SetRxFifoDMA (Thumb, 14 bytes, Stack size 0 bytes, flexcan_driver.o(.text.FLEXCAN_SetRxFifoDMA))
  [Called By]

  - >> FLEXCAN_DRV_Init

  FLEXCAN_SetSelfReception (Thumb, 10 bytes, Stack size 0 bytes, flexcan_driver.o(.text.FLEXCAN_SetSelfReception))
  [Called By]

  - >> FLEXCAN_DRV_Init

  FLEXCAN_SetStuffBitCount (Thumb, 14 bytes, Stack size 0 bytes, flexcan_driver.o(.text.FLEXCAN_SetStuffBitCount))
  [Called By]

  - >> FLEXCAN_DRV_Init

  FLEXCAN_SetTimeSegments (Thumb, 66 bytes, Stack size 8 bytes, flexcan_driver.o(.text.FLEXCAN_SetTimeSegments))
  [Stack]

  - Max Depth = 8
  - Call Chain = FLEXCAN_SetTimeSegments
  [Called By]
  - >> FLEXCAN_DRV_Init

  FLEXCAN_StartRxMessageBufferData (Thumb, 136 bytes, Stack size 32 bytes, flexcan_driver.o(.text.FLEXCAN_StartRxMessageBufferData))
  [Stack]

  - Max Depth = 48
  - Call Chain = FLEXCAN_StartRxMessageBufferData ⇒ FLEXCAN_SetMsgBuffIntCmd
  [Calls]
  - >> FLEXCAN_SetMsgBuffIntCmd
  - >> FLEXCAN_GetMaxMbNum
  - >> RxFifoOcuppiedLastMsgBuff
  - >> FLEXCAN_IsRxFifoEnabled
  [Called By]
  - >> FLEXCAN_DRV_Receive

  FLEXCAN_UnlockRxMsgBuff (Thumb, 4 bytes, Stack size 0 bytes, flexcan_driver.o(.text.FLEXCAN_UnlockRxMsgBuff))
  [Called By]

  - >> FLEXCAN_IRQHandler
  - >> FLEXCAN_IRQHandlerRxMB

  RxFifoOcuppiedLastMsgBuff (Thumb, 14 bytes, Stack size 0 bytes, flexcan_driver.o(.text.RxFifoOcuppiedLastMsgBuff))
  [Called By]

  - >> FLEXCAN_StartRxMessageBufferData

  FLEXCAN_ClearRAM (Thumb, 66 bytes, Stack size 8 bytes, flexcan_hw_access.o(.text.FLEXCAN_ClearRAM))
  [Stack]

  - Max Depth = 16
  - Call Chain = FLEXCAN_ClearRAM ⇒ FLEXCAN_GetMaxMbNum
  [Calls]
  - >> FLEXCAN_GetMaxMbNum
  [Called By]
  - >> FLEXCAN_Init

  FLEXCAN_ComputeDLCValue (Thumb, 18 bytes, Stack size 0 bytes, flexcan_hw_access.o(.text.FLEXCAN_ComputeDLCValue))
  [Called By]

  - >> FLEXCAN_SetTxMsgBuff

  FLEXCAN_ComputePayloadSize (Thumb, 56 bytes, Stack size 0 bytes, flexcan_hw_access.o(.text.FLEXCAN_ComputePayloadSize))
  [Called By]

  - >> FLEXCAN_SetTxMsgBuff
  - >> FLEXCAN_ReadRxFifo
  - >> FLEXCAN_GetMsgBuff

  FLEXCAN_GetFreezeMode (Thumb, 8 bytes, Stack size 0 bytes, flexcan_hw_access.o(.text.FLEXCAN_GetFreezeMode))
  [Called By]

  - >> FLEXCAN_EnterFreezeMode

  FLEXCAN_IsFDEnabled (Thumb, 8 bytes, Stack size 0 bytes, flexcan_hw_access.o(.text.FLEXCAN_IsFDEnabled))
  [Called By]

  - >> FLEXCAN_SetTxMsgBuff
  - >> FLEXCAN_SetPayloadSize
  - >> FLEXCAN_EnterFreezeMode
  - >> FLEXCAN_EnableRxFifo
  - >> FLEXCAN_GetPayloadSize

  FLEXCAN_IsRxFifoEnabled (Thumb, 8 bytes, Stack size 0 bytes, flexcan_hw_access.o(.text.FLEXCAN_IsRxFifoEnabled))
  [Called By]

  - >> FLEXCAN_SetMaxMsgBuffNum
  - >> FLEXCAN_IsOutOfRangeMbIdx

  FLEXCAN_SetSelfReception (Thumb, 10 bytes, Stack size 0 bytes, flexcan_hw_access.o(.text.FLEXCAN_SetSelfReception))
  [Called By]

  - >> FLEXCAN_SetOperationMode

  RxFifoOcuppiedLastMsgBuff (Thumb, 14 bytes, Stack size 0 bytes, flexcan_hw_access.o(.text.RxFifoOcuppiedLastMsgBuff))
  [Called By]

  - >> FLEXCAN_SetTxMsgBuff
  - >> FLEXCAN_SetRxMsgBuff
  - >> FLEXCAN_IsOutOfRangeMbIdx

  UART_DRV_CompleteReceiveDataUsingInt (Thumb, 94 bytes, Stack size 24 bytes, uart_driver.o(.text.UART_DRV_CompleteReceiveDataUsingInt))
  [Stack]

  - Max Depth = 56
  - Call Chain = UART_DRV_CompleteReceiveDataUsingInt ⇒ UART_DRV_SetErrorInterrupts ⇒ UART_SetErrorInterrupts
  [Calls]
  - >> UART_SetIntMode
  - >> UART_SetReceiverCmd
  - >> UART_ResetRxFifo
  - >> UART_DRV_SetErrorInterrupts
  - >> OSIF_SemaPost
  [Called By]
  - >> UART_DRV_RxIrqHandler
  - >> UART_DRV_ErrIrqHandler

  UART_DRV_CompleteSendDataUsingInt (Thumb, 86 bytes, Stack size 16 bytes, uart_driver.o(.text.UART_DRV_CompleteSendDataUsingInt))
  [Stack]

  - Max Depth = 32
  - Call Chain = UART_DRV_CompleteSendDataUsingInt ⇒ OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> UART_SetIntMode
  - >> UART_SetTransmitterCmd
  - >> OSIF_SemaPost
  [Called By]
  - >> UART_DRV_TxCompleteIrqHandler

  UART_DRV_ErrIrqHandler (Thumb, 312 bytes, Stack size 16 bytes, uart_driver.o(.text.UART_DRV_ErrIrqHandler))
  [Stack]

  - Max Depth = 72
  - Call Chain = UART_DRV_ErrIrqHandler ⇒ UART_DRV_StopRxDma ⇒ UART_DRV_SetErrorInterrupts ⇒ UART_SetErrorInterrupts
  [Calls]
  - >> UART_GetStatusFlag
  - >> UART_GetIntMode
  - >> UART_ClearStatusFlag
  - >> UART_DRV_StopRxDma
  - >> UART_DRV_CompleteReceiveDataUsingInt
  [Called By]
  - >> UART_DRV_IRQHandler

  UART_DRV_GetData (Thumb, 96 bytes, Stack size 16 bytes, uart_driver.o(.text.UART_DRV_GetData))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_DRV_GetData
  [Calls]
  - >> UART_Getchar9
  - >> UART_Getchar8
  - >> UART_Getchar7
  - >> UART_Getchar10
  [Called By]
  - >> UART_DRV_RxIrqHandler

  UART_DRV_PutData (Thumb, 62 bytes, Stack size 8 bytes, uart_driver.o(.text.UART_DRV_PutData))
  [Stack]

  - Max Depth = 8
  - Call Chain = UART_DRV_PutData
  [Calls]
  - >> UART_Putchar9
  - >> UART_Putchar10
  - >> UART_Putchar
  [Called By]
  - >> UART_DRV_SendDataPolling
  - >> UART_DRV_TxEmptyIrqHandler

  UART_DRV_RxIrqHandler (Thumb, 134 bytes, Stack size 16 bytes, uart_driver.o(.text.UART_DRV_RxIrqHandler))
  [Stack]

  - Max Depth = 72
  - Call Chain = UART_DRV_RxIrqHandler ⇒ UART_DRV_CompleteReceiveDataUsingInt ⇒ UART_DRV_SetErrorInterrupts ⇒ UART_SetErrorInterrupts
  [Calls]
  - >> UART_GetWordCountInRxFifo
  - >> UART_DRV_GetData
  - >> UART_DRV_CompleteReceiveDataUsingInt
  [Called By]
  - >> UART_DRV_IRQHandler

  UART_DRV_SetErrorInterrupts (Thumb, 58 bytes, Stack size 16 bytes, uart_driver.o(.text.UART_DRV_SetErrorInterrupts))
  [Stack]

  - Max Depth = 32
  - Call Chain = UART_DRV_SetErrorInterrupts ⇒ UART_SetErrorInterrupts
  [Calls]
  - >> UART_SetIntMode
  - >> UART_SetErrorInterrupts
  [Called By]
  - >> UART_DRV_StopRxDma
  - >> UART_DRV_CompleteReceiveDataUsingInt

  UART_DRV_StopRxDma (Thumb, 102 bytes, Stack size 24 bytes, uart_driver.o(.text.UART_DRV_StopRxDma))
  [Stack]

  - Max Depth = 56
  - Call Chain = UART_DRV_StopRxDma ⇒ UART_DRV_SetErrorInterrupts ⇒ UART_SetErrorInterrupts
  [Calls]
  - >> DMA_DRV_StopChannel
  - >> UART_SetRxDmaCmd
  - >> UART_SetReceiverCmd
  - >> UART_ResetRxFifo
  - >> UART_DRV_SetErrorInterrupts
  - >> OSIF_SemaPost
  [Called By]
  - >> UART_DRV_ErrIrqHandler

  UART_DRV_StopTxDma (Thumb, 90 bytes, Stack size 16 bytes, uart_driver.o(.text.UART_DRV_StopTxDma))
  [Stack]

  - Max Depth = 32
  - Call Chain = UART_DRV_StopTxDma ⇒ OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> DMA_DRV_StopChannel
  - >> UART_SetIntMode
  - >> UART_SetTxDmaCmd
  - >> UART_SetTransmitterCmd
  - >> OSIF_SemaPost
  [Called By]
  - >> UART_DRV_TxCompleteIrqHandler

  UART_DRV_TxCompleteIrqHandler (Thumb, 56 bytes, Stack size 8 bytes, uart_driver.o(.text.UART_DRV_TxCompleteIrqHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = UART_DRV_TxCompleteIrqHandler ⇒ UART_DRV_StopTxDma ⇒ OSIF_SemaPost ⇒ osif_EnableIrqGlobal
  [Calls]
  - >> UART_DRV_StopTxDma
  - >> UART_DRV_CompleteSendDataUsingInt
  [Called By]
  - >> UART_DRV_IRQHandler

  UART_DRV_TxEmptyIrqHandler (Thumb, 152 bytes, Stack size 24 bytes, uart_driver.o(.text.UART_DRV_TxEmptyIrqHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = UART_DRV_TxEmptyIrqHandler ⇒ UART_DRV_PutData
  [Calls]
  - >> UART_SetIntMode
  - >> UART_GetWordCountInTxFifo
  - >> UART_GetTxFifoSize
  - >> UART_DRV_PutData
  [Called By]
  - >> UART_DRV_IRQHandler

  UART_EnableBothEdgeSamplingCmd (Thumb, 10 bytes, Stack size 0 bytes, uart_driver.o(.text.UART_EnableBothEdgeSamplingCmd))
  [Called By]

  - >> UART_DRV_SetBaudRate

  UART_GetTxFifoSize (Thumb, 14 bytes, Stack size 0 bytes, uart_driver.o(.text.UART_GetTxFifoSize))
  [Called By]

  - >> UART_DRV_TxEmptyIrqHandler

  UART_GetWordCountInRxFifo (Thumb, 8 bytes, Stack size 0 bytes, uart_driver.o(.text.UART_GetWordCountInRxFifo))
  [Called By]

  - >> UART_DRV_RxIrqHandler

  UART_GetWordCountInTxFifo (Thumb, 8 bytes, Stack size 0 bytes, uart_driver.o(.text.UART_GetWordCountInTxFifo))
  [Called By]

  - >> UART_DRV_TxEmptyIrqHandler

  UART_Putchar (Thumb, 4 bytes, Stack size 0 bytes, uart_driver.o(.text.UART_Putchar))
  [Called By]

  - >> UART_DRV_PutData

  UART_ResetRxFifo (Thumb, 8 bytes, Stack size 0 bytes, uart_driver.o(.text.UART_ResetRxFifo))
  [Called By]

  - >> UART_DRV_StopRxDma
  - >> UART_DRV_CompleteReceiveDataUsingInt

  UART_SetBaudRateDivisor (Thumb, 10 bytes, Stack size 0 bytes, uart_driver.o(.text.UART_SetBaudRateDivisor))
  [Called By]

  - >> UART_DRV_SetBaudRate

  UART_SetLineIdleSize (Thumb, 22 bytes, Stack size 0 bytes, uart_driver.o(.text.UART_SetLineIdleSize))
  [Called By]

  - >> UART_DRV_SetLineIdleDetect

  UART_SetOversamplingRatio (Thumb, 10 bytes, Stack size 0 bytes, uart_driver.o(.text.UART_SetOversamplingRatio))
  [Called By]

  - >> UART_DRV_SetBaudRate

  UART_SetReceiverCmd (Thumb, 24 bytes, Stack size 0 bytes, uart_driver.o(.text.UART_SetReceiverCmd))
  [Called By]

  - >> UART_DRV_StopRxDma
  - >> UART_DRV_CompleteReceiveDataUsingInt

  UART_SetRxDmaCmd (Thumb, 14 bytes, Stack size 0 bytes, uart_driver.o(.text.UART_SetRxDmaCmd))
  [Called By]

  - >> UART_DRV_StopRxDma

  UART_SetStopBitCount (Thumb, 14 bytes, Stack size 0 bytes, uart_driver.o(.text.UART_SetStopBitCount))
  [Called By]

  - >> UART_DRV_Init

  UART_SetTransmitterCmd (Thumb, 32 bytes, Stack size 0 bytes, uart_driver.o(.text.UART_SetTransmitterCmd))
  [Called By]

  - >> UART_DRV_SendDataPolling
  - >> UART_DRV_StopTxDma
  - >> UART_DRV_CompleteSendDataUsingInt

  UART_SetTxDmaCmd (Thumb, 14 bytes, Stack size 0 bytes, uart_driver.o(.text.UART_SetTxDmaCmd))
  [Called By]

  - >> UART_DRV_StopTxDma

  osif_DisableIrqGlobal (Thumb, 8 bytes, Stack size 8 bytes, osif_baremetal.o(.text.osif_DisableIrqGlobal))
  [Stack]

  - Max Depth = 8
  - Call Chain = osif_DisableIrqGlobal
  [Calls]
  - >> INT_SYS_DisableIRQGlobal
  [Called By]
  - >> OSIF_SemaCreate
  - >> OSIF_SemaPost

  osif_EnableIrqGlobal (Thumb, 8 bytes, Stack size 8 bytes, osif_baremetal.o(.text.osif_EnableIrqGlobal))
  [Stack]

  - Max Depth = 8
  - Call Chain = osif_EnableIrqGlobal
  [Calls]
  - >> INT_SYS_EnableIRQGlobal
  [Called By]
  - >> OSIF_SemaCreate
  - >> OSIF_SemaPost

  osif_Tick (Thumb, 16 bytes, Stack size 0 bytes, osif_baremetal.o(.text.osif_Tick))
  [Called By]

  - >> SysTick_Handler

  _atoi (Thumb, 64 bytes, Stack size 16 bytes, printf.o(.text._atoi))
  [Stack]

  - Max Depth = 16
  - Call Chain = _atoi
  [Calls]
  - >> _is_digit
  [Called By]
  - >> _vsnprintf

  _etoa (Thumb, 974 bytes, Stack size 96 bytes, printf.o(.text._etoa))
  [Stack]

  - Max Depth = 304 + In Cycle
  - Call Chain = _etoa ⇒ _ftoa (Cycle)
  [Calls]
  - >> __aeabi_i2d
  - >> __aeabi_dsub
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dcmplt
  - >> __aeabi_dcmpgt
  - >> __aeabi_dcmpge
  - >> __aeabi_dadd
  - >> __aeabi_d2iz
  - >> _ntoa_long
  - >> _ftoa
  [Called By]
  - >> _vsnprintf
  - >> _ftoa

  _ftoa (Thumb, 876 bytes, Stack size 120 bytes, printf.o(.text._ftoa))
  [Stack]

  - Max Depth = 424
  - Call Chain = _ftoa ⇒ _etoa ⇒ _ftoa (Cycle)
  [Calls]
  - >> __aeabi_memset4
  - >> __aeabi_memset
  - >> __aeabi_ui2d
  - >> __aeabi_i2d
  - >> __aeabi_dsub
  - >> __aeabi_dmul
  - >> __aeabi_dcmplt
  - >> __aeabi_dcmple
  - >> __aeabi_dcmpgt
  - >> __aeabi_dcmpge
  - >> __aeabi_d2uiz
  - >> __aeabi_d2iz
  - >> _out_rev
  - >> _etoa
  [Called By]
  - >> _vsnprintf
  - >> _etoa

  _is_digit (Thumb, 14 bytes, Stack size 0 bytes, printf.o(.text._is_digit))
  [Called By]

  - >> _vsnprintf
  - >> _atoi

  _ntoa_format (Thumb, 290 bytes, Stack size 56 bytes, printf.o(.text._ntoa_format))
  [Stack]

  - Max Depth = 104
  - Call Chain = _ntoa_format ⇒ _out_rev
  [Calls]
  - >> __aeabi_memset
  - >> _out_rev
  [Called By]
  - >> _ntoa_long_long
  - >> _ntoa_long

  _ntoa_long (Thumb, 148 bytes, Stack size 104 bytes, printf.o(.text._ntoa_long))
  [Stack]

  - Max Depth = 208
  - Call Chain = _ntoa_long ⇒ _ntoa_format ⇒ _out_rev
  [Calls]
  - >> _ntoa_format
  [Called By]
  - >> _vsnprintf
  - >> _etoa

  _ntoa_long_long (Thumb, 164 bytes, Stack size 112 bytes, printf.o(.text._ntoa_long_long))
  [Stack]

  - Max Depth = 216
  - Call Chain = _ntoa_long_long ⇒ _ntoa_format ⇒ _out_rev
  [Calls]
  - >> __aeabi_uldivmod
  - >> _ntoa_format
  [Called By]
  - >> _vsnprintf

  _out_char (Thumb, 18 bytes, Stack size 8 bytes, printf.o(.text._out_char))
  [Stack]

  - Max Depth = 56
  - Call Chain = _out_char ⇒ printf_char ⇒ UART_DRV_SendDataPolling ⇒ UART_DRV_PutData
  [Calls]
  - >> printf_char
  [Address Reference Count : 1]
  - printf.o(.text.printf_)

  _out_null (Thumb, 2 bytes, Stack size 0 bytes, printf.o(.text._out_null))
  [Address Reference Count : 1]

  - printf.o(.text._vsnprintf)

  _out_rev (Thumb, 168 bytes, Stack size 48 bytes, printf.o(.text._out_rev))
  [Stack]

  - Max Depth = 48
  - Call Chain = _out_rev
  [Called By]
  - >> _ntoa_format
  - >> _ftoa

  _strnlen_s (Thumb, 32 bytes, Stack size 0 bytes, printf.o(.text._strnlen_s))
  [Called By]

  - >> _vsnprintf

  _vsnprintf (Thumb, 1506 bytes, Stack size 104 bytes, printf.o(.text._vsnprintf))
  [Stack]

  - Max Depth = 528
  - Call Chain = _vsnprintf ⇒ _ftoa ⇒ _etoa ⇒ _ftoa (Cycle)
  [Calls]
  - >> _strnlen_s
  - >> _ntoa_long_long
  - >> _ntoa_long
  - >> _is_digit
  - >> _ftoa
  - >> _etoa
  - >> _atoi
  [Called By]
  - >> printf_

  ### Undefined Global Symbols