# Project Name: CddSent_Int_Demo

## Functional Description

- This demo shows MCAL-based SENT receive using interrupt mode.
- CH0 is configured as the active SENT receive channel.
- Fast and slow messages are received by SENT interrupts and printed through `CddUart`.
- DMA is not used in this demo.

## Operation Instructions

- Step 1: Open `CddSent_Int_Demo.yct` with YCT.
- Step 2: Generate code if you need to adapt pins, clocks, or UART settings.
- Step 3: Build the project and flash `build/CddSent_Int_Demo.elf`.
- Step 4: Open a serial terminal at `115200 8N1`.
- Step 5: Start the SENT sender and observe fast/slow receive statistics on UART.

## Key Files

- `app/main.c`
- `board/sent_config.c`
- `Mcal/CddSent/inc/sent_port_adapter.h`

## Hardware Requirement

- EVB: `YTM32B1MD1-EVB-Q100-Rev.A/B`
- Debugger: J-Link HW v9 or later

## Software Requirement

- YCT v2.7.0 or later
- GCC v10.3 or later, or equivalent supported toolchain
