{
  "project": {
    "clangd": {
      "enable": false,
      "path": ""
    },
    "cmakeGcc": {
      "optimization": "-O1",
      "funcSection": true,
      "dataSection": true,
      "compOthers": "",
      "removeSection": true,
      "linkOthers": "",
      "charSigned": false,
      "bitunsigned": false,
      "oninline": false,
      "floatABI": "",
      "library": "-specs=nosys.specs",
      "debuglevel": "-g",
      "gcov": false,
      "debugformat": "",
      "nocommon": false,
      "ffreestanding": false,
      "fnobuiltin": false,
      "singleprecisionconstant": false,
      "flto": false,
      "fnomoveloopinvariants": false,
      "printremoveSection": false,
      "noStartup": true,
      "suppress": {
        "variable": true,
        "parameter": true,
        "function": true,
        "setVariable": true,
        "result": true,
        "uninitialized": true,
        "compare": true,
        "aliasing": true,
        "pragmas": true,
        "format": true
      }
    },
    "cmakeGeneral": {
      "genbin": false,
      "genhex": true,
      "genlst": false,
      "gens19": false,
      "userDefine": ""
    },
    "debug": {
      "enable": false,
      "servertype": "jlink",
      "interface": "swd",
      "runToEntryPoint": "main",
      "gdbPath": "C:\\Program Files (x86)\\SEGGER\\JLink\\JLinkGDBServerCL.exe",
      "svdPath": "${workspaceFolder}/.vscode/chip.svd",
      "rttConfig": {
        "enable": false,
        "port": 0
      },
      "liveWatch": {
        "enable": true,
        "samplesPerSecond": 4
      }
    },
    "family": "YTM32B1MD1",
    "flexLink": true,
    "generate": {
      "folder": "board",
      "keepUserCode": true,
      "initBoard": true,
      "initBoardFuncName": "Board_Init",
      "enableVariants": false,
      "variantName": "",
      "variantList": [],
      "lockConfigCode": true,
      "lockSourceCode": true
    },
    "git": {
      "enable": false,
      "path": ".cache,build,.vscode"
    },
    "heapSize": "200",
    "hfVersion": "001",
    "ideDeviceName": "YTM32B1MD14",
    "initList": [
      {
        "funcName": "CLOCK_SYS_Init  ",
        "value": "CLOCK_SYS_Init(g_clockManConfigsArr,CLOCK_MANAGER_CONFIG_CNT,g_clockManCallbacksArr,CLOCK_MANAGER_CALLBACK_CNT);",
        "id": "91c1d80e-c3be-4420-8537-a01c5385bac1",
        "errorHandler": false,
        "successLabel": "0"
      },
      {
        "funcName": "CLOCK_SYS_UpdateConfiguration",
        "value": "CLOCK_SYS_UpdateConfiguration(CLOCK_MANAGER_ACTIVE_INDEX,CLOCK_MANAGER_POLICY_AGREEMENT);",
        "id": "16243663-9f35-49c9-bc83-02390dc32933",
        "errorHandler": false,
        "successLabel": "0"
      },
      {
        "funcName": "PINS_DRV_Init   ",
        "value": "PINS_DRV_Init(NUM_OF_CONFIGURED_PINS0,g_pin_mux_InitConfigArr0);",
        "id": "e57d801f-23f3-489f-9042-dd382818c31c",
        "errorHandler": false,
        "successLabel": "0"
      },
      {
        "funcName": "WDG_DRV_Init    ",
        "value": "WDG_DRV_Init(0,&wdg_config0);",
        "id": "1c679ea4-175f-4f3d-98b3-9bf2d31d2ddf",
        "errorHandler": false,
        "successLabel": "0"
      },
      {
        "funcName": "DMA_DRV_Init    ",
        "value": "DMA_DRV_Init(&dmaState,&dmaController_InitConfig,dmaChnState,dmaChnConfigArray,NUM_OF_CONFIGURED_DMA_CHANNEL);",
        "id": "96cee43e-5888-4f27-bd30-5635b1427240",
        "errorHandler": false,
        "successLabel": "0"
      },
      {
        "funcName": "FLEXCAN_DRV_Init",
        "value": "FLEXCAN_DRV_Init(0,&flexcanInitConfig0_State,&flexcanInitConfig0);",
        "id": "a6e3e496-c4f7-48f8-ae3c-57fdfb172647",
        "errorHandler": false,
        "successLabel": "0"
      },
      {
        "funcName": "eTMR_DRV_Init   ",
        "value": "eTMR_DRV_Init(0,&ETMR_CM_Config0,&ETMR_CM_Config0_State);",
        "id": "c2c77164-0127-4c98-8e40-a1c061ded499",
        "errorHandler": false,
        "successLabel": "0"
      },
      {
        "funcName": "eTMR_DRV_Init   ",
        "value": "eTMR_DRV_Init(1,&ETMR_CM_Config1,&ETMR_CM_Config1_State);",
        "id": "b428ef4b-81b3-412d-93fb-da4beeb6cf6d",
        "errorHandler": false,
        "successLabel": "0"
      },
      {
        "funcName": "eTMR_DRV_Init   ",
        "value": "eTMR_DRV_Init(2,&ETMR_CM_Config2,&ETMR_CM_Config2_State);",
        "id": "4c1dcfc5-009a-499c-9698-910e85789b76",
        "errorHandler": false,
        "successLabel": "0"
      },
      {
        "funcName": "ADC_DRV_ConfigConverter",
        "value": "ADC_DRV_ConfigConverter(0,&adc_config0);",
        "id": "c86e1f51-0e23-4ebc-a6b3-38d6b4039044",
        "errorHandler": false,
        "successLabel": "0"
      },
      {
        "funcName": "Fee_Init        ",
        "value": "Fee_Init(&FEEGenConfig);",
        "id": "8b26ff1b-1e25-485b-94ed-09a16e30e110",
        "errorHandler": false,
        "successLabel": "0"
      },
      {
        "funcName": "SPI_DRV_MasterInit",
        "value": "SPI_DRV_MasterInit(2,&spi_MasterConfig0_State,&spi_MasterConfig0);",
        "id": "a8196d5d-0047-4622-b8e3-0eb1664d65cd",
        "errorHandler": false,
        "successLabel": "0"
      },
      {
        "funcName": "HCU_DRV_Init    ",
        "value": "HCU_DRV_Init(&hcu_config0,&hcu_config0_State);",
        "id": "508c013c-346e-44fe-b52c-7058f4249ba8",
        "errorHandler": false,
        "successLabel": "0"
      },
      {
        "funcName": "lpTMR_DRV_InitConfigStruct",
        "value": "lpTMR_DRV_InitConfigStruct(lptmr_config_t * const config);",
        "id": "1b383465-31b0-4d2f-885a-ac6cba2e2f06",
        "errorHandler": false,
        "successLabel": "0"
      },
      {
        "funcName": "SPI_DRV_MasterInit",
        "value": "SPI_DRV_MasterInit(0,&spi_MasterConfig0_State,&spi_MasterConfig0);",
        "id": "16c01679-243f-4ccb-b512-6a054c9bce6d",
        "errorHandler": false,
        "successLabel": "0"
      },
      {
        "funcName": "POWER_SYS_Init  ",
        "value": "POWER_SYS_Init(&powerConfigsArr,POWER_MANAGER_CONFIG_CNT,&powerStaticCallbacksConfigsArr,POWER_MANAGER_CALLBACK_CNT);",
        "id": "f52f8cac-54d8-49e2-bade-7579ee288710",
        "errorHandler": false,
        "successLabel": "0"
      },
      {
        "funcName": "Fee_EraseImmediateBlock",
        "value": "Fee_EraseImmediateBlock(uint16_t BlockNumber);",
        "id": "b4e25e31-ea1c-4130-9ae3-cae5d010ad35",
        "errorHandler": false,
        "successLabel": "0"
      }
    ],
    "linkfile": "",
    "links": [],
    "name": "H24_100PIN",
    "ozone": {
      "enable": false,
      "interface": "SWD",
      "path": ""
    },
    "partNumber": "YTM32B1MD14G0MLLT",
    "sdkVersion": "1_3_1",
    "sections": [],
    "stackSize": "400",
    "targetToolOpt": {
      "KEIL": {
        "device": {
          "depends": [],
          "cdefines": []
        },
        "ytlink": {
          "linkflags": [
            "--no_startup",
            "--diag_suppress=L6314W,L6221E,L6329W",
            "--keep=*(.isr_vector)"
          ]
        }
      },
      "EWARM": {
        "device": {
          "depends": [],
          "cdefines": []
        }
      },
      "CMakeKEIL": {
        "device": {
          "depends": [],
          "cdefines": []
        },
        "ytlink": {
          "linkflags": [
            "--no_startup",
            "--diag_suppress=L6314W,L6221E,L6329W",
            "--keep=*(.isr_vector)"
          ]
        }
      },
      "CMakeGCC": {
        "device": {
          "depends": [],
          "cdefines": []
        }
      },
      "CMakeEWARM": {
        "device": {
          "depends": [],
          "cdefines": []
        }
      },
      "CMakeGHS": {
        "device": {
          "depends": [],
          "cdefines": []
        }
      }
    },
    "toolOpt": {
      "addData": {
        "cdefines": [],
        "asmdefines": [],
        "cincludes": [],
        "aincludes": [],
        "cflags": [],
        "aflags": [],
        "linkflags": [],
        "depends": []
      },
      "deleteData": {
        "cdefines": [],
        "asmdefines": [],
        "cincludes": [],
        "aincludes": [],
        "cflags": [],
        "aflags": [],
        "linkflags": [],
        "depends": []
      }
    },
    "toolchain": "KEIL",
    "toolchainPath": "",
    "toolchainVer": "",
    "type": "sdk",
    "useYtLink": true,
    "yctFileName": "project.yct"
  },
  "data": {
    "pins": {
      "enable": {},
      "data": [
        {
          "base": "PCTRLE",
          "gpioBase": "GPIOE",
          "num": "1",
          "label": "PTE_16",
          "feature": "eTMR2_CH7",
          "alt": "PCTRL_MUX_ALT4",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLE",
          "gpioBase": "GPIOE",
          "num": "17",
          "label": "PTE_14",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_INPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLE",
          "gpioBase": "GPIOE",
          "num": "19",
          "label": "PTE_12",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_OUTPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": "0",
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLD",
          "gpioBase": "GPIOD",
          "num": "22",
          "label": "PTD_15",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_OUTPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLE",
          "gpioBase": "GPIOE",
          "num": "26",
          "label": "PTE_8",
          "feature": "eTMR0_CH6",
          "alt": "PCTRL_MUX_ALT2",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLC",
          "gpioBase": "GPIOC",
          "num": "29",
          "label": "PTC_3",
          "feature": "CAN0_TX",
          "alt": "PCTRL_MUX_ALT3",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLC",
          "gpioBase": "GPIOC",
          "num": "30",
          "label": "PTC_2",
          "feature": "CAN0_RX",
          "alt": "PCTRL_MUX_ALT3",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLB",
          "gpioBase": "GPIOB",
          "num": "27",
          "label": "PTB_5",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_OUTPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": "1",
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLB",
          "gpioBase": "GPIOB",
          "num": "28",
          "label": "PTB_4",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_OUTPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLD",
          "gpioBase": "GPIOD",
          "num": "33",
          "label": "PTD_5",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_INPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLD",
          "gpioBase": "GPIOD",
          "num": "41",
          "label": "PTD_9",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_OUTPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": "1",
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLD",
          "gpioBase": "GPIOD",
          "num": "42",
          "label": "PTD_8",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_INPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLC",
          "gpioBase": "GPIOC",
          "num": "43",
          "label": "PTC_17",
          "feature": "ADC0_SE15",
          "alt": "PCTRL_PIN_DISABLED",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLC",
          "gpioBase": "GPIOC",
          "num": "46",
          "label": "PTC_14",
          "feature": "SPI2_PCS0",
          "alt": "PCTRL_MUX_ALT3",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLC",
          "gpioBase": "GPIOC",
          "num": "45",
          "label": "PTC_15",
          "feature": "SPI2_SCK",
          "alt": "PCTRL_MUX_ALT3",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLC",
          "gpioBase": "GPIOC",
          "num": "52",
          "label": "PTC_10",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_OUTPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLC",
          "gpioBase": "GPIOC",
          "num": "55",
          "label": "PTC_9",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_INPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLC",
          "gpioBase": "GPIOC",
          "num": "56",
          "label": "PTC_8",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_OUTPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLB",
          "gpioBase": "GPIOB",
          "num": "65",
          "label": "PTB_15",
          "feature": "ADC0_SE30",
          "alt": "PCTRL_PIN_DISABLED",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLB",
          "gpioBase": "GPIOB",
          "num": "66",
          "label": "PTB_14",
          "feature": "ADC0_SE25",
          "alt": "PCTRL_PIN_DISABLED",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLD",
          "gpioBase": "GPIOD",
          "num": "69",
          "label": "PTD_4",
          "feature": "ADC0_SE22",
          "alt": "PCTRL_PIN_DISABLED",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLD",
          "gpioBase": "GPIOD",
          "num": "70",
          "label": "PTD_3",
          "feature": "I2C1_SCL",
          "alt": "PCTRL_MUX_ALT4",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLD",
          "gpioBase": "GPIOD",
          "num": "71",
          "label": "PTD_2",
          "feature": "I2C1_SDA",
          "alt": "PCTRL_MUX_ALT4",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLA",
          "gpioBase": "GPIOA",
          "num": "72",
          "label": "PTA_3",
          "feature": "ADC0_SE17",
          "alt": "PCTRL_PIN_DISABLED",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLA",
          "gpioBase": "GPIOA",
          "num": "73",
          "label": "PTA_2",
          "feature": "ADC0_SE16",
          "alt": "PCTRL_PIN_DISABLED",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLA",
          "gpioBase": "GPIOA",
          "num": "82",
          "label": "PTA_16",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_OUTPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": "0",
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLA",
          "gpioBase": "GPIOA",
          "num": "83",
          "label": "PTA_15",
          "feature": "eTMR1_CH2",
          "alt": "PCTRL_MUX_ALT2",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLA",
          "gpioBase": "GPIOA",
          "num": "91",
          "label": "PTA_11",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_OUTPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLD",
          "gpioBase": "GPIOD",
          "num": "20",
          "label": "PTD_17",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_OUTPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": "1",
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLD",
          "gpioBase": "GPIOD",
          "num": "31",
          "label": "PTD_7",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_INPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLA",
          "gpioBase": "GPIOA",
          "num": "57",
          "label": "PTA_7",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_OUTPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": "1",
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLA",
          "gpioBase": "GPIOA",
          "num": "62",
          "label": "PTA_17",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_INPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLB",
          "gpioBase": "GPIOB",
          "num": "64",
          "label": "PTB_16",
          "feature": "GPIO",
          "alt": "PCTRL_MUX_AS_GPIO",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "GPIO_OUTPUT_DIRECTION",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": "1",
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLC",
          "gpioBase": "GPIOC",
          "num": "39",
          "label": "PTC_1",
          "feature": "SPI2_SOUT",
          "alt": "PCTRL_MUX_ALT3",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        },
        {
          "base": "PCTRLC",
          "gpioBase": "GPIOC",
          "num": "40",
          "label": "PTC_0",
          "feature": "SPI2_SIN",
          "alt": "PCTRL_MUX_ALT3",
          "intCfg": "PCTRL_DMA_INT_DISABLED",
          "direction": "",
          "pullEnable": 0,
          "pullSelect": "",
          "filter": false,
          "passiveFilter": false,
          "strength": "PCTRL_LOW_DRIVE_STRENGTH",
          "intFlag": false,
          "init": 0,
          "userLabel": "",
          "rateSelect": "PCTRL_FAST_SLEW_RATE"
        }
      ],
      "updateTime": 1776006607612,
      "lock": false
    },
    "clock": {
      "enable": {},
      "data": {
        "activeInst": 0,
        "version": "1",
        "clockArray": [
          {
            "name": "clock_config0",
            "data": {
              "firc": {
                "enable": true,
                "dsEnable": false,
                "freq": {
                  "value": 96,
                  "unit": "MHz",
                  "raw": 96000000
                }
              },
              "fxosc": {
                "enable": true,
                "dsEnable": false,
                "freq": {
                  "value": 24,
                  "unit": "MHz",
                  "raw": 24000000
                },
                "gain": 5,
                "mode": 0
              },
              "sirc": {
                "enable": true,
                "dsEnable": false,
                "stbEnable": false,
                "pdEnable": false,
                "freq": {
                  "value": 12,
                  "unit": "MHz",
                  "raw": 12000000
                }
              },
              "sxosc": {
                "enable": false,
                "dsEnable": false,
                "pdEnable": false,
                "stbEnable": false,
                "freq": {
                  "value": 32768,
                  "unit": "Hz",
                  "raw": 32768
                },
                "gain": 0,
                "mode": 0
              },
              "pll": {
                "enable": true,
                "refdivV": 1,
                "fbdivV": 10,
                "ref": 1,
                "freq": {
                  "value": 120,
                  "unit": "MHz",
                  "raw": 120000000
                },
                "dsEnable": false
              },
              "cmu0": {
                "reset": true,
                "ref": 0,
                "enable": true,
                "compareHigh": 50,
                "compareLow": 30
              },
              "cmu1": {
                "reset": true,
                "ref": 0,
                "enable": true,
                "compareHigh": 120,
                "compareLow": 72
              },
              "cmu2": {
                "reset": true,
                "ref": 0,
                "enable": true,
                "compareHigh": 150,
                "compareLow": 90
              },
              "cmu3": {
                "reset": true,
                "enable": true,
                "ref": 0,
                "compareHigh": 30,
                "compareLow": 18
              },
              "clkOut": {
                "enable": false,
                "div": 1,
                "ref": 0
              },
              "coreClock": {
                "div": 0,
                "ref": 1,
                "freq": {
                  "value": 120,
                  "unit": "MHz",
                  "raw": 120000000
                }
              },
              "fastClock": {
                "div": 0,
                "freq": {
                  "value": 120,
                  "unit": "MHz",
                  "raw": 120000000
                }
              },
              "slowClock": {
                "div": 2,
                "freq": {
                  "value": 40,
                  "unit": "MHz",
                  "raw": 40000000
                }
              },
              "periClocks": [
                {
                  "name": "DMA_CLK",
                  "gate": true,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": true,
                  "div": 0,
                  "busClock": [
                    "CORE_CLK"
                  ]
                },
                {
                  "name": "TRACE_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "div": 0,
                  "busClock": [
                    "FAST_BUS_CLK"
                  ],
                  "periClock": [
                    "CLK_SRC_DISABLED",
                    "CLK_SRC_FIRC",
                    "CLK_SRC_SIRC",
                    "CLK_SRC_FXOSC",
                    "CLK_SRC_PLL"
                  ]
                },
                {
                  "name": "EFM_CLK",
                  "gate": true,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": true,
                  "div": 0,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ]
                },
                {
                  "name": "GPIO_CLK",
                  "gate": true,
                  "busSrc": 0,
                  "periSrc": 2,
                  "userCtrl": true,
                  "div": 0,
                  "busClock": [
                    "CORE_CLK"
                  ],
                  "periClock": [
                    "CLK_SRC_DISABLED",
                    "CLK_SRC_FIRC",
                    "CLK_SRC_SIRC",
                    "CLK_SRC_FXOSC",
                    "CLK_SRC_PLL"
                  ]
                },
                {
                  "name": "PCTRLA_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "div": 0,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ]
                },
                {
                  "name": "PCTRLB_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "div": 0,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ]
                },
                {
                  "name": "PCTRLC_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "div": 0
                },
                {
                  "name": "PCTRLD_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "div": 0
                },
                {
                  "name": "PCTRLE_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "div": 0
                },
                {
                  "name": "LINFlexD0_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "periClock": [
                    "CLK_SRC_DISABLED",
                    "CLK_SRC_FIRC",
                    "CLK_SRC_SIRC",
                    "CLK_SRC_FXOSC",
                    "CLK_SRC_PLL"
                  ],
                  "div": 0
                },
                {
                  "name": "LINFlexD1_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "periClock": [
                    "CLK_SRC_DISABLED",
                    "CLK_SRC_FIRC",
                    "CLK_SRC_SIRC",
                    "CLK_SRC_FXOSC",
                    "CLK_SRC_PLL"
                  ],
                  "div": 0
                },
                {
                  "name": "LINFlexD2_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "periClock": [
                    "CLK_SRC_DISABLED",
                    "CLK_SRC_FIRC",
                    "CLK_SRC_SIRC",
                    "CLK_SRC_FXOSC",
                    "CLK_SRC_PLL"
                  ],
                  "div": 0
                },
                {
                  "name": "SENT0_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "periClock": [
                    "CLK_SRC_DISABLED",
                    "CLK_SRC_FIRC",
                    "CLK_SRC_SIRC",
                    "CLK_SRC_FXOSC",
                    "CLK_SRC_PLL"
                  ],
                  "div": 0
                },
                {
                  "name": "I2C0_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "periClock": [
                    "CLK_SRC_DISABLED",
                    "CLK_SRC_FIRC",
                    "CLK_SRC_SIRC",
                    "CLK_SRC_FXOSC",
                    "CLK_SRC_PLL"
                  ],
                  "div": 0
                },
                {
                  "name": "I2C1_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "periClock": [
                    "CLK_SRC_DISABLED",
                    "CLK_SRC_FIRC",
                    "CLK_SRC_SIRC",
                    "CLK_SRC_FXOSC",
                    "CLK_SRC_PLL"
                  ],
                  "div": 0
                },
                {
                  "name": "SPI0_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 2,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "periClock": [
                    "CLK_SRC_DISABLED",
                    "CLK_SRC_FIRC",
                    "CLK_SRC_SIRC",
                    "CLK_SRC_FXOSC",
                    "CLK_SRC_PLL"
                  ],
                  "div": 0
                },
                {
                  "name": "SPI1_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 2,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "periClock": [
                    "CLK_SRC_DISABLED",
                    "CLK_SRC_FIRC",
                    "CLK_SRC_SIRC",
                    "CLK_SRC_FXOSC",
                    "CLK_SRC_PLL"
                  ],
                  "div": 0
                },
                {
                  "name": "SPI2_CLK",
                  "gate": true,
                  "busSrc": 0,
                  "periSrc": 3,
                  "userCtrl": true,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "periClock": [
                    "CLK_SRC_DISABLED",
                    "CLK_SRC_FIRC",
                    "CLK_SRC_SIRC",
                    "CLK_SRC_FXOSC",
                    "CLK_SRC_PLL"
                  ],
                  "div": 0
                },
                {
                  "name": "SPI3_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "periClock": [
                    "CLK_SRC_DISABLED",
                    "CLK_SRC_FIRC",
                    "CLK_SRC_SIRC",
                    "CLK_SRC_FXOSC",
                    "CLK_SRC_PLL"
                  ],
                  "div": 0
                },
                {
                  "name": "FlexCAN0_CLK",
                  "gate": true,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": true,
                  "busClock": [
                    "FAST_BUS_CLK",
                    "FXOSC_CLK"
                  ],
                  "div": 0
                },
                {
                  "name": "FlexCAN1_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "FAST_BUS_CLK",
                    "FXOSC_CLK"
                  ],
                  "div": 0
                },
                {
                  "name": "FlexCAN2_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "FAST_BUS_CLK",
                    "FXOSC_CLK"
                  ],
                  "div": 0
                },
                {
                  "name": "ADC0_CLK",
                  "gate": true,
                  "busSrc": 0,
                  "periSrc": 1,
                  "userCtrl": true,
                  "busClock": [
                    "FAST_BUS_CLK"
                  ],
                  "periClock": [
                    "CLK_SRC_DISABLED",
                    "CLK_SRC_FIRC",
                    "CLK_SRC_SIRC",
                    "CLK_SRC_FXOSC",
                    "CLK_SRC_PLL"
                  ],
                  "div": 0
                },
                {
                  "name": "ACMP0_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "periClock": [
                    "CLK_SRC_DISABLED",
                    "CLK_SRC_FIRC",
                    "CLK_SRC_SIRC",
                    "CLK_SRC_FXOSC",
                    "CLK_SRC_PLL"
                  ],
                  "div": 0
                },
                {
                  "name": "PTU0_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "FAST_BUS_CLK"
                  ],
                  "div": 0
                },
                {
                  "name": "TMU_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "div": 0
                },
                {
                  "name": "eTMR0_CLK",
                  "gate": true,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": true,
                  "busClock": [
                    "FAST_BUS_CLK",
                    "TCLK0",
                    "TCLK1",
                    "TCLK2"
                  ],
                  "div": 0
                },
                {
                  "name": "eTMR1_CLK",
                  "gate": true,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": true,
                  "busClock": [
                    "FAST_BUS_CLK",
                    "TCLK0",
                    "TCLK1",
                    "TCLK2"
                  ],
                  "div": 0
                },
                {
                  "name": "eTMR2_CLK",
                  "gate": true,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": true,
                  "busClock": [
                    "FAST_BUS_CLK",
                    "TCLK0",
                    "TCLK1",
                    "TCLK2"
                  ],
                  "div": 0
                },
                {
                  "name": "eTMR3_CLK",
                  "gate": true,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": true,
                  "busClock": [
                    "FAST_BUS_CLK",
                    "TCLK0",
                    "TCLK1",
                    "TCLK2"
                  ],
                  "div": 0
                },
                {
                  "name": "TMR0_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "div": 0
                },
                {
                  "name": "pTMR0_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "div": 0
                },
                {
                  "name": "lpTMR0_CLK",
                  "gate": true,
                  "busSrc": 0,
                  "periSrc": 2,
                  "userCtrl": true,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "periClock": [
                    "CLK_SRC_DISABLED",
                    "CLK_SRC_FIRC",
                    "CLK_SRC_SIRC",
                    "CLK_SRC_FXOSC",
                    "CLK_SRC_PLL"
                  ],
                  "div": 0
                },
                {
                  "name": "RTC_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK",
                    "RTC_CLK_OSCIN",
                    "RTC_CLK_CLKIN"
                  ],
                  "periClock": [
                    "CLK_SRC_DISABLED",
                    "CLK_SRC_FIRC",
                    "CLK_SRC_SIRC",
                    "CLK_SRC_FXOSC",
                    "CLK_SRC_PLL"
                  ],
                  "div": 0
                },
                {
                  "name": "WKU_CLK",
                  "gate": true,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": true,
                  "div": 0
                },
                {
                  "name": "CRC_CLK",
                  "gate": false,
                  "busClock": [
                    "CORE_CLK"
                  ],
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "div": 0
                },
                {
                  "name": "TRNG_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "div": 0
                },
                {
                  "name": "HCU_CLK",
                  "gate": true,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": true,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "div": 0
                },
                {
                  "name": "WDG0_CLK",
                  "gate": true,
                  "busSrc": 0,
                  "periSrc": 2,
                  "userCtrl": true,
                  "busClock": [
                    "SLOW_BUS_CLK",
                    "SIRC_CLK",
                    "SXOSC_CLK"
                  ],
                  "periClock": [
                    "CLK_SRC_DISABLED",
                    "CLK_SRC_FIRC",
                    "CLK_SRC_SIRC",
                    "CLK_SRC_FXOSC",
                    "CLK_SRC_PLL"
                  ],
                  "div": 0
                },
                {
                  "name": "EWDG0_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "div": 0
                },
                {
                  "name": "EMU0_CLK",
                  "gate": true,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": true,
                  "busClock": [
                    "CORE_CLK"
                  ],
                  "div": 0
                },
                {
                  "name": "CIM_CLK",
                  "gate": false,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "div": 0
                },
                {
                  "name": "SCU_CLK",
                  "gate": true,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "div": 0
                },
                {
                  "name": "PCU_CLK",
                  "gate": true,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK"
                  ],
                  "div": 0
                },
                {
                  "name": "RCU_CLK",
                  "gate": true,
                  "busSrc": 0,
                  "periSrc": 0,
                  "userCtrl": false,
                  "busClock": [
                    "SLOW_BUS_CLK",
                    "SIRC_CLK"
                  ],
                  "div": 0
                }
              ]
            }
          }
        ]
      },
      "updateTime": 1776007064464,
      "lock": false
    },
    "interrupt": {
      "enable": {},
      "data": [
        {
          "name": "NMI_IRQn",
          "num": -14,
          "enable": false,
          "priority": -2,
          "callback": "NMI_Handler"
        },
        {
          "name": "HardFault_IRQn",
          "num": -13,
          "enable": false,
          "priority": -1,
          "callback": "HardFault_Handler"
        },
        {
          "name": "MemManage_IRQn",
          "num": -12,
          "enable": false,
          "priority": 0,
          "callback": "MemManage_Handler"
        },
        {
          "name": "BusFault_IRQn",
          "num": -11,
          "enable": false,
          "priority": 0,
          "callback": "BusFault_Handler"
        },
        {
          "name": "UsageFault_IRQn",
          "num": -10,
          "enable": false,
          "priority": 0,
          "callback": "UsageFault_Handler"
        },
        {
          "name": "SVC_IRQn",
          "num": -5,
          "enable": false,
          "priority": 0,
          "callback": "SVC_Handler"
        },
        {
          "name": "DebugMon_IRQn",
          "num": -4,
          "enable": false,
          "priority": 0,
          "callback": "DebugMon_Handler"
        },
        {
          "name": "PendSV_IRQn",
          "num": -2,
          "enable": false,
          "priority": 0,
          "callback": "PendSV_Handler"
        },
        {
          "name": "SysTick_IRQn",
          "num": -1,
          "enable": false,
          "priority": 0,
          "callback": "SysTick_Handler"
        },
        {
          "name": "DMA0_IRQn",
          "num": 0,
          "enable": false,
          "priority": 0,
          "callback": "DMA0_IRQHandler"
        },
        {
          "name": "DMA1_IRQn",
          "num": 1,
          "enable": false,
          "priority": 0,
          "callback": "DMA1_IRQHandler"
        },
        {
          "name": "DMA2_IRQn",
          "num": 2,
          "enable": false,
          "priority": 0,
          "callback": "DMA2_IRQHandler"
        },
        {
          "name": "DMA3_IRQn",
          "num": 3,
          "enable": false,
          "priority": 0,
          "callback": "DMA3_IRQHandler"
        },
        {
          "name": "DMA4_IRQn",
          "num": 4,
          "enable": false,
          "priority": 0,
          "callback": "DMA4_IRQHandler"
        },
        {
          "name": "DMA5_IRQn",
          "num": 5,
          "enable": false,
          "priority": 0,
          "callback": "DMA5_IRQHandler"
        },
        {
          "name": "DMA6_IRQn",
          "num": 6,
          "enable": false,
          "priority": 0,
          "callback": "DMA6_IRQHandler"
        },
        {
          "name": "DMA7_IRQn",
          "num": 7,
          "enable": false,
          "priority": 0,
          "callback": "DMA7_IRQHandler"
        },
        {
          "name": "DMA8_IRQn",
          "num": 8,
          "enable": false,
          "priority": 0,
          "callback": "DMA8_IRQHandler"
        },
        {
          "name": "DMA9_IRQn",
          "num": 9,
          "enable": false,
          "priority": 0,
          "callback": "DMA9_IRQHandler"
        },
        {
          "name": "DMA10_IRQn",
          "num": 10,
          "enable": false,
          "priority": 0,
          "callback": "DMA10_IRQHandler"
        },
        {
          "name": "DMA11_IRQn",
          "num": 11,
          "enable": false,
          "priority": 0,
          "callback": "DMA11_IRQHandler"
        },
        {
          "name": "DMA12_IRQn",
          "num": 12,
          "enable": false,
          "priority": 0,
          "callback": "DMA12_IRQHandler"
        },
        {
          "name": "DMA13_IRQn",
          "num": 13,
          "enable": false,
          "priority": 0,
          "callback": "DMA13_IRQHandler"
        },
        {
          "name": "DMA14_IRQn",
          "num": 14,
          "enable": false,
          "priority": 0,
          "callback": "DMA14_IRQHandler"
        },
        {
          "name": "DMA15_IRQn",
          "num": 15,
          "enable": false,
          "priority": 0,
          "callback": "DMA15_IRQHandler"
        },
        {
          "name": "DMA_Error_IRQn",
          "num": 16,
          "enable": false,
          "priority": 0,
          "callback": "DMA_Error_IRQHandler"
        },
        {
          "name": "FPU_IRQn",
          "num": 17,
          "enable": false,
          "priority": 0,
          "callback": "FPU_IRQHandler"
        },
        {
          "name": "EFM_IRQn",
          "num": 18,
          "enable": false,
          "priority": 0,
          "callback": "EFM_IRQHandler"
        },
        {
          "name": "EFM_Error_IRQn",
          "num": 19,
          "enable": false,
          "priority": 0,
          "callback": "EFM_Error_IRQHandler"
        },
        {
          "name": "PCU_IRQn",
          "num": 20,
          "enable": false,
          "priority": 0,
          "callback": "PCU_IRQHandler"
        },
        {
          "name": "EFM_Ecc_IRQn",
          "num": 21,
          "enable": false,
          "priority": 0,
          "callback": "EFM_Ecc_IRQHandler"
        },
        {
          "name": "WDG0_IRQn",
          "num": 22,
          "enable": false,
          "priority": 0,
          "callback": "WDG0_IRQHandler"
        },
        {
          "name": "Reserved5_IRQn",
          "num": 23,
          "enable": false,
          "priority": 0,
          "callback": "Reserved5_IRQHandler"
        },
        {
          "name": "I2C0_Master_IRQn",
          "num": 24,
          "enable": false,
          "priority": 0,
          "callback": "I2C0_Master_IRQHandler"
        },
        {
          "name": "I2C0_Slave_IRQn",
          "num": 25,
          "enable": false,
          "priority": 0,
          "callback": "I2C0_Slave_IRQHandler"
        },
        {
          "name": "SPI0_IRQn",
          "num": 26,
          "enable": false,
          "priority": 0,
          "callback": "SPI0_IRQHandler"
        },
        {
          "name": "SPI1_IRQn",
          "num": 27,
          "enable": false,
          "priority": 0,
          "callback": "SPI1_IRQHandler"
        },
        {
          "name": "SPI2_IRQn",
          "num": 28,
          "enable": false,
          "priority": 0,
          "callback": "SPI2_IRQHandler"
        },
        {
          "name": "I2C1_Master_IRQn",
          "num": 29,
          "enable": false,
          "priority": 0,
          "callback": "I2C1_Master_IRQHandler"
        },
        {
          "name": "Reserved6_IRQn",
          "num": 30,
          "enable": false,
          "priority": 0,
          "callback": "Reserved6_IRQHandler"
        },
        {
          "name": "LINFlexD0_IRQn",
          "num": 31,
          "enable": false,
          "priority": 0,
          "callback": "LINFlexD0_IRQHandler"
        },
        {
          "name": "Reserved7_IRQn",
          "num": 32,
          "enable": false,
          "priority": 0,
          "callback": "Reserved7_IRQHandler"
        },
        {
          "name": "LINFlexD1_IRQn",
          "num": 33,
          "enable": false,
          "priority": 0,
          "callback": "LINFlexD1_IRQHandler"
        },
        {
          "name": "Reserved8_IRQn",
          "num": 34,
          "enable": false,
          "priority": 0,
          "callback": "Reserved8_IRQHandler"
        },
        {
          "name": "LINFlexD2_IRQn",
          "num": 35,
          "enable": false,
          "priority": 0,
          "callback": "LINFlexD2_IRQHandler"
        },
        {
          "name": "Reserved9_IRQn",
          "num": 36,
          "enable": false,
          "priority": 0,
          "callback": "Reserved9_IRQHandler"
        },
        {
          "name": "Reserved10_IRQn",
          "num": 37,
          "enable": false,
          "priority": 0,
          "callback": "Reserved10_IRQHandler"
        },
        {
          "name": "Reserved11_IRQn",
          "num": 38,
          "enable": false,
          "priority": 0,
          "callback": "Reserved11_IRQHandler"
        },
        {
          "name": "ADC0_IRQn",
          "num": 39,
          "enable": false,
          "priority": 0,
          "callback": "ADC0_IRQHandler"
        },
        {
          "name": "Reserved12_IRQn",
          "num": 40,
          "enable": false,
          "priority": 0,
          "callback": "Reserved12_IRQHandler"
        },
        {
          "name": "ACMP0_IRQn",
          "num": 41,
          "enable": false,
          "priority": 0,
          "callback": "ACMP0_IRQHandler"
        },
        {
          "name": "Reserved13_IRQn",
          "num": 42,
          "enable": false,
          "priority": 0,
          "callback": "Reserved13_IRQHandler"
        },
        {
          "name": "Reserved14_IRQn",
          "num": 43,
          "enable": false,
          "priority": 0,
          "callback": "Reserved14_IRQHandler"
        },
        {
          "name": "EMU0_SB_IRQn",
          "num": 44,
          "enable": false,
          "priority": 0,
          "callback": "EMU0_SB_IRQHandler"
        },
        {
          "name": "EMU0_DB_IRQn",
          "num": 45,
          "enable": false,
          "priority": 0,
          "callback": "EMU0_DB_IRQHandler"
        },
        {
          "name": "RTC_IRQn",
          "num": 46,
          "enable": false,
          "priority": 0,
          "callback": "RTC_IRQHandler"
        },
        {
          "name": "RTC_Seconds_IRQn",
          "num": 47,
          "enable": false,
          "priority": 0,
          "callback": "RTC_Seconds_IRQHandler"
        },
        {
          "name": "pTMR0_Ch0_IRQn",
          "num": 48,
          "enable": false,
          "priority": 0,
          "callback": "pTMR0_Ch0_IRQHandler"
        },
        {
          "name": "pTMR0_Ch1_IRQn",
          "num": 49,
          "enable": false,
          "priority": 0,
          "callback": "pTMR0_Ch1_IRQHandler"
        },
        {
          "name": "pTMR0_Ch2_IRQn",
          "num": 50,
          "enable": false,
          "priority": 0,
          "callback": "pTMR0_Ch2_IRQHandler"
        },
        {
          "name": "pTMR0_Ch3_IRQn",
          "num": 51,
          "enable": false,
          "priority": 0,
          "callback": "pTMR0_Ch3_IRQHandler"
        },
        {
          "name": "PTU0_IRQn",
          "num": 52,
          "enable": false,
          "priority": 0,
          "callback": "PTU0_IRQHandler"
        },
        {
          "name": "Reserved15_IRQn",
          "num": 53,
          "enable": false,
          "priority": 0,
          "callback": "Reserved15_IRQHandler"
        },
        {
          "name": "Reserved16_IRQn",
          "num": 54,
          "enable": false,
          "priority": 0,
          "callback": "Reserved16_IRQHandler"
        },
        {
          "name": "Reserved17_IRQn",
          "num": 55,
          "enable": false,
          "priority": 0,
          "callback": "Reserved17_IRQHandler"
        },
        {
          "name": "Reserved18_IRQn",
          "num": 56,
          "enable": false,
          "priority": 0,
          "callback": "Reserved18_IRQHandler"
        },
        {
          "name": "SCU_IRQn",
          "num": 57,
          "enable": false,
          "priority": 0,
          "callback": "SCU_IRQHandler"
        },
        {
          "name": "lpTMR0_IRQn",
          "num": 58,
          "enable": false,
          "priority": 0,
          "callback": "lpTMR0_IRQHandler"
        },
        {
          "name": "GPIOA_IRQn",
          "num": 59,
          "enable": false,
          "priority": 0,
          "callback": "GPIOA_IRQHandler"
        },
        {
          "name": "GPIOB_IRQn",
          "num": 60,
          "enable": false,
          "priority": 0,
          "callback": "GPIOB_IRQHandler"
        },
        {
          "name": "GPIOC_IRQn",
          "num": 61,
          "enable": false,
          "priority": 0,
          "callback": "GPIOC_IRQHandler"
        },
        {
          "name": "GPIOD_IRQn",
          "num": 62,
          "enable": false,
          "priority": 0,
          "callback": "GPIOD_IRQHandler"
        },
        {
          "name": "GPIOE_IRQn",
          "num": 63,
          "enable": false,
          "priority": 0,
          "callback": "GPIOE_IRQHandler"
        },
        {
          "name": "Reserved19_IRQn",
          "num": 64,
          "enable": false,
          "priority": 0,
          "callback": "Reserved19_IRQHandler"
        },
        {
          "name": "Reserved20_IRQn",
          "num": 65,
          "enable": false,
          "priority": 0,
          "callback": "Reserved20_IRQHandler"
        },
        {
          "name": "Reserved21_IRQn",
          "num": 66,
          "enable": false,
          "priority": 0,
          "callback": "Reserved21_IRQHandler"
        },
        {
          "name": "Reserved22_IRQn",
          "num": 67,
          "enable": false,
          "priority": 0,
          "callback": "Reserved22_IRQHandler"
        },
        {
          "name": "Reserved23_IRQn",
          "num": 68,
          "enable": false,
          "priority": 0,
          "callback": "Reserved23_IRQHandler"
        },
        {
          "name": "Reserved24_IRQn",
          "num": 69,
          "enable": false,
          "priority": 0,
          "callback": "Reserved24_IRQHandler"
        },
        {
          "name": "Reserved25_IRQn",
          "num": 70,
          "enable": false,
          "priority": 0,
          "callback": "Reserved25_IRQHandler"
        },
        {
          "name": "Reserved26_IRQn",
          "num": 71,
          "enable": false,
          "priority": 0,
          "callback": "Reserved26_IRQHandler"
        },
        {
          "name": "Reserved27_IRQn",
          "num": 72,
          "enable": false,
          "priority": 0,
          "callback": "Reserved27_IRQHandler"
        },
        {
          "name": "Reserved28_IRQn",
          "num": 73,
          "enable": false,
          "priority": 0,
          "callback": "Reserved28_IRQHandler"
        },
        {
          "name": "Reserved29_IRQn",
          "num": 74,
          "enable": false,
          "priority": 0,
          "callback": "Reserved29_IRQHandler"
        },
        {
          "name": "Reserved30_IRQn",
          "num": 75,
          "enable": false,
          "priority": 0,
          "callback": "Reserved30_IRQHandler"
        },
        {
          "name": "Reserved31_IRQn",
          "num": 76,
          "enable": false,
          "priority": 0,
          "callback": "Reserved31_IRQHandler"
        },
        {
          "name": "Reserved32_IRQn",
          "num": 77,
          "enable": false,
          "priority": 0,
          "callback": "Reserved32_IRQHandler"
        },
        {
          "name": "CAN0_ORed_IRQn",
          "num": 78,
          "enable": false,
          "priority": 0,
          "callback": "CAN0_ORed_IRQHandler"
        },
        {
          "name": "CAN0_Error_IRQn",
          "num": 79,
          "enable": false,
          "priority": 0,
          "callback": "CAN0_Error_IRQHandler"
        },
        {
          "name": "CAN0_Wake_Up_IRQn",
          "num": 80,
          "enable": false,
          "priority": 0,
          "callback": "CAN0_Wake_Up_IRQHandler"
        },
        {
          "name": "CAN0_ORed_0_15_MB_IRQn",
          "num": 81,
          "enable": false,
          "priority": 0,
          "callback": "CAN0_ORed_0_15_MB_IRQHandler"
        },
        {
          "name": "CAN0_ORed_16_31_MB_IRQn",
          "num": 82,
          "enable": false,
          "priority": 0,
          "callback": "CAN0_ORed_16_31_MB_IRQHandler"
        },
        {
          "name": "CAN0_ORed_32_47_MB_IRQn",
          "num": 83,
          "enable": false,
          "priority": 0,
          "callback": "CAN0_ORed_32_47_MB_IRQHandler"
        },
        {
          "name": "CAN0_ORed_48_63_MB_IRQn",
          "num": 84,
          "enable": false,
          "priority": 0,
          "callback": "CAN0_ORed_48_63_MB_IRQHandler"
        },
        {
          "name": "CAN1_ORed_IRQn",
          "num": 85,
          "enable": false,
          "priority": 0,
          "callback": "CAN1_ORed_IRQHandler"
        },
        {
          "name": "CAN1_Error_IRQn",
          "num": 86,
          "enable": false,
          "priority": 0,
          "callback": "CAN1_Error_IRQHandler"
        },
        {
          "name": "CAN1_Wake_Up_IRQn",
          "num": 87,
          "enable": false,
          "priority": 0,
          "callback": "CAN1_Wake_Up_IRQHandler"
        },
        {
          "name": "CAN1_ORed_0_15_MB_IRQn",
          "num": 88,
          "enable": false,
          "priority": 0,
          "callback": "CAN1_ORed_0_15_MB_IRQHandler"
        },
        {
          "name": "CAN1_ORed_16_31_MB_IRQn",
          "num": 89,
          "enable": false,
          "priority": 0,
          "callback": "CAN1_ORed_16_31_MB_IRQHandler"
        },
        {
          "name": "Reserved33_IRQn",
          "num": 90,
          "enable": false,
          "priority": 0,
          "callback": "Reserved33_IRQHandler"
        },
        {
          "name": "Reserved34_IRQn",
          "num": 91,
          "enable": false,
          "priority": 0,
          "callback": "Reserved34_IRQHandler"
        },
        {
          "name": "CAN2_ORed_IRQn",
          "num": 92,
          "enable": false,
          "priority": 0,
          "callback": "CAN2_ORed_IRQHandler"
        },
        {
          "name": "CAN2_Error_IRQn",
          "num": 93,
          "enable": false,
          "priority": 0,
          "callback": "CAN2_Error_IRQHandler"
        },
        {
          "name": "CAN2_Wake_Up_IRQn",
          "num": 94,
          "enable": false,
          "priority": 0,
          "callback": "CAN2_Wake_Up_IRQHandler"
        },
        {
          "name": "CAN2_ORed_0_15_MB_IRQn",
          "num": 95,
          "enable": false,
          "priority": 0,
          "callback": "CAN2_ORed_0_15_MB_IRQHandler"
        },
        {
          "name": "CAN2_ORed_16_31_MB_IRQn",
          "num": 96,
          "enable": false,
          "priority": 0,
          "callback": "CAN2_ORed_16_31_MB_IRQHandler"
        },
        {
          "name": "Reserved35_IRQn",
          "num": 97,
          "enable": false,
          "priority": 0,
          "callback": "Reserved35_IRQHandler"
        },
        {
          "name": "Reserved36_IRQn",
          "num": 98,
          "enable": false,
          "priority": 0,
          "callback": "Reserved36_IRQHandler"
        },
        {
          "name": "eTMR0_Ch0_Ch1_IRQn",
          "num": 99,
          "enable": false,
          "priority": 0,
          "callback": "eTMR0_Ch0_Ch1_IRQHandler"
        },
        {
          "name": "eTMR0_Ch2_Ch3_IRQn",
          "num": 100,
          "enable": false,
          "priority": 0,
          "callback": "eTMR0_Ch2_Ch3_IRQHandler"
        },
        {
          "name": "eTMR0_Ch4_Ch5_IRQn",
          "num": 101,
          "enable": false,
          "priority": 0,
          "callback": "eTMR0_Ch4_Ch5_IRQHandler"
        },
        {
          "name": "eTMR0_Ch6_Ch7_IRQn",
          "num": 102,
          "enable": false,
          "priority": 0,
          "callback": "eTMR0_Ch6_Ch7_IRQHandler"
        },
        {
          "name": "eTMR0_Fault_IRQn",
          "num": 103,
          "enable": false,
          "priority": 0,
          "callback": "eTMR0_Fault_IRQHandler"
        },
        {
          "name": "eTMR0_Ovf_IRQn",
          "num": 104,
          "enable": false,
          "priority": 0,
          "callback": "eTMR0_Ovf_IRQHandler"
        },
        {
          "name": "eTMR1_Ch0_Ch1_IRQn",
          "num": 105,
          "enable": false,
          "priority": 0,
          "callback": "eTMR1_Ch0_Ch1_IRQHandler"
        },
        {
          "name": "eTMR1_Ch2_Ch3_IRQn",
          "num": 106,
          "enable": false,
          "priority": 0,
          "callback": "eTMR1_Ch2_Ch3_IRQHandler"
        },
        {
          "name": "eTMR1_Ch4_Ch5_IRQn",
          "num": 107,
          "enable": false,
          "priority": 0,
          "callback": "eTMR1_Ch4_Ch5_IRQHandler"
        },
        {
          "name": "eTMR1_Ch6_Ch7_IRQn",
          "num": 108,
          "enable": false,
          "priority": 0,
          "callback": "eTMR1_Ch6_Ch7_IRQHandler"
        },
        {
          "name": "eTMR1_Fault_IRQn",
          "num": 109,
          "enable": false,
          "priority": 0,
          "callback": "eTMR1_Fault_IRQHandler"
        },
        {
          "name": "eTMR1_Ovf_IRQn",
          "num": 110,
          "enable": false,
          "priority": 0,
          "callback": "eTMR1_Ovf_IRQHandler"
        },
        {
          "name": "eTMR2_Ch0_Ch1_IRQn",
          "num": 111,
          "enable": false,
          "priority": 0,
          "callback": "eTMR2_Ch0_Ch1_IRQHandler"
        },
        {
          "name": "eTMR2_Ch2_Ch3_IRQn",
          "num": 112,
          "enable": false,
          "priority": 0,
          "callback": "eTMR2_Ch2_Ch3_IRQHandler"
        },
        {
          "name": "eTMR2_Ch4_Ch5_IRQn",
          "num": 113,
          "enable": false,
          "priority": 0,
          "callback": "eTMR2_Ch4_Ch5_IRQHandler"
        },
        {
          "name": "eTMR2_Ch6_Ch7_IRQn",
          "num": 114,
          "enable": false,
          "priority": 0,
          "callback": "eTMR2_Ch6_Ch7_IRQHandler"
        },
        {
          "name": "eTMR2_Fault_IRQn",
          "num": 115,
          "enable": false,
          "priority": 0,
          "callback": "eTMR2_Fault_IRQHandler"
        },
        {
          "name": "eTMR2_Ovf_IRQn",
          "num": 116,
          "enable": false,
          "priority": 0,
          "callback": "eTMR2_Ovf_IRQHandler"
        },
        {
          "name": "eTMR3_Ch0_Ch1_IRQn",
          "num": 117,
          "enable": false,
          "priority": 0,
          "callback": "eTMR3_Ch0_Ch1_IRQHandler"
        },
        {
          "name": "eTMR3_Ch2_Ch3_IRQn",
          "num": 118,
          "enable": false,
          "priority": 0,
          "callback": "eTMR3_Ch2_Ch3_IRQHandler"
        },
        {
          "name": "eTMR3_Ch4_Ch5_IRQn",
          "num": 119,
          "enable": false,
          "priority": 0,
          "callback": "eTMR3_Ch4_Ch5_IRQHandler"
        },
        {
          "name": "eTMR3_Ch6_Ch7_IRQn",
          "num": 120,
          "enable": false,
          "priority": 0,
          "callback": "eTMR3_Ch6_Ch7_IRQHandler"
        },
        {
          "name": "eTMR3_Fault_IRQn",
          "num": 121,
          "enable": false,
          "priority": 0,
          "callback": "eTMR3_Fault_IRQHandler"
        },
        {
          "name": "eTMR3_Ovf_IRQn",
          "num": 122,
          "enable": false,
          "priority": 0,
          "callback": "eTMR3_Ovf_IRQHandler"
        },
        {
          "name": "Reserved37_IRQn",
          "num": 123,
          "enable": false,
          "priority": 0,
          "callback": "Reserved37_IRQHandler"
        },
        {
          "name": "Reserved38_IRQn",
          "num": 124,
          "enable": false,
          "priority": 0,
          "callback": "Reserved38_IRQHandler"
        },
        {
          "name": "Reserved39_IRQn",
          "num": 125,
          "enable": false,
          "priority": 0,
          "callback": "Reserved39_IRQHandler"
        },
        {
          "name": "Reserved40_IRQn",
          "num": 126,
          "enable": false,
          "priority": 0,
          "callback": "Reserved40_IRQHandler"
        },
        {
          "name": "Reserved41_IRQn",
          "num": 127,
          "enable": false,
          "priority": 0,
          "callback": "Reserved41_IRQHandler"
        },
        {
          "name": "Reserved42_IRQn",
          "num": 128,
          "enable": false,
          "priority": 0,
          "callback": "Reserved42_IRQHandler"
        },
        {
          "name": "Reserved43_IRQn",
          "num": 129,
          "enable": false,
          "priority": 0,
          "callback": "Reserved43_IRQHandler"
        },
        {
          "name": "Reserved44_IRQn",
          "num": 130,
          "enable": false,
          "priority": 0,
          "callback": "Reserved44_IRQHandler"
        },
        {
          "name": "Reserved45_IRQn",
          "num": 131,
          "enable": false,
          "priority": 0,
          "callback": "Reserved45_IRQHandler"
        },
        {
          "name": "Reserved46_IRQn",
          "num": 132,
          "enable": false,
          "priority": 0,
          "callback": "Reserved46_IRQHandler"
        },
        {
          "name": "Reserved47_IRQn",
          "num": 133,
          "enable": false,
          "priority": 0,
          "callback": "Reserved47_IRQHandler"
        },
        {
          "name": "Reserved48_IRQn",
          "num": 134,
          "enable": false,
          "priority": 0,
          "callback": "Reserved48_IRQHandler"
        },
        {
          "name": "Reserved49_IRQn",
          "num": 135,
          "enable": false,
          "priority": 0,
          "callback": "Reserved49_IRQHandler"
        },
        {
          "name": "Reserved50_IRQn",
          "num": 136,
          "enable": false,
          "priority": 0,
          "callback": "Reserved50_IRQHandler"
        },
        {
          "name": "Reserved51_IRQn",
          "num": 137,
          "enable": false,
          "priority": 0,
          "callback": "Reserved51_IRQHandler"
        },
        {
          "name": "Reserved52_IRQn",
          "num": 138,
          "enable": false,
          "priority": 0,
          "callback": "Reserved52_IRQHandler"
        },
        {
          "name": "Reserved53_IRQn",
          "num": 139,
          "enable": false,
          "priority": 0,
          "callback": "Reserved53_IRQHandler"
        },
        {
          "name": "Reserved54_IRQn",
          "num": 140,
          "enable": false,
          "priority": 0,
          "callback": "Reserved54_IRQHandler"
        },
        {
          "name": "Reserved55_IRQn",
          "num": 141,
          "enable": false,
          "priority": 0,
          "callback": "Reserved55_IRQHandler"
        },
        {
          "name": "Reserved56_IRQn",
          "num": 142,
          "enable": false,
          "priority": 0,
          "callback": "Reserved56_IRQHandler"
        },
        {
          "name": "Reserved57_IRQn",
          "num": 143,
          "enable": false,
          "priority": 0,
          "callback": "Reserved57_IRQHandler"
        },
        {
          "name": "Reserved58_IRQn",
          "num": 144,
          "enable": false,
          "priority": 0,
          "callback": "Reserved58_IRQHandler"
        },
        {
          "name": "Reserved59_IRQn",
          "num": 145,
          "enable": false,
          "priority": 0,
          "callback": "Reserved59_IRQHandler"
        },
        {
          "name": "Reserved60_IRQn",
          "num": 146,
          "enable": false,
          "priority": 0,
          "callback": "Reserved60_IRQHandler"
        },
        {
          "name": "Reserved61_IRQn",
          "num": 147,
          "enable": false,
          "priority": 0,
          "callback": "Reserved61_IRQHandler"
        },
        {
          "name": "Reserved62_IRQn",
          "num": 148,
          "enable": false,
          "priority": 0,
          "callback": "Reserved62_IRQHandler"
        },
        {
          "name": "Reserved63_IRQn",
          "num": 149,
          "enable": false,
          "priority": 0,
          "callback": "Reserved63_IRQHandler"
        },
        {
          "name": "Reserved64_IRQn",
          "num": 150,
          "enable": false,
          "priority": 0,
          "callback": "Reserved64_IRQHandler"
        },
        {
          "name": "Reserved65_IRQn",
          "num": 151,
          "enable": false,
          "priority": 0,
          "callback": "Reserved65_IRQHandler"
        },
        {
          "name": "Reserved66_IRQn",
          "num": 152,
          "enable": false,
          "priority": 0,
          "callback": "Reserved66_IRQHandler"
        },
        {
          "name": "Reserved67_IRQn",
          "num": 153,
          "enable": false,
          "priority": 0,
          "callback": "Reserved67_IRQHandler"
        },
        {
          "name": "Reserved68_IRQn",
          "num": 154,
          "enable": false,
          "priority": 0,
          "callback": "Reserved68_IRQHandler"
        },
        {
          "name": "Reserved69_IRQn",
          "num": 155,
          "enable": false,
          "priority": 0,
          "callback": "Reserved69_IRQHandler"
        },
        {
          "name": "TRNG_IRQn",
          "num": 156,
          "enable": false,
          "priority": 0,
          "callback": "TRNG_IRQHandler"
        },
        {
          "name": "HCU_IRQn",
          "num": 157,
          "enable": false,
          "priority": 0,
          "callback": "HCU_IRQHandler"
        },
        {
          "name": "Reserved70_IRQn",
          "num": 158,
          "enable": false,
          "priority": 0,
          "callback": "Reserved70_IRQHandler"
        },
        {
          "name": "TMR0_Ch0_IRQn",
          "num": 159,
          "enable": false,
          "priority": 0,
          "callback": "TMR0_Ch0_IRQHandler"
        },
        {
          "name": "TMR0_Ch1_IRQn",
          "num": 160,
          "enable": false,
          "priority": 0,
          "callback": "TMR0_Ch1_IRQHandler"
        },
        {
          "name": "TMR0_Ch2_IRQn",
          "num": 161,
          "enable": false,
          "priority": 0,
          "callback": "TMR0_Ch2_IRQHandler"
        },
        {
          "name": "TMR0_Ch3_IRQn",
          "num": 162,
          "enable": false,
          "priority": 0,
          "callback": "TMR0_Ch3_IRQHandler"
        },
        {
          "name": "Reserved71_IRQn",
          "num": 163,
          "enable": false,
          "priority": 0,
          "callback": "Reserved71_IRQHandler"
        },
        {
          "name": "Reserved72_IRQn",
          "num": 164,
          "enable": false,
          "priority": 0,
          "callback": "Reserved72_IRQHandler"
        },
        {
          "name": "Reserved73_IRQn",
          "num": 165,
          "enable": false,
          "priority": 0,
          "callback": "Reserved73_IRQHandler"
        },
        {
          "name": "Reserved74_IRQn",
          "num": 166,
          "enable": false,
          "priority": 0,
          "callback": "Reserved74_IRQHandler"
        },
        {
          "name": "Reserved75_IRQn",
          "num": 167,
          "enable": false,
          "priority": 0,
          "callback": "Reserved75_IRQHandler"
        },
        {
          "name": "SPI3_IRQn",
          "num": 168,
          "enable": false,
          "priority": 0,
          "callback": "SPI3_IRQHandler"
        },
        {
          "name": "Reserved76_IRQn",
          "num": 169,
          "enable": false,
          "priority": 0,
          "callback": "Reserved76_IRQHandler"
        },
        {
          "name": "Reserved77_IRQn",
          "num": 170,
          "enable": false,
          "priority": 0,
          "callback": "Reserved77_IRQHandler"
        },
        {
          "name": "Reserved78_IRQn",
          "num": 171,
          "enable": false,
          "priority": 0,
          "callback": "Reserved78_IRQHandler"
        },
        {
          "name": "Reserved79_IRQn",
          "num": 172,
          "enable": false,
          "priority": 0,
          "callback": "Reserved79_IRQHandler"
        },
        {
          "name": "Reserved80_IRQn",
          "num": 173,
          "enable": false,
          "priority": 0,
          "callback": "Reserved80_IRQHandler"
        },
        {
          "name": "Reserved81_IRQn",
          "num": 174,
          "enable": false,
          "priority": 0,
          "callback": "Reserved81_IRQHandler"
        },
        {
          "name": "Reserved82_IRQn",
          "num": 175,
          "enable": false,
          "priority": 0,
          "callback": "Reserved82_IRQHandler"
        },
        {
          "name": "Reserved83_IRQn",
          "num": 176,
          "enable": false,
          "priority": 0,
          "callback": "Reserved83_IRQHandler"
        },
        {
          "name": "Reserved84_IRQn",
          "num": 177,
          "enable": false,
          "priority": 0,
          "callback": "Reserved84_IRQHandler"
        },
        {
          "name": "Reserved85_IRQn",
          "num": 178,
          "enable": false,
          "priority": 0,
          "callback": "Reserved85_IRQHandler"
        },
        {
          "name": "Reserved86_IRQn",
          "num": 179,
          "enable": false,
          "priority": 0,
          "callback": "Reserved86_IRQHandler"
        },
        {
          "name": "SENT0_IRQn",
          "num": 180,
          "enable": false,
          "priority": 0,
          "callback": "SENT0_IRQHandler"
        },
        {
          "name": "Reserved87_IRQn",
          "num": 181,
          "enable": false,
          "priority": 0,
          "callback": "Reserved87_IRQHandler"
        },
        {
          "name": "Reserved88_IRQn",
          "num": 182,
          "enable": false,
          "priority": 0,
          "callback": "Reserved88_IRQHandler"
        },
        {
          "name": "Reserved89_IRQn",
          "num": 183,
          "enable": false,
          "priority": 0,
          "callback": "Reserved89_IRQHandler"
        },
        {
          "name": "Reserved90_IRQn",
          "num": 184,
          "enable": false,
          "priority": 0,
          "callback": "Reserved90_IRQHandler"
        },
        {
          "name": "Reserved91_IRQn",
          "num": 185,
          "enable": false,
          "priority": 0,
          "callback": "Reserved91_IRQHandler"
        },
        {
          "name": "Reserved92_IRQn",
          "num": 186,
          "enable": false,
          "priority": 0,
          "callback": "Reserved92_IRQHandler"
        },
        {
          "name": "Reserved93_IRQn",
          "num": 187,
          "enable": false,
          "priority": 0,
          "callback": "Reserved93_IRQHandler"
        },
        {
          "name": "Reserved94_IRQn",
          "num": 188,
          "enable": false,
          "priority": 0,
          "callback": "Reserved94_IRQHandler"
        },
        {
          "name": "Reserved95_IRQn",
          "num": 189,
          "enable": false,
          "priority": 0,
          "callback": "Reserved95_IRQHandler"
        },
        {
          "name": "WKU_IRQn",
          "num": 190,
          "enable": false,
          "priority": 0,
          "callback": "WKU_IRQHandler"
        },
        {
          "name": "ALIGN_0_IRQn",
          "num": 191,
          "enable": false,
          "priority": 0,
          "callback": "ALIGN_0_IRQHandler"
        }
      ],
      "updateTime": 1745887890437,
      "lock": false
    },
    "device": {
      "enable": {},
      "data": {
        "pn": "YTM32B1MD14G0MLLT",
        "sdkVer": "1_3_1",
        "useFreeRtos": false,
        "useSecureBoot": false,
        "stack_top": "STACK_end",
        "vector_ram": "IVT_RAM_start",
        "vector_flash_region": ".isr_vector",
        "vector_flash": "IVT_start",
        "vector_flash_end": "IVT_end",
        "vectors": [
          "NMI_Handler",
          "HardFault_Handler",
          "MemManage_Handler",
          "BusFault_Handler",
          "UsageFault_Handler",
          "Reserved",
          "Reserved",
          "Reserved",
          "Reserved",
          "SVC_Handler",
          "DebugMon_Handler",
          "Reserved",
          "PendSV_Handler",
          "SysTick_Handler",
          "DMA0_IRQHandler",
          "DMA1_IRQHandler",
          "DMA2_IRQHandler",
          "DMA3_IRQHandler",
          "DMA4_IRQHandler",
          "DMA5_IRQHandler",
          "DMA6_IRQHandler",
          "DMA7_IRQHandler",
          "DMA8_IRQHandler",
          "DMA9_IRQHandler",
          "DMA10_IRQHandler",
          "DMA11_IRQHandler",
          "DMA12_IRQHandler",
          "DMA13_IRQHandler",
          "DMA14_IRQHandler",
          "DMA15_IRQHandler",
          "DMA_Error_IRQHandler",
          "FPU_IRQHandler",
          "EFM_IRQHandler",
          "EFM_Error_IRQHandler",
          "PCU_IRQHandler",
          "EFM_Ecc_IRQHandler",
          "WDG0_IRQHandler",
          "Reserved5_IRQHandler",
          "I2C0_Master_IRQHandler",
          "I2C0_Slave_IRQHandler",
          "SPI0_IRQHandler",
          "SPI1_IRQHandler",
          "SPI2_IRQHandler",
          "I2C1_Master_IRQHandler",
          "Reserved6_IRQHandler",
          "LINFlexD0_IRQHandler",
          "Reserved7_IRQHandler",
          "LINFlexD1_IRQHandler",
          "Reserved8_IRQHandler",
          "LINFlexD2_IRQHandler",
          "Reserved9_IRQHandler",
          "Reserved10_IRQHandler",
          "Reserved11_IRQHandler",
          "ADC0_IRQHandler",
          "Reserved12_IRQHandler",
          "ACMP0_IRQHandler",
          "Reserved13_IRQHandler",
          "Reserved14_IRQHandler",
          "EMU0_SB_IRQHandler",
          "EMU0_DB_IRQHandler",
          "RTC_IRQHandler",
          "RTC_Seconds_IRQHandler",
          "pTMR0_Ch0_IRQHandler",
          "pTMR0_Ch1_IRQHandler",
          "pTMR0_Ch2_IRQHandler",
          "pTMR0_Ch3_IRQHandler",
          "PTU0_IRQHandler",
          "Reserved15_IRQHandler",
          "Reserved16_IRQHandler",
          "Reserved17_IRQHandler",
          "Reserved18_IRQHandler",
          "SCU_IRQHandler",
          "lpTMR0_IRQHandler",
          "GPIOA_IRQHandler",
          "GPIOB_IRQHandler",
          "GPIOC_IRQHandler",
          "GPIOD_IRQHandler",
          "GPIOE_IRQHandler",
          "Reserved19_IRQHandler",
          "Reserved20_IRQHandler",
          "Reserved21_IRQHandler",
          "Reserved22_IRQHandler",
          "Reserved23_IRQHandler",
          "Reserved24_IRQHandler",
          "Reserved25_IRQHandler",
          "Reserved26_IRQHandler",
          "Reserved27_IRQHandler",
          "Reserved28_IRQHandler",
          "Reserved29_IRQHandler",
          "Reserved30_IRQHandler",
          "Reserved31_IRQHandler",
          "Reserved32_IRQHandler",
          "CAN0_ORed_IRQHandler",
          "CAN0_Error_IRQHandler",
          "CAN0_Wake_Up_IRQHandler",
          "CAN0_ORed_0_15_MB_IRQHandler",
          "CAN0_ORed_16_31_MB_IRQHandler",
          "CAN0_ORed_32_47_MB_IRQHandler",
          "CAN0_ORed_48_63_MB_IRQHandler",
          "CAN1_ORed_IRQHandler",
          "CAN1_Error_IRQHandler",
          "CAN1_Wake_Up_IRQHandler",
          "CAN1_ORed_0_15_MB_IRQHandler",
          "CAN1_ORed_16_31_MB_IRQHandler",
          "Reserved33_IRQHandler",
          "Reserved34_IRQHandler",
          "CAN2_ORed_IRQHandler",
          "CAN2_Error_IRQHandler",
          "CAN2_Wake_Up_IRQHandler",
          "CAN2_ORed_0_15_MB_IRQHandler",
          "CAN2_ORed_16_31_MB_IRQHandler",
          "Reserved35_IRQHandler",
          "Reserved36_IRQHandler",
          "eTMR0_Ch0_Ch1_IRQHandler",
          "eTMR0_Ch2_Ch3_IRQHandler",
          "eTMR0_Ch4_Ch5_IRQHandler",
          "eTMR0_Ch6_Ch7_IRQHandler",
          "eTMR0_Fault_IRQHandler",
          "eTMR0_Ovf_IRQHandler",
          "eTMR1_Ch0_Ch1_IRQHandler",
          "eTMR1_Ch2_Ch3_IRQHandler",
          "eTMR1_Ch4_Ch5_IRQHandler",
          "eTMR1_Ch6_Ch7_IRQHandler",
          "eTMR1_Fault_IRQHandler",
          "eTMR1_Ovf_IRQHandler",
          "eTMR2_Ch0_Ch1_IRQHandler",
          "eTMR2_Ch2_Ch3_IRQHandler",
          "eTMR2_Ch4_Ch5_IRQHandler",
          "eTMR2_Ch6_Ch7_IRQHandler",
          "eTMR2_Fault_IRQHandler",
          "eTMR2_Ovf_IRQHandler",
          "eTMR3_Ch0_Ch1_IRQHandler",
          "eTMR3_Ch2_Ch3_IRQHandler",
          "eTMR3_Ch4_Ch5_IRQHandler",
          "eTMR3_Ch6_Ch7_IRQHandler",
          "eTMR3_Fault_IRQHandler",
          "eTMR3_Ovf_IRQHandler",
          "Reserved37_IRQHandler",
          "Reserved38_IRQHandler",
          "Reserved39_IRQHandler",
          "Reserved40_IRQHandler",
          "Reserved41_IRQHandler",
          "Reserved42_IRQHandler",
          "Reserved43_IRQHandler",
          "Reserved44_IRQHandler",
          "Reserved45_IRQHandler",
          "Reserved46_IRQHandler",
          "Reserved47_IRQHandler",
          "Reserved48_IRQHandler",
          "Reserved49_IRQHandler",
          "Reserved50_IRQHandler",
          "Reserved51_IRQHandler",
          "Reserved52_IRQHandler",
          "Reserved53_IRQHandler",
          "Reserved54_IRQHandler",
          "Reserved55_IRQHandler",
          "Reserved56_IRQHandler",
          "Reserved57_IRQHandler",
          "Reserved58_IRQHandler",
          "Reserved59_IRQHandler",
          "Reserved60_IRQHandler",
          "Reserved61_IRQHandler",
          "Reserved62_IRQHandler",
          "Reserved63_IRQHandler",
          "Reserved64_IRQHandler",
          "Reserved65_IRQHandler",
          "Reserved66_IRQHandler",
          "Reserved67_IRQHandler",
          "Reserved68_IRQHandler",
          "Reserved69_IRQHandler",
          "TRNG_IRQHandler",
          "HCU_IRQHandler",
          "Reserved70_IRQHandler",
          "TMR0_Ch0_IRQHandler",
          "TMR0_Ch1_IRQHandler",
          "TMR0_Ch2_IRQHandler",
          "TMR0_Ch3_IRQHandler",
          "Reserved71_IRQHandler",
          "Reserved72_IRQHandler",
          "Reserved73_IRQHandler",
          "Reserved74_IRQHandler",
          "Reserved75_IRQHandler",
          "SPI3_IRQHandler",
          "Reserved76_IRQHandler",
          "Reserved77_IRQHandler",
          "Reserved78_IRQHandler",
          "Reserved79_IRQHandler",
          "Reserved80_IRQHandler",
          "Reserved81_IRQHandler",
          "Reserved82_IRQHandler",
          "Reserved83_IRQHandler",
          "Reserved84_IRQHandler",
          "Reserved85_IRQHandler",
          "Reserved86_IRQHandler",
          "SENT0_IRQHandler",
          "Reserved87_IRQHandler",
          "Reserved88_IRQHandler",
          "Reserved89_IRQHandler",
          "Reserved90_IRQHandler",
          "Reserved91_IRQHandler",
          "Reserved92_IRQHandler",
          "Reserved93_IRQHandler",
          "Reserved94_IRQHandler",
          "Reserved95_IRQHandler",
          "WKU_IRQHandler",
          "ALIGN_0_IRQHandler"
        ]
      },
      "updateTime": 1741914735337,
      "lock": false
    },
    "ytlink": {
      "enable": {},
      "data": [
        {
          "name": "P_FLASH",
          "level": 0,
          "isFlash": true,
          "id": "9ffa6a74-339d-44c8-ae55-7afd70fcecd7",
          "size": "0x80000",
          "startAddress": 0,
          "flags": "84.38%",
          "children": [
            {
              "name": "IVT",
              "level": 1,
              "id": "2315c9ba-7031-4f64-a7ef-e6879fd98618",
              "size": "1024",
              "order": 1,
              "startAddress": "0x0",
              "isFlash": true,
              "boundary": "UPPER",
              "x": 200,
              "y": -280,
              "children": [
                {
                  "name": "IVT",
                  "level": 2,
                  "id": "6baab512-6f23-40fc-ace2-3895338576d4",
                  "size": "",
                  "order": 0,
                  "startAddress": 0,
                  "isFlash": true,
                  "x": 500,
                  "y": -270,
                  "children": [
                    {
                      "name": "IVT",
                      "level": 3,
                      "id": "0627beab-7123-40c5-a18d-b9bcf8e1296d",
                      "size": "",
                      "order": 0,
                      "startAddress": 0,
                      "isFlash": true,
                      "x": 790,
                      "y": -270,
                      "children": [
                        {
                          "name": "isr_vector",
                          "level": 4,
                          "id": "10a3d117-4a5c-428f-8462-c10daca96e93",
                          "size": "",
                          "order": 0,
                          "startAddress": 0,
                          "isFlash": true,
                          "flags": "KEEP",
                          "x": 1130,
                          "y": -270
                        }
                      ]
                    }
                  ]
                }
              ]
            },
            {
              "name": "TEXT",
              "level": 1,
              "id": "5dacd8b2-a943-4507-a9df-17ddcbbd07d5",
              "size": "0x6BC00",
              "order": 2,
              "startAddress": "0x400",
              "isFlash": true,
              "boundary": "UPPER",
              "x": 200,
              "y": -230,
              "children": [
                {
                  "name": "COPY",
                  "level": 2,
                  "id": "a27335d8-5cf1-4761-8494-6dad793d4095",
                  "size": "",
                  "order": 2,
                  "startAddress": 0,
                  "isFlash": true,
                  "x": 500,
                  "y": 160,
                  "children": [
                    {
                      "name": "CODE_FLASH",
                      "level": 3,
                      "id": "4c03ad2b-89c2-410f-a6d5-1ac63e348b28",
                      "size": "",
                      "order": 0,
                      "align": 4,
                      "startAddress": 0,
                      "flags": "NULL",
                      "isFlash": true,
                      "x": 780,
                      "y": 160
                    },
                    {
                      "name": "DATA_FLASH",
                      "level": 3,
                      "id": "0670194a-8864-4c69-bab9-c9abf3e2cdcb",
                      "size": "",
                      "order": 0,
                      "align": 4,
                      "startAddress": 0,
                      "flags": "NULL",
                      "isFlash": true,
                      "x": 950,
                      "y": 230
                    }
                  ]
                },
                {
                  "name": "TEXT",
                  "level": 2,
                  "id": "7b2b296e-e4ab-4ac2-a7c2-d4ef382a74a8",
                  "size": "",
                  "order": 0,
                  "startAddress": 0,
                  "isFlash": true,
                  "x": 500,
                  "y": -60,
                  "children": [
                    {
                      "name": "TEXT",
                      "level": 3,
                      "id": "79ac2245-96a6-45c2-bcde-7c487fdad01c",
                      "size": "",
                      "order": 0,
                      "startAddress": 0,
                      "flags": "NULL",
                      "isFlash": true,
                      "x": 790,
                      "y": -60,
                      "children": [
                        {
                          "name": "text",
                          "level": 4,
                          "id": "732b76e1-9154-44bd-82dc-dfce0db96064",
                          "size": "",
                          "order": 0,
                          "startAddress": 0,
                          "flags": "NULL",
                          "isFlash": true,
                          "x": 1130,
                          "y": -70,
                          "wildcard": true
                        },
                        {
                          "name": "rodata",
                          "level": 4,
                          "id": "aa3d2cd7-5f0e-46fa-9861-ee1ee470efa4",
                          "size": "",
                          "order": 0,
                          "startAddress": 0,
                          "flags": "NULL",
                          "isFlash": true,
                          "x": 1130,
                          "y": -130,
                          "binFile": "",
                          "wildcard": true
                        }
                      ]
                    }
                  ]
                },
                {
                  "name": "ARM",
                  "level": 2,
                  "id": "70d2211e-2e86-40d9-8441-f391dc248280",
                  "size": "",
                  "order": 1,
                  "startAddress": "",
                  "flags": "",
                  "isFlash": true,
                  "x": 500,
                  "y": 40,
                  "children": [
                    {
                      "name": "ARM",
                      "level": 3,
                      "id": "d3a2d077-bba9-4bdf-b6e2-735d90480621",
                      "size": "",
                      "order": 0,
                      "startAddress": "",
                      "flags": "",
                      "isFlash": true,
                      "x": 790,
                      "y": 40,
                      "children": [
                        {
                          "name": "ARM.exidx",
                          "level": 4,
                          "id": "71c48f4c-5d57-408d-98a8-acf8835d4f5c",
                          "size": "",
                          "order": 0,
                          "startAddress": "",
                          "flags": "NULL",
                          "isFlash": true,
                          "wildcard": true,
                          "x": 1130,
                          "y": 40
                        }
                      ]
                    }
                  ]
                }
              ]
            }
          ],
          "x": -180,
          "y": -260
        },
        {
          "name": "RAM",
          "level": 0,
          "isFlash": false,
          "id": "71eff99e-ec18-4495-b4d3-8748da44c927",
          "size": "0x10000",
          "startAddress": "0x1FFF8000",
          "y": 530,
          "flags": "100.00%",
          "x": -180,
          "children": [
            {
              "name": "RAM",
              "level": 1,
              "id": "041e1a12-a38d-474a-8611-3c5fe39ad680",
              "size": "0xF800",
              "order": 1,
              "startAddress": "0x1fff8400",
              "isFlash": false,
              "boundary": "UPPER",
              "x": 200,
              "y": 520,
              "children": [
                {
                  "name": "BSS",
                  "level": 2,
                  "id": "8512e2b3-ab47-456f-9c32-b532eb942f24",
                  "size": "",
                  "order": 1,
                  "startAddress": 0,
                  "isFlash": false,
                  "clear": true,
                  "x": 510,
                  "y": 440,
                  "children": [
                    {
                      "name": "BSS",
                      "level": 3,
                      "id": "c9976186-8bd7-4212-b091-574a82d6befd",
                      "size": "",
                      "order": 0,
                      "startAddress": 0,
                      "flags": "NOLOAD",
                      "isFlash": false,
                      "x": 780,
                      "y": 440,
                      "clear": true,
                      "children": [
                        {
                          "name": "bss",
                          "level": 4,
                          "id": "6f24916e-dd23-4673-9c01-734802c0155a",
                          "size": "",
                          "order": 0,
                          "startAddress": 0,
                          "flags": "NULL",
                          "isFlash": false,
                          "x": 1110,
                          "y": 440,
                          "wildcard": true
                        }
                      ]
                    }
                  ]
                },
                {
                  "name": "DATA",
                  "level": 2,
                  "id": "fb79c358-1b80-4539-9e23-8d08877dcdd0",
                  "size": "",
                  "order": 1,
                  "startAddress": 0,
                  "isFlash": false,
                  "x": 510,
                  "y": 550,
                  "children": [
                    {
                      "name": "CODE_RAM",
                      "level": 3,
                      "id": "ecd50e6e-163f-4c04-a0fc-18a14c4c86f7",
                      "size": "",
                      "order": 0,
                      "startAddress": 0,
                      "flags": "NULL",
                      "isFlash": false,
                      "x": 780,
                      "y": 540,
                      "align": 4,
                      "copyFrom": "4c03ad2b-89c2-410f-a6d5-1ac63e348b28",
                      "children": [
                        {
                          "name": "code_ram",
                          "level": 4,
                          "id": "f767db5f-c8bb-4683-b572-e39617dccb6c",
                          "size": "",
                          "order": 0,
                          "startAddress": 0,
                          "flags": "NULL",
                          "isFlash": false,
                          "x": 1110,
                          "y": 540
                        }
                      ]
                    },
                    {
                      "name": "DATA_RAM",
                      "level": 3,
                      "id": "de9985d9-e89a-4e88-8da6-2c6128c635ec",
                      "size": "",
                      "order": 0,
                      "startAddress": 0,
                      "flags": "NULL",
                      "isFlash": false,
                      "x": 780,
                      "y": 630,
                      "copyFrom": "0670194a-8864-4c69-bab9-c9abf3e2cdcb",
                      "children": [
                        {
                          "name": "data",
                          "level": 4,
                          "id": "c5361333-f443-40b9-8566-ac8d8ef209e2",
                          "size": "",
                          "order": 0,
                          "startAddress": 0,
                          "flags": "NULL",
                          "isFlash": false,
                          "x": 1110,
                          "y": 630,
                          "wildcard": true
                        }
                      ]
                    }
                  ]
                }
              ],
              "init": "NORMAL"
            },
            {
              "name": "STACK",
              "level": 1,
              "id": "1c0909ef-5ee3-4499-b278-40e777069370",
              "size": "0x400",
              "order": 0,
              "startAddress": "0x20007c00",
              "isFlash": false,
              "boundary": "LOWER",
              "x": 200,
              "y": 700,
              "children": [
                {
                  "name": "STACK",
                  "level": 2,
                  "id": "0d1dd0ef-0478-4096-880a-db88f3301f88",
                  "size": "",
                  "order": 0,
                  "startAddress": 0,
                  "isFlash": false,
                  "x": 510,
                  "y": 740,
                  "children": [
                    {
                      "name": "STACK",
                      "level": 3,
                      "id": "08b94bc2-7906-47c6-b1f0-f9afcecff0f4",
                      "size": "",
                      "order": 0,
                      "startAddress": 0,
                      "flags": "NULL",
                      "isFlash": false,
                      "x": 780,
                      "y": 740,
                      "groupSize": "1024"
                    }
                  ]
                }
              ],
              "init": "NORMAL"
            },
            {
              "name": "IVT_RAM",
              "level": 1,
              "id": "91022760-091d-4db2-9815-f7feb273710d",
              "size": "0x400",
              "order": 0,
              "startAddress": "0x1fff8000",
              "isFlash": false,
              "init": "NORMAL",
              "boundary": "UPPER",
              "x": 200,
              "y": 390,
              "children": [
                {
                  "name": "IVT_RAM",
                  "level": 2,
                  "id": "9755c110-d819-47e1-a09d-abb77c1f76da",
                  "size": "",
                  "order": 0,
                  "startAddress": 0,
                  "isFlash": false,
                  "x": 500,
                  "y": 320,
                  "children": [
                    {
                      "name": "IVT_RAM",
                      "level": 3,
                      "id": "8d153954-ea4e-4071-898e-2531bdfc2fa2",
                      "size": "",
                      "order": 0,
                      "startAddress": 0,
                      "flags": "NULL",
                      "isFlash": false,
                      "groupSize": "0X400",
                      "align": 1024,
                      "x": 780,
                      "y": 320
                    }
                  ]
                }
              ]
            }
          ]
        }
      ],
      "updateTime": 1752735667778,
      "lock": false
    },
    "can": {
      "enable": {},
      "data": [
        {
          "name": "flexcanInitConfig0",
          "readonly": true,
          "inst": 0,
          "max_num_mb": 32,
          "num_id_filters": "FLEXCAN_RX_FIFO_ID_FILTERS_8",
          "flexcanMode": "FLEXCAN_NORMAL_MODE",
          "payload": "FLEXCAN_PAYLOAD_SIZE_8",
          "fd_enable": false,
          "pe_clock": "FLEXCAN_CLK_SOURCE_OSC",
          "transfer_type": "FLEXCAN_RXFIFO_USING_INTERRUPTS",
          "rxFifoDMAChannel": 0,
          "rxFifoDMALastWord": 0,
          "is_enhance_rx_fifo_needed": false,
          "num_enhance_rx_fifo_filters": 0,
          "num_enhance_rx_fifo_extid_filters": 0,
          "num_enhance_rx_fifo_min_messages": 0,
          "is_rx_fifo_needed": false,
          "bte": false,
          "bitrate": {
            "propSeg": 5,
            "phaseSeg1": 8,
            "phaseSeg2": 2,
            "preDivider": 3,
            "rJumpwidth": 2
          },
          "bitrate_cbt": {
            "propSeg": 6,
            "phaseSeg1": 3,
            "phaseSeg2": 2,
            "preDivider": 1,
            "rJumpwidth": 2
          }
        }
      ],
      "updateTime": 1742454782724,
      "lock": false
    },
    "dma": {
      "enable": {},
      "data": {
        "userConfig": {
          "haltOnError": false
        },
        "chs": [
          {
            "name": "dma_config0",
            "readonly": true,
            "virtChnConfig": 0,
            "source": "DMA_REQ_SPI2_TX",
            "callback": "NULL",
            "callbackParam": "NULL"
          },
          {
            "name": "dma_config1",
            "readonly": true,
            "virtChnConfig": 1,
            "source": "DMA_REQ_SPI2_RX",
            "callback": "NULL",
            "callbackParam": "NULL"
          }
        ],
        "transEnable": false,
        "trans": [
          {
            "name": "dma_transfer_config0",
            "srcAddr": 0,
            "destAddr": 0,
            "srcOffset": 0,
            "destOffset": 0,
            "srcTransferSize": "DMA_TRANSFER_SIZE_1B",
            "destTransferSize": "DMA_TRANSFER_SIZE_1B",
            "srcModulo": "DMA_MODULO_OFF",
            "destModulo": "DMA_MODULO_OFF",
            "loopTransferConfig": {
              "triggerLoopIterationCount": 1,
              "srcOffsetEnable": false,
              "dstOffsetEnable": false,
              "triggerLoopOffset": 0,
              "transferLoopChnLinkEnable": false,
              "transferLoopChnLinkNumber": 0,
              "triggerLoopChnLinkEnable": false,
              "triggerLoopChnLinkNumber": 0
            },
            "transferLoopByteCount": 0,
            "srcLastAddrAdjust": 0,
            "destLastAddrAdjust": 0,
            "interruptEnable": false
          }
        ]
      },
      "updateTime": 1746778559582,
      "lock": false
    },
    "wdg": {
      "enable": {},
      "data": [
        {
          "name": "wdg_config0",
          "readonly": true,
          "clockSource": "WDG_IPC_CLOCK",
          "opMode": {
            "deepsleep": false,
            "debug": false
          },
          "updateEnable": false,
          "intEnable": false,
          "winEnable": false,
          "windowValue": 0,
          "timeoutValue": 192000000,
          "apbErrorResetEnable": 0
        }
      ],
      "updateTime": 1742464618244,
      "lock": false
    },
    "adc": {
      "enable": {},
      "data": [
        {
          "name": "adc_config0",
          "readonly": true,
          "inst": 0,
          "clockDivider": 3,
          "startTime": 60,
          "sampleTime": 40,
          "overrunMode": false,
          "autoOffEnable": false,
          "waitEnable": false,
          "triggerSource": 0,
          "trigger": "ADC_TRIGGER_SOFTWARE",
          "align": "ADC_ALIGN_RIGHT",
          "resolution": "ADC_RESOLUTION_12BIT",
          "dmaWaterMark": 0,
          "dmaEnable": false,
          "sequenceConfig": {
            "channels": [
              {
                "channel": "ADC_INPUTCHAN_EXT16"
              },
              {
                "channel": "ADC_INPUTCHAN_EXT17"
              },
              {
                "channel": "ADC_INPUTCHAN_EXT22"
              },
              {
                "channel": "ADC_INPUTCHAN_EXT15"
              },
              {
                "channel": "ADC_INPUTCHAN_EXT25"
              },
              {
                "channel": "ADC_INPUTCHAN_EXT30"
              }
            ],
            "sequenceMode": "ADC_CONV_LOOP",
            "sequenceIntEnable": true,
            "convIntEnable": false,
            "readyIntEnable": false,
            "sampIntEnable": false,
            "ovrunIntEnable": false
          },
          "adcCompareCnt": 1,
          "compareConfig": [
            {
              "resolution": "ADC_RESOLUTION_12BIT",
              "compareEnable": false,
              "compareAllChannelEnable": false,
              "compHigh": 4095,
              "compLow": 0,
              "comWdchIndex": 0,
              "compIntEnable": false,
              "effectiveMode": "ADC_AWG_EFFECTIVE_OUTSIDE"
            },
            {
              "resolution": "ADC_RESOLUTION_12BIT",
              "compareEnable": false,
              "compareAllChannelEnable": false,
              "compHigh": 4095,
              "compLow": 0,
              "comWdchIndex": 0,
              "compIntEnable": false,
              "effectiveMode": "ADC_AWG_EFFECTIVE_OUTSIDE"
            },
            {
              "resolution": "ADC_RESOLUTION_12BIT",
              "compareEnable": false,
              "compareAllChannelEnable": false,
              "compHigh": 4095,
              "compLow": 0,
              "comWdchIndex": 0,
              "compIntEnable": false,
              "effectiveMode": "ADC_AWG_EFFECTIVE_OUTSIDE"
            },
            {
              "resolution": "ADC_RESOLUTION_12BIT",
              "compareEnable": false,
              "compareAllChannelEnable": false,
              "compHigh": 4095,
              "compLow": 0,
              "comWdchIndex": 0,
              "compIntEnable": false,
              "effectiveMode": "ADC_AWG_EFFECTIVE_OUTSIDE"
            }
          ]
        }
      ],
      "updateTime": 1754613782311,
      "lock": false
    },
    "etmr": {
      "enable": {},
      "data": {
        "common": [
          {
            "name": "ETMR_CM_Config0",
            "readonly": false,
            "etmrClockSource": "eTMR_CLOCK_SOURCE_INTERNALCLK",
            "etmrPrescaler": 120,
            "debugMode": false,
            "isTofIntEnabled": false,
            "syncMethod": {
              "regSyncFreq": 1,
              "regSyncSel": "REG_SYNC_WITH_MOD",
              "cntInitSyncSel": "CNT_SYNC_WITH_REG",
              "maskOutputSyncSel": "CHMASK_SYNC_WITH_REG",
              "regSyncTrigSrc": "DISABLE_TRIGGER",
              "cntInitSyncTrigSrc": "DISABLE_TRIGGER",
              "maskOutputSyncTrigSrc": "DISABLE_TRIGGER",
              "hwTrigRegLoadEnable": false,
              "hwTrigCounterLoadEnable": false,
              "hwTrigMaskLoadEnable": false
            },
            "outputTrigConfig": {
              "trigSrc": "TRIGGER_FROM_MATCHING_EVENT",
              "pwmOutputChannel": 0,
              "outputTrigWidth": 0,
              "outputTrigFreq": 1,
              "modMatchTrigEnable": false,
              "midMatchTrigEnable": false,
              "initMatchTrigEnable": false,
              "channelTrigParamConfig": []
            }
          },
          {
            "name": "ETMR_CM_Config1",
            "readonly": false,
            "etmrClockSource": "eTMR_CLOCK_SOURCE_INTERNALCLK",
            "etmrPrescaler": 120,
            "debugMode": false,
            "isTofIntEnabled": false,
            "syncMethod": {
              "regSyncFreq": 1,
              "regSyncSel": "REG_SYNC_WITH_MOD",
              "cntInitSyncSel": "CNT_SYNC_WITH_REG",
              "maskOutputSyncSel": "CHMASK_SYNC_WITH_REG",
              "regSyncTrigSrc": "DISABLE_TRIGGER",
              "cntInitSyncTrigSrc": "DISABLE_TRIGGER",
              "maskOutputSyncTrigSrc": "DISABLE_TRIGGER",
              "hwTrigRegLoadEnable": false,
              "hwTrigCounterLoadEnable": false,
              "hwTrigMaskLoadEnable": false
            },
            "outputTrigConfig": {
              "trigSrc": "TRIGGER_FROM_MATCHING_EVENT",
              "pwmOutputChannel": 0,
              "outputTrigWidth": 0,
              "outputTrigFreq": 1,
              "modMatchTrigEnable": false,
              "midMatchTrigEnable": false,
              "initMatchTrigEnable": false,
              "channelTrigParamConfig": []
            }
          },
          {
            "name": "ETMR_CM_Config2",
            "readonly": false,
            "etmrClockSource": "eTMR_CLOCK_SOURCE_INTERNALCLK",
            "etmrPrescaler": 120,
            "debugMode": false,
            "isTofIntEnabled": false,
            "syncMethod": {
              "regSyncFreq": 1,
              "regSyncSel": "REG_SYNC_WITH_MOD",
              "cntInitSyncSel": "CNT_SYNC_WITH_REG",
              "maskOutputSyncSel": "CHMASK_SYNC_WITH_REG",
              "regSyncTrigSrc": "DISABLE_TRIGGER",
              "cntInitSyncTrigSrc": "DISABLE_TRIGGER",
              "maskOutputSyncTrigSrc": "DISABLE_TRIGGER",
              "hwTrigRegLoadEnable": false,
              "hwTrigCounterLoadEnable": false,
              "hwTrigMaskLoadEnable": false
            },
            "outputTrigConfig": {
              "trigSrc": "TRIGGER_FROM_MATCHING_EVENT",
              "pwmOutputChannel": 0,
              "outputTrigWidth": 0,
              "outputTrigFreq": 1,
              "modMatchTrigEnable": false,
              "midMatchTrigEnable": false,
              "initMatchTrigEnable": false,
              "channelTrigParamConfig": []
            }
          }
        ],
        "pwm": {
          "enable": true,
          "data": [
            {
              "name": "ETMR_PWM_Config0",
              "readonly": false,
              "nNumIndependentPwmChannels": 1,
              "mode": "eTMR_PWM_MODE",
              "uFrequencyHZ": 2500,
              "counterInitValFromInitReg": false,
              "counterInitSrc": "COUNTER_VAL_FROM_CNT",
              "pwmIndependentChannelConfig": [
                {
                  "hwChannelId": 6,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_CENTER_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": "0x0",
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 5,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": true,
                  "align": "eTMR_PWM_CENTER_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 1,
                  "dutyCycle": "0x0",
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 6,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_CENTER_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": "0x0",
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 3,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_CENTER_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": "0x0",
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 0,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": 0,
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 0,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": 0,
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 0,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": 0,
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 0,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": 0,
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                }
              ],
              "deadtimeConfig": {
                "prs": 1,
                "evenDeadTime": 0,
                "oddDeadTime": 0
              },
              "faultConfig": {
                "pwmFaultInterrupt": false,
                "faultFilterSampleCounter": 0,
                "faultFilterSamplePeriod": 0,
                "faultInputStrentch": 0,
                "pwmRecoveryOpportunity": "eTMR_FAULT_PWM_RECOVERY_DISABLED",
                "pwmAutoRecoveryMode": "eTMR_MANUAL_CLEAR_FAULT_FLAG_THEN_AUTO_RECOVERY",
                "faultMode": "eTMR_FAULT_WITH_CLK",
                "etmrFaultChannelParam": [
                  {
                    "faultChannelEnabled": false,
                    "faultInputPolarity": "eTMR_FAULT_SIGNAL_HIGH"
                  },
                  {
                    "faultChannelEnabled": false,
                    "faultInputPolarity": "eTMR_FAULT_SIGNAL_HIGH"
                  },
                  {
                    "faultChannelEnabled": false,
                    "faultInputPolarity": "eTMR_FAULT_SIGNAL_HIGH"
                  },
                  {
                    "faultChannelEnabled": false,
                    "faultInputPolarity": "eTMR_FAULT_SIGNAL_HIGH"
                  }
                ],
                "safeState": [
                  {
                    "val": "eTMR_LOW_STATE"
                  },
                  {
                    "val": "eTMR_LOW_STATE"
                  },
                  {
                    "val": "eTMR_LOW_STATE"
                  },
                  {
                    "val": "eTMR_LOW_STATE"
                  }
                ]
              }
            },
            {
              "name": "ETMR_PWM_Config1",
              "readonly": false,
              "nNumIndependentPwmChannels": 1,
              "mode": "eTMR_PWM_MODE",
              "uFrequencyHZ": 400,
              "counterInitValFromInitReg": false,
              "counterInitSrc": "COUNTER_VAL_FROM_CNT",
              "pwmIndependentChannelConfig": [
                {
                  "hwChannelId": 2,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_CENTER_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": "0x0",
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 3,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": "0x0",
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 0,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": 0,
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 0,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": 0,
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 0,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": 0,
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 0,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": 0,
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 0,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": 0,
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 0,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": 0,
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                }
              ],
              "deadtimeConfig": {
                "prs": 1,
                "evenDeadTime": 0,
                "oddDeadTime": 0
              },
              "faultConfig": {
                "pwmFaultInterrupt": false,
                "faultFilterSampleCounter": 0,
                "faultFilterSamplePeriod": 0,
                "faultInputStrentch": 0,
                "pwmRecoveryOpportunity": "eTMR_FAULT_PWM_RECOVERY_DISABLED",
                "pwmAutoRecoveryMode": "eTMR_MANUAL_CLEAR_FAULT_FLAG_THEN_AUTO_RECOVERY",
                "faultMode": "eTMR_FAULT_WITH_CLK",
                "etmrFaultChannelParam": [
                  {
                    "faultChannelEnabled": false,
                    "faultInputPolarity": "eTMR_FAULT_SIGNAL_HIGH"
                  },
                  {
                    "faultChannelEnabled": false,
                    "faultInputPolarity": "eTMR_FAULT_SIGNAL_HIGH"
                  },
                  {
                    "faultChannelEnabled": false,
                    "faultInputPolarity": "eTMR_FAULT_SIGNAL_HIGH"
                  },
                  {
                    "faultChannelEnabled": false,
                    "faultInputPolarity": "eTMR_FAULT_SIGNAL_HIGH"
                  }
                ],
                "safeState": [
                  {
                    "val": "eTMR_LOW_STATE"
                  },
                  {
                    "val": "eTMR_LOW_STATE"
                  },
                  {
                    "val": "eTMR_LOW_STATE"
                  },
                  {
                    "val": "eTMR_LOW_STATE"
                  }
                ]
              }
            },
            {
              "name": "ETMR_PWM_Config2",
              "readonly": false,
              "nNumIndependentPwmChannels": 1,
              "mode": "eTMR_PWM_MODE",
              "uFrequencyHZ": 200,
              "counterInitValFromInitReg": false,
              "counterInitSrc": "COUNTER_VAL_FROM_CNT",
              "pwmIndependentChannelConfig": [
                {
                  "hwChannelId": 7,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_CENTER_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": "0x0",
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 0,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": 0,
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 0,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": 0,
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 0,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": 0,
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 0,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": 0,
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 0,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": 0,
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 0,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": 0,
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                },
                {
                  "hwChannelId": 0,
                  "polarity": "eTMR_POLARITY_NORMAL",
                  "pwmSrcInvert": false,
                  "align": "eTMR_PWM_RIGHT_EDGE_ALIGN",
                  "typeOfUpdate": "eTMR_PWM_UPDATE_IN_DUTY_CYCLE",
                  "channelInitVal": 0,
                  "dutyCycle": 0,
                  "offset": 0,
                  "enableSecondChannelOutput": false,
                  "secondChannelPolarity": "eTMR_POLARITY_NORMAL",
                  "evenDeadTime": 0,
                  "oddDeadTime": 0,
                  "enableDoubleSwitch": false,
                  "interruptEnable": false
                }
              ],
              "deadtimeConfig": {
                "prs": 1,
                "evenDeadTime": 0,
                "oddDeadTime": 0
              },
              "faultConfig": {
                "pwmFaultInterrupt": false,
                "faultFilterSampleCounter": 0,
                "faultFilterSamplePeriod": 0,
                "faultInputStrentch": 0,
                "pwmRecoveryOpportunity": "eTMR_FAULT_PWM_RECOVERY_DISABLED",
                "pwmAutoRecoveryMode": "eTMR_MANUAL_CLEAR_FAULT_FLAG_THEN_AUTO_RECOVERY",
                "faultMode": "eTMR_FAULT_WITH_CLK",
                "etmrFaultChannelParam": [
                  {
                    "faultChannelEnabled": false,
                    "faultInputPolarity": "eTMR_FAULT_SIGNAL_HIGH"
                  },
                  {
                    "faultChannelEnabled": false,
                    "faultInputPolarity": "eTMR_FAULT_SIGNAL_HIGH"
                  },
                  {
                    "faultChannelEnabled": false,
                    "faultInputPolarity": "eTMR_FAULT_SIGNAL_HIGH"
                  },
                  {
                    "faultChannelEnabled": false,
                    "faultInputPolarity": "eTMR_FAULT_SIGNAL_HIGH"
                  }
                ],
                "safeState": [
                  {
                    "val": "eTMR_LOW_STATE"
                  },
                  {
                    "val": "eTMR_LOW_STATE"
                  },
                  {
                    "val": "eTMR_LOW_STATE"
                  },
                  {
                    "val": "eTMR_LOW_STATE"
                  }
                ]
              }
            }
          ]
        },
        "ic": {
          "enable": false,
          "data": []
        },
        "oc": {
          "enable": false,
          "data": []
        },
        "qd": {
          "enable": false,
          "data": []
        },
        "mc": {
          "enable": false,
          "data": []
        }
      },
      "updateTime": 1776010820706,
      "lock": false
    },
    "fee": {
      "enable": {},
      "data": {
        "flashConfig": {
          "name": "FEEGenConfig",
          "readonly": true,
          "acEraseFunPtr": "NULL",
          "acWriteFunPtr": "NULL",
          "jobEndNotificationFunPtr": "Fee_JobEndNotification",
          "jobErrorNotificationFunPtr": "Fee_JobErrorNotification",
          "eDefaultMode": "MEMIF_MODE_SLOW",
          "maxReadFastMode": 256,
          "maxReadNormalMode": 256,
          "maxWriteFastMode": 128,
          "maxWriteNormalMode": 8,
          "sectorList": [
            {
              "sectorId": 0,
              "sectorStartAddress": "0x0",
              "sectorSize": "0x400",
              "pageSize": 8,
              "sectorHwStartAddress": "0x7c000",
              "asyncAccess": false
            },
            {
              "sectorId": 1,
              "sectorStartAddress": "0x400",
              "sectorSize": "0x400",
              "pageSize": 8,
              "sectorHwStartAddress": "0x7c400",
              "asyncAccess": false
            },
            {
              "sectorId": 2,
              "sectorStartAddress": "0x800",
              "sectorSize": "0x400",
              "pageSize": 8,
              "sectorHwStartAddress": "0x7c800",
              "asyncAccess": false
            },
            {
              "sectorId": 3,
              "sectorStartAddress": "0xc00",
              "sectorSize": "0x400",
              "pageSize": 8,
              "sectorHwStartAddress": "0x7cc00",
              "asyncAccess": false
            },
            {
              "sectorId": 4,
              "sectorStartAddress": "0x1000",
              "sectorSize": "0x400",
              "pageSize": 8,
              "sectorHwStartAddress": "0x7d000",
              "asyncAccess": false
            },
            {
              "sectorId": 5,
              "sectorStartAddress": "0x1400",
              "sectorSize": "0x400",
              "pageSize": 8,
              "sectorHwStartAddress": "0x7d400",
              "asyncAccess": false
            },
            {
              "sectorId": 6,
              "sectorStartAddress": "0x1800",
              "sectorSize": "0x400",
              "pageSize": 8,
              "sectorHwStartAddress": "0x7d800",
              "asyncAccess": false
            },
            {
              "sectorId": 7,
              "sectorStartAddress": "0x1c00",
              "sectorSize": "0x400",
              "pageSize": 8,
              "sectorHwStartAddress": "0x7dc00",
              "asyncAccess": false
            }
          ]
        },
        "clusterConfig": [
          {
            "ReservedSize": 256,
            "clusterList": [
              {
                "StartAddr": "0x0",
                "Length": "0x400"
              },
              {
                "StartAddr": "0x400",
                "Length": "0x400"
              }
            ]
          },
          {
            "ReservedSize": 384,
            "clusterList": [
              {
                "StartAddr": "0x800",
                "Length": "0x400"
              },
              {
                "StartAddr": "0xc00",
                "Length": "0x400"
              },
              {
                "StartAddr": "0x1000",
                "Length": "0x400"
              },
              {
                "StartAddr": "0x1400",
                "Length": "0x400"
              }
            ]
          },
          {
            "ReservedSize": 128,
            "clusterList": [
              {
                "StartAddr": "0x1800",
                "Length": "0x400"
              },
              {
                "StartAddr": "0x1c00",
                "Length": "0x400"
              }
            ]
          }
        ],
        "blockConfig": [
          {
            "BlockName": "FEE_BLOCK_1",
            "BlockNumber": 1,
            "BlockSize": 96,
            "ClrGrp": 0,
            "ImmediateData": true,
            "BlockAssignment": "FEE_PROJECT_RESERVED"
          },
          {
            "BlockName": "FEE_BLOCK_2",
            "BlockNumber": 2,
            "BlockSize": 96,
            "ClrGrp": 0,
            "ImmediateData": true,
            "BlockAssignment": "FEE_PROJECT_RESERVED"
          },
          {
            "BlockName": "FEE_BLOCK_3",
            "BlockNumber": 3,
            "BlockSize": 96,
            "ClrGrp": 1,
            "ImmediateData": true,
            "BlockAssignment": "FEE_PROJECT_RESERVED"
          },
          {
            "BlockName": "FEE_BLOCK_4",
            "BlockNumber": 4,
            "BlockSize": 96,
            "ClrGrp": 1,
            "ImmediateData": true,
            "BlockAssignment": "FEE_PROJECT_RESERVED"
          },
          {
            "BlockName": "FEE_BLOCK_5",
            "BlockNumber": 5,
            "BlockSize": 96,
            "ClrGrp": 1,
            "ImmediateData": true,
            "BlockAssignment": "FEE_PROJECT_RESERVED"
          },
          {
            "BlockName": "FEE_BLOCK_6",
            "BlockNumber": 6,
            "BlockSize": 96,
            "ClrGrp": 2,
            "ImmediateData": true,
            "BlockAssignment": "FEE_PROJECT_RESERVED"
          }
        ]
      },
      "updateTime": 1750322790334,
      "lock": false
    },
    "spi": {
      "enable": {},
      "data": {
        "master": [
          {
            "name": "spi_MasterConfig0",
            "readonly": true,
            "baudrate": 100000,
            "pcs": "SPI_PCS0",
            "polarity": "SPI_ACTIVE_LOW",
            "isPcsContinuous": true,
            "bitcount": 16,
            "clkPhase": "SPI_CLOCK_PHASE_2ND_EDGE",
            "clkPolarity": "SPI_SCK_ACTIVE_HIGH",
            "lsbFirst": true,
            "txDMAChannel": 0,
            "rxDMAChannel": 1,
            "transferType": "SPI_USING_DMA",
            "callback": "NULL",
            "callbackParam": "NULL",
            "width": "SPI_SINGLE_BIT_XFER"
          }
        ],
        "slave": []
      },
      "updateTime": 1747205571613,
      "lock": false
    },
    "hcu": {
      "enable": {},
      "data": [
        {
          "name": "hcu_config0",
          "readonly": true,
          "swap": "MODE_SWAPPING_NO",
          "carryType": "HCU_USING_POLLING",
          "ingressDMAChannel": 0,
          "egressDMAChannel": 0
        }
      ],
      "updateTime": 1748930236200,
      "lock": false
    },
    "lptmr": {
      "enable": {},
      "data": {
        "name": "LPTMR_Config",
        "readonly": true,
        "dmaRequest": false,
        "interruptEnable": true,
        "freeRun": false,
        "workMode": "lpTMR_WORKMODE_TIMER",
        "prescaler": "lpTMR_PRESCALE_2",
        "bypassPrescaler": false,
        "compareValue": 1000,
        "counterUnits": "lpTMR_COUNTER_UNITS_MICROSECONDS",
        "pinSelect": "lpTMR_PINSELECT_TMU",
        "pinPolarity": "lpTMR_PINPOLARITY_RISING",
        "clockSource": "lpTMR_CLOCK_SOURCE_IPC"
      },
      "updateTime": 1752736133192,
      "lock": false
    },
    "wkup": {
      "enable": {},
      "data": [
        {
          "resetName": "wkup_resetConfig0",
          "pinsName": "wkup_pinsConfig0",
          "readonly": true,
          "wakeupEn": true,
          "filterEn": false,
          "filterClkSrc": "WKU_FILTER_CLK_SIRC",
          "wkupPins": []
        }
      ],
      "updateTime": 1767722599541,
      "lock": false
    },
    "power": {
      "enable": {},
      "data": {
        "user": [
          {
            "name": "Power_down",
            "powerMode": "POWER_MANAGER_STANDBY",
            "sleepOnExitValue": false
          }
        ],
        "callback": []
      },
      "updateTime": 1767722685820,
      "lock": false
    }
  }
}