VERSION ""


NS_ : 
	NS_DESC_
	CM_
	BA_DEF_
	BA_
	VAL_
	CAT_DEF_
	CAT_
	FILTER
	BA_DEF_DEF_
	EV_DATA_
	ENVVAR_DATA_
	SGTYPE_
	SGTYPE_VAL_
	BA_DEF_SGTYPE_
	BA_SGTYPE_
	SIG_TYPE_REF_
	VAL_TABLE_
	SIG_GROUP_
	SIG_VALTYPE_
	SIGTYPE_VALTYPE_
	BO_TX_BU_
	BA_DEF_REL_
	BA_REL_
	BA_DEF_DEF_REL_
	BU_SG_REL_
	BU_EV_REL_
	BU_BO_REL_
	SG_MUL_VAL_

BS_:

BU_: ACP AC VCU EC GW


BO_ 2566851609 HVAC: 8 AC
 SG_ HVAC_Cool_heat_mode_resp : 0|2@1+ (1,0) [0|3] ""  VCU
 SG_ HVAC_Mode_sele_button : 2|3@1+ (1,0) [0|7] ""  VCU
 SG_ HVAC_Auto_button : 5|2@1+ (1,0) [0|3] ""  VCU
 SG_ HVAC_OFF_ON_button : 8|2@1+ (1,0) [0|3] ""  VCU
 SG_ HVAC_Fan_Adj_button : 10|4@1+ (1,0) [0|15] ""  VCU
 SG_ HVAC_AC_OUT : 14|2@1+ (1,0) [0|3] ""  VCU
 SG_ HVAC_AC_Req : 16|2@1+ (1,0) [0|3] ""  VCU
 SG_ HVAC_Defrost_Sts : 18|2@1+ (1,0) [0|3] ""  VCU
 SG_ HVAC_AC_Wrok_Mode : 20|2@1+ (1,0) [0|3] ""  VCU
 SG_ HVAC_Negative_ion_state : 22|2@1+ (1,0) [0|3] ""  VCU
 SG_ HVAC_Left_Temp_adj_button : 24|8@1+ (0.1,16.5) [16.5|32.5] "℃"  VCU
 SG_ HVAC_DUAL_Setting : 32|2@1+ (1,0) [0|3] ""  VCU
 SG_ HVAC_Circulation_button : 34|3@1+ (1,0) [0|7] ""  VCU
 SG_ HVAC_Parking_Heating : 37|2@1+ (1,0) [0|3] ""  VCU
 SG_ HVAC_Right_Temp_adj_button : 40|8@1+ (0.1,16.5) [16.5|32.5] ""  VCU
 SG_ HVAC_Battery_Volt_sts : 48|2@1+ (1,0) [0|3] ""  VCU
 SG_ HVAC_Humidity : 56|8@1+ (1,0) [0|255] ""  VCU

BO_ 2583632680 IDCU: 8 VCU
 SG_ IDCU_mode_key : 2|3@1+ (1,0) [0|7] ""  AC
 SG_ IDCU_auto_key : 5|2@1+ (1,0) [0|3] ""  AC
 SG_ ICDU_OFF_ON : 8|2@1+ (1,0) [0|3] ""  AC
 SG_ IDCU_FAN_Adj : 10|4@1+ (1,0) [0|15] ""  AC
 SG_ IDCU_AC_Req : 16|2@1+ (1,0) [0|3] ""  AC
 SG_ IDCU_Lefg_Adj_Key : 24|8@1+ (0.1,16.5) [16.5|32.5] ""  AC
 SG_ IDCU_Circulation_Adj_Key : 34|3@1+ (1,0) [0|7] ""  AC
 SG_ IDCU_Rgt_Adj_Key : 40|8@1+ (0.1,16.5) [16.5|32.5] ""  AC
 SG_ IDCU_DUAL_Setting : 48|2@1+ (1,0) [0|3] ""  AC
 SG_ IDCU_key_defrost : 50|2@1+ (1,0) [0|3] ""  AC
 SG_ IDCU_key_dehum : 52|2@1+ (1,0) [0|3] ""  AC
 SG_ IDCU_Init : 54|2@1+ (1,1) [1|3] ""  AC
 SG_ IDCU_PARKING_Timeing : 56|7@1+ (0.1,0) [0|120] ""  AC

BO_ 2566845719 AMB: 8 VCU
 SG_ AMB : 24|16@1+ (0.03125,-273) [-273|1734] "℃"  AC

BO_ 2364539904 Engine_Speed: 8 VCU
 SG_ Engine_Speed : 24|16@1+ (0.125,0) [0|8031] "℃"  AC

BO_ 2566907929 HVAC_1: 8 VCU
 SG_ AC_DUAL_configuration : 0|2@1+ (1,0) [0|7] ""  VCU
 SG_ AC_ION_configuration : 2|2@1+ (1,0) [0|3] ""  VCU
 SG_ AC_PM2_5_configuration : 4|2@1+ (1,-40) [0|3] ""  VCU
 SG_ EVAP_Temp : 8|8@1+ (1,-40) [-40|255] ""  VCU
 SG_ Incar_Temp : 16|8@1+ (1,-40) [-40|255] ""  VCU

BO_ 2566851865 HVAC_VERSION: 8 VCU
 SG_ SW_VERS : 0|16@1+ (0.01,0) [9.99|9.99] ""  VCU
 SG_ HW_VERS : 16|16@1+ (0.01,0) [9.99|9.99] ""  VCU
 SG_ SUPPLIER_CODE : 32|32@1+ (1,0) [4294967295|4294967295] ""  VCU

BO_ 2566907417 HVAC_ACSpeed: 8 VCU
 SG_ HVAC_timing_countdown : 0|16@1+ (0.1,0) [0|127] ""  VCU
 SG_ HVAC_M_pressure_switch : 16|2@1+ (1,0) [0|2] ""  VCU
 SG_ HVAC_initialization : 18|2@1+ (1,0) [0|2] ""  VCU
 SG_ HVAC_COMP_ComprSpd : 24|16@1+ (1,0) [0|16000] ""  VCU
 SG_ HVAC_COMP_ComprSt : 40|8@1+ (1,0) [0|255] ""  VCU

BO_ 2566866351 CO: 8 VCU
 SG_ CO : 48|16@1+ (1,0) [0|1000] ""  AC

BO_ 2566874003 CeWei: 8 VCU
 SG_ ACSwt : 0|2@1+ (1,0) [0|3] ""  AC
 SG_ HeaterMechSet : 2|4@1+ (1,0) [0|16] ""  AC
 SG_ HeaterSwt : 6|2@1+ (1,0) [0|3] ""  AC
 SG_ TempSet : 8|8@1+ (0.1,16.5) [0|255] ""  AC
 SG_ TimeSet : 16|8@1+ (0.1,0) [0|24] ""  AC

BO_ 2565812505 HVAC_TMS: 8 VCU
 SG_ HVACS_Acc_ReqSt : 0|2@1+ (1,0) [0|3] ""  VCU
 SG_ HVACS_Compr_CtrlSt : 2|2@1+ (1,0) [0|3] ""  VCU
 SG_ HVACS_ComprSpd : 8|16@1+ (0.125,0) [0|65535] ""  VCU
 SG_ HVACS_CondFanCtrlSt : 24|2@1+ (1,0) [0|3] ""  VCU
 SG_ HVACS_Press_lSt : 26|2@1+ (1,0) [0|3] ""  VCU

BO_ 2565812696 Park_AC_Feedback: 8 VCU
 SG_ COMP_ComprSpd : 0|16@1+ (1,0) [0|16000] ""  AC
 SG_ COMP_ComprSt : 24|2@1+ (1,0) [0|3] ""  AC
 SG_ COMP_CompErrCode : 32|8@1+ (1,0) [0|255] ""  AC
 SG_ COMP_CompErrCode1 : 40|8@1+ (1,0) [0|255] ""  AC
 SG_ COMP_CompRunCurr : 48|8@1+ (0.1,0) [0|25.4] ""  AC
 SG_ COMP_CompDCVol : 56|8@1+ (4,0) [0|1016] ""  AC

BO_ 2566892357 PHCU: 8 VCU
 SG_ Sts : 16|8@1+ (1,0) [0|256] ""  AC

BO_ 2583646233 AC_PANEL: 8 VCU
 SG_ key_Left_Set_Add : 0|4@1+ (1,0) [0|2] ""  AC
 SG_ key_Left_Set_Subb : 4|4@1+ (1,0) [0|2] ""  AC
 SG_ key_Blower_Set_Add : 8|4@1+ (1,0) [0|2] ""  AC
 SG_ key_Blower_Set_Subb : 12|4@1+ (1,0) [0|2] ""  AC
 SG_ key_CyclButton : 16|4@1+ (1,0) [0|2] ""  AC
 SG_ key_OFFButton : 20|4@1+ (1,0) [0|2] ""  AC
 SG_ key_ACButton : 24|4@1+ (1,0) [0|2] ""  AC
 SG_ key_AUTOButton : 28|4@1+ (1,0) [0|2] ""  AC
 SG_ key_ModeButton : 32|4@1+ (1,0) [0|2] ""  AC
 SG_ key_DefButton : 36|4@1+ (1,0) [0|2] ""  AC

BO_ 2566912281 ACCA_TMS_EPAC2: 8 VCU
 SG_ HVACS_Acc_ReqSt : 0|2@1+ (1,0) [0|3] ""  VCU
 SG_ HVACS_Press_lSt : 2|2@1+ (1,0) [0|3] ""  VCU
 SG_ Heating_cooling_mode : 4|2@1+ (1,0) [0|3] ""  VCU
 SG_ Heating_Tag_Temp : 8|8@1+ (1,-50) [-50|255] ""  VCU
 SG_ T_EVAP : 16|8@1+ (0.5,-40) [-50|255] ""  VCU
 SG_ EvpTemp : 32|8@1+ (0.5,-40) [-50|255] ""  VCU
 SG_ HVAC_Fan_Adj : 24|4@1+ (1,0) [0|15] ""  VCU

BO_ 2565855257 ACCA_EPAC: 8 VCU
 SG_ AC_speed_of_compressor : 0|16@1+ (1,0) [0|65534] ""  VCU
 SG_ AC_max_perm_compressor_power : 16|8@1+ (0.1,0) [0|25.4] ""  VCU
 SG_ AC_compressor_enable : 24|8@1+ (1,0) [0|255] ""  VCU



CM_ SG_ 2566851609 HVAC_Cool_heat_mode_resp "制冷或制热模式应答";
CM_ SG_ 2566851609 HVAC_Mode_sele_button "模式选择按键";
CM_ SG_ 2566851609 HVAC_Auto_button "AUTO按键";
CM_ SG_ 2566851609 HVAC_OFF_ON_button "OFF/ON";
CM_ SG_ 2566851609 HVAC_Fan_Adj_button "风量调节按键";
CM_ SG_ 2566851609 HVAC_AC_OUT "AC输出";
CM_ SG_ 2566851609 HVAC_AC_Req "AC请求";
CM_ SG_ 2566851609 HVAC_Defrost_Sts "除霜状态";
CM_ SG_ 2566851609 HVAC_AC_Wrok_Mode "空调工作模式";
CM_ SG_ 2566851609 HVAC_Negative_ion_state "负离子状态";
CM_ SG_ 2566851609 HVAC_Left_Temp_adj_button "左温度调节按键";
CM_ SG_ 2566851609 HVAC_DUAL_Setting "双温区驱动";
CM_ SG_ 2566851609 HVAC_Circulation_button "内外循环切换按键";
CM_ SG_ 2566851609 HVAC_Parking_Heating "驻车暖风";
CM_ SG_ 2566851609 HVAC_Right_Temp_adj_button "右温区温度调节";
CM_ SG_ 2566851609 HVAC_Battery_Volt_sts "电池电压状态";
CM_ SG_ 2566851609 HVAC_Humidity "室内湿度";
CM_ SG_ 2583632680 IDCU_mode_key "模式选择按键";
CM_ SG_ 2583632680 IDCU_auto_key "AUTO按键";
CM_ SG_ 2583632680 ICDU_OFF_ON "OFF/ON";
CM_ SG_ 2583632680 IDCU_FAN_Adj "风量调节按键";
CM_ SG_ 2583632680 IDCU_AC_Req "AC请求";
CM_ SG_ 2583632680 IDCU_Lefg_Adj_Key "左温度调节按键";
CM_ SG_ 2583632680 IDCU_Circulation_Adj_Key "内外循环切换按键";
CM_ SG_ 2583632680 IDCU_Rgt_Adj_Key "右温度调节按键";
CM_ SG_ 2583632680 IDCU_DUAL_Setting "双温区驱动";
CM_ SG_ 2583632680 IDCU_key_defrost "一键除霜";
CM_ SG_ 2583632680 IDCU_key_dehum "一键除湿";
CM_ SG_ 2583632680 IDCU_Init "初始化";
CM_ SG_ 2583632680 IDCU_PARKING_Timeing "驻车空调定时";
CM_ SG_ 2566845719 AMB "环境温度";
CM_ SG_ 2364539904 Engine_Speed "转速信号";
CM_ SG_ 2566907929 AC_DUAL_configuration "空调单/双温区配置";
CM_ SG_ 2566907929 AC_ION_configuration "空调负离子配置";
CM_ SG_ 2566907929 AC_PM2_5_configuration "空调PM2.5配置";
CM_ SG_ 2566907929 EVAP_Temp "蒸发器温度传感器";
CM_ SG_ 2566907929 Incar_Temp "车内温度传感器";
CM_ SG_ 2566851865 SW_VERS "软件版本号";
CM_ SG_ 2566851865 HW_VERS "硬件版本号";
CM_ SG_ 2566851865 SUPPLIER_CODE "供应商代码";
CM_ SG_ 2566907417 HVAC_timing_countdown "空调定时-倒计时";
CM_ SG_ 2566907417 HVAC_M_pressure_switch "中压开关";
CM_ SG_ 2566907417 HVAC_initialization "初始化执行";
CM_ SG_ 2566907417 HVAC_COMP_ComprSpd "驻车空调压缩机转速";
CM_ SG_ 2566907417 HVAC_COMP_ComprSt "驻车空调压缩机状态";
CM_ SG_ 2566866351 CO "CO浓度值";
CM_ SG_ 2566874003 ACSwt "唤醒开关
";
CM_ SG_ 2566874003 HeaterMechSet "驻车暖风档位
";
CM_ SG_ 2566874003 HeaterSwt "驻车暖风开关";
CM_ SG_ 2566874003 TempSet "空调温度设置，行车模式温度16.5-32.5，驻车模式温度24°-30°";
CM_ SG_ 2566874003 TimeSet "驻车空调/驻车暖风定时设置";
CM_ SG_ 2565812505 HVACS_Acc_ReqSt "AC请求状态";
CM_ SG_ 2565812505 HVACS_Compr_CtrlSt "空调压缩机控制状态";
CM_ SG_ 2565812505 HVACS_ComprSpd "压缩机转速";
CM_ SG_ 2565812505 HVACS_CondFanCtrlSt "冷凝风扇状态";
CM_ SG_ 2565812505 HVACS_Press_lSt "压力开关状态";
CM_ SG_ 2565812696 COMP_ComprSpd "空调压缩机转速";
CM_ SG_ 2565812696 COMP_ComprSt "空调压缩机状态";
CM_ SG_ 2565812696 COMP_CompErrCode "空调压缩机故障码";
CM_ SG_ 2565812696 COMP_CompErrCode1 "空调压缩机故障码";
CM_ SG_ 2565812696 COMP_CompRunCurr "空调压缩机直流电流";
CM_ SG_ 2565812696 COMP_CompDCVol "空调压缩机直流电压";
CM_ SG_ 2566892357 Sts "CO浓度值";
CM_ SG_ 2583646233 key_Left_Set_Add "左设定按键+";
CM_ SG_ 2583646233 key_Left_Set_Subb "左设定按键-";
CM_ SG_ 2583646233 key_Blower_Set_Add "风量按键+";
CM_ SG_ 2583646233 key_Blower_Set_Subb "风量按键-";
CM_ SG_ 2583646233 key_CyclButton "循环按键";
CM_ SG_ 2583646233 key_OFFButton "开关机按键";
CM_ SG_ 2583646233 key_ACButton "AC按键";
CM_ SG_ 2583646233 key_AUTOButton "AUTO按键";
CM_ SG_ 2583646233 key_ModeButton "模式按键";
CM_ SG_ 2583646233 key_DefButton "强制除霜按键";
CM_ SG_ 2566912281 HVACS_Acc_ReqSt "AC请求状态";
CM_ SG_ 2566912281 HVACS_Press_lSt "压力开关状态";
CM_ SG_ 2566912281 Heating_cooling_mode "驾驶室需求模式（制热，制冷，除湿）";
CM_ SG_ 2566912281 Heating_Tag_Temp "制热目标温度-T";
CM_ SG_ 2566912281 T_EVAP "蒸发器目标温度";
CM_ SG_ 2566912281 EvpTemp "蒸发器实际温度";
CM_ SG_ 2566912281 HVAC_Fan_Adj "风量调节按键";
CM_ SG_ 2565855257 AC_speed_of_compressor "压缩机目标转速";
CM_ SG_ 2565855257 AC_max_perm_compressor_power "最大运行压缩机消耗的功率";
CM_ SG_ 2565855257 AC_compressor_enable "压缩机开关机命令";
BA_DEF_ SG_  "GenSigStartValue" INT 0 0;
BA_DEF_ SG_  "GenSigInvalidValue" INT 0 0;
BA_DEF_ SG_  "GenSigInactiveValue" INT 0 0;
BA_DEF_ BO_  "DiagMessage" ENUM  "No","Yes";
BA_DEF_ BO_  "NmMessage" ENUM  "No","Yes";
BA_DEF_ BO_  "GenMsgCycleTimeFast" INT 0 0;
BA_DEF_ BO_  "GenMsgNrOfRepetition" INT 0 0;
BA_DEF_ BO_  "GenMsgCycleTime" INT 0 0;
BA_DEF_ BO_  "GenMsgDelayTime" INT 0 0;
BA_DEF_ SG_  "GenSigSendType" ENUM  "Cyclic","OnWrite","OnWriteWithRepetition","OnChange","OnChangeWithRepetition","IfActive","IfActiveWithRepetition";
BA_DEF_ BO_  "GenMsgSendType" ENUM  "Cyclic","Event","IfActive","CE","CA";
BA_DEF_ BO_  "GenMsgILSupport" ENUM  "No","Yes";
BA_DEF_ BU_  "ILUsed" ENUM  "No","Yes";
BA_DEF_ BO_  "CANFD_BRS" ENUM  "0","1";
BA_DEF_  "DBName" STRING ;
BA_DEF_  "BusType" STRING ;
BA_DEF_ BU_  "NodeLayerModules" STRING ;
BA_DEF_ BU_  "ECU" STRING ;
BA_DEF_ BU_  "CANoeJitterMax" INT 0 0;
BA_DEF_ BU_  "CANoeJitterMin" INT 0 0;
BA_DEF_ BU_  "CANoeDrift" INT 0 0;
BA_DEF_ BU_  "CANoeStartDelay" INT 0 0;
BA_DEF_ BO_  "VFrameFormat" ENUM  "StandardCAN","ExtendedCAN","reserved","reserved","reserved","reserved","reserved","reserved","reserved","reserved","reserved","reserved","reserved","reserved","StandardCAN_FD","ExtendedCAN_FD";
BA_DEF_DEF_  "GenSigStartValue" 0;
BA_DEF_DEF_  "GenSigInvalidValue" 0;
BA_DEF_DEF_  "GenSigInactiveValue" 0;
BA_DEF_DEF_  "DiagMessage" "";
BA_DEF_DEF_  "NmMessage" "";
BA_DEF_DEF_  "GenMsgCycleTimeFast" 0;
BA_DEF_DEF_  "GenMsgNrOfRepetition" 0;
BA_DEF_DEF_  "GenMsgCycleTime" 0;
BA_DEF_DEF_  "GenMsgDelayTime" 0;
BA_DEF_DEF_  "GenSigSendType" "Cyclic";
BA_DEF_DEF_  "GenMsgSendType" "Cyclic";
BA_DEF_DEF_  "GenMsgILSupport" "Yes";
BA_DEF_DEF_  "ILUsed" "Yes";
BA_DEF_DEF_  "CANFD_BRS" "0";
BA_DEF_DEF_  "DBName" "";
BA_DEF_DEF_  "BusType" "";
BA_DEF_DEF_  "NodeLayerModules" "";
BA_DEF_DEF_  "ECU" "";
BA_DEF_DEF_  "CANoeJitterMax" 0;
BA_DEF_DEF_  "CANoeJitterMin" 0;
BA_DEF_DEF_  "CANoeDrift" 0;
BA_DEF_DEF_  "CANoeStartDelay" 0;
BA_DEF_DEF_  "VFrameFormat" "";
BA_ "BusType" "CAN";
BA_ "DBName" "CANMatrix";
BA_ "VFrameFormat" BO_ 2566851609 1;
BA_ "GenMsgCycleTime" BO_ 2566851609 100;
BA_ "GenMsgSendType" BO_ 2566851609 0;
BA_ "GenMsgDelayTime" BO_ 2566851609 0;
BA_ "GenMsgNrOfRepetition" BO_ 2566851609 0;
BA_ "GenMsgCycleTimeFast" BO_ 2566851609 0;
BA_ "VFrameFormat" BO_ 2583632680 1;
BA_ "GenMsgCycleTime" BO_ 2583632680 100;
BA_ "GenMsgSendType" BO_ 2583632680 0;
BA_ "GenMsgDelayTime" BO_ 2583632680 0;
BA_ "GenMsgNrOfRepetition" BO_ 2583632680 0;
BA_ "GenMsgCycleTimeFast" BO_ 2583632680 0;
BA_ "VFrameFormat" BO_ 2566845719 1;
BA_ "GenMsgCycleTime" BO_ 2566845719 100;
BA_ "GenMsgSendType" BO_ 2566845719 0;
BA_ "GenMsgDelayTime" BO_ 2566845719 0;
BA_ "GenMsgNrOfRepetition" BO_ 2566845719 0;
BA_ "GenMsgCycleTimeFast" BO_ 2566845719 0;
BA_ "VFrameFormat" BO_ 2364539904 1;
BA_ "GenMsgCycleTime" BO_ 2364539904 100;
BA_ "GenMsgSendType" BO_ 2364539904 0;
BA_ "GenMsgDelayTime" BO_ 2364539904 0;
BA_ "GenMsgNrOfRepetition" BO_ 2364539904 0;
BA_ "GenMsgCycleTimeFast" BO_ 2364539904 0;
BA_ "VFrameFormat" BO_ 2566907929 1;
BA_ "GenMsgCycleTime" BO_ 2566907929 200;
BA_ "GenMsgSendType" BO_ 2566907929 0;
BA_ "GenMsgDelayTime" BO_ 2566907929 0;
BA_ "GenMsgNrOfRepetition" BO_ 2566907929 0;
BA_ "GenMsgCycleTimeFast" BO_ 2566907929 0;
BA_ "VFrameFormat" BO_ 2566851865 1;
BA_ "GenMsgCycleTime" BO_ 2566851865 200;
BA_ "GenMsgSendType" BO_ 2566851865 0;
BA_ "GenMsgDelayTime" BO_ 2566851865 0;
BA_ "GenMsgNrOfRepetition" BO_ 2566851865 0;
BA_ "GenMsgCycleTimeFast" BO_ 2566851865 0;
BA_ "VFrameFormat" BO_ 2566907417 1;
BA_ "GenMsgCycleTime" BO_ 2566907417 100;
BA_ "GenMsgSendType" BO_ 2566907417 0;
BA_ "GenMsgDelayTime" BO_ 2566907417 0;
BA_ "GenMsgNrOfRepetition" BO_ 2566907417 0;
BA_ "GenMsgCycleTimeFast" BO_ 2566907417 0;
BA_ "VFrameFormat" BO_ 2566866351 1;
BA_ "GenMsgCycleTime" BO_ 2566866351 100;
BA_ "GenMsgSendType" BO_ 2566866351 0;
BA_ "GenMsgDelayTime" BO_ 2566866351 0;
BA_ "GenMsgNrOfRepetition" BO_ 2566866351 0;
BA_ "GenMsgCycleTimeFast" BO_ 2566866351 0;
BA_ "VFrameFormat" BO_ 2566874003 1;
BA_ "GenMsgCycleTime" BO_ 2566874003 100;
BA_ "GenMsgSendType" BO_ 2566874003 0;
BA_ "GenMsgDelayTime" BO_ 2566874003 0;
BA_ "GenMsgNrOfRepetition" BO_ 2566874003 0;
BA_ "GenMsgCycleTimeFast" BO_ 2566874003 0;
BA_ "VFrameFormat" BO_ 2565812505 1;
BA_ "GenMsgCycleTime" BO_ 2565812505 100;
BA_ "GenMsgSendType" BO_ 2565812505 0;
BA_ "GenMsgDelayTime" BO_ 2565812505 0;
BA_ "GenMsgNrOfRepetition" BO_ 2565812505 0;
BA_ "GenMsgCycleTimeFast" BO_ 2565812505 0;
BA_ "VFrameFormat" BO_ 2565812696 1;
BA_ "GenMsgCycleTime" BO_ 2565812696 100;
BA_ "GenMsgSendType" BO_ 2565812696 0;
BA_ "GenMsgDelayTime" BO_ 2565812696 0;
BA_ "GenMsgNrOfRepetition" BO_ 2565812696 0;
BA_ "GenMsgCycleTimeFast" BO_ 2565812696 0;
BA_ "VFrameFormat" BO_ 2566892357 1;
BA_ "GenMsgCycleTime" BO_ 2566892357 100;
BA_ "GenMsgSendType" BO_ 2566892357 0;
BA_ "GenMsgDelayTime" BO_ 2566892357 0;
BA_ "GenMsgNrOfRepetition" BO_ 2566892357 0;
BA_ "GenMsgCycleTimeFast" BO_ 2566892357 0;
BA_ "VFrameFormat" BO_ 2583646233 1;
BA_ "GenMsgCycleTime" BO_ 2583646233 100;
BA_ "GenMsgSendType" BO_ 2583646233 0;
BA_ "GenMsgDelayTime" BO_ 2583646233 0;
BA_ "GenMsgNrOfRepetition" BO_ 2583646233 0;
BA_ "GenMsgCycleTimeFast" BO_ 2583646233 0;
BA_ "VFrameFormat" BO_ 2566912281 1;
BA_ "GenMsgCycleTime" BO_ 2566912281 200;
BA_ "GenMsgSendType" BO_ 2566912281 0;
BA_ "GenMsgDelayTime" BO_ 2566912281 0;
BA_ "GenMsgNrOfRepetition" BO_ 2566912281 0;
BA_ "GenMsgCycleTimeFast" BO_ 2566912281 0;
BA_ "VFrameFormat" BO_ 2565855257 1;
BA_ "GenMsgCycleTime" BO_ 2565855257 100;
BA_ "GenMsgSendType" BO_ 2565855257 0;
BA_ "GenMsgDelayTime" BO_ 2565855257 0;
BA_ "GenMsgNrOfRepetition" BO_ 2565855257 0;
BA_ "GenMsgCycleTimeFast" BO_ 2565855257 0;
BA_ "GenSigSendType" SG_ 2566851609 HVAC_Cool_heat_mode_resp 0;
BA_ "GenSigInactiveValue" SG_ 2566851609 HVAC_Cool_heat_mode_resp 0;
BA_ "GenSigStartValue" SG_ 2566851609 HVAC_Cool_heat_mode_resp 3;
BA_ "GenSigSendType" SG_ 2566851609 HVAC_Mode_sele_button 0;
BA_ "GenSigInactiveValue" SG_ 2566851609 HVAC_Mode_sele_button 0;
BA_ "GenSigStartValue" SG_ 2566851609 HVAC_Mode_sele_button 7;
BA_ "GenSigSendType" SG_ 2566851609 HVAC_Auto_button 0;
BA_ "GenSigInactiveValue" SG_ 2566851609 HVAC_Auto_button 0;
BA_ "GenSigStartValue" SG_ 2566851609 HVAC_Auto_button 3;
BA_ "GenSigSendType" SG_ 2566851609 HVAC_OFF_ON_button 0;
BA_ "GenSigInactiveValue" SG_ 2566851609 HVAC_OFF_ON_button 0;
BA_ "GenSigStartValue" SG_ 2566851609 HVAC_OFF_ON_button 3;
BA_ "GenSigSendType" SG_ 2566851609 HVAC_Fan_Adj_button 0;
BA_ "GenSigInactiveValue" SG_ 2566851609 HVAC_Fan_Adj_button 0;
BA_ "GenSigStartValue" SG_ 2566851609 HVAC_Fan_Adj_button 15;
BA_ "GenSigSendType" SG_ 2566851609 HVAC_AC_OUT 0;
BA_ "GenSigInactiveValue" SG_ 2566851609 HVAC_AC_OUT 0;
BA_ "GenSigStartValue" SG_ 2566851609 HVAC_AC_OUT 3;
BA_ "GenSigSendType" SG_ 2566851609 HVAC_AC_Req 0;
BA_ "GenSigInactiveValue" SG_ 2566851609 HVAC_AC_Req 0;
BA_ "GenSigStartValue" SG_ 2566851609 HVAC_AC_Req 3;
BA_ "GenSigSendType" SG_ 2566851609 HVAC_Defrost_Sts 0;
BA_ "GenSigInactiveValue" SG_ 2566851609 HVAC_Defrost_Sts 0;
BA_ "GenSigStartValue" SG_ 2566851609 HVAC_Defrost_Sts 3;
BA_ "GenSigSendType" SG_ 2566851609 HVAC_AC_Wrok_Mode 0;
BA_ "GenSigInactiveValue" SG_ 2566851609 HVAC_AC_Wrok_Mode 0;
BA_ "GenSigStartValue" SG_ 2566851609 HVAC_AC_Wrok_Mode 3;
BA_ "GenSigSendType" SG_ 2566851609 HVAC_Negative_ion_state 0;
BA_ "GenSigInactiveValue" SG_ 2566851609 HVAC_Negative_ion_state 0;
BA_ "GenSigStartValue" SG_ 2566851609 HVAC_Negative_ion_state 3;
BA_ "GenSigSendType" SG_ 2566851609 HVAC_Left_Temp_adj_button 0;
BA_ "GenSigInactiveValue" SG_ 2566851609 HVAC_Left_Temp_adj_button 0;
BA_ "GenSigStartValue" SG_ 2566851609 HVAC_Left_Temp_adj_button 255;
BA_ "GenSigSendType" SG_ 2566851609 HVAC_DUAL_Setting 0;
BA_ "GenSigInactiveValue" SG_ 2566851609 HVAC_DUAL_Setting 0;
BA_ "GenSigStartValue" SG_ 2566851609 HVAC_DUAL_Setting 3;
BA_ "GenSigSendType" SG_ 2566851609 HVAC_Circulation_button 0;
BA_ "GenSigInactiveValue" SG_ 2566851609 HVAC_Circulation_button 0;
BA_ "GenSigStartValue" SG_ 2566851609 HVAC_Circulation_button 7;
BA_ "GenSigSendType" SG_ 2566851609 HVAC_Parking_Heating 0;
BA_ "GenSigInactiveValue" SG_ 2566851609 HVAC_Parking_Heating 0;
BA_ "GenSigStartValue" SG_ 2566851609 HVAC_Parking_Heating 3;
BA_ "GenSigSendType" SG_ 2566851609 HVAC_Right_Temp_adj_button 0;
BA_ "GenSigInactiveValue" SG_ 2566851609 HVAC_Right_Temp_adj_button 0;
BA_ "GenSigStartValue" SG_ 2566851609 HVAC_Right_Temp_adj_button 255;
BA_ "GenSigSendType" SG_ 2566851609 HVAC_Battery_Volt_sts 0;
BA_ "GenSigInactiveValue" SG_ 2566851609 HVAC_Battery_Volt_sts 0;
BA_ "GenSigStartValue" SG_ 2566851609 HVAC_Battery_Volt_sts 3;
BA_ "GenSigSendType" SG_ 2566851609 HVAC_Humidity 0;
BA_ "GenSigInactiveValue" SG_ 2566851609 HVAC_Humidity 0;
BA_ "GenSigStartValue" SG_ 2566851609 HVAC_Humidity 255;
BA_ "GenSigSendType" SG_ 2583632680 IDCU_mode_key 0;
BA_ "GenSigInactiveValue" SG_ 2583632680 IDCU_mode_key 0;
BA_ "GenSigStartValue" SG_ 2583632680 IDCU_mode_key 7;
BA_ "GenSigSendType" SG_ 2583632680 IDCU_auto_key 0;
BA_ "GenSigInactiveValue" SG_ 2583632680 IDCU_auto_key 0;
BA_ "GenSigStartValue" SG_ 2583632680 IDCU_auto_key 3;
BA_ "GenSigSendType" SG_ 2583632680 ICDU_OFF_ON 0;
BA_ "GenSigInactiveValue" SG_ 2583632680 ICDU_OFF_ON 0;
BA_ "GenSigStartValue" SG_ 2583632680 ICDU_OFF_ON 3;
BA_ "GenSigSendType" SG_ 2583632680 IDCU_FAN_Adj 0;
BA_ "GenSigInactiveValue" SG_ 2583632680 IDCU_FAN_Adj 0;
BA_ "GenSigStartValue" SG_ 2583632680 IDCU_FAN_Adj 15;
BA_ "GenSigSendType" SG_ 2583632680 IDCU_AC_Req 0;
BA_ "GenSigInactiveValue" SG_ 2583632680 IDCU_AC_Req 0;
BA_ "GenSigStartValue" SG_ 2583632680 IDCU_AC_Req 3;
BA_ "GenSigSendType" SG_ 2583632680 IDCU_Lefg_Adj_Key 0;
BA_ "GenSigInactiveValue" SG_ 2583632680 IDCU_Lefg_Adj_Key 0;
BA_ "GenSigStartValue" SG_ 2583632680 IDCU_Lefg_Adj_Key 255;
BA_ "GenSigSendType" SG_ 2583632680 IDCU_Circulation_Adj_Key 0;
BA_ "GenSigInactiveValue" SG_ 2583632680 IDCU_Circulation_Adj_Key 0;
BA_ "GenSigStartValue" SG_ 2583632680 IDCU_Circulation_Adj_Key 3;
BA_ "GenSigSendType" SG_ 2583632680 IDCU_Rgt_Adj_Key 0;
BA_ "GenSigInactiveValue" SG_ 2583632680 IDCU_Rgt_Adj_Key 0;
BA_ "GenSigStartValue" SG_ 2583632680 IDCU_Rgt_Adj_Key 255;
BA_ "GenSigSendType" SG_ 2583632680 IDCU_DUAL_Setting 0;
BA_ "GenSigInactiveValue" SG_ 2583632680 IDCU_DUAL_Setting 0;
BA_ "GenSigStartValue" SG_ 2583632680 IDCU_DUAL_Setting 3;
BA_ "GenSigSendType" SG_ 2583632680 IDCU_key_defrost 0;
BA_ "GenSigInactiveValue" SG_ 2583632680 IDCU_key_defrost 0;
BA_ "GenSigStartValue" SG_ 2583632680 IDCU_key_defrost 3;
BA_ "GenSigSendType" SG_ 2583632680 IDCU_key_dehum 0;
BA_ "GenSigInactiveValue" SG_ 2583632680 IDCU_key_dehum 0;
BA_ "GenSigStartValue" SG_ 2583632680 IDCU_key_dehum 3;
BA_ "GenSigSendType" SG_ 2583632680 IDCU_Init 0;
BA_ "GenSigInactiveValue" SG_ 2583632680 IDCU_Init 0;
BA_ "GenSigStartValue" SG_ 2583632680 IDCU_Init 3;
BA_ "GenSigSendType" SG_ 2583632680 IDCU_PARKING_Timeing 0;
BA_ "GenSigInactiveValue" SG_ 2583632680 IDCU_PARKING_Timeing 0;
BA_ "GenSigStartValue" SG_ 2583632680 IDCU_PARKING_Timeing 127;
BA_ "GenSigSendType" SG_ 2566845719 AMB 0;
BA_ "GenSigInactiveValue" SG_ 2566845719 AMB 0;
BA_ "GenSigStartValue" SG_ 2566845719 AMB 0;
BA_ "GenSigSendType" SG_ 2364539904 Engine_Speed 0;
BA_ "GenSigInactiveValue" SG_ 2364539904 Engine_Speed 0;
BA_ "GenSigStartValue" SG_ 2364539904 Engine_Speed 0;
BA_ "GenSigSendType" SG_ 2566907929 AC_DUAL_configuration 0;
BA_ "GenSigInactiveValue" SG_ 2566907929 AC_DUAL_configuration 0;
BA_ "GenSigStartValue" SG_ 2566907929 AC_DUAL_configuration 7;
BA_ "GenSigSendType" SG_ 2566907929 AC_ION_configuration 0;
BA_ "GenSigInactiveValue" SG_ 2566907929 AC_ION_configuration 0;
BA_ "GenSigStartValue" SG_ 2566907929 AC_ION_configuration 0;
BA_ "GenSigSendType" SG_ 2566907929 AC_PM2_5_configuration 0;
BA_ "GenSigInactiveValue" SG_ 2566907929 AC_PM2_5_configuration 0;
BA_ "GenSigStartValue" SG_ 2566907929 AC_PM2_5_configuration 0;
BA_ "GenSigSendType" SG_ 2566907929 EVAP_Temp 0;
BA_ "GenSigInactiveValue" SG_ 2566907929 EVAP_Temp 0;
BA_ "GenSigStartValue" SG_ 2566907929 EVAP_Temp 0;
BA_ "GenSigSendType" SG_ 2566907929 Incar_Temp 0;
BA_ "GenSigInactiveValue" SG_ 2566907929 Incar_Temp 0;
BA_ "GenSigStartValue" SG_ 2566907929 Incar_Temp 0;
BA_ "GenSigSendType" SG_ 2566851865 SW_VERS 0;
BA_ "GenSigInactiveValue" SG_ 2566851865 SW_VERS 0;
BA_ "GenSigStartValue" SG_ 2566851865 SW_VERS 0;
BA_ "GenSigSendType" SG_ 2566851865 HW_VERS 0;
BA_ "GenSigInactiveValue" SG_ 2566851865 HW_VERS 0;
BA_ "GenSigStartValue" SG_ 2566851865 HW_VERS 0;
BA_ "GenSigSendType" SG_ 2566851865 SUPPLIER_CODE 0;
BA_ "GenSigInactiveValue" SG_ 2566851865 SUPPLIER_CODE 0;
BA_ "GenSigStartValue" SG_ 2566851865 SUPPLIER_CODE 0;
BA_ "GenSigSendType" SG_ 2566907417 HVAC_timing_countdown 0;
BA_ "GenSigInactiveValue" SG_ 2566907417 HVAC_timing_countdown 0;
BA_ "GenSigStartValue" SG_ 2566907417 HVAC_timing_countdown 7;
BA_ "GenSigSendType" SG_ 2566907417 HVAC_M_pressure_switch 0;
BA_ "GenSigInactiveValue" SG_ 2566907417 HVAC_M_pressure_switch 0;
BA_ "GenSigStartValue" SG_ 2566907417 HVAC_M_pressure_switch 0;
BA_ "GenSigSendType" SG_ 2566907417 HVAC_initialization 0;
BA_ "GenSigInactiveValue" SG_ 2566907417 HVAC_initialization 0;
BA_ "GenSigStartValue" SG_ 2566907417 HVAC_initialization 0;
BA_ "GenSigSendType" SG_ 2566907417 HVAC_COMP_ComprSpd 0;
BA_ "GenSigInactiveValue" SG_ 2566907417 HVAC_COMP_ComprSpd 0;
BA_ "GenSigStartValue" SG_ 2566907417 HVAC_COMP_ComprSpd 0;
BA_ "GenSigSendType" SG_ 2566907417 HVAC_COMP_ComprSt 0;
BA_ "GenSigInactiveValue" SG_ 2566907417 HVAC_COMP_ComprSt 0;
BA_ "GenSigStartValue" SG_ 2566907417 HVAC_COMP_ComprSt 0;
BA_ "GenSigSendType" SG_ 2566866351 CO 0;
BA_ "GenSigInactiveValue" SG_ 2566866351 CO 0;
BA_ "GenSigStartValue" SG_ 2566866351 CO 0;
BA_ "GenSigSendType" SG_ 2566874003 ACSwt 0;
BA_ "GenSigInactiveValue" SG_ 2566874003 ACSwt 0;
BA_ "GenSigStartValue" SG_ 2566874003 ACSwt 3;
BA_ "GenSigSendType" SG_ 2566874003 HeaterMechSet 0;
BA_ "GenSigInactiveValue" SG_ 2566874003 HeaterMechSet 0;
BA_ "GenSigStartValue" SG_ 2566874003 HeaterMechSet 15;
BA_ "GenSigSendType" SG_ 2566874003 HeaterSwt 0;
BA_ "GenSigInactiveValue" SG_ 2566874003 HeaterSwt 0;
BA_ "GenSigStartValue" SG_ 2566874003 HeaterSwt 3;
BA_ "GenSigSendType" SG_ 2566874003 TempSet 0;
BA_ "GenSigInactiveValue" SG_ 2566874003 TempSet 0;
BA_ "GenSigStartValue" SG_ 2566874003 TempSet 255;
BA_ "GenSigSendType" SG_ 2566874003 TimeSet 0;
BA_ "GenSigInactiveValue" SG_ 2566874003 TimeSet 0;
BA_ "GenSigStartValue" SG_ 2566874003 TimeSet 255;
BA_ "GenSigSendType" SG_ 2565812505 HVACS_Acc_ReqSt 0;
BA_ "GenSigInactiveValue" SG_ 2565812505 HVACS_Acc_ReqSt 0;
BA_ "GenSigStartValue" SG_ 2565812505 HVACS_Acc_ReqSt 0;
BA_ "GenSigSendType" SG_ 2565812505 HVACS_Compr_CtrlSt 0;
BA_ "GenSigInactiveValue" SG_ 2565812505 HVACS_Compr_CtrlSt 0;
BA_ "GenSigStartValue" SG_ 2565812505 HVACS_Compr_CtrlSt 0;
BA_ "GenSigSendType" SG_ 2565812505 HVACS_ComprSpd 0;
BA_ "GenSigInactiveValue" SG_ 2565812505 HVACS_ComprSpd 0;
BA_ "GenSigStartValue" SG_ 2565812505 HVACS_ComprSpd 0;
BA_ "GenSigSendType" SG_ 2565812505 HVACS_CondFanCtrlSt 0;
BA_ "GenSigInactiveValue" SG_ 2565812505 HVACS_CondFanCtrlSt 0;
BA_ "GenSigStartValue" SG_ 2565812505 HVACS_CondFanCtrlSt 0;
BA_ "GenSigSendType" SG_ 2565812505 HVACS_Press_lSt 0;
BA_ "GenSigInactiveValue" SG_ 2565812505 HVACS_Press_lSt 0;
BA_ "GenSigStartValue" SG_ 2565812505 HVACS_Press_lSt 0;
BA_ "GenSigSendType" SG_ 2565812696 COMP_ComprSpd 0;
BA_ "GenSigInactiveValue" SG_ 2565812696 COMP_ComprSpd 0;
BA_ "GenSigStartValue" SG_ 2565812696 COMP_ComprSpd 0;
BA_ "GenSigSendType" SG_ 2565812696 COMP_ComprSt 0;
BA_ "GenSigInactiveValue" SG_ 2565812696 COMP_ComprSt 0;
BA_ "GenSigStartValue" SG_ 2565812696 COMP_ComprSt 0;
BA_ "GenSigSendType" SG_ 2565812696 COMP_CompErrCode 0;
BA_ "GenSigInactiveValue" SG_ 2565812696 COMP_CompErrCode 0;
BA_ "GenSigStartValue" SG_ 2565812696 COMP_CompErrCode 0;
BA_ "GenSigSendType" SG_ 2565812696 COMP_CompErrCode1 0;
BA_ "GenSigInactiveValue" SG_ 2565812696 COMP_CompErrCode1 0;
BA_ "GenSigStartValue" SG_ 2565812696 COMP_CompErrCode1 255;
BA_ "GenSigSendType" SG_ 2565812696 COMP_CompRunCurr 0;
BA_ "GenSigInactiveValue" SG_ 2565812696 COMP_CompRunCurr 0;
BA_ "GenSigStartValue" SG_ 2565812696 COMP_CompRunCurr 255;
BA_ "GenSigSendType" SG_ 2565812696 COMP_CompDCVol 0;
BA_ "GenSigInactiveValue" SG_ 2565812696 COMP_CompDCVol 0;
BA_ "GenSigStartValue" SG_ 2565812696 COMP_CompDCVol 255;
BA_ "GenSigSendType" SG_ 2566892357 Sts 0;
BA_ "GenSigInactiveValue" SG_ 2566892357 Sts 0;
BA_ "GenSigStartValue" SG_ 2566892357 Sts 0;
BA_ "GenSigSendType" SG_ 2583646233 key_Left_Set_Add 0;
BA_ "GenSigInactiveValue" SG_ 2583646233 key_Left_Set_Add 0;
BA_ "GenSigStartValue" SG_ 2583646233 key_Left_Set_Add 0;
BA_ "GenSigSendType" SG_ 2583646233 key_Left_Set_Subb 0;
BA_ "GenSigInactiveValue" SG_ 2583646233 key_Left_Set_Subb 0;
BA_ "GenSigStartValue" SG_ 2583646233 key_Left_Set_Subb 0;
BA_ "GenSigSendType" SG_ 2583646233 key_Blower_Set_Add 0;
BA_ "GenSigInactiveValue" SG_ 2583646233 key_Blower_Set_Add 0;
BA_ "GenSigStartValue" SG_ 2583646233 key_Blower_Set_Add 0;
BA_ "GenSigSendType" SG_ 2583646233 key_Blower_Set_Subb 0;
BA_ "GenSigInactiveValue" SG_ 2583646233 key_Blower_Set_Subb 0;
BA_ "GenSigStartValue" SG_ 2583646233 key_Blower_Set_Subb 0;
BA_ "GenSigSendType" SG_ 2583646233 key_CyclButton 0;
BA_ "GenSigInactiveValue" SG_ 2583646233 key_CyclButton 0;
BA_ "GenSigStartValue" SG_ 2583646233 key_CyclButton 0;
BA_ "GenSigSendType" SG_ 2583646233 key_OFFButton 0;
BA_ "GenSigInactiveValue" SG_ 2583646233 key_OFFButton 0;
BA_ "GenSigStartValue" SG_ 2583646233 key_OFFButton 0;
BA_ "GenSigSendType" SG_ 2583646233 key_ACButton 0;
BA_ "GenSigInactiveValue" SG_ 2583646233 key_ACButton 0;
BA_ "GenSigStartValue" SG_ 2583646233 key_ACButton 0;
BA_ "GenSigSendType" SG_ 2583646233 key_AUTOButton 0;
BA_ "GenSigInactiveValue" SG_ 2583646233 key_AUTOButton 0;
BA_ "GenSigStartValue" SG_ 2583646233 key_AUTOButton 0;
BA_ "GenSigSendType" SG_ 2583646233 key_ModeButton 0;
BA_ "GenSigInactiveValue" SG_ 2583646233 key_ModeButton 0;
BA_ "GenSigStartValue" SG_ 2583646233 key_ModeButton 0;
BA_ "GenSigSendType" SG_ 2583646233 key_DefButton 0;
BA_ "GenSigInactiveValue" SG_ 2583646233 key_DefButton 0;
BA_ "GenSigStartValue" SG_ 2583646233 key_DefButton 0;
BA_ "GenSigSendType" SG_ 2566912281 HVACS_Acc_ReqSt 0;
BA_ "GenSigInactiveValue" SG_ 2566912281 HVACS_Acc_ReqSt 0;
BA_ "GenSigStartValue" SG_ 2566912281 HVACS_Acc_ReqSt 0;
BA_ "GenSigSendType" SG_ 2566912281 HVACS_Press_lSt 0;
BA_ "GenSigInactiveValue" SG_ 2566912281 HVACS_Press_lSt 0;
BA_ "GenSigStartValue" SG_ 2566912281 HVACS_Press_lSt 0;
BA_ "GenSigSendType" SG_ 2566912281 Heating_cooling_mode 0;
BA_ "GenSigInactiveValue" SG_ 2566912281 Heating_cooling_mode 0;
BA_ "GenSigStartValue" SG_ 2566912281 Heating_cooling_mode 0;
BA_ "GenSigSendType" SG_ 2566912281 Heating_Tag_Temp 0;
BA_ "GenSigInactiveValue" SG_ 2566912281 Heating_Tag_Temp 0;
BA_ "GenSigStartValue" SG_ 2566912281 Heating_Tag_Temp 0;
BA_ "GenSigSendType" SG_ 2566912281 T_EVAP 0;
BA_ "GenSigInactiveValue" SG_ 2566912281 T_EVAP 0;
BA_ "GenSigStartValue" SG_ 2566912281 T_EVAP 0;
BA_ "GenSigSendType" SG_ 2566912281 EvpTemp 0;
BA_ "GenSigInactiveValue" SG_ 2566912281 EvpTemp 0;
BA_ "GenSigStartValue" SG_ 2566912281 EvpTemp 0;
BA_ "GenSigSendType" SG_ 2566912281 HVAC_Fan_Adj 0;
BA_ "GenSigInactiveValue" SG_ 2566912281 HVAC_Fan_Adj 0;
BA_ "GenSigStartValue" SG_ 2566912281 HVAC_Fan_Adj 0;
BA_ "GenSigSendType" SG_ 2565855257 AC_speed_of_compressor 0;
BA_ "GenSigInactiveValue" SG_ 2565855257 AC_speed_of_compressor 0;
BA_ "GenSigStartValue" SG_ 2565855257 AC_speed_of_compressor 0;
BA_ "GenSigSendType" SG_ 2565855257 AC_max_perm_compressor_power 0;
BA_ "GenSigInactiveValue" SG_ 2565855257 AC_max_perm_compressor_power 0;
BA_ "GenSigStartValue" SG_ 2565855257 AC_max_perm_compressor_power 0;
BA_ "GenSigSendType" SG_ 2565855257 AC_compressor_enable 0;
BA_ "GenSigInactiveValue" SG_ 2565855257 AC_compressor_enable 0;
BA_ "GenSigStartValue" SG_ 2565855257 AC_compressor_enable 0;
VAL_ 2566851609 HVAC_Cool_heat_mode_resp 0 " 制冷模式 " 1 "制热模式 " 3 "无效信号 " ;
VAL_ 2566851609 HVAC_Mode_sele_button 1 "吹面  " 2 "吹面吹脚   " 3 "吹脚 " 4 "吹脚除霜 " 5 "吹脚吹面除霜 " 7 "无效信号 " ;
VAL_ 2566851609 HVAC_Auto_button 0 "非AUTO " 1 "AUTO状态 " 3 "无效信号 " ;
VAL_ 2566851609 HVAC_OFF_ON_button 0 "OFF " 1 "ON " 3 "无效信号 " ;
VAL_ 2566851609 HVAC_Fan_Adj_button 0 "预留  " 1 "1档  " 2 "2档   " 3 "3档  " 4 "4档  " 5 "5档   " 6 "6档  " 7 "7档  " 8 "8档  " 15 "无效信号 " ;
VAL_ 2566851609 HVAC_AC_OUT 0 "压缩机关闭状态  " 1 " 压缩机开启状态 " 2 "驻车制冷（电动压缩机开启，冷凝器风扇开启） " 3 "无效信号  " ;
VAL_ 2566851609 HVAC_AC_Req 0 "关AC " 1 " 开AC " 3 "无效信号 " ;
VAL_ 2566851609 HVAC_Defrost_Sts 0 "非除霜 " 1 "除霜状态 " 3 "无效信号 " ;
VAL_ 2566851609 HVAC_AC_Wrok_Mode 0 "行车模式 " 1 "驻车模式 " 3 "无效信号 " ;
VAL_ 2566851609 HVAC_Negative_ion_state 0 "负离子关 " 1 "负离子开 " 3 "无效信号 " ;
VAL_ 2566851609 HVAC_Left_Temp_adj_button 255 "无效信号 " ;
VAL_ 2566851609 HVAC_DUAL_Setting 1 "双驱  " 0 " 单驱 " 3 " 无效信号 " ;
VAL_ 2566851609 HVAC_Circulation_button 0 "内循环 " 1 "外循环 " 7 "无效信号 " ;
VAL_ 2566851609 HVAC_Parking_Heating 0 "驻车暖风关闭 " 1 "驻车暖风开启 " 3 "无效信号 " ;
VAL_ 2566851609 HVAC_Right_Temp_adj_button 255 "无效信号 " ;
VAL_ 2566851609 HVAC_Battery_Volt_sts 0 "电压低，驻车空调不开启 " 1 "电压正常，驻车空调可开启 " 3 "无效信号 " ;
VAL_ 2566851609 HVAC_Humidity 255 "无效信号 " ;
VAL_ 2583632680 IDCU_mode_key 1 "吹面  " 2 "吹面吹脚 " 3 "吹脚   " 4 "吹脚除霜 " 5 "吹脚吹面除霜 " 7 "无效信号 " ;
VAL_ 2583632680 IDCU_auto_key 0 "非AUTO " 1 "AUTO状态 " 3 "无效信号 " ;
VAL_ 2583632680 ICDU_OFF_ON 0 "OFF " 1 "ON " 3 "无效信号 " ;
VAL_ 2583632680 IDCU_FAN_Adj 0 "预留   " 1 "1档   " 2 "2档   " 3 "3档    " 4 "4档   " 5 "5档   " 6 "6档   " 7 "7档  " 8 "8档 " 15 "无效信号 " ;
VAL_ 2583632680 IDCU_AC_Req 0 "无动作 " 1 "制冷（包含驻车制冷，行车制冷） " 3 "无效信号 " ;
VAL_ 2583632680 IDCU_Lefg_Adj_Key 255 "无效信号 " ;
VAL_ 2583632680 IDCU_Circulation_Adj_Key 0 "内循环 " 1 "外循环 " 3 "无效信号 " ;
VAL_ 2583632680 IDCU_Rgt_Adj_Key 255 "无效信号 " ;
VAL_ 2583632680 IDCU_DUAL_Setting 1 "双驱  " 0 " 单驱 " 3 " 无效信号 " ;
VAL_ 2583632680 IDCU_key_defrost 1 "开启  " 0 "关闭 " 3 "无效信号 " ;
VAL_ 2583632680 IDCU_key_dehum 1 "开启  " 0 "关闭 " 3 "无效信号 " ;
VAL_ 2583632680 IDCU_Init 1 "开启  " 0 "关闭 " 3 "无效信号 " ;
VAL_ 2566907929 AC_DUAL_configuration 0 "单温区 " 1 "双温区 " ;
VAL_ 2566907929 AC_ION_configuration 0 "无负离子 " 1 "有负离子 " ;
VAL_ 2566907929 AC_PM2_5_configuration 0 "无PM2.5 " 1 "有PM2.5 " ;
VAL_ 2566907417 HVAC_M_pressure_switch 0 "断开 " 1 "闭合 " ;
VAL_ 2566907417 HVAC_initialization 0 "无动作 " 1 "初始化 " ;
VAL_ 2566907417 HVAC_COMP_ComprSt 0 "停机 " 1 "运转 " ;
VAL_ 2566874003 ACSwt 0 "OFF " 1 "ON " 3 "无效信号 " ;
VAL_ 2566874003 HeaterMechSet 0 "预留  " 1 "1档  " 2 "2档   " 3 "3档  " 4 "4档  " 5 "5档   " 6 "6档  " 7 "7档  " 8 "8档  " 15 "无效信号 " ;
VAL_ 2566874003 HeaterSwt 0 "行车模式 " 1 "驻车白天模式 " 2 "驻车夜晚模式 " 3 "无效信号； " ;
VAL_ 2566874003 TempSet 255 "无效信号 " ;
VAL_ 2566874003 TimeSet 255 "无效信号 " ;
VAL_ 2565812505 HVACS_Acc_ReqSt 0 "关AC " 1 " 开AC " ;
VAL_ 2565812505 HVACS_Compr_CtrlSt 0 "关AC " 1 " 开AC " ;
VAL_ 2565812505 HVACS_CondFanCtrlSt 0 "关闭 " 1 "开启 " ;
VAL_ 2565812505 HVACS_Press_lSt 0 "闭合 " 1 "断开 " ;
VAL_ 2565812696 COMP_ComprSt 0 "停机 " 1 "运转 " 2 "无效 " 3 "故障 " ;
VAL_ 2565812696 COMP_CompErrCode 0 " No Error " 1 " Over Current " 8 "Over Voltage " 16 " UnderVoltage " 32 "Communication Error " ;
VAL_ 2565812696 COMP_CompErrCode1 0 " No Error " 1 "IPM Over Heat Error " 2 "Scroll Over Heat Error " 4 " Start Failure Error " 8 "Scroll Over Heat Warning " 16 " Over Power Warning " 32 "Over LoadAdaption Warning " 64 "IPM Over Heat Warning " 128 " Missing Speed " ;
VAL_ 2565812696 COMP_CompRunCurr 255 "无效信号 " ;
VAL_ 2565812696 COMP_CompDCVol 255 "无效信号 " ;
VAL_ 2566892357 Sts 0 "休眠状态 " 129 "启动准备状态 " 130 "点火状态 " 132 "稳定运转状态 " 136 "只送风状态 " 144 "准备休眠状态 " ;
VAL_ 2583646233 key_Left_Set_Add 0 "抬起 " 1 "按下 " 2 "预留 " ;
VAL_ 2583646233 key_Left_Set_Subb 0 "抬起 " 1 "按下 " 2 "预留 " ;
VAL_ 2583646233 key_Blower_Set_Add 0 "抬起 " 1 "按下 " 2 "预留 " ;
VAL_ 2583646233 key_Blower_Set_Subb 0 "抬起 " 1 "按下 " 2 "预留 " ;
VAL_ 2583646233 key_CyclButton 0 "抬起 " 1 "按下 " 2 "预留 " ;
VAL_ 2583646233 key_OFFButton 0 "抬起 " 1 "按下 " 2 "预留 " ;
VAL_ 2583646233 key_ACButton 0 "抬起 " 1 "按下 " 2 "预留 " ;
VAL_ 2583646233 key_AUTOButton 0 "抬起 " 1 "按下 " 2 "预留 " ;
VAL_ 2583646233 key_ModeButton 0 "抬起 " 1 "按下 " 2 "预留 " ;
VAL_ 2583646233 key_DefButton 0 "抬起 " 1 "按下 " 2 "预留 " ;
VAL_ 2566912281 HVACS_Acc_ReqSt 0 "关AC " 1 " 开AC " 3 " 无效 " ;
VAL_ 2566912281 HVACS_Press_lSt 0 "闭合 " 1 " 断开 " ;
VAL_ 2566912281 Heating_cooling_mode 0 "无需求 " 1 " 制冷模式 " 2 " 制热模式 " 3 "除湿 " ;
VAL_ 2565855257 AC_compressor_enable 0 "关压缩机 " 1 "开压缩机 " ;

